// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "NEC Aterm WF1200CR";
	compatible = "nec,wf1200cr", "qca,qca9561";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	leds {
		compatible = "gpio-leds";
		/* other LEDs are connected to ath10k (QCA9888) gpiochip */

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led_power_red: power_red {
			label = "red:power";
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		router {
			label = "rt";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "devdata";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				label = "devconf";
				reg = <0x050000 0x010000>;
				read-only;
			};

			partition@60000 {
				label = "misc";
				reg = <0x060000 0x010000>;
				read-only;
			};

			partition@70000 {
				compatible = "seama";
				label = "firmware";
				reg = <0x070000 0x780000>;
			};

			partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x03000101 0x00000101 0x00001919>;

	phy-handle = <&swphy0>;

	gmac-config {
		device = <&gmac>;

		switch-phy-swap = <1>;
		switch-phy-addr-swap = <0>;
	};
};

&eth1 {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinmux_swled_enable_pins>;
};

&gpio {
	switch_leds {
		gpio-hog;
		gpios = <14 GPIO_ACTIVE_HIGH>,	/* WAN */
			<19 GPIO_ACTIVE_HIGH>;	/* LAN */
		output-high;
		line-name = "led:wan-lan";
	};
};

&pinmux {
	pinmux_swled_enable_pins: swled_enable_pins {
		pinctrl-single,bits =
			<0xc 0x240000 0xff0000>,	/* WAN */
			<0x10 0x10000000 0xff000000>;	/* LAN */
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;
	};
};

&wmac {
	status = "okay";

	qca,no-eeprom;
};
