From 226383600be58dcf2e070e4ac8a371640024fe54 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Wed, 17 Jun 2020 12:50:38 +0200
Subject: [PATCH 6/9] mips: bmips: dts: add BCM6362 reset controller support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM6362 SoCs have a reset controller for certain components.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Acked-by: Florian Fainelli <f.fainelli@gmail.com>
Reviewed-by: Rob Herring <robh@kernel.org>
Signed-off-by: Thomas Bogendoerfer <tsbogend@alpha.franken.de>
---
 arch/mips/boot/dts/brcm/bcm6362.dtsi      |  6 ++++++
 include/dt-bindings/reset/bcm6362-reset.h | 22 ++++++++++++++++++++++
 2 files changed, 28 insertions(+)
 create mode 100644 include/dt-bindings/reset/bcm6362-reset.h

--- a/arch/mips/boot/dts/brcm/bcm6362.dtsi
+++ b/arch/mips/boot/dts/brcm/bcm6362.dtsi
@@ -70,6 +70,12 @@
 			mask = <0x1>;
 		};
 
+		periph_rst: reset-controller@10000010 {
+			compatible = "brcm,bcm6345-reset";
+			reg = <0x10000010 0x4>;
+			#reset-cells = <1>;
+		};
+
 		periph_intc: interrupt-controller@10000020 {
 			compatible = "brcm,bcm6345-l1-intc";
 			reg = <0x10000020 0x10>,
--- /dev/null
+++ b/include/dt-bindings/reset/bcm6362-reset.h
@@ -0,0 +1,22 @@
+/* SPDX-License-Identifier: GPL-2.0+ */
+
+#ifndef __DT_BINDINGS_RESET_BCM6362_H
+#define __DT_BINDINGS_RESET_BCM6362_H
+
+#define BCM6362_RST_SPI		0
+#define BCM6362_RST_IPSEC	1
+#define BCM6362_RST_EPHY	2
+#define BCM6362_RST_SAR		3
+#define BCM6362_RST_ENETSW	4
+#define BCM6362_RST_USBD	5
+#define BCM6362_RST_USBH	6
+#define BCM6362_RST_PCM		7
+#define BCM6362_RST_PCIE_CORE	8
+#define BCM6362_RST_PCIE	9
+#define BCM6362_RST_PCIE_EXT	10
+#define BCM6362_RST_WLAN_SHIM	11
+#define BCM6362_RST_DDR_PHY	12
+#define BCM6362_RST_FAP		13
+#define BCM6362_RST_WLAN_UBUS	14
+
+#endif /* __DT_BINDINGS_RESET_BCM6362_H */
