// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "ubnt,xw", "qca,ar9342";
	model = "Ubiquiti Networks XW board";

	aliases {
		led-boot = &led_link4;
		led-running = &led_link4;
		led-upgrade = &led_link4;
		led-failsafe = &led_link4;
		label-mac-device = &wmac;
	};

	leds {
		compatible = "gpio-leds";

		link1 {
			label = "red:link1";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		link2 {
			label = "orange:link2";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		link3 {
			label = "green:link3";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led_link4: link4 {
			label = "green:link4";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x050000 0x760000>;
			};

			partition@7b0000 {
				label = "cfg";
				reg = <0x7b0000 0x040000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&eth0 {
	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
