From 5d9e068402dcf7354cc8ee66c2152845306d2ccb Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Fri, 14 May 2021 22:59:51 +0200
Subject: [PATCH] net: dsa: qca8k: change simple print to dev variant

Change pr_err and pr_warn to dev variant.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/dsa/qca8k.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/dsa/qca8k.c
+++ b/drivers/net/dsa/qca8k.c
@@ -701,7 +701,7 @@ qca8k_setup(struct dsa_switch *ds)
 
 	/* Make sure that port 0 is the cpu port */
 	if (!dsa_is_cpu_port(ds, 0)) {
-		pr_err("port 0 is not the CPU port\n");
+		dev_err(priv->dev, "port 0 is not the CPU port");
 		return -EINVAL;
 	}
 
@@ -711,7 +711,7 @@ qca8k_setup(struct dsa_switch *ds)
 	priv->regmap = devm_regmap_init(ds->dev, NULL, priv,
 					&qca8k_regmap_config);
 	if (IS_ERR(priv->regmap))
-		pr_warn("regmap initialization failed");
+		dev_warn(priv->dev, "regmap initialization failed");
 
 	ret = qca8k_setup_mdio_bus(priv);
 	if (ret)
