
. /lib/functions.sh
. /lib/functions/uci-defaults.sh
. /lib/functions/system.sh

mediatek_setup_interfaces()
{
	local board="$1"

	case $board in
	mediatek,mt7629-rfb)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "6@eth0"
		;;
	esac
}

mediatek_setup_macs()
{
	local board="$1"

	case $board in
	esac
}

board_config_update
board=$(board_name)
mediatek_setup_interfaces $board
mediatek_setup_macs $board
board_config_flush

exit 0
