From 13bcdf07cb2ecff5d45d2c141df2539b15211448 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Tue, 30 Nov 2021 18:29:09 +0100
Subject: [PATCH] PCI: aardvark: Mask all interrupts when unbinding driver
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Ensure that no interrupt can be triggered after driver unbind.

Link: https://lore.kernel.org/r/20211130172913.9727-8-kabel@kernel.org
Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
Signed-off-by: Lorenzo Pieralisi <lorenzo.pieralisi@arm.com>
---
 drivers/pci/controller/pci-aardvark.c | 21 +++++++++++++++++++++
 1 file changed, 21 insertions(+)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -1704,6 +1704,27 @@ static int advk_pcie_remove(struct platf
 	val &= ~(PCI_COMMAND_IO | PCI_COMMAND_MEMORY | PCI_COMMAND_MASTER);
 	advk_writel(pcie, val, PCIE_CORE_CMD_STATUS_REG);
 
+	/* Disable MSI */
+	val = advk_readl(pcie, PCIE_CORE_CTRL2_REG);
+	val &= ~PCIE_CORE_CTRL2_MSI_ENABLE;
+	advk_writel(pcie, val, PCIE_CORE_CTRL2_REG);
+
+	/* Clear MSI address */
+	advk_writel(pcie, 0, PCIE_MSI_ADDR_LOW_REG);
+	advk_writel(pcie, 0, PCIE_MSI_ADDR_HIGH_REG);
+
+	/* Mask all interrupts */
+	advk_writel(pcie, PCIE_MSI_ALL_MASK, PCIE_MSI_MASK_REG);
+	advk_writel(pcie, PCIE_ISR0_ALL_MASK, PCIE_ISR0_MASK_REG);
+	advk_writel(pcie, PCIE_ISR1_ALL_MASK, PCIE_ISR1_MASK_REG);
+	advk_writel(pcie, PCIE_IRQ_ALL_MASK, HOST_CTRL_INT_MASK_REG);
+
+	/* Clear all interrupts */
+	advk_writel(pcie, PCIE_MSI_ALL_MASK, PCIE_MSI_STATUS_REG);
+	advk_writel(pcie, PCIE_ISR0_ALL_MASK, PCIE_ISR0_REG);
+	advk_writel(pcie, PCIE_ISR1_ALL_MASK, PCIE_ISR1_REG);
+	advk_writel(pcie, PCIE_IRQ_ALL_MASK, HOST_CTRL_INT_STATUS_REG);
+
 	/* Remove IRQ domains */
 	advk_pcie_remove_msi_irq_domain(pcie);
 	advk_pcie_remove_irq_domain(pcie);
