// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7628an_iptime.dtsi"

/ {
	compatible = "iptime,a604m", "mediatek,mt7628an-soc";
	model = "ipTIME A604M";

	aliases {
		led-boot = &led_cpu;
		led-failsafe = &led_cpu;
		led-running = &led_cpu;
		led-upgrade = &led_cpu;
	};

	leds {
		compatible = "gpio-leds";

		wlan5g {
			label = "blue:wlan5g";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led_cpu: cpu {
			label = "blue:cpu";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "blue:wlan2g";
			gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "uart1", "wdt";
		function = "gpio";
	};
};
