
. /lib/functions/leds.sh
. /lib/functions/uci-defaults.sh

board=$(board_name)

board_config_update

case $board in
belkin,f9k1109v1)
	ucidef_set_led_netdev "lan" "lan" "blue:wps" "eth0"
	;;
edimax,br-6475nd)
	ucidef_set_led_netdev "wifi_led" "wifi" "amber:wlan" "wlan0"
	;;
omnima,hpm)
	ucidef_set_led_netdev "eth" "ETH" "green:eth" "eth0"
	ucidef_set_led_netdev "wifi_led" "wifi" "green:wifi" "wlan0"
	;;
esac

board_config_flush

exit 0
