From dcb56d61d5a8acca0a357cc603397bc0272ce4cb Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Mon, 29 Mar 2021 10:04:09 +0200
Subject: [PATCH] ARM: dts: BCM5301X: Set Linksys EA9500 power LED
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Set Linux default trigger to default on, just like it's normally done
for power LEDs.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm47094-linksys-panamera.dts | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/boot/dts/bcm47094-linksys-panamera.dts
+++ b/arch/arm/boot/dts/bcm47094-linksys-panamera.dts
@@ -75,6 +75,7 @@
 		power {
 			label = "bcm53xx:white:power";
 			gpios = <&chipcommon 4 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-on";
 		};
 
 		wifi-disabled {
