
. /lib/functions/leds.sh
. /lib/functions/uci-defaults.sh

board=$(board_name)
boardname="${board##*,}"

board_config_update

case $board in
extreme-networks,ws-ap3825i)
	ucidef_set_led_netdev "lan1" "LAN1" "green:lan1" "eth1"
	ucidef_set_led_netdev "lan2" "LAN2" "green:lan2" "eth0"
	;;
esac

board_config_flush

exit 0
