// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "tplink,re200-v1", "ralink,mt7620a-soc";
	model = "TP-Link RE200 v1";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &ethernet;
	};

	chosen {
		bootargs = "console=ttyS0,57600n8";
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "re200-v1:green:power";
			gpios = <&gpio1 0 GPIO_ACTIVE_LOW>;
		};

		lan {
			label = "re200-v1:green:lan";
			gpios = <&gpio2 0 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "re200-v1:green:wlan";
			gpios = <&gpio1 3 GPIO_ACTIVE_LOW>;
		};

		qss {
			label = "re200-v1:green:qss";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
		};

		wlan2g_red {
			label = "re200-v1:red:wlan2g";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
		};

		wlan2g_green {
			label = "re200-v1:green:wlan2g";
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};
};


&state_default {
	gpio {
		ralink,group = "i2c", "uartf", "ephy", "wled", "rgmii1", "spi refclk";
		ralink,function = "gpio";
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x0 0x20000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x20000 0x7c0000>;
			};

			partition@7e0000 {
				label = "userconfig";
				reg = <0x7e0000 0x10000>;
				read-only;
			};

			radio: partition@7f0000 {
				label = "radio";
				reg = <0x7f0000 0x10000>;
				read-only;
			};
		};
	};
};

&gpio1 {
	status = "okay";
};

&gpio2 {
	status = "okay";
};

&gpio3 {
	status = "okay";
};

&ethernet {
	mtd-mac-address = <&uboot 0x1fc00>;
};

&wmac {
	ralink,mtd-eeprom = <&radio 0x0>;
	mtd-mac-address = <&uboot 0x1fc00>;
};

&pcie {
	status = "okay";
};

&pcie0 {
	mt76@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&radio 0x8000>;
		mtd-mac-address = <&uboot 0x1fc00>;
		mtd-mac-address-increment = <2>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};
