This patch squashes the following upstream commits:

5ca1b1c5cd98 pinctrl: mediatek: mt8183: Add pm_ops
5c0904488a20 pinctrl: mediatek: Add pm_ops to pinctrl-paris
1802d0beecaf treewide: Replace GPLv2 boilerplate/reference with SPDX - rule 174
ec8f24b7faaf treewide: Add SPDX license identifier - Makefile/Kconfig
264667112ef0 pinctrl: mediatek: Add MT8516 Pinctrl driver
5e73de3413c5 pinctrl: add drive for I2C related pins on MT8183
e65372124cd7 Merge tag 'v5.0-rc6' into devel
2d2d478576d7 pinctrl: mediatek: fix Kconfig build errors for moore core
6e737a4e921e pinctrl: mediatek: add EINT support to virtual GPIOs
b5af33df50e9 pinctrl: mediatek: improve Kconfig dependencies
9ede2a76f66e pinctrl: mediatek: Convert to using %pOFn instead of device_node.name
b44677375fee pinctrl: mediatek: add pinctrl support for MT7629 SoC
f969b7aac980 pinctrl: mediatek: Add initial pinctrl driver for MT6797 SoC
7c68024a82a2 pinctrl: mediatek: Fix dependencies for EINT_MTK
78bf386daf8a pinctrl: mediatek: clean up indentation issues, add missing tab
28e0603c4df4 pinctrl: mediatek: Make eint_m u16
71a9d395aa12 pinctrl: mediatek: select GPIOLIB
ad335bee6ced pinctrl: mediatek: mark dummy helpers as 'static inline'
7a52127e3cf1 pinctrl: mediatek: fix check on EINT_NA comparison
bb8d8466ca25 pinctrl: mediatek: add eint support to MT6765 pinctrl driver
477fecee7ca9 pinctrl: mediatek: add MT6765 pinctrl driver
ecfcfb498860 pinctrl: mediatek: add no eint function for pin define
7f2e29e133ea pinctrl: mediatek: fix static checker warning caused by EINT_NA
068cfb9a0fd9 pinctrl: mediatek: moore: fix return value check in mtk_moore_pinctrl_probe()
07c6b037c2ba pinctrl: mediatek: make symbol 'mtk_drive' static
184744e9a014 pinctrl: mediatek: paris: fix return value check in mtk_paris_pinctrl_probe()
22d7fe4984a2 pinctrl: mtk: Fix up GPIO includes
55818b90233b Merge branch 'ib-mtk' into devel
6561859b067f pinctrl: mediatek: add eint support to MT8183 pinctrl driver
89132dd8ffd2 pinctrl: mediatek: extend eint build to pinctrl-mtk-common-v2.c
29686f0151df pintcrl: mediatek: add pull tweaks for I2C related pins on MT8183
79348f6fb713 pinctrl: mediatek: extend advanced pull support in pinctrl-mtk-common-v2.c
750cd15d9081 pinctrl: mediatek: add MT8183 pinctrl driver
805250982bb5 pinctrl: mediatek: add pinctrl-paris that implements the vendor dt-bindings
b7d7f9eeca55 pinctrl: mediatek: extend struct mtk_pin_desc which per-pin driver depends on
9d9b171c6897 pinctrl: mediatek: adjust error code and message when some register not supported is found
2bc47dfe4f8b pinctrl: mediatek: add multiple register bases support to pinctrl-mtk-common-v2.c
ea051eb38413 pinctrl: mediatek: use pin descriptor all in pinctrl-mtk-common-v2.c
e7507f57a93a pinctrl: mediatek: add MT7623 pinctrl driver based on generic pinctrl binding
9afc305bfad7 pinctrl: mediatek: add pullen, pullsel register support to pinctrl-mtk-common-v2.c
182c842fd5e6 pinctrl: mediatek: add ies register support to pinctrl-mtk-common-v2.c
0d7ca772148f pinctrl: mediatek: add advanced pull related support to pinctrl-mtk-common-v2.c
85430152ba46 pinctrl: mediatek: add pull related support to pinctrl-mtk-common-v2.c
3ad38a14e13c pinctrl: mediatek: add drv register support to pinctrl-mtk-common-v2.c
c28321979ba8 pinctrl: mediatek: add driving strength related support to pinctrl-mtk-common-v2.c
1dc5e5369159 pinctrl: mediatek: extend struct mtk_pin_soc to pinctrl-mtk-common-v2.c
fb5fa8dc151b pinctrl: mediatek: extend struct mtk_pin_desc to pinctrl-mtk-common-v2.c
b906faf7b61d pinctrl: mediatek: extend struct mtk_pin_field_calc to pinctrl-mtk-common-v2.c
e78d57b2f87c pinctrl: mediatek: add pinctrl-moore that implements the generic pinctrl dt-bindings
a1a503a8c332 pinctrl: mediatek: add pinctrl-mtk-common-v2 for all MediaTek pinctrls
1c5fb66afa2a pinctrl: Include <linux/gpio/driver.h> nothing else
94f4e54cecaf pinctrl: Convert to using %pOFn instead of device_node.name

--- a/drivers/pinctrl/mediatek/Kconfig
+++ b/drivers/pinctrl/mediatek/Kconfig
@@ -3,7 +3,8 @@ menu "MediaTek pinctrl drivers"
 
 config EINT_MTK
 	bool "MediaTek External Interrupt Support"
-	depends on PINCTRL_MTK || PINCTRL_MT7622 || COMPILE_TEST
+	depends on PINCTRL_MTK || PINCTRL_MTK_MOORE || PINCTRL_MTK_PARIS || COMPILE_TEST
+	select GPIOLIB
 	select IRQ_DOMAIN
 
 config PINCTRL_MTK
@@ -15,6 +16,24 @@ config PINCTRL_MTK
 	select EINT_MTK
 	select OF_GPIO
 
+config PINCTRL_MTK_MOORE
+	bool
+	depends on OF
+	select GENERIC_PINCONF
+	select GENERIC_PINCTRL_GROUPS
+	select GENERIC_PINMUX_FUNCTIONS
+	select GPIOLIB
+	select OF_GPIO
+
+config PINCTRL_MTK_PARIS
+	bool
+	depends on OF
+	select PINMUX
+	select GENERIC_PINCONF
+	select GPIOLIB
+	select EINT_MTK
+	select OF_GPIO
+
 # For ARMv7 SoCs
 config PINCTRL_MT2701
 	bool "Mediatek MT2701 pin control"
@@ -23,6 +42,20 @@ config PINCTRL_MT2701
 	default MACH_MT2701
 	select PINCTRL_MTK
 
+config PINCTRL_MT7623
+	bool "Mediatek MT7623 pin control with generic binding"
+	depends on MACH_MT7623 || COMPILE_TEST
+	depends on OF
+	default MACH_MT7623
+	select PINCTRL_MTK_MOORE
+
+config PINCTRL_MT7629
+	bool "Mediatek MT7629 pin control"
+	depends on MACH_MT7629 || COMPILE_TEST
+	depends on OF
+	default MACH_MT7629
+	select PINCTRL_MTK_MOORE
+
 config PINCTRL_MT8135
 	bool "Mediatek MT8135 pin control"
 	depends on MACH_MT8135 || COMPILE_TEST
@@ -45,21 +78,46 @@ config PINCTRL_MT2712
 	default ARM64 && ARCH_MEDIATEK
 	select PINCTRL_MTK
 
+config PINCTRL_MT6765
+	bool "Mediatek MT6765 pin control"
+	depends on OF
+	depends on ARM64 || COMPILE_TEST
+	default ARM64 && ARCH_MEDIATEK
+	select PINCTRL_MTK_PARIS
+
+config PINCTRL_MT6797
+	bool "Mediatek MT6797 pin control"
+	depends on OF
+	depends on ARM64 || COMPILE_TEST
+	default ARM64 && ARCH_MEDIATEK
+	select PINCTRL_MTK_PARIS
+
 config PINCTRL_MT7622
 	bool "MediaTek MT7622 pin control"
 	depends on OF
 	depends on ARM64 || COMPILE_TEST
-	select GENERIC_PINCONF
-	select GENERIC_PINCTRL_GROUPS
-	select GENERIC_PINMUX_FUNCTIONS
-	select GPIOLIB
-	select OF_GPIO
+	default ARM64 && ARCH_MEDIATEK
+	select PINCTRL_MTK_MOORE
 
 config PINCTRL_MT8173
 	bool "Mediatek MT8173 pin control"
 	depends on OF
 	depends on ARM64 || COMPILE_TEST
 	default ARM64 && ARCH_MEDIATEK
+	select PINCTRL_MTK
+
+config PINCTRL_MT8183
+	bool "Mediatek MT8183 pin control"
+	depends on OF
+	depends on ARM64 || COMPILE_TEST
+	default ARM64 && ARCH_MEDIATEK
+	select PINCTRL_MTK_PARIS
+
+config PINCTRL_MT8516
+	bool "Mediatek MT8516 pin control"
+	depends on OF
+	depends on ARM64 || COMPILE_TEST
+	default ARM64 && ARCH_MEDIATEK
 	select PINCTRL_MTK
 
 # For PMIC
--- a/drivers/pinctrl/mediatek/Makefile
+++ b/drivers/pinctrl/mediatek/Makefile
@@ -2,12 +2,20 @@
 # Core
 obj-$(CONFIG_EINT_MTK)		+= mtk-eint.o
 obj-$(CONFIG_PINCTRL_MTK)	+= pinctrl-mtk-common.o
+obj-$(CONFIG_PINCTRL_MTK_MOORE) += pinctrl-moore.o pinctrl-mtk-common-v2.o
+obj-$(CONFIG_PINCTRL_MTK_PARIS) += pinctrl-paris.o pinctrl-mtk-common-v2.o
 
 # SoC Drivers
 obj-$(CONFIG_PINCTRL_MT2701)	+= pinctrl-mt2701.o
 obj-$(CONFIG_PINCTRL_MT2712)	+= pinctrl-mt2712.o
 obj-$(CONFIG_PINCTRL_MT8135)	+= pinctrl-mt8135.o
 obj-$(CONFIG_PINCTRL_MT8127)	+= pinctrl-mt8127.o
+obj-$(CONFIG_PINCTRL_MT6765)	+= pinctrl-mt6765.o
+obj-$(CONFIG_PINCTRL_MT6797)	+= pinctrl-mt6797.o
 obj-$(CONFIG_PINCTRL_MT7622)	+= pinctrl-mt7622.o
+obj-$(CONFIG_PINCTRL_MT7623)	+= pinctrl-mt7623.o
+obj-$(CONFIG_PINCTRL_MT7629)	+= pinctrl-mt7629.o
 obj-$(CONFIG_PINCTRL_MT8173)	+= pinctrl-mt8173.o
+obj-$(CONFIG_PINCTRL_MT8183)	+= pinctrl-mt8183.o
+obj-$(CONFIG_PINCTRL_MT8516)	+= pinctrl-mt8516.o
 obj-$(CONFIG_PINCTRL_MT6397)	+= pinctrl-mt6397.o
--- a/drivers/pinctrl/mediatek/mtk-eint.c
+++ b/drivers/pinctrl/mediatek/mtk-eint.c
@@ -11,7 +11,7 @@
 
 #include <linux/delay.h>
 #include <linux/err.h>
-#include <linux/gpio.h>
+#include <linux/gpio/driver.h>
 #include <linux/io.h>
 #include <linux/irqchip/chained_irq.h>
 #include <linux/irqdomain.h>
--- a/drivers/pinctrl/mediatek/mtk-eint.h
+++ b/drivers/pinctrl/mediatek/mtk-eint.h
@@ -92,13 +92,13 @@ static inline int mtk_eint_do_resume(str
 	return -EOPNOTSUPP;
 }
 
-int mtk_eint_set_debounce(struct mtk_eint *eint, unsigned long eint_n,
+static inline int mtk_eint_set_debounce(struct mtk_eint *eint, unsigned long eint_n,
 			  unsigned int debounce)
 {
 	return -EOPNOTSUPP;
 }
 
-int mtk_eint_find_irq(struct mtk_eint *eint, unsigned long eint_n)
+static inline int mtk_eint_find_irq(struct mtk_eint *eint, unsigned long eint_n)
 {
 	return -EOPNOTSUPP;
 }
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-moore.c
@@ -0,0 +1,690 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * MediaTek Pinctrl Moore Driver, which implement the generic dt-binding
+ * pinctrl-bindings.txt for MediaTek SoC.
+ *
+ * Copyright (C) 2017-2018 MediaTek Inc.
+ * Author: Sean Wang <sean.wang@mediatek.com>
+ *
+ */
+
+#include <linux/gpio/driver.h>
+#include "pinctrl-moore.h"
+
+#define PINCTRL_PINCTRL_DEV		KBUILD_MODNAME
+
+/* Custom pinconf parameters */
+#define MTK_PIN_CONFIG_TDSEL	(PIN_CONFIG_END + 1)
+#define MTK_PIN_CONFIG_RDSEL	(PIN_CONFIG_END + 2)
+#define MTK_PIN_CONFIG_PU_ADV	(PIN_CONFIG_END + 3)
+#define MTK_PIN_CONFIG_PD_ADV	(PIN_CONFIG_END + 4)
+
+static const struct pinconf_generic_params mtk_custom_bindings[] = {
+	{"mediatek,tdsel",	MTK_PIN_CONFIG_TDSEL,		0},
+	{"mediatek,rdsel",	MTK_PIN_CONFIG_RDSEL,		0},
+	{"mediatek,pull-up-adv", MTK_PIN_CONFIG_PU_ADV,		1},
+	{"mediatek,pull-down-adv", MTK_PIN_CONFIG_PD_ADV,	1},
+};
+
+#ifdef CONFIG_DEBUG_FS
+static const struct pin_config_item mtk_conf_items[] = {
+	PCONFDUMP(MTK_PIN_CONFIG_TDSEL, "tdsel", NULL, true),
+	PCONFDUMP(MTK_PIN_CONFIG_RDSEL, "rdsel", NULL, true),
+	PCONFDUMP(MTK_PIN_CONFIG_PU_ADV, "pu-adv", NULL, true),
+	PCONFDUMP(MTK_PIN_CONFIG_PD_ADV, "pd-adv", NULL, true),
+};
+#endif
+
+static int mtk_pinmux_set_mux(struct pinctrl_dev *pctldev,
+			      unsigned int selector, unsigned int group)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	struct function_desc *func;
+	struct group_desc *grp;
+	int i;
+
+	func = pinmux_generic_get_function(pctldev, selector);
+	if (!func)
+		return -EINVAL;
+
+	grp = pinctrl_generic_get_group(pctldev, group);
+	if (!grp)
+		return -EINVAL;
+
+	dev_dbg(pctldev->dev, "enable function %s group %s\n",
+		func->name, grp->name);
+
+	for (i = 0; i < grp->num_pins; i++) {
+		const struct mtk_pin_desc *desc;
+		int *pin_modes = grp->data;
+		int pin = grp->pins[i];
+
+		desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+		mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_MODE,
+				 pin_modes[i]);
+	}
+
+	return 0;
+}
+
+static int mtk_pinmux_gpio_request_enable(struct pinctrl_dev *pctldev,
+					  struct pinctrl_gpio_range *range,
+					  unsigned int pin)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+	return mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_MODE,
+				hw->soc->gpio_m);
+}
+
+static int mtk_pinmux_gpio_set_direction(struct pinctrl_dev *pctldev,
+					 struct pinctrl_gpio_range *range,
+					 unsigned int pin, bool input)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+	/* hardware would take 0 as input direction */
+	return mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR, !input);
+}
+
+static int mtk_pinconf_get(struct pinctrl_dev *pctldev,
+			   unsigned int pin, unsigned long *config)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	u32 param = pinconf_to_config_param(*config);
+	int val, val2, err, reg, ret = 1;
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+	switch (param) {
+	case PIN_CONFIG_BIAS_DISABLE:
+		if (hw->soc->bias_disable_get) {
+			err = hw->soc->bias_disable_get(hw, desc, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_BIAS_PULL_UP:
+		if (hw->soc->bias_get) {
+			err = hw->soc->bias_get(hw, desc, 1, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_BIAS_PULL_DOWN:
+		if (hw->soc->bias_get) {
+			err = hw->soc->bias_get(hw, desc, 0, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_SLEW_RATE:
+		err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_SR, &val);
+		if (err)
+			return err;
+
+		if (!val)
+			return -EINVAL;
+
+		break;
+	case PIN_CONFIG_INPUT_ENABLE:
+	case PIN_CONFIG_OUTPUT_ENABLE:
+		err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DIR, &val);
+		if (err)
+			return err;
+
+		/* HW takes input mode as zero; output mode as non-zero */
+		if ((val && param == PIN_CONFIG_INPUT_ENABLE) ||
+		    (!val && param == PIN_CONFIG_OUTPUT_ENABLE))
+			return -EINVAL;
+
+		break;
+	case PIN_CONFIG_INPUT_SCHMITT_ENABLE:
+		err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DIR, &val);
+		if (err)
+			return err;
+
+		err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_SMT, &val2);
+		if (err)
+			return err;
+
+		if (val || !val2)
+			return -EINVAL;
+
+		break;
+	case PIN_CONFIG_DRIVE_STRENGTH:
+		if (hw->soc->drive_get) {
+			err = hw->soc->drive_get(hw, desc, &ret);
+			if (err)
+				return err;
+		} else {
+			err = -ENOTSUPP;
+		}
+		break;
+	case MTK_PIN_CONFIG_TDSEL:
+	case MTK_PIN_CONFIG_RDSEL:
+		reg = (param == MTK_PIN_CONFIG_TDSEL) ?
+		       PINCTRL_PIN_REG_TDSEL : PINCTRL_PIN_REG_RDSEL;
+
+		err = mtk_hw_get_value(hw, desc, reg, &val);
+		if (err)
+			return err;
+
+		ret = val;
+
+		break;
+	case MTK_PIN_CONFIG_PU_ADV:
+	case MTK_PIN_CONFIG_PD_ADV:
+		if (hw->soc->adv_pull_get) {
+			bool pullup;
+
+			pullup = param == MTK_PIN_CONFIG_PU_ADV;
+			err = hw->soc->adv_pull_get(hw, desc, pullup, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	default:
+		return -ENOTSUPP;
+	}
+
+	*config = pinconf_to_config_packed(param, ret);
+
+	return 0;
+}
+
+static int mtk_pinconf_set(struct pinctrl_dev *pctldev, unsigned int pin,
+			   unsigned long *configs, unsigned int num_configs)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	const struct mtk_pin_desc *desc;
+	u32 reg, param, arg;
+	int cfg, err = 0;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+	for (cfg = 0; cfg < num_configs; cfg++) {
+		param = pinconf_to_config_param(configs[cfg]);
+		arg = pinconf_to_config_argument(configs[cfg]);
+
+		switch (param) {
+		case PIN_CONFIG_BIAS_DISABLE:
+			if (hw->soc->bias_disable_set) {
+				err = hw->soc->bias_disable_set(hw, desc);
+				if (err)
+					return err;
+			} else {
+				return -ENOTSUPP;
+			}
+			break;
+		case PIN_CONFIG_BIAS_PULL_UP:
+			if (hw->soc->bias_set) {
+				err = hw->soc->bias_set(hw, desc, 1);
+				if (err)
+					return err;
+			} else {
+				return -ENOTSUPP;
+			}
+			break;
+		case PIN_CONFIG_BIAS_PULL_DOWN:
+			if (hw->soc->bias_set) {
+				err = hw->soc->bias_set(hw, desc, 0);
+				if (err)
+					return err;
+			} else {
+				return -ENOTSUPP;
+			}
+			break;
+		case PIN_CONFIG_OUTPUT_ENABLE:
+			err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_SMT,
+					       MTK_DISABLE);
+			if (err)
+				goto err;
+
+			err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR,
+					       MTK_OUTPUT);
+			if (err)
+				goto err;
+			break;
+		case PIN_CONFIG_INPUT_ENABLE:
+
+			if (hw->soc->ies_present) {
+				mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_IES,
+						 MTK_ENABLE);
+			}
+
+			err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR,
+					       MTK_INPUT);
+			if (err)
+				goto err;
+			break;
+		case PIN_CONFIG_SLEW_RATE:
+			err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_SR,
+					       arg);
+			if (err)
+				goto err;
+
+			break;
+		case PIN_CONFIG_OUTPUT:
+			err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR,
+					       MTK_OUTPUT);
+			if (err)
+				goto err;
+
+			err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DO,
+					       arg);
+			if (err)
+				goto err;
+			break;
+		case PIN_CONFIG_INPUT_SCHMITT_ENABLE:
+			/* arg = 1: Input mode & SMT enable ;
+			 * arg = 0: Output mode & SMT disable
+			 */
+			arg = arg ? 2 : 1;
+			err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR,
+					       arg & 1);
+			if (err)
+				goto err;
+
+			err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_SMT,
+					       !!(arg & 2));
+			if (err)
+				goto err;
+			break;
+		case PIN_CONFIG_DRIVE_STRENGTH:
+			if (hw->soc->drive_set) {
+				err = hw->soc->drive_set(hw, desc, arg);
+				if (err)
+					return err;
+			} else {
+				err = -ENOTSUPP;
+			}
+			break;
+		case MTK_PIN_CONFIG_TDSEL:
+		case MTK_PIN_CONFIG_RDSEL:
+			reg = (param == MTK_PIN_CONFIG_TDSEL) ?
+			       PINCTRL_PIN_REG_TDSEL : PINCTRL_PIN_REG_RDSEL;
+
+			err = mtk_hw_set_value(hw, desc, reg, arg);
+			if (err)
+				goto err;
+			break;
+		case MTK_PIN_CONFIG_PU_ADV:
+		case MTK_PIN_CONFIG_PD_ADV:
+			if (hw->soc->adv_pull_set) {
+				bool pullup;
+
+				pullup = param == MTK_PIN_CONFIG_PU_ADV;
+				err = hw->soc->adv_pull_set(hw, desc, pullup,
+							    arg);
+				if (err)
+					return err;
+			} else {
+				return -ENOTSUPP;
+			}
+			break;
+		default:
+			err = -ENOTSUPP;
+		}
+	}
+err:
+	return err;
+}
+
+static int mtk_pinconf_group_get(struct pinctrl_dev *pctldev,
+				 unsigned int group, unsigned long *config)
+{
+	const unsigned int *pins;
+	unsigned int i, npins, old = 0;
+	int ret;
+
+	ret = pinctrl_generic_get_group_pins(pctldev, group, &pins, &npins);
+	if (ret)
+		return ret;
+
+	for (i = 0; i < npins; i++) {
+		if (mtk_pinconf_get(pctldev, pins[i], config))
+			return -ENOTSUPP;
+
+		/* configs do not match between two pins */
+		if (i && old != *config)
+			return -ENOTSUPP;
+
+		old = *config;
+	}
+
+	return 0;
+}
+
+static int mtk_pinconf_group_set(struct pinctrl_dev *pctldev,
+				 unsigned int group, unsigned long *configs,
+				 unsigned int num_configs)
+{
+	const unsigned int *pins;
+	unsigned int i, npins;
+	int ret;
+
+	ret = pinctrl_generic_get_group_pins(pctldev, group, &pins, &npins);
+	if (ret)
+		return ret;
+
+	for (i = 0; i < npins; i++) {
+		ret = mtk_pinconf_set(pctldev, pins[i], configs, num_configs);
+		if (ret)
+			return ret;
+	}
+
+	return 0;
+}
+
+static const struct pinctrl_ops mtk_pctlops = {
+	.get_groups_count = pinctrl_generic_get_group_count,
+	.get_group_name = pinctrl_generic_get_group_name,
+	.get_group_pins = pinctrl_generic_get_group_pins,
+	.dt_node_to_map = pinconf_generic_dt_node_to_map_all,
+	.dt_free_map = pinconf_generic_dt_free_map,
+};
+
+static const struct pinmux_ops mtk_pmxops = {
+	.get_functions_count = pinmux_generic_get_function_count,
+	.get_function_name = pinmux_generic_get_function_name,
+	.get_function_groups = pinmux_generic_get_function_groups,
+	.set_mux = mtk_pinmux_set_mux,
+	.gpio_request_enable = mtk_pinmux_gpio_request_enable,
+	.gpio_set_direction = mtk_pinmux_gpio_set_direction,
+	.strict = true,
+};
+
+static const struct pinconf_ops mtk_confops = {
+	.is_generic = true,
+	.pin_config_get = mtk_pinconf_get,
+	.pin_config_set = mtk_pinconf_set,
+	.pin_config_group_get = mtk_pinconf_group_get,
+	.pin_config_group_set = mtk_pinconf_group_set,
+	.pin_config_config_dbg_show = pinconf_generic_dump_config,
+};
+
+static struct pinctrl_desc mtk_desc = {
+	.name = PINCTRL_PINCTRL_DEV,
+	.pctlops = &mtk_pctlops,
+	.pmxops = &mtk_pmxops,
+	.confops = &mtk_confops,
+	.owner = THIS_MODULE,
+};
+
+static int mtk_gpio_get(struct gpio_chip *chip, unsigned int gpio)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+	int value, err;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[gpio];
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DI, &value);
+	if (err)
+		return err;
+
+	return !!value;
+}
+
+static void mtk_gpio_set(struct gpio_chip *chip, unsigned int gpio, int value)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[gpio];
+
+	mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DO, !!value);
+}
+
+static int mtk_gpio_direction_input(struct gpio_chip *chip, unsigned int gpio)
+{
+	return pinctrl_gpio_direction_input(chip->base + gpio);
+}
+
+static int mtk_gpio_direction_output(struct gpio_chip *chip, unsigned int gpio,
+				     int value)
+{
+	mtk_gpio_set(chip, gpio, value);
+
+	return pinctrl_gpio_direction_output(chip->base + gpio);
+}
+
+static int mtk_gpio_to_irq(struct gpio_chip *chip, unsigned int offset)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+
+	if (!hw->eint)
+		return -ENOTSUPP;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[offset];
+
+	if (desc->eint.eint_n == (u16)EINT_NA)
+		return -ENOTSUPP;
+
+	return mtk_eint_find_irq(hw->eint, desc->eint.eint_n);
+}
+
+static int mtk_gpio_set_config(struct gpio_chip *chip, unsigned int offset,
+			       unsigned long config)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+	u32 debounce;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[offset];
+
+	if (!hw->eint ||
+	    pinconf_to_config_param(config) != PIN_CONFIG_INPUT_DEBOUNCE ||
+	    desc->eint.eint_n == (u16)EINT_NA)
+		return -ENOTSUPP;
+
+	debounce = pinconf_to_config_argument(config);
+
+	return mtk_eint_set_debounce(hw->eint, desc->eint.eint_n, debounce);
+}
+
+static int mtk_build_gpiochip(struct mtk_pinctrl *hw, struct device_node *np)
+{
+	struct gpio_chip *chip = &hw->chip;
+	int ret;
+
+	chip->label		= PINCTRL_PINCTRL_DEV;
+	chip->parent		= hw->dev;
+	chip->request		= gpiochip_generic_request;
+	chip->free		= gpiochip_generic_free;
+	chip->direction_input	= mtk_gpio_direction_input;
+	chip->direction_output	= mtk_gpio_direction_output;
+	chip->get		= mtk_gpio_get;
+	chip->set		= mtk_gpio_set;
+	chip->to_irq		= mtk_gpio_to_irq,
+	chip->set_config	= mtk_gpio_set_config,
+	chip->base		= -1;
+	chip->ngpio		= hw->soc->npins;
+	chip->of_node		= np;
+	chip->of_gpio_n_cells	= 2;
+
+	ret = gpiochip_add_data(chip, hw);
+	if (ret < 0)
+		return ret;
+
+	/* Just for backward compatible for these old pinctrl nodes without
+	 * "gpio-ranges" property. Otherwise, called directly from a
+	 * DeviceTree-supported pinctrl driver is DEPRECATED.
+	 * Please see Section 2.1 of
+	 * Documentation/devicetree/bindings/gpio/gpio.txt on how to
+	 * bind pinctrl and gpio drivers via the "gpio-ranges" property.
+	 */
+	if (!of_find_property(np, "gpio-ranges", NULL)) {
+		ret = gpiochip_add_pin_range(chip, dev_name(hw->dev), 0, 0,
+					     chip->ngpio);
+		if (ret < 0) {
+			gpiochip_remove(chip);
+			return ret;
+		}
+	}
+
+	return 0;
+}
+
+static int mtk_build_groups(struct mtk_pinctrl *hw)
+{
+	int err, i;
+
+	for (i = 0; i < hw->soc->ngrps; i++) {
+		const struct group_desc *group = hw->soc->grps + i;
+
+		err = pinctrl_generic_add_group(hw->pctrl, group->name,
+						group->pins, group->num_pins,
+						group->data);
+		if (err < 0) {
+			dev_err(hw->dev, "Failed to register group %s\n",
+				group->name);
+			return err;
+		}
+	}
+
+	return 0;
+}
+
+static int mtk_build_functions(struct mtk_pinctrl *hw)
+{
+	int i, err;
+
+	for (i = 0; i < hw->soc->nfuncs ; i++) {
+		const struct function_desc *func = hw->soc->funcs + i;
+
+		err = pinmux_generic_add_function(hw->pctrl, func->name,
+						  func->group_names,
+						  func->num_group_names,
+						  func->data);
+		if (err < 0) {
+			dev_err(hw->dev, "Failed to register function %s\n",
+				func->name);
+			return err;
+		}
+	}
+
+	return 0;
+}
+
+int mtk_moore_pinctrl_probe(struct platform_device *pdev,
+			    const struct mtk_pin_soc *soc)
+{
+	struct pinctrl_pin_desc *pins;
+	struct resource *res;
+	struct mtk_pinctrl *hw;
+	int err, i;
+
+	hw = devm_kzalloc(&pdev->dev, sizeof(*hw), GFP_KERNEL);
+	if (!hw)
+		return -ENOMEM;
+
+	hw->soc = soc;
+	hw->dev = &pdev->dev;
+
+	if (!hw->soc->nbase_names) {
+		dev_err(&pdev->dev,
+			"SoC should be assigned at least one register base\n");
+		return -EINVAL;
+	}
+
+	hw->base = devm_kmalloc_array(&pdev->dev, hw->soc->nbase_names,
+				      sizeof(*hw->base), GFP_KERNEL);
+	if (!hw->base)
+		return -ENOMEM;
+
+	for (i = 0; i < hw->soc->nbase_names; i++) {
+		res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
+						   hw->soc->base_names[i]);
+		if (!res) {
+			dev_err(&pdev->dev, "missing IO resource\n");
+			return -ENXIO;
+		}
+
+		hw->base[i] = devm_ioremap_resource(&pdev->dev, res);
+		if (IS_ERR(hw->base[i]))
+			return PTR_ERR(hw->base[i]);
+	}
+
+	hw->nbase = hw->soc->nbase_names;
+
+	/* Copy from internal struct mtk_pin_desc to register to the core */
+	pins = devm_kmalloc_array(&pdev->dev, hw->soc->npins, sizeof(*pins),
+				  GFP_KERNEL);
+	if (!pins)
+		return -ENOMEM;
+
+	for (i = 0; i < hw->soc->npins; i++) {
+		pins[i].number = hw->soc->pins[i].number;
+		pins[i].name = hw->soc->pins[i].name;
+	}
+
+	/* Setup pins descriptions per SoC types */
+	mtk_desc.pins = (const struct pinctrl_pin_desc *)pins;
+	mtk_desc.npins = hw->soc->npins;
+	mtk_desc.num_custom_params = ARRAY_SIZE(mtk_custom_bindings);
+	mtk_desc.custom_params = mtk_custom_bindings;
+#ifdef CONFIG_DEBUG_FS
+	mtk_desc.custom_conf_items = mtk_conf_items;
+#endif
+
+	err = devm_pinctrl_register_and_init(&pdev->dev, &mtk_desc, hw,
+					     &hw->pctrl);
+	if (err)
+		return err;
+
+	/* Setup groups descriptions per SoC types */
+	err = mtk_build_groups(hw);
+	if (err) {
+		dev_err(&pdev->dev, "Failed to build groups\n");
+		return err;
+	}
+
+	/* Setup functions descriptions per SoC types */
+	err = mtk_build_functions(hw);
+	if (err) {
+		dev_err(&pdev->dev, "Failed to build functions\n");
+		return err;
+	}
+
+	/* For able to make pinctrl_claim_hogs, we must not enable pinctrl
+	 * until all groups and functions are being added one.
+	 */
+	err = pinctrl_enable(hw->pctrl);
+	if (err)
+		return err;
+
+	err = mtk_build_eint(hw, pdev);
+	if (err)
+		dev_warn(&pdev->dev,
+			 "Failed to add EINT, but pinctrl still can work\n");
+
+	/* Build gpiochip should be after pinctrl_enable is done */
+	err = mtk_build_gpiochip(hw, pdev->dev.of_node);
+	if (err) {
+		dev_err(&pdev->dev, "Failed to add gpio_chip\n");
+		return err;
+	}
+
+	platform_set_drvdata(pdev, hw);
+
+	return 0;
+}
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-moore.h
@@ -0,0 +1,51 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2017-2018 MediaTek Inc.
+ *
+ * Author: Sean Wang <sean.wang@mediatek.com>
+ *
+ */
+#ifndef __PINCTRL_MOORE_H
+#define __PINCTRL_MOORE_H
+
+#include <linux/io.h>
+#include <linux/init.h>
+#include <linux/of.h>
+#include <linux/of_platform.h>
+#include <linux/platform_device.h>
+#include <linux/pinctrl/pinctrl.h>
+#include <linux/pinctrl/pinmux.h>
+#include <linux/pinctrl/pinconf.h>
+#include <linux/pinctrl/pinconf-generic.h>
+
+#include "../core.h"
+#include "../pinconf.h"
+#include "../pinmux.h"
+#include "mtk-eint.h"
+#include "pinctrl-mtk-common-v2.h"
+
+#define MTK_RANGE(_a)		{ .range = (_a), .nranges = ARRAY_SIZE(_a), }
+
+#define MTK_PIN(_number, _name, _eint_m, _eint_n, _drv_n) {	\
+		.number = _number,			\
+		.name = _name,				\
+		.eint = {				\
+			.eint_m = _eint_m,		\
+			.eint_n = _eint_n,		\
+		},					\
+		.drv_n = _drv_n,			\
+		.funcs = NULL,				\
+	}
+
+#define PINCTRL_PIN_GROUP(name, id)			\
+	{						\
+		name,					\
+		id##_pins,				\
+		ARRAY_SIZE(id##_pins),			\
+		id##_funcs,				\
+	}
+
+int mtk_moore_pinctrl_probe(struct platform_device *pdev,
+			    const struct mtk_pin_soc *soc);
+
+#endif /* __PINCTRL_MOORE_H */
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mt6765.c
@@ -0,0 +1,1108 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: ZH Chen <zh.chen@mediatek.com>
+ *
+ */
+
+#include "pinctrl-mtk-mt6765.h"
+#include "pinctrl-paris.h"
+
+/* MT6765 have multiple bases to program pin configuration listed as the below:
+ * iocfg[0]:0x10005000, iocfg[1]:0x10002C00, iocfg[2]:0x10002800,
+ * iocfg[3]:0x10002A00, iocfg[4]:0x10002000, iocfg[5]:0x10002200,
+ * iocfg[6]:0x10002500, iocfg[7]:0x10002600.
+ * _i_base could be used to indicate what base the pin should be mapped into.
+ */
+
+#define PIN_FIELD_BASE(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit,	\
+		       _x_bits, 32, 0)
+
+#define PINS_FIELD_BASE(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit,	\
+		      _x_bits, 32, 1)
+
+static const struct mtk_pin_field_calc mt6765_pin_mode_range[] = {
+	PIN_FIELD(0, 202, 0x300, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_dir_range[] = {
+	PIN_FIELD(0, 202, 0x0, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_di_range[] = {
+	PIN_FIELD(0, 202, 0x200, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_do_range[] = {
+	PIN_FIELD(0, 202, 0x100, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_smt_range[] = {
+	PINS_FIELD_BASE(0, 3, 2, 0x00b0, 0x10, 4, 1),
+	PINS_FIELD_BASE(4, 7, 2, 0x00b0, 0x10, 5, 1),
+	PIN_FIELD_BASE(8, 8, 3, 0x0080, 0x10, 3, 1),
+	PINS_FIELD_BASE(9, 11, 2, 0x00b0, 0x10, 6, 1),
+	PIN_FIELD_BASE(12, 12, 5, 0x0060, 0x10, 9, 1),
+	PINS_FIELD_BASE(13, 16, 6, 0x00b0, 0x10, 10, 1),
+	PINS_FIELD_BASE(17, 20, 6, 0x00b0, 0x10, 8, 1),
+	PINS_FIELD_BASE(21, 24, 6, 0x00b0, 0x10, 9, 1),
+	PINS_FIELD_BASE(25, 28, 6, 0x00b0, 0x10, 7, 1),
+	PIN_FIELD_BASE(29, 29, 6, 0x00b0, 0x10, 0, 1),
+	PIN_FIELD_BASE(30, 30, 6, 0x00b0, 0x10, 1, 1),
+	PINS_FIELD_BASE(31, 34, 6, 0x00b0, 0x10, 2, 1),
+	PINS_FIELD_BASE(35, 36, 6, 0x00b0, 0x10, 5, 1),
+	PIN_FIELD_BASE(37, 37, 6, 0x00b0, 0x10, 6, 1),
+	PIN_FIELD_BASE(38, 38, 6, 0x00b0, 0x10, 4, 1),
+	PINS_FIELD_BASE(39, 40, 6, 0x00b0, 0x10, 3, 1),
+	PINS_FIELD_BASE(41, 42, 7, 0x00c0, 0x10, 6, 1),
+	PIN_FIELD_BASE(43, 43, 7, 0x00c0, 0x10, 3, 1),
+	PIN_FIELD_BASE(44, 44, 7, 0x00c0, 0x10, 4, 1),
+	PIN_FIELD_BASE(45, 45, 7, 0x00c0, 0x10, 8, 1),
+	PINS_FIELD_BASE(46, 47, 7, 0x00c0, 0x10, 7, 1),
+	PIN_FIELD_BASE(48, 48, 7, 0x00c0, 0x10, 15, 1),
+	PIN_FIELD_BASE(49, 49, 7, 0x00c0, 0x10, 17, 1),
+	PIN_FIELD_BASE(50, 50, 7, 0x00c0, 0x10, 14, 1),
+	PIN_FIELD_BASE(51, 51, 7, 0x00c0, 0x10, 16, 1),
+	PINS_FIELD_BASE(52, 57, 7, 0x00c0, 0x10, 0, 1),
+	PINS_FIELD_BASE(58, 60, 7, 0x00c0, 0x10, 12, 1),
+	PINS_FIELD_BASE(61, 62, 3, 0x0080, 0x10, 5, 1),
+	PINS_FIELD_BASE(63, 64, 3, 0x0080, 0x10, 4, 1),
+	PINS_FIELD_BASE(65, 66, 3, 0x0080, 0x10, 7, 1),
+	PINS_FIELD_BASE(67, 68, 3, 0x0080, 0x10, 6, 1),
+	PINS_FIELD_BASE(69, 73, 3, 0x0080, 0x10, 1, 1),
+	PINS_FIELD_BASE(74, 78, 3, 0x0080, 0x10, 2, 1),
+	PINS_FIELD_BASE(79, 80, 3, 0x0080, 0x10, 0, 1),
+	PIN_FIELD_BASE(81, 81, 3, 0x0080, 0x10, 12, 1),
+	PIN_FIELD_BASE(82, 82, 3, 0x0080, 0x10, 11, 1),
+	PIN_FIELD_BASE(83, 83, 3, 0x0080, 0x10, 9, 1),
+	PIN_FIELD_BASE(84, 84, 3, 0x0080, 0x10, 10, 1),
+	PIN_FIELD_BASE(85, 85, 7, 0x00c0, 0x10, 12, 1),
+	PIN_FIELD_BASE(86, 86, 7, 0x00c0, 0x10, 13, 1),
+	PIN_FIELD_BASE(87, 87, 7, 0x00c0, 0x10, 2, 1),
+	PIN_FIELD_BASE(88, 88, 7, 0x00c0, 0x10, 1, 1),
+	PIN_FIELD_BASE(89, 89, 2, 0x00b0, 0x10, 13, 1),
+	PIN_FIELD_BASE(90, 90, 3, 0x0080, 0x10, 8, 1),
+	PINS_FIELD_BASE(91, 92, 2, 0x00b0, 0x10, 8, 1),
+	PINS_FIELD_BASE(93, 94, 2, 0x00b0, 0x10, 7, 1),
+	PINS_FIELD_BASE(95, 96, 2, 0x00b0, 0x10, 14, 1),
+	PINS_FIELD_BASE(97, 98, 2, 0x00b0, 0x10, 2, 1),
+	PIN_FIELD_BASE(99, 99, 2, 0x00b0, 0x10, 0, 1),
+	PIN_FIELD_BASE(100, 100, 2, 0x00b0, 0x10, 1, 1),
+	PINS_FIELD_BASE(101, 102, 2, 0x00b0, 0x10, 3, 1),
+	PIN_FIELD_BASE(103, 103, 2, 0x00b0, 0x10, 9, 1),
+	PIN_FIELD_BASE(104, 104, 2, 0x00b0, 0x10, 11, 1),
+	PIN_FIELD_BASE(105, 105, 2, 0x00b0, 0x10, 10, 1),
+	PIN_FIELD_BASE(106, 106, 2, 0x00b0, 0x10, 12, 1),
+	PIN_FIELD_BASE(107, 107, 1, 0x0080, 0x10, 4, 1),
+	PIN_FIELD_BASE(108, 108, 1, 0x0080, 0x10, 3, 1),
+	PIN_FIELD_BASE(109, 109, 1, 0x0080, 0x10, 5, 1),
+	PIN_FIELD_BASE(110, 110, 1, 0x0080, 0x10, 0, 1),
+	PIN_FIELD_BASE(111, 111, 1, 0x0080, 0x10, 1, 1),
+	PIN_FIELD_BASE(112, 112, 1, 0x0080, 0x10, 2, 1),
+	PIN_FIELD_BASE(113, 113, 1, 0x0080, 0x10, 9, 1),
+	PIN_FIELD_BASE(114, 114, 1, 0x0080, 0x10, 10, 1),
+	PIN_FIELD_BASE(115, 115, 1, 0x0080, 0x10, 6, 1),
+	PIN_FIELD_BASE(116, 116, 1, 0x0080, 0x10, 7, 1),
+	PIN_FIELD_BASE(117, 117, 1, 0x0080, 0x10, 12, 1),
+	PIN_FIELD_BASE(118, 118, 1, 0x0080, 0x10, 13, 1),
+	PIN_FIELD_BASE(119, 119, 1, 0x0080, 0x10, 14, 1),
+	PIN_FIELD_BASE(120, 120, 1, 0x0080, 0x10, 11, 1),
+	PIN_FIELD_BASE(121, 121, 1, 0x0080, 0x10, 8, 1),
+	PIN_FIELD_BASE(122, 122, 4, 0x0080, 0x10, 2, 1),
+	PIN_FIELD_BASE(123, 123, 4, 0x0080, 0x10, 3, 1),
+	PIN_FIELD_BASE(124, 124, 4, 0x0080, 0x10, 1, 1),
+	PIN_FIELD_BASE(125, 125, 4, 0x0080, 0x10, 5, 1),
+	PIN_FIELD_BASE(126, 126, 4, 0x0080, 0x10, 7, 1),
+	PIN_FIELD_BASE(127, 127, 4, 0x0080, 0x10, 9, 1),
+	PIN_FIELD_BASE(128, 128, 4, 0x0080, 0x10, 4, 1),
+	PIN_FIELD_BASE(129, 129, 4, 0x0080, 0x10, 8, 1),
+	PIN_FIELD_BASE(130, 130, 4, 0x0080, 0x10, 10, 1),
+	PIN_FIELD_BASE(131, 131, 4, 0x0080, 0x10, 11, 1),
+	PIN_FIELD_BASE(132, 132, 4, 0x0080, 0x10, 6, 1),
+	PIN_FIELD_BASE(133, 133, 4, 0x0080, 0x10, 12, 1),
+	PIN_FIELD_BASE(134, 134, 5, 0x0060, 0x10, 11, 1),
+	PIN_FIELD_BASE(135, 135, 5, 0x0060, 0x10, 13, 1),
+	PIN_FIELD_BASE(136, 136, 5, 0x0060, 0x10, 1, 1),
+	PIN_FIELD_BASE(137, 137, 5, 0x0060, 0x10, 7, 1),
+	PIN_FIELD_BASE(138, 138, 5, 0x0060, 0x10, 4, 1),
+	PIN_FIELD_BASE(139, 139, 5, 0x0060, 0x10, 5, 1),
+	PIN_FIELD_BASE(140, 140, 5, 0x0060, 0x10, 0, 1),
+	PIN_FIELD_BASE(141, 141, 5, 0x0060, 0x10, 6, 1),
+	PIN_FIELD_BASE(142, 142, 5, 0x0060, 0x10, 2, 1),
+	PIN_FIELD_BASE(143, 143, 5, 0x0060, 0x10, 3, 1),
+	PINS_FIELD_BASE(144, 147, 5, 0x0060, 0x10, 10, 1),
+	PINS_FIELD_BASE(148, 149, 5, 0x0060, 0x10, 12, 1),
+	PINS_FIELD_BASE(150, 151, 7, 0x00c0, 0x10, 9, 1),
+	PINS_FIELD_BASE(152, 153, 7, 0x00c0, 0x10, 10, 1),
+	PIN_FIELD_BASE(154, 154, 7, 0x00c0, 0x10, 11, 1),
+	PINS_FIELD_BASE(155, 158, 3, 0x0080, 0x10, 13, 1),
+	PIN_FIELD_BASE(159, 159, 7, 0x00c0, 0x10, 11, 1),
+	PIN_FIELD_BASE(160, 160, 5, 0x0060, 0x10, 8, 1),
+	PIN_FIELD_BASE(161, 161, 1, 0x0080, 0x10, 15, 1),
+	PIN_FIELD_BASE(162, 162, 1, 0x0080, 0x10, 16, 1),
+	PINS_FIELD_BASE(163, 170, 4, 0x0080, 0x10, 0, 1),
+	PINS_FIELD_BASE(171, 179, 7, 0x00c0, 0x10, 5, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_pd_range[] = {
+	PIN_FIELD_BASE(0, 0, 2, 0x0040, 0x10, 6, 1),
+	PIN_FIELD_BASE(1, 1, 2, 0x0040, 0x10, 7, 1),
+	PIN_FIELD_BASE(2, 2, 2, 0x0040, 0x10, 10, 1),
+	PIN_FIELD_BASE(3, 3, 2, 0x0040, 0x10, 11, 1),
+	PIN_FIELD_BASE(4, 4, 2, 0x0040, 0x10, 12, 1),
+	PIN_FIELD_BASE(5, 5, 2, 0x0040, 0x10, 13, 1),
+	PIN_FIELD_BASE(6, 6, 2, 0x0040, 0x10, 14, 1),
+	PIN_FIELD_BASE(7, 7, 2, 0x0040, 0x10, 15, 1),
+	PIN_FIELD_BASE(8, 8, 3, 0x0040, 0x10, 12, 1),
+	PIN_FIELD_BASE(9, 9, 2, 0x0040, 0x10, 16, 1),
+	PIN_FIELD_BASE(10, 10, 2, 0x0040, 0x10, 8, 1),
+	PIN_FIELD_BASE(11, 11, 2, 0x0040, 0x10, 9, 1),
+	PIN_FIELD_BASE(12, 12, 5, 0x0030, 0x10, 9, 1),
+	PIN_FIELD_BASE(13, 13, 6, 0x0040, 0x10, 14, 1),
+	PIN_FIELD_BASE(14, 14, 6, 0x0040, 0x10, 13, 1),
+	PIN_FIELD_BASE(15, 15, 6, 0x0040, 0x10, 15, 1),
+	PIN_FIELD_BASE(16, 16, 6, 0x0040, 0x10, 12, 1),
+	PIN_FIELD_BASE(17, 17, 6, 0x0040, 0x10, 7, 1),
+	PIN_FIELD_BASE(18, 18, 6, 0x0040, 0x10, 4, 1),
+	PIN_FIELD_BASE(19, 19, 6, 0x0040, 0x10, 6, 1),
+	PIN_FIELD_BASE(20, 20, 6, 0x0040, 0x10, 5, 1),
+	PIN_FIELD_BASE(21, 21, 6, 0x0040, 0x10, 10, 1),
+	PIN_FIELD_BASE(22, 22, 6, 0x0040, 0x10, 9, 1),
+	PIN_FIELD_BASE(23, 23, 6, 0x0040, 0x10, 11, 1),
+	PIN_FIELD_BASE(24, 24, 6, 0x0040, 0x10, 8, 1),
+	PIN_FIELD_BASE(25, 25, 6, 0x0040, 0x10, 2, 1),
+	PIN_FIELD_BASE(26, 26, 6, 0x0040, 0x10, 1, 1),
+	PIN_FIELD_BASE(27, 27, 6, 0x0040, 0x10, 3, 1),
+	PINS_FIELD_BASE(28, 40, 6, 0x0040, 0x10, 0, 1),
+	PIN_FIELD_BASE(41, 41, 7, 0x0060, 0x10, 19, 1),
+	PIN_FIELD_BASE(42, 42, 7, 0x0060, 0x10, 9, 1),
+	PIN_FIELD_BASE(43, 43, 7, 0x0060, 0x10, 8, 1),
+	PIN_FIELD_BASE(44, 44, 7, 0x0060, 0x10, 10, 1),
+	PIN_FIELD_BASE(45, 45, 7, 0x0060, 0x10, 22, 1),
+	PIN_FIELD_BASE(46, 46, 7, 0x0060, 0x10, 21, 1),
+	PIN_FIELD_BASE(47, 47, 7, 0x0060, 0x10, 20, 1),
+	PIN_FIELD_BASE(48, 48, 7, 0x0070, 0x10, 3, 1),
+	PIN_FIELD_BASE(49, 49, 7, 0x0070, 0x10, 5, 1),
+	PIN_FIELD_BASE(50, 50, 7, 0x0070, 0x10, 2, 1),
+	PIN_FIELD_BASE(51, 51, 7, 0x0070, 0x10, 4, 1),
+	PIN_FIELD_BASE(52, 52, 7, 0x0060, 0x10, 1, 1),
+	PIN_FIELD_BASE(53, 53, 7, 0x0060, 0x10, 0, 1),
+	PIN_FIELD_BASE(54, 54, 7, 0x0060, 0x10, 5, 1),
+	PIN_FIELD_BASE(55, 55, 7, 0x0060, 0x10, 3, 1),
+	PIN_FIELD_BASE(56, 56, 7, 0x0060, 0x10, 4, 1),
+	PIN_FIELD_BASE(57, 57, 7, 0x0060, 0x10, 2, 1),
+	PIN_FIELD_BASE(58, 58, 7, 0x0070, 0x10, 0, 1),
+	PIN_FIELD_BASE(59, 59, 7, 0x0060, 0x10, 31, 1),
+	PIN_FIELD_BASE(60, 60, 7, 0x0060, 0x10, 30, 1),
+	PIN_FIELD_BASE(61, 61, 3, 0x0040, 0x10, 18, 1),
+	PIN_FIELD_BASE(62, 62, 3, 0x0040, 0x10, 14, 1),
+	PIN_FIELD_BASE(63, 63, 3, 0x0040, 0x10, 17, 1),
+	PIN_FIELD_BASE(64, 64, 3, 0x0040, 0x10, 13, 1),
+	PIN_FIELD_BASE(65, 65, 3, 0x0040, 0x10, 20, 1),
+	PIN_FIELD_BASE(66, 66, 3, 0x0040, 0x10, 16, 1),
+	PIN_FIELD_BASE(67, 67, 3, 0x0040, 0x10, 19, 1),
+	PIN_FIELD_BASE(68, 68, 3, 0x0040, 0x10, 15, 1),
+	PIN_FIELD_BASE(69, 69, 3, 0x0040, 0x10, 8, 1),
+	PIN_FIELD_BASE(70, 70, 3, 0x0040, 0x10, 7, 1),
+	PIN_FIELD_BASE(71, 71, 3, 0x0040, 0x10, 6, 1),
+	PIN_FIELD_BASE(72, 72, 3, 0x0040, 0x10, 5, 1),
+	PIN_FIELD_BASE(73, 73, 3, 0x0040, 0x10, 4, 1),
+	PIN_FIELD_BASE(74, 74, 3, 0x0040, 0x10, 3, 1),
+	PIN_FIELD_BASE(75, 75, 3, 0x0040, 0x10, 2, 1),
+	PIN_FIELD_BASE(76, 76, 3, 0x0040, 0x10, 1, 1),
+	PIN_FIELD_BASE(77, 77, 3, 0x0040, 0x10, 0, 1),
+	PIN_FIELD_BASE(78, 78, 3, 0x0040, 0x10, 9, 1),
+	PIN_FIELD_BASE(79, 79, 3, 0x0040, 0x10, 11, 1),
+	PIN_FIELD_BASE(80, 80, 3, 0x0040, 0x10, 10, 1),
+	PIN_FIELD_BASE(81, 81, 3, 0x0040, 0x10, 25, 1),
+	PIN_FIELD_BASE(82, 82, 3, 0x0040, 0x10, 24, 1),
+	PIN_FIELD_BASE(83, 83, 3, 0x0040, 0x10, 22, 1),
+	PIN_FIELD_BASE(84, 84, 3, 0x0040, 0x10, 23, 1),
+	PIN_FIELD_BASE(85, 85, 7, 0x0070, 0x10, 1, 1),
+	PIN_FIELD_BASE(86, 86, 7, 0x0060, 0x10, 29, 1),
+	PIN_FIELD_BASE(87, 87, 7, 0x0060, 0x10, 7, 1),
+	PIN_FIELD_BASE(88, 88, 7, 0x0060, 0x10, 6, 1),
+	PIN_FIELD_BASE(89, 89, 2, 0x0040, 0x10, 21, 1),
+	PINS_FIELD_BASE(90, 94, 3, 0x0040, 0x10, 21, 1),
+	PIN_FIELD_BASE(95, 95, 2, 0x0040, 0x10, 22, 1),
+	PIN_FIELD_BASE(96, 96, 2, 0x0040, 0x10, 23, 1),
+	PIN_FIELD_BASE(97, 97, 2, 0x0040, 0x10, 2, 1),
+	PIN_FIELD_BASE(98, 98, 2, 0x0040, 0x10, 3, 1),
+	PIN_FIELD_BASE(99, 99, 2, 0x0040, 0x10, 0, 1),
+	PIN_FIELD_BASE(100, 100, 2, 0x0040, 0x10, 1, 1),
+	PIN_FIELD_BASE(101, 101, 2, 0x0040, 0x10, 4, 1),
+	PIN_FIELD_BASE(102, 102, 2, 0x0040, 0x10, 5, 1),
+	PIN_FIELD_BASE(103, 103, 2, 0x0040, 0x10, 17, 1),
+	PIN_FIELD_BASE(104, 104, 2, 0x0040, 0x10, 19, 1),
+	PIN_FIELD_BASE(105, 105, 2, 0x0040, 0x10, 18, 1),
+	PIN_FIELD_BASE(106, 106, 2, 0x0040, 0x10, 20, 1),
+	PIN_FIELD_BASE(107, 107, 1, 0x0040, 0x10, 4, 1),
+	PIN_FIELD_BASE(108, 108, 1, 0x0040, 0x10, 3, 1),
+	PIN_FIELD_BASE(109, 109, 1, 0x0040, 0x10, 5, 1),
+	PIN_FIELD_BASE(110, 110, 1, 0x0040, 0x10, 0, 1),
+	PIN_FIELD_BASE(111, 111, 1, 0x0040, 0x10, 1, 1),
+	PIN_FIELD_BASE(112, 112, 1, 0x0040, 0x10, 2, 1),
+	PIN_FIELD_BASE(113, 113, 1, 0x0040, 0x10, 9, 1),
+	PIN_FIELD_BASE(114, 114, 1, 0x0040, 0x10, 10, 1),
+	PIN_FIELD_BASE(115, 115, 1, 0x0040, 0x10, 6, 1),
+	PIN_FIELD_BASE(116, 116, 1, 0x0040, 0x10, 7, 1),
+	PIN_FIELD_BASE(117, 117, 1, 0x0040, 0x10, 12, 1),
+	PIN_FIELD_BASE(118, 118, 1, 0x0040, 0x10, 13, 1),
+	PIN_FIELD_BASE(119, 119, 1, 0x0040, 0x10, 14, 1),
+	PIN_FIELD_BASE(120, 120, 1, 0x0040, 0x10, 11, 1),
+	PINS_FIELD_BASE(121, 133, 1, 0x0040, 0x10, 8, 1),
+	PIN_FIELD_BASE(134, 134, 5, 0x0030, 0x10, 14, 1),
+	PIN_FIELD_BASE(135, 135, 5, 0x0030, 0x10, 19, 1),
+	PIN_FIELD_BASE(136, 136, 5, 0x0030, 0x10, 1, 1),
+	PIN_FIELD_BASE(137, 137, 5, 0x0030, 0x10, 7, 1),
+	PIN_FIELD_BASE(138, 138, 5, 0x0030, 0x10, 4, 1),
+	PIN_FIELD_BASE(139, 139, 5, 0x0030, 0x10, 5, 1),
+	PIN_FIELD_BASE(140, 140, 5, 0x0030, 0x10, 0, 1),
+	PIN_FIELD_BASE(141, 141, 5, 0x0030, 0x10, 6, 1),
+	PIN_FIELD_BASE(142, 142, 5, 0x0030, 0x10, 2, 1),
+	PIN_FIELD_BASE(143, 143, 5, 0x0030, 0x10, 3, 1),
+	PIN_FIELD_BASE(144, 144, 5, 0x0030, 0x10, 12, 1),
+	PIN_FIELD_BASE(145, 145, 5, 0x0030, 0x10, 11, 1),
+	PIN_FIELD_BASE(146, 146, 5, 0x0030, 0x10, 13, 1),
+	PIN_FIELD_BASE(147, 147, 5, 0x0030, 0x10, 10, 1),
+	PIN_FIELD_BASE(148, 148, 5, 0x0030, 0x10, 15, 1),
+	PIN_FIELD_BASE(149, 149, 5, 0x0030, 0x10, 16, 1),
+	PIN_FIELD_BASE(150, 150, 7, 0x0060, 0x10, 23, 1),
+	PIN_FIELD_BASE(151, 151, 7, 0x0060, 0x10, 24, 1),
+	PIN_FIELD_BASE(152, 152, 7, 0x0060, 0x10, 25, 1),
+	PIN_FIELD_BASE(153, 153, 7, 0x0060, 0x10, 26, 1),
+	PIN_FIELD_BASE(154, 154, 7, 0x0060, 0x10, 28, 1),
+	PIN_FIELD_BASE(155, 155, 3, 0x0040, 0x10, 28, 1),
+	PIN_FIELD_BASE(156, 156, 3, 0x0040, 0x10, 27, 1),
+	PIN_FIELD_BASE(157, 157, 3, 0x0040, 0x10, 29, 1),
+	PIN_FIELD_BASE(158, 158, 3, 0x0040, 0x10, 26, 1),
+	PIN_FIELD_BASE(159, 159, 7, 0x0060, 0x10, 27, 1),
+	PIN_FIELD_BASE(160, 160, 5, 0x0030, 0x10, 8, 1),
+	PIN_FIELD_BASE(161, 161, 1, 0x0040, 0x10, 15, 1),
+	PIN_FIELD_BASE(162, 162, 1, 0x0040, 0x10, 16, 1),
+	PIN_FIELD_BASE(163, 163, 4, 0x0020, 0x10, 0, 1),
+	PIN_FIELD_BASE(164, 164, 4, 0x0020, 0x10, 1, 1),
+	PIN_FIELD_BASE(165, 165, 4, 0x0020, 0x10, 2, 1),
+	PIN_FIELD_BASE(166, 166, 4, 0x0020, 0x10, 3, 1),
+	PIN_FIELD_BASE(167, 167, 4, 0x0020, 0x10, 4, 1),
+	PIN_FIELD_BASE(168, 168, 4, 0x0020, 0x10, 5, 1),
+	PIN_FIELD_BASE(169, 169, 4, 0x0020, 0x10, 6, 1),
+	PIN_FIELD_BASE(170, 170, 4, 0x0020, 0x10, 7, 1),
+	PIN_FIELD_BASE(171, 171, 7, 0x0060, 0x10, 17, 1),
+	PIN_FIELD_BASE(172, 172, 7, 0x0060, 0x10, 18, 1),
+	PIN_FIELD_BASE(173, 173, 7, 0x0060, 0x10, 11, 1),
+	PIN_FIELD_BASE(174, 174, 7, 0x0060, 0x10, 12, 1),
+	PIN_FIELD_BASE(175, 175, 7, 0x0060, 0x10, 13, 1),
+	PIN_FIELD_BASE(176, 176, 7, 0x0060, 0x10, 14, 1),
+	PIN_FIELD_BASE(177, 177, 7, 0x0060, 0x10, 15, 1),
+	PINS_FIELD_BASE(178, 179, 7, 0x0060, 0x10, 16, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_pu_range[] = {
+	PIN_FIELD_BASE(0, 0, 2, 0x0060, 0x10, 6, 1),
+	PIN_FIELD_BASE(1, 1, 2, 0x0060, 0x10, 7, 1),
+	PIN_FIELD_BASE(2, 2, 2, 0x0060, 0x10, 10, 1),
+	PIN_FIELD_BASE(3, 3, 2, 0x0060, 0x10, 11, 1),
+	PIN_FIELD_BASE(4, 4, 2, 0x0060, 0x10, 12, 1),
+	PIN_FIELD_BASE(5, 5, 2, 0x0060, 0x10, 13, 1),
+	PIN_FIELD_BASE(6, 6, 2, 0x0060, 0x10, 14, 1),
+	PIN_FIELD_BASE(7, 7, 2, 0x0060, 0x10, 15, 1),
+	PIN_FIELD_BASE(8, 8, 3, 0x0050, 0x10, 12, 1),
+	PIN_FIELD_BASE(9, 9, 2, 0x0060, 0x10, 16, 1),
+	PIN_FIELD_BASE(10, 10, 2, 0x0060, 0x10, 8, 1),
+	PIN_FIELD_BASE(11, 11, 2, 0x0060, 0x10, 9, 1),
+	PIN_FIELD_BASE(12, 12, 5, 0x0040, 0x10, 9, 1),
+	PIN_FIELD_BASE(13, 13, 6, 0x0060, 0x10, 14, 1),
+	PIN_FIELD_BASE(14, 14, 6, 0x0060, 0x10, 13, 1),
+	PIN_FIELD_BASE(15, 15, 6, 0x0060, 0x10, 15, 1),
+	PIN_FIELD_BASE(16, 16, 6, 0x0060, 0x10, 12, 1),
+	PIN_FIELD_BASE(17, 17, 6, 0x0060, 0x10, 7, 1),
+	PIN_FIELD_BASE(18, 18, 6, 0x0060, 0x10, 4, 1),
+	PIN_FIELD_BASE(19, 19, 6, 0x0060, 0x10, 6, 1),
+	PIN_FIELD_BASE(20, 20, 6, 0x0060, 0x10, 5, 1),
+	PIN_FIELD_BASE(21, 21, 6, 0x0060, 0x10, 10, 1),
+	PIN_FIELD_BASE(22, 22, 6, 0x0060, 0x10, 9, 1),
+	PIN_FIELD_BASE(23, 23, 6, 0x0060, 0x10, 11, 1),
+	PIN_FIELD_BASE(24, 24, 6, 0x0060, 0x10, 8, 1),
+	PIN_FIELD_BASE(25, 25, 6, 0x0060, 0x10, 2, 1),
+	PIN_FIELD_BASE(26, 26, 6, 0x0060, 0x10, 1, 1),
+	PIN_FIELD_BASE(27, 27, 6, 0x0060, 0x10, 3, 1),
+	PINS_FIELD_BASE(28, 40, 6, 0x0060, 0x10, 0, 1),
+	PIN_FIELD_BASE(41, 41, 7, 0x0080, 0x10, 19, 1),
+	PIN_FIELD_BASE(42, 42, 7, 0x0080, 0x10, 9, 1),
+	PIN_FIELD_BASE(43, 43, 7, 0x0080, 0x10, 8, 1),
+	PIN_FIELD_BASE(44, 44, 7, 0x0080, 0x10, 10, 1),
+	PIN_FIELD_BASE(45, 45, 7, 0x0080, 0x10, 22, 1),
+	PIN_FIELD_BASE(46, 46, 7, 0x0080, 0x10, 21, 1),
+	PIN_FIELD_BASE(47, 47, 7, 0x0080, 0x10, 20, 1),
+	PIN_FIELD_BASE(48, 48, 7, 0x0090, 0x10, 3, 1),
+	PIN_FIELD_BASE(49, 49, 7, 0x0090, 0x10, 5, 1),
+	PIN_FIELD_BASE(50, 50, 7, 0x0090, 0x10, 2, 1),
+	PIN_FIELD_BASE(51, 51, 7, 0x0090, 0x10, 4, 1),
+	PIN_FIELD_BASE(52, 52, 7, 0x0080, 0x10, 1, 1),
+	PIN_FIELD_BASE(53, 53, 7, 0x0080, 0x10, 0, 1),
+	PIN_FIELD_BASE(54, 54, 7, 0x0080, 0x10, 5, 1),
+	PIN_FIELD_BASE(55, 55, 7, 0x0080, 0x10, 3, 1),
+	PIN_FIELD_BASE(56, 56, 7, 0x0080, 0x10, 4, 1),
+	PIN_FIELD_BASE(57, 57, 7, 0x0080, 0x10, 2, 1),
+	PIN_FIELD_BASE(58, 58, 7, 0x0090, 0x10, 0, 1),
+	PIN_FIELD_BASE(59, 59, 7, 0x0080, 0x10, 31, 1),
+	PIN_FIELD_BASE(60, 60, 7, 0x0080, 0x10, 30, 1),
+	PIN_FIELD_BASE(61, 61, 3, 0x0050, 0x10, 18, 1),
+	PIN_FIELD_BASE(62, 62, 3, 0x0050, 0x10, 14, 1),
+	PIN_FIELD_BASE(63, 63, 3, 0x0050, 0x10, 17, 1),
+	PIN_FIELD_BASE(64, 64, 3, 0x0050, 0x10, 13, 1),
+	PIN_FIELD_BASE(65, 65, 3, 0x0050, 0x10, 20, 1),
+	PIN_FIELD_BASE(66, 66, 3, 0x0050, 0x10, 16, 1),
+	PIN_FIELD_BASE(67, 67, 3, 0x0050, 0x10, 19, 1),
+	PIN_FIELD_BASE(68, 68, 3, 0x0050, 0x10, 15, 1),
+	PIN_FIELD_BASE(69, 69, 3, 0x0050, 0x10, 8, 1),
+	PIN_FIELD_BASE(70, 70, 3, 0x0050, 0x10, 7, 1),
+	PIN_FIELD_BASE(71, 71, 3, 0x0050, 0x10, 6, 1),
+	PIN_FIELD_BASE(72, 72, 3, 0x0050, 0x10, 5, 1),
+	PIN_FIELD_BASE(73, 73, 3, 0x0050, 0x10, 4, 1),
+	PIN_FIELD_BASE(74, 74, 3, 0x0050, 0x10, 3, 1),
+	PIN_FIELD_BASE(75, 75, 3, 0x0050, 0x10, 2, 1),
+	PIN_FIELD_BASE(76, 76, 3, 0x0050, 0x10, 1, 1),
+	PIN_FIELD_BASE(77, 77, 3, 0x0050, 0x10, 0, 1),
+	PIN_FIELD_BASE(78, 78, 3, 0x0050, 0x10, 9, 1),
+	PIN_FIELD_BASE(79, 79, 3, 0x0050, 0x10, 11, 1),
+	PIN_FIELD_BASE(80, 80, 3, 0x0050, 0x10, 10, 1),
+	PIN_FIELD_BASE(81, 81, 3, 0x0050, 0x10, 25, 1),
+	PIN_FIELD_BASE(82, 82, 3, 0x0050, 0x10, 24, 1),
+	PIN_FIELD_BASE(83, 83, 3, 0x0050, 0x10, 22, 1),
+	PIN_FIELD_BASE(84, 84, 3, 0x0050, 0x10, 23, 1),
+	PIN_FIELD_BASE(85, 85, 7, 0x0090, 0x10, 1, 1),
+	PIN_FIELD_BASE(86, 86, 7, 0x0080, 0x10, 29, 1),
+	PIN_FIELD_BASE(87, 87, 7, 0x0080, 0x10, 7, 1),
+	PIN_FIELD_BASE(88, 88, 7, 0x0080, 0x10, 6, 1),
+	PIN_FIELD_BASE(89, 89, 2, 0x0060, 0x10, 21, 1),
+	PINS_FIELD_BASE(90, 94, 3, 0x0050, 0x10, 21, 1),
+	PIN_FIELD_BASE(95, 95, 2, 0x0060, 0x10, 22, 1),
+	PIN_FIELD_BASE(96, 96, 2, 0x0060, 0x10, 23, 1),
+	PIN_FIELD_BASE(97, 97, 2, 0x0060, 0x10, 2, 1),
+	PIN_FIELD_BASE(98, 98, 2, 0x0060, 0x10, 3, 1),
+	PIN_FIELD_BASE(99, 99, 2, 0x0060, 0x10, 0, 1),
+	PIN_FIELD_BASE(100, 100, 2, 0x0060, 0x10, 1, 1),
+	PIN_FIELD_BASE(101, 101, 2, 0x0060, 0x10, 4, 1),
+	PIN_FIELD_BASE(102, 102, 2, 0x0060, 0x10, 5, 1),
+	PIN_FIELD_BASE(103, 103, 2, 0x0060, 0x10, 17, 1),
+	PIN_FIELD_BASE(104, 104, 2, 0x0060, 0x10, 19, 1),
+	PIN_FIELD_BASE(105, 105, 2, 0x0060, 0x10, 18, 1),
+	PIN_FIELD_BASE(106, 106, 2, 0x0060, 0x10, 20, 1),
+	PIN_FIELD_BASE(107, 107, 1, 0x0050, 0x10, 4, 1),
+	PIN_FIELD_BASE(108, 108, 1, 0x0050, 0x10, 3, 1),
+	PIN_FIELD_BASE(109, 109, 1, 0x0050, 0x10, 5, 1),
+	PIN_FIELD_BASE(110, 110, 1, 0x0050, 0x10, 0, 1),
+	PIN_FIELD_BASE(111, 111, 1, 0x0050, 0x10, 1, 1),
+	PIN_FIELD_BASE(112, 112, 1, 0x0050, 0x10, 2, 1),
+	PIN_FIELD_BASE(113, 113, 1, 0x0050, 0x10, 9, 1),
+	PIN_FIELD_BASE(114, 114, 1, 0x0050, 0x10, 10, 1),
+	PIN_FIELD_BASE(115, 115, 1, 0x0050, 0x10, 6, 1),
+	PIN_FIELD_BASE(116, 116, 1, 0x0050, 0x10, 7, 1),
+	PIN_FIELD_BASE(117, 117, 1, 0x0050, 0x10, 12, 1),
+	PIN_FIELD_BASE(118, 118, 1, 0x0050, 0x10, 13, 1),
+	PIN_FIELD_BASE(119, 119, 1, 0x0050, 0x10, 14, 1),
+	PIN_FIELD_BASE(120, 120, 1, 0x0050, 0x10, 11, 1),
+	PINS_FIELD_BASE(121, 133, 1, 0x0050, 0x10, 8, 1),
+	PIN_FIELD_BASE(134, 134, 5, 0x0040, 0x10, 14, 1),
+	PIN_FIELD_BASE(135, 135, 5, 0x0040, 0x10, 19, 1),
+	PIN_FIELD_BASE(136, 136, 5, 0x0040, 0x10, 1, 1),
+	PIN_FIELD_BASE(137, 137, 5, 0x0040, 0x10, 7, 1),
+	PIN_FIELD_BASE(138, 138, 5, 0x0040, 0x10, 4, 1),
+	PIN_FIELD_BASE(139, 139, 5, 0x0040, 0x10, 5, 1),
+	PIN_FIELD_BASE(140, 140, 5, 0x0040, 0x10, 0, 1),
+	PIN_FIELD_BASE(141, 141, 5, 0x0040, 0x10, 6, 1),
+	PIN_FIELD_BASE(142, 142, 5, 0x0040, 0x10, 2, 1),
+	PIN_FIELD_BASE(143, 143, 5, 0x0040, 0x10, 3, 1),
+	PIN_FIELD_BASE(144, 144, 5, 0x0040, 0x10, 12, 1),
+	PIN_FIELD_BASE(145, 145, 5, 0x0040, 0x10, 11, 1),
+	PIN_FIELD_BASE(146, 146, 5, 0x0040, 0x10, 13, 1),
+	PIN_FIELD_BASE(147, 147, 5, 0x0040, 0x10, 10, 1),
+	PIN_FIELD_BASE(148, 148, 5, 0x0040, 0x10, 15, 1),
+	PIN_FIELD_BASE(149, 149, 5, 0x0040, 0x10, 16, 1),
+	PIN_FIELD_BASE(150, 150, 7, 0x0080, 0x10, 23, 1),
+	PIN_FIELD_BASE(151, 151, 7, 0x0080, 0x10, 24, 1),
+	PIN_FIELD_BASE(152, 152, 7, 0x0080, 0x10, 25, 1),
+	PIN_FIELD_BASE(153, 153, 7, 0x0080, 0x10, 26, 1),
+	PIN_FIELD_BASE(154, 154, 7, 0x0080, 0x10, 28, 1),
+	PIN_FIELD_BASE(155, 155, 3, 0x0050, 0x10, 28, 1),
+	PIN_FIELD_BASE(156, 156, 3, 0x0050, 0x10, 27, 1),
+	PIN_FIELD_BASE(157, 157, 3, 0x0050, 0x10, 29, 1),
+	PIN_FIELD_BASE(158, 158, 3, 0x0050, 0x10, 26, 1),
+	PIN_FIELD_BASE(159, 159, 7, 0x0080, 0x10, 27, 1),
+	PIN_FIELD_BASE(160, 160, 5, 0x0040, 0x10, 8, 1),
+	PIN_FIELD_BASE(161, 161, 1, 0x0050, 0x10, 15, 1),
+	PIN_FIELD_BASE(162, 162, 1, 0x0050, 0x10, 16, 1),
+	PIN_FIELD_BASE(163, 163, 4, 0x0040, 0x10, 0, 1),
+	PIN_FIELD_BASE(164, 164, 4, 0x0040, 0x10, 1, 1),
+	PIN_FIELD_BASE(165, 165, 4, 0x0040, 0x10, 2, 1),
+	PIN_FIELD_BASE(166, 166, 4, 0x0040, 0x10, 3, 1),
+	PIN_FIELD_BASE(167, 167, 4, 0x0040, 0x10, 4, 1),
+	PIN_FIELD_BASE(168, 168, 4, 0x0040, 0x10, 5, 1),
+	PIN_FIELD_BASE(169, 169, 4, 0x0040, 0x10, 6, 1),
+	PIN_FIELD_BASE(170, 170, 4, 0x0040, 0x10, 7, 1),
+	PIN_FIELD_BASE(171, 171, 7, 0x0080, 0x10, 17, 1),
+	PIN_FIELD_BASE(172, 172, 7, 0x0080, 0x10, 18, 1),
+	PIN_FIELD_BASE(173, 173, 7, 0x0080, 0x10, 11, 1),
+	PIN_FIELD_BASE(174, 174, 7, 0x0080, 0x10, 12, 1),
+	PIN_FIELD_BASE(175, 175, 7, 0x0080, 0x10, 13, 1),
+	PIN_FIELD_BASE(176, 176, 7, 0x0080, 0x10, 14, 1),
+	PIN_FIELD_BASE(177, 177, 7, 0x0080, 0x10, 15, 1),
+	PINS_FIELD_BASE(178, 179, 7, 0x0080, 0x10, 16, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_tdsel_range[] = {
+	PINS_FIELD_BASE(0, 3, 2, 0x00c0, 0x10, 16, 4),
+	PINS_FIELD_BASE(4, 7, 2, 0x00c0, 0x10, 20, 4),
+	PIN_FIELD_BASE(8, 8, 3, 0x0090, 0x10, 12, 4),
+	PINS_FIELD_BASE(9, 11, 2, 0x00c0, 0x10, 24, 4),
+	PIN_FIELD_BASE(12, 12, 5, 0x0080, 0x10, 4, 4),
+	PINS_FIELD_BASE(13, 16, 6, 0x00e0, 0x10, 8, 4),
+	PINS_FIELD_BASE(17, 20, 6, 0x00e0, 0x10, 0, 4),
+	PINS_FIELD_BASE(21, 24, 6, 0x00e0, 0x10, 4, 4),
+	PINS_FIELD_BASE(25, 28, 6, 0x00d0, 0x10, 28, 4),
+	PIN_FIELD_BASE(29, 29, 6, 0x00d0, 0x10, 0, 4),
+	PIN_FIELD_BASE(30, 30, 6, 0x00d0, 0x10, 4, 4),
+	PINS_FIELD_BASE(31, 34, 6, 0x00d0, 0x10, 8, 4),
+	PINS_FIELD_BASE(35, 36, 6, 0x00d0, 0x10, 20, 4),
+	PIN_FIELD_BASE(37, 37, 6, 0x00d0, 0x10, 24, 4),
+	PIN_FIELD_BASE(38, 38, 6, 0x00d0, 0x10, 16, 4),
+	PINS_FIELD_BASE(39, 40, 6, 0x00d0, 0x10, 12, 4),
+	PINS_FIELD_BASE(41, 42, 7, 0x00d0, 0x10, 24, 4),
+	PIN_FIELD_BASE(43, 43, 7, 0x00d0, 0x10, 12, 4),
+	PIN_FIELD_BASE(44, 44, 7, 0x00d0, 0x10, 16, 4),
+	PIN_FIELD_BASE(45, 45, 7, 0x00e0, 0x10, 0, 4),
+	PINS_FIELD_BASE(46, 47, 7, 0x00d0, 0x10, 28, 4),
+	PINS_FIELD_BASE(48, 49, 7, 0x00e0, 0x10, 28, 4),
+	PINS_FIELD_BASE(50, 51, 7, 0x00e0, 0x10, 24, 4),
+	PINS_FIELD_BASE(52, 57, 7, 0x00d0, 0x10, 0, 4),
+	PINS_FIELD_BASE(58, 60, 7, 0x00e0, 0x10, 16, 4),
+	PINS_FIELD_BASE(61, 62, 3, 0x0090, 0x10, 20, 4),
+	PINS_FIELD_BASE(63, 64, 3, 0x0090, 0x10, 16, 4),
+	PINS_FIELD_BASE(65, 66, 3, 0x0090, 0x10, 28, 4),
+	PINS_FIELD_BASE(67, 68, 3, 0x0090, 0x10, 24, 4),
+	PINS_FIELD_BASE(69, 73, 3, 0x0090, 0x10, 4, 4),
+	PINS_FIELD_BASE(74, 78, 3, 0x0090, 0x10, 8, 4),
+	PINS_FIELD_BASE(79, 80, 3, 0x0090, 0x10, 0, 4),
+	PIN_FIELD_BASE(81, 81, 3, 0x00a0, 0x10, 8, 4),
+	PINS_FIELD_BASE(82, 83, 3, 0x00a0, 0x10, 4, 4),
+	PIN_FIELD_BASE(84, 84, 3, 0x00a0, 0x10, 8, 4),
+	PIN_FIELD_BASE(85, 85, 7, 0x00e0, 0x10, 16, 4),
+	PIN_FIELD_BASE(86, 86, 7, 0x00e0, 0x10, 20, 4),
+	PIN_FIELD_BASE(87, 87, 7, 0x00d0, 0x10, 8, 4),
+	PIN_FIELD_BASE(88, 88, 7, 0x00d0, 0x10, 4, 4),
+	PIN_FIELD_BASE(89, 89, 2, 0x00d0, 0x10, 12, 4),
+	PIN_FIELD_BASE(90, 90, 3, 0x00a0, 0x10, 0, 4),
+	PINS_FIELD_BASE(91, 92, 2, 0x00d0, 0x10, 0, 4),
+	PINS_FIELD_BASE(93, 94, 2, 0x00c0, 0x10, 28, 4),
+	PINS_FIELD_BASE(95, 96, 2, 0x00d0, 0x10, 16, 4),
+	PINS_FIELD_BASE(97, 98, 2, 0x00c0, 0x10, 8, 4),
+	PIN_FIELD_BASE(99, 99, 2, 0x00c0, 0x10, 0, 4),
+	PIN_FIELD_BASE(100, 100, 2, 0x00c0, 0x10, 4, 4),
+	PINS_FIELD_BASE(101, 102, 2, 0x00c0, 0x10, 12, 4),
+	PINS_FIELD_BASE(103, 104, 2, 0x00d0, 0x10, 4, 4),
+	PINS_FIELD_BASE(105, 106, 2, 0x00d0, 0x10, 8, 4),
+	PIN_FIELD_BASE(107, 107, 1, 0x0090, 0x10, 16, 4),
+	PIN_FIELD_BASE(108, 108, 1, 0x0090, 0x10, 12, 4),
+	PIN_FIELD_BASE(109, 109, 1, 0x0090, 0x10, 20, 4),
+	PIN_FIELD_BASE(110, 110, 1, 0x0090, 0x10, 0, 4),
+	PIN_FIELD_BASE(111, 111, 1, 0x0090, 0x10, 4, 4),
+	PIN_FIELD_BASE(112, 112, 1, 0x0090, 0x10, 8, 4),
+	PIN_FIELD_BASE(113, 113, 1, 0x00a0, 0x10, 4, 4),
+	PIN_FIELD_BASE(114, 114, 1, 0x00a0, 0x10, 8, 4),
+	PIN_FIELD_BASE(115, 115, 1, 0x0090, 0x10, 24, 4),
+	PIN_FIELD_BASE(116, 116, 1, 0x0090, 0x10, 28, 4),
+	PIN_FIELD_BASE(117, 117, 1, 0x00a0, 0x10, 16, 4),
+	PIN_FIELD_BASE(118, 118, 1, 0x00a0, 0x10, 20, 4),
+	PIN_FIELD_BASE(119, 119, 1, 0x00a0, 0x10, 24, 4),
+	PIN_FIELD_BASE(120, 120, 1, 0x00a0, 0x10, 12, 4),
+	PIN_FIELD_BASE(121, 121, 1, 0x00a0, 0x10, 0, 4),
+	PIN_FIELD_BASE(122, 122, 4, 0x0090, 0x10, 8, 4),
+	PIN_FIELD_BASE(123, 123, 4, 0x0090, 0x10, 12, 4),
+	PIN_FIELD_BASE(124, 124, 4, 0x0090, 0x10, 4, 4),
+	PINS_FIELD_BASE(125, 130, 4, 0x0090, 0x10, 12, 4),
+	PIN_FIELD_BASE(131, 131, 4, 0x0090, 0x10, 16, 4),
+	PIN_FIELD_BASE(132, 132, 4, 0x0090, 0x10, 12, 4),
+	PIN_FIELD_BASE(133, 133, 4, 0x0090, 0x10, 20, 4),
+	PIN_FIELD_BASE(134, 134, 5, 0x0080, 0x10, 12, 4),
+	PIN_FIELD_BASE(135, 135, 5, 0x0080, 0x10, 20, 4),
+	PIN_FIELD_BASE(136, 136, 5, 0x0070, 0x10, 4, 4),
+	PIN_FIELD_BASE(137, 137, 5, 0x0070, 0x10, 28, 4),
+	PIN_FIELD_BASE(138, 138, 5, 0x0070, 0x10, 16, 4),
+	PIN_FIELD_BASE(139, 139, 5, 0x0070, 0x10, 20, 4),
+	PIN_FIELD_BASE(140, 140, 5, 0x0070, 0x10, 0, 4),
+	PIN_FIELD_BASE(141, 141, 5, 0x0070, 0x10, 24, 4),
+	PIN_FIELD_BASE(142, 142, 5, 0x0070, 0x10, 8, 4),
+	PIN_FIELD_BASE(143, 143, 5, 0x0070, 0x10, 12, 4),
+	PINS_FIELD_BASE(144, 147, 5, 0x0080, 0x10, 8, 4),
+	PINS_FIELD_BASE(148, 149, 5, 0x0080, 0x10, 16, 4),
+	PINS_FIELD_BASE(150, 151, 7, 0x00e0, 0x10, 4, 4),
+	PINS_FIELD_BASE(152, 153, 7, 0x00e0, 0x10, 8, 4),
+	PIN_FIELD_BASE(154, 154, 7, 0x00e0, 0x10, 12, 4),
+	PINS_FIELD_BASE(155, 158, 3, 0x00a0, 0x10, 12, 4),
+	PIN_FIELD_BASE(159, 159, 7, 0x00e0, 0x10, 12, 4),
+	PIN_FIELD_BASE(160, 160, 5, 0x0080, 0x10, 0, 4),
+	PINS_FIELD_BASE(161, 162, 1, 0x00a0, 0x10, 28, 4),
+	PINS_FIELD_BASE(163, 170, 4, 0x0090, 0x10, 0, 4),
+	PINS_FIELD_BASE(171, 179, 7, 0x00d0, 0x10, 20, 4),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_rdsel_range[] = {
+	PINS_FIELD_BASE(0, 3, 2, 0x0090, 0x10, 8, 2),
+	PINS_FIELD_BASE(4, 7, 2, 0x0090, 0x10, 10, 2),
+	PIN_FIELD_BASE(8, 8, 3, 0x0060, 0x10, 6, 2),
+	PINS_FIELD_BASE(9, 11, 2, 0x0090, 0x10, 12, 2),
+	PIN_FIELD_BASE(12, 12, 5, 0x0050, 0x10, 18, 2),
+	PINS_FIELD_BASE(13, 16, 6, 0x00a0, 0x10, 18, 2),
+	PINS_FIELD_BASE(17, 20, 6, 0x00a0, 0x10, 14, 2),
+	PINS_FIELD_BASE(21, 24, 6, 0x00a0, 0x10, 16, 2),
+	PINS_FIELD_BASE(25, 28, 6, 0x00a0, 0x10, 12, 2),
+	PIN_FIELD_BASE(29, 29, 6, 0x0090, 0x10, 0, 6),
+	PIN_FIELD_BASE(30, 30, 6, 0x0090, 0x10, 6, 6),
+	PINS_FIELD_BASE(31, 34, 6, 0x0090, 0x10, 12, 6),
+	PINS_FIELD_BASE(35, 36, 6, 0x00a0, 0x10, 0, 6),
+	PIN_FIELD_BASE(37, 37, 6, 0x00a0, 0x10, 6, 6),
+	PIN_FIELD_BASE(38, 38, 6, 0x0090, 0x10, 24, 6),
+	PINS_FIELD_BASE(39, 40, 6, 0x0090, 0x10, 18, 6),
+	PINS_FIELD_BASE(41, 42, 7, 0x00a0, 0x10, 12, 2),
+	PIN_FIELD_BASE(43, 43, 7, 0x00a0, 0x10, 6, 2),
+	PIN_FIELD_BASE(44, 44, 7, 0x00a0, 0x10, 8, 2),
+	PIN_FIELD_BASE(45, 45, 7, 0x00a0, 0x10, 16, 2),
+	PINS_FIELD_BASE(46, 47, 7, 0x00a0, 0x10, 14, 2),
+	PINS_FIELD_BASE(48, 49, 7, 0x00a0, 0x10, 30, 2),
+	PINS_FIELD_BASE(50, 51, 7, 0x00a0, 0x10, 28, 2),
+	PINS_FIELD_BASE(52, 57, 7, 0x00a0, 0x10, 0, 2),
+	PINS_FIELD_BASE(58, 60, 7, 0x00a0, 0x10, 24, 2),
+	PINS_FIELD_BASE(61, 62, 3, 0x0060, 0x10, 10, 2),
+	PINS_FIELD_BASE(63, 64, 3, 0x0060, 0x10, 8, 2),
+	PINS_FIELD_BASE(65, 66, 3, 0x0060, 0x10, 14, 2),
+	PINS_FIELD_BASE(67, 68, 3, 0x0060, 0x10, 12, 2),
+	PINS_FIELD_BASE(69, 73, 3, 0x0060, 0x10, 2, 2),
+	PINS_FIELD_BASE(74, 78, 3, 0x0060, 0x10, 4, 2),
+	PINS_FIELD_BASE(79, 80, 3, 0x0060, 0x10, 0, 2),
+	PIN_FIELD_BASE(81, 81, 3, 0x0060, 0x10, 20, 2),
+	PINS_FIELD_BASE(82, 83, 3, 0x0060, 0x10, 18, 2),
+	PIN_FIELD_BASE(84, 84, 3, 0x0060, 0x10, 20, 2),
+	PIN_FIELD_BASE(85, 85, 7, 0x00a0, 0x10, 24, 2),
+	PIN_FIELD_BASE(86, 86, 7, 0x00a0, 0x10, 26, 2),
+	PIN_FIELD_BASE(87, 87, 7, 0x00a0, 0x10, 4, 2),
+	PIN_FIELD_BASE(88, 88, 7, 0x00a0, 0x10, 2, 2),
+	PIN_FIELD_BASE(89, 89, 2, 0x0090, 0x10, 22, 2),
+	PIN_FIELD_BASE(90, 90, 3, 0x0060, 0x10, 16, 2),
+	PINS_FIELD_BASE(91, 92, 2, 0x0090, 0x10, 16, 2),
+	PINS_FIELD_BASE(93, 94, 2, 0x0090, 0x10, 14, 2),
+	PINS_FIELD_BASE(95, 96, 2, 0x0090, 0x10, 24, 2),
+	PINS_FIELD_BASE(97, 98, 2, 0x0090, 0x10, 4, 2),
+	PIN_FIELD_BASE(99, 99, 2, 0x0090, 0x10, 0, 2),
+	PIN_FIELD_BASE(100, 100, 2, 0x0090, 0x10, 2, 2),
+	PINS_FIELD_BASE(101, 102, 2, 0x0090, 0x10, 6, 2),
+	PINS_FIELD_BASE(103, 104, 2, 0x0090, 0x10, 18, 2),
+	PINS_FIELD_BASE(105, 106, 2, 0x0090, 0x10, 20, 2),
+	PIN_FIELD_BASE(107, 107, 1, 0x0060, 0x10, 8, 2),
+	PIN_FIELD_BASE(108, 108, 1, 0x0060, 0x10, 6, 2),
+	PIN_FIELD_BASE(109, 109, 1, 0x0060, 0x10, 10, 2),
+	PIN_FIELD_BASE(110, 110, 1, 0x0060, 0x10, 0, 2),
+	PIN_FIELD_BASE(111, 111, 1, 0x0060, 0x10, 2, 2),
+	PIN_FIELD_BASE(112, 112, 1, 0x0060, 0x10, 4, 2),
+	PIN_FIELD_BASE(113, 113, 1, 0x0060, 0x10, 18, 2),
+	PIN_FIELD_BASE(114, 114, 1, 0x0060, 0x10, 20, 2),
+	PIN_FIELD_BASE(115, 115, 1, 0x0060, 0x10, 12, 2),
+	PIN_FIELD_BASE(116, 116, 1, 0x0060, 0x10, 14, 2),
+	PIN_FIELD_BASE(117, 117, 1, 0x0060, 0x10, 24, 2),
+	PIN_FIELD_BASE(118, 118, 1, 0x0060, 0x10, 26, 2),
+	PIN_FIELD_BASE(119, 119, 1, 0x0060, 0x10, 28, 2),
+	PIN_FIELD_BASE(120, 120, 1, 0x0060, 0x10, 22, 2),
+	PIN_FIELD_BASE(121, 121, 1, 0x0060, 0x10, 16, 2),
+	PIN_FIELD_BASE(122, 122, 4, 0x0070, 0x10, 8, 6),
+	PIN_FIELD_BASE(123, 123, 4, 0x0070, 0x10, 14, 6),
+	PIN_FIELD_BASE(124, 124, 4, 0x0070, 0x10, 2, 6),
+	PINS_FIELD_BASE(125, 130, 4, 0x0070, 0x10, 14, 6),
+	PIN_FIELD_BASE(131, 131, 4, 0x0070, 0x10, 20, 6),
+	PIN_FIELD_BASE(132, 132, 4, 0x0070, 0x10, 14, 6),
+	PIN_FIELD_BASE(133, 133, 4, 0x0070, 0x10, 26, 6),
+	PIN_FIELD_BASE(134, 134, 5, 0x0050, 0x10, 22, 2),
+	PIN_FIELD_BASE(135, 135, 5, 0x0050, 0x10, 30, 2),
+	PIN_FIELD_BASE(136, 136, 5, 0x0050, 0x10, 2, 2),
+	PIN_FIELD_BASE(137, 137, 5, 0x0050, 0x10, 14, 2),
+	PIN_FIELD_BASE(138, 138, 5, 0x0050, 0x10, 8, 2),
+	PIN_FIELD_BASE(139, 139, 5, 0x0050, 0x10, 10, 2),
+	PIN_FIELD_BASE(140, 140, 5, 0x0050, 0x10, 0, 2),
+	PIN_FIELD_BASE(141, 141, 5, 0x0050, 0x10, 12, 2),
+	PIN_FIELD_BASE(142, 142, 5, 0x0050, 0x10, 4, 2),
+	PIN_FIELD_BASE(143, 143, 5, 0x0050, 0x10, 6, 2),
+	PINS_FIELD_BASE(144, 147, 5, 0x0050, 0x10, 20, 2),
+	PINS_FIELD_BASE(148, 149, 5, 0x0050, 0x10, 24, 2),
+	PINS_FIELD_BASE(150, 151, 7, 0x00a0, 0x10, 18, 2),
+	PINS_FIELD_BASE(152, 153, 7, 0x00a0, 0x10, 20, 2),
+	PIN_FIELD_BASE(154, 154, 7, 0x00a0, 0x10, 22, 2),
+	PINS_FIELD_BASE(155, 158, 3, 0x0060, 0x10, 22, 2),
+	PIN_FIELD_BASE(159, 159, 7, 0x00a0, 0x10, 22, 2),
+	PIN_FIELD_BASE(160, 160, 5, 0x0050, 0x10, 16, 2),
+	PINS_FIELD_BASE(161, 162, 1, 0x0060, 0x10, 30, 2),
+	PINS_FIELD_BASE(163, 170, 4, 0x0070, 0x10, 0, 2),
+	PINS_FIELD_BASE(171, 179, 7, 0x00a0, 0x10, 10, 2),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_drv_range[] = {
+	PINS_FIELD_BASE(0, 2, 2, 0x0000, 0x10, 12, 3),
+	PIN_FIELD_BASE(3, 3, 2, 0x0000, 0x10, 15, 3),
+	PINS_FIELD_BASE(4, 6, 2, 0x0000, 0x10, 18, 3),
+	PIN_FIELD_BASE(7, 7, 2, 0x0000, 0x10, 21, 3),
+	PIN_FIELD_BASE(8, 8, 3, 0x0000, 0x10, 9, 3),
+	PINS_FIELD_BASE(9, 11, 2, 0x0000, 0x10, 24, 3),
+	PIN_FIELD_BASE(12, 12, 5, 0x0000, 0x10, 27, 3),
+	PINS_FIELD_BASE(13, 15, 6, 0x0010, 0x10, 3, 3),
+	PIN_FIELD_BASE(16, 16, 6, 0x0010, 0x10, 6, 3),
+	PIN_FIELD_BASE(17, 17, 6, 0x0000, 0x10, 23, 3),
+	PIN_FIELD_BASE(18, 18, 6, 0x0000, 0x10, 26, 3),
+	PINS_FIELD_BASE(19, 20, 6, 0x0000, 0x10, 23, 3),
+	PINS_FIELD_BASE(21, 23, 6, 0x0000, 0x10, 29, 3),
+	PIN_FIELD_BASE(24, 24, 6, 0x0010, 0x10, 0, 3),
+	PINS_FIELD_BASE(25, 27, 6, 0x0000, 0x10, 17, 3),
+	PIN_FIELD_BASE(28, 28, 6, 0x0000, 0x10, 20, 3),
+	PIN_FIELD_BASE(29, 29, 6, 0x0000, 0x10, 0, 3),
+	PIN_FIELD_BASE(30, 30, 6, 0x0000, 0x10, 3, 3),
+	PINS_FIELD_BASE(31, 34, 6, 0x0000, 0x10, 6, 3),
+	PINS_FIELD_BASE(35, 36, 6, 0x0000, 0x10, 13, 2),
+	PIN_FIELD_BASE(37, 37, 6, 0x0000, 0x10, 15, 2),
+	PIN_FIELD_BASE(38, 38, 6, 0x0000, 0x10, 11, 2),
+	PINS_FIELD_BASE(39, 40, 6, 0x0000, 0x10, 9, 2),
+	PINS_FIELD_BASE(41, 42, 7, 0x0000, 0x10, 21, 3),
+	PIN_FIELD_BASE(43, 43, 7, 0x0000, 0x10, 9, 3),
+	PIN_FIELD_BASE(44, 44, 7, 0x0000, 0x10, 12, 3),
+	PIN_FIELD_BASE(45, 45, 7, 0x0000, 0x10, 27, 3),
+	PINS_FIELD_BASE(46, 47, 7, 0x0000, 0x10, 24, 3),
+	PINS_FIELD_BASE(48, 49, 7, 0x0010, 0x10, 18, 3),
+	PINS_FIELD_BASE(50, 51, 7, 0x0010, 0x10, 15, 3),
+	PINS_FIELD_BASE(52, 57, 7, 0x0000, 0x10, 0, 3),
+	PINS_FIELD_BASE(58, 60, 7, 0x0010, 0x10, 9, 3),
+	PINS_FIELD_BASE(61, 62, 3, 0x0000, 0x10, 15, 3),
+	PINS_FIELD_BASE(63, 64, 3, 0x0000, 0x10, 12, 3),
+	PINS_FIELD_BASE(65, 66, 3, 0x0000, 0x10, 21, 3),
+	PINS_FIELD_BASE(67, 68, 3, 0x0000, 0x10, 18, 3),
+	PINS_FIELD_BASE(69, 73, 3, 0x0000, 0x10, 3, 3),
+	PINS_FIELD_BASE(74, 78, 3, 0x0000, 0x10, 6, 3),
+	PINS_FIELD_BASE(79, 80, 3, 0x0000, 0x10, 0, 3),
+	PIN_FIELD_BASE(81, 81, 3, 0x0010, 0x10, 0, 3),
+	PINS_FIELD_BASE(82, 83, 3, 0x0000, 0x10, 27, 3),
+	PIN_FIELD_BASE(84, 84, 3, 0x0010, 0x10, 0, 3),
+	PIN_FIELD_BASE(85, 85, 7, 0x0010, 0x10, 9, 3),
+	PIN_FIELD_BASE(86, 86, 7, 0x0010, 0x10, 12, 3),
+	PIN_FIELD_BASE(87, 87, 7, 0x0000, 0x10, 6, 3),
+	PIN_FIELD_BASE(88, 88, 7, 0x0000, 0x10, 3, 3),
+	PIN_FIELD_BASE(89, 89, 2, 0x0010, 0x10, 15, 3),
+	PIN_FIELD_BASE(90, 90, 3, 0x0000, 0x10, 24, 3),
+	PIN_FIELD_BASE(91, 91, 2, 0x0010, 0x10, 6, 3),
+	PIN_FIELD_BASE(92, 92, 2, 0x0010, 0x10, 3, 3),
+	PIN_FIELD_BASE(93, 93, 2, 0x0000, 0x10, 27, 3),
+	PIN_FIELD_BASE(94, 94, 2, 0x0010, 0x10, 0, 3),
+	PINS_FIELD_BASE(95, 96, 2, 0x0010, 0x10, 18, 3),
+	PINS_FIELD_BASE(97, 98, 2, 0x0000, 0x10, 6, 3),
+	PIN_FIELD_BASE(99, 99, 2, 0x0000, 0x10, 0, 3),
+	PIN_FIELD_BASE(100, 100, 2, 0x0000, 0x10, 3, 3),
+	PINS_FIELD_BASE(101, 102, 2, 0x0000, 0x10, 9, 3),
+	PINS_FIELD_BASE(103, 104, 2, 0x0010, 0x10, 9, 3),
+	PINS_FIELD_BASE(105, 106, 2, 0x0010, 0x10, 12, 3),
+	PIN_FIELD_BASE(107, 107, 1, 0x0000, 0x10, 12, 3),
+	PIN_FIELD_BASE(108, 108, 1, 0x0000, 0x10, 9, 3),
+	PIN_FIELD_BASE(109, 109, 1, 0x0000, 0x10, 15, 3),
+	PIN_FIELD_BASE(110, 110, 1, 0x0000, 0x10, 0, 3),
+	PIN_FIELD_BASE(111, 111, 1, 0x0000, 0x10, 3, 3),
+	PIN_FIELD_BASE(112, 112, 1, 0x0000, 0x10, 6, 3),
+	PIN_FIELD_BASE(113, 113, 1, 0x0000, 0x10, 27, 3),
+	PIN_FIELD_BASE(114, 114, 1, 0x0010, 0x10, 0, 3),
+	PIN_FIELD_BASE(115, 115, 1, 0x0000, 0x10, 18, 3),
+	PIN_FIELD_BASE(116, 116, 1, 0x0000, 0x10, 21, 3),
+	PIN_FIELD_BASE(117, 117, 1, 0x0010, 0x10, 6, 3),
+	PIN_FIELD_BASE(118, 118, 1, 0x0010, 0x10, 9, 3),
+	PIN_FIELD_BASE(119, 119, 1, 0x0010, 0x10, 12, 3),
+	PIN_FIELD_BASE(120, 120, 1, 0x0010, 0x10, 3, 3),
+	PIN_FIELD_BASE(121, 121, 1, 0x0000, 0x10, 24, 3),
+	PIN_FIELD_BASE(122, 122, 4, 0x0000, 0x10, 9, 3),
+	PIN_FIELD_BASE(123, 123, 4, 0x0000, 0x10, 12, 3),
+	PIN_FIELD_BASE(124, 124, 4, 0x0000, 0x10, 6, 3),
+	PINS_FIELD_BASE(125, 130, 4, 0x0000, 0x10, 12, 3),
+	PIN_FIELD_BASE(131, 131, 4, 0x0000, 0x10, 15, 3),
+	PIN_FIELD_BASE(132, 132, 4, 0x0000, 0x10, 12, 3),
+	PIN_FIELD_BASE(133, 133, 4, 0x0000, 0x10, 18, 3),
+	PIN_FIELD_BASE(134, 134, 5, 0x0010, 0x10, 6, 3),
+	PIN_FIELD_BASE(135, 135, 5, 0x0010, 0x10, 12, 3),
+	PIN_FIELD_BASE(136, 136, 5, 0x0000, 0x10, 3, 3),
+	PIN_FIELD_BASE(137, 137, 5, 0x0000, 0x10, 21, 3),
+	PIN_FIELD_BASE(138, 138, 5, 0x0000, 0x10, 12, 3),
+	PIN_FIELD_BASE(139, 139, 5, 0x0000, 0x10, 15, 3),
+	PIN_FIELD_BASE(140, 140, 5, 0x0000, 0x10, 0, 3),
+	PIN_FIELD_BASE(141, 141, 5, 0x0000, 0x10, 18, 3),
+	PIN_FIELD_BASE(142, 142, 5, 0x0000, 0x10, 6, 3),
+	PIN_FIELD_BASE(143, 143, 5, 0x0000, 0x10, 9, 3),
+	PINS_FIELD_BASE(144, 146, 5, 0x0010, 0x10, 0, 3),
+	PIN_FIELD_BASE(147, 147, 5, 0x0010, 0x10, 3, 3),
+	PINS_FIELD_BASE(148, 149, 5, 0x0010, 0x10, 9, 3),
+	PINS_FIELD_BASE(150, 151, 7, 0x0010, 0x10, 0, 3),
+	PINS_FIELD_BASE(152, 153, 7, 0x0010, 0x10, 3, 3),
+	PIN_FIELD_BASE(154, 154, 7, 0x0010, 0x10, 6, 3),
+	PINS_FIELD_BASE(155, 157, 3, 0x0010, 0x10, 3, 3),
+	PIN_FIELD_BASE(158, 158, 3, 0x0010, 0x10, 6, 3),
+	PIN_FIELD_BASE(159, 159, 7, 0x0010, 0x10, 6, 3),
+	PIN_FIELD_BASE(160, 160, 5, 0x0000, 0x10, 24, 3),
+	PINS_FIELD_BASE(161, 162, 1, 0x0010, 0x10, 15, 3),
+	PINS_FIELD_BASE(163, 166, 4, 0x0000, 0x10, 0, 3),
+	PINS_FIELD_BASE(167, 170, 4, 0x0000, 0x10, 3, 3),
+	PINS_FIELD_BASE(171, 174, 7, 0x0000, 0x10, 18, 3),
+	PINS_FIELD_BASE(175, 179, 7, 0x0000, 0x10, 15, 3),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_pupd_range[] = {
+	PINS_FIELD_BASE(0, 28, 0, 0x0050, 0x10, 18, 1),
+	PIN_FIELD_BASE(29, 29, 6, 0x0050, 0x10, 0, 1),
+	PIN_FIELD_BASE(30, 30, 6, 0x0050, 0x10, 1, 1),
+	PIN_FIELD_BASE(31, 31, 6, 0x0050, 0x10, 5, 1),
+	PIN_FIELD_BASE(32, 32, 6, 0x0050, 0x10, 2, 1),
+	PIN_FIELD_BASE(33, 33, 6, 0x0050, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, 6, 0x0050, 0x10, 3, 1),
+	PIN_FIELD_BASE(35, 35, 6, 0x0050, 0x10, 10, 1),
+	PIN_FIELD_BASE(36, 36, 6, 0x0050, 0x10, 11, 1),
+	PIN_FIELD_BASE(37, 37, 6, 0x0050, 0x10, 9, 1),
+	PIN_FIELD_BASE(38, 38, 6, 0x0050, 0x10, 6, 1),
+	PIN_FIELD_BASE(39, 39, 6, 0x0050, 0x10, 8, 1),
+	PINS_FIELD_BASE(40, 90, 6, 0x0050, 0x10, 7, 1),
+	PIN_FIELD_BASE(91, 91, 2, 0x0050, 0x10, 3, 1),
+	PIN_FIELD_BASE(92, 92, 2, 0x0050, 0x10, 2, 1),
+	PIN_FIELD_BASE(93, 93, 2, 0x0050, 0x10, 0, 1),
+	PINS_FIELD_BASE(94, 121, 2, 0x0050, 0x10, 1, 1),
+	PIN_FIELD_BASE(122, 122, 4, 0x0030, 0x10, 1, 1),
+	PIN_FIELD_BASE(123, 123, 4, 0x0030, 0x10, 2, 1),
+	PIN_FIELD_BASE(124, 124, 4, 0x0030, 0x10, 0, 1),
+	PIN_FIELD_BASE(125, 125, 4, 0x0030, 0x10, 4, 1),
+	PIN_FIELD_BASE(126, 126, 4, 0x0030, 0x10, 6, 1),
+	PIN_FIELD_BASE(127, 127, 4, 0x0030, 0x10, 8, 1),
+	PIN_FIELD_BASE(128, 128, 4, 0x0030, 0x10, 3, 1),
+	PIN_FIELD_BASE(129, 129, 4, 0x0030, 0x10, 7, 1),
+	PIN_FIELD_BASE(130, 130, 4, 0x0030, 0x10, 9, 1),
+	PIN_FIELD_BASE(131, 131, 4, 0x0030, 0x10, 10, 1),
+	PIN_FIELD_BASE(132, 132, 4, 0x0030, 0x10, 5, 1),
+	PINS_FIELD_BASE(133, 179, 4, 0x0030, 0x10, 11, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_r0_range[] = {
+	PINS_FIELD_BASE(0, 28, 4, 0x0030, 0x10, 11, 1),
+	PIN_FIELD_BASE(29, 29, 6, 0x0070, 0x10, 0, 1),
+	PIN_FIELD_BASE(30, 30, 6, 0x0070, 0x10, 1, 1),
+	PIN_FIELD_BASE(31, 31, 6, 0x0070, 0x10, 5, 1),
+	PIN_FIELD_BASE(32, 32, 6, 0x0070, 0x10, 2, 1),
+	PIN_FIELD_BASE(33, 33, 6, 0x0070, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, 6, 0x0070, 0x10, 3, 1),
+	PIN_FIELD_BASE(35, 35, 6, 0x0070, 0x10, 10, 1),
+	PIN_FIELD_BASE(36, 36, 6, 0x0070, 0x10, 11, 1),
+	PIN_FIELD_BASE(37, 37, 6, 0x0070, 0x10, 9, 1),
+	PIN_FIELD_BASE(38, 38, 6, 0x0070, 0x10, 6, 1),
+	PIN_FIELD_BASE(39, 39, 6, 0x0070, 0x10, 8, 1),
+	PINS_FIELD_BASE(40, 90, 6, 0x0070, 0x10, 7, 1),
+	PIN_FIELD_BASE(91, 91, 2, 0x0070, 0x10, 3, 1),
+	PIN_FIELD_BASE(92, 92, 2, 0x0070, 0x10, 2, 1),
+	PIN_FIELD_BASE(93, 93, 2, 0x0070, 0x10, 0, 1),
+	PINS_FIELD_BASE(94, 121, 2, 0x0070, 0x10, 1, 1),
+	PIN_FIELD_BASE(122, 122, 4, 0x0050, 0x10, 1, 1),
+	PIN_FIELD_BASE(123, 123, 4, 0x0050, 0x10, 2, 1),
+	PIN_FIELD_BASE(124, 124, 4, 0x0050, 0x10, 0, 1),
+	PIN_FIELD_BASE(125, 125, 4, 0x0050, 0x10, 4, 1),
+	PIN_FIELD_BASE(126, 126, 4, 0x0050, 0x10, 6, 1),
+	PIN_FIELD_BASE(127, 127, 4, 0x0050, 0x10, 8, 1),
+	PIN_FIELD_BASE(128, 128, 4, 0x0050, 0x10, 3, 1),
+	PIN_FIELD_BASE(129, 129, 4, 0x0050, 0x10, 7, 1),
+	PIN_FIELD_BASE(130, 130, 4, 0x0050, 0x10, 9, 1),
+	PIN_FIELD_BASE(131, 131, 4, 0x0050, 0x10, 10, 1),
+	PIN_FIELD_BASE(132, 132, 4, 0x0050, 0x10, 5, 1),
+	PINS_FIELD_BASE(133, 179, 4, 0x0050, 0x10, 11, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_r1_range[] = {
+	PINS_FIELD_BASE(0, 28, 4, 0x0050, 0x10, 11, 1),
+	PIN_FIELD_BASE(29, 29, 6, 0x0080, 0x10, 0, 1),
+	PIN_FIELD_BASE(30, 30, 6, 0x0080, 0x10, 1, 1),
+	PIN_FIELD_BASE(31, 31, 6, 0x0080, 0x10, 5, 1),
+	PIN_FIELD_BASE(32, 32, 6, 0x0080, 0x10, 2, 1),
+	PIN_FIELD_BASE(33, 33, 6, 0x0080, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, 6, 0x0080, 0x10, 3, 1),
+	PIN_FIELD_BASE(35, 35, 6, 0x0080, 0x10, 10, 1),
+	PIN_FIELD_BASE(36, 36, 6, 0x0080, 0x10, 11, 1),
+	PIN_FIELD_BASE(37, 37, 6, 0x0080, 0x10, 9, 1),
+	PIN_FIELD_BASE(38, 38, 6, 0x0080, 0x10, 6, 1),
+	PIN_FIELD_BASE(39, 39, 6, 0x0080, 0x10, 8, 1),
+	PINS_FIELD_BASE(40, 90, 6, 0x0080, 0x10, 7, 1),
+	PIN_FIELD_BASE(91, 91, 2, 0x0080, 0x10, 3, 1),
+	PIN_FIELD_BASE(92, 92, 2, 0x0080, 0x10, 2, 1),
+	PIN_FIELD_BASE(93, 93, 2, 0x0080, 0x10, 0, 1),
+	PINS_FIELD_BASE(94, 121, 2, 0x0080, 0x10, 1, 1),
+	PIN_FIELD_BASE(122, 122, 4, 0x0060, 0x10, 1, 1),
+	PIN_FIELD_BASE(123, 123, 4, 0x0060, 0x10, 2, 1),
+	PIN_FIELD_BASE(124, 124, 4, 0x0060, 0x10, 0, 1),
+	PIN_FIELD_BASE(125, 125, 4, 0x0060, 0x10, 4, 1),
+	PIN_FIELD_BASE(126, 126, 4, 0x0060, 0x10, 6, 1),
+	PIN_FIELD_BASE(127, 127, 4, 0x0060, 0x10, 8, 1),
+	PIN_FIELD_BASE(128, 128, 4, 0x0060, 0x10, 3, 1),
+	PIN_FIELD_BASE(129, 129, 4, 0x0060, 0x10, 7, 1),
+	PIN_FIELD_BASE(130, 130, 4, 0x0060, 0x10, 9, 1),
+	PIN_FIELD_BASE(131, 131, 4, 0x0060, 0x10, 10, 1),
+	PIN_FIELD_BASE(132, 132, 4, 0x0060, 0x10, 5, 1),
+	PINS_FIELD_BASE(133, 179, 4, 0x0060, 0x10, 11, 1),
+};
+
+static const struct mtk_pin_field_calc mt6765_pin_ies_range[] = {
+	PIN_FIELD_BASE(0, 0, 2, 0x0030, 0x10, 6, 1),
+	PIN_FIELD_BASE(1, 1, 2, 0x0030, 0x10, 7, 1),
+	PIN_FIELD_BASE(2, 2, 2, 0x0030, 0x10, 10, 1),
+	PIN_FIELD_BASE(3, 3, 2, 0x0030, 0x10, 11, 1),
+	PIN_FIELD_BASE(4, 4, 2, 0x0030, 0x10, 12, 1),
+	PIN_FIELD_BASE(5, 5, 2, 0x0030, 0x10, 13, 1),
+	PIN_FIELD_BASE(6, 6, 2, 0x0030, 0x10, 14, 1),
+	PIN_FIELD_BASE(7, 7, 2, 0x0030, 0x10, 15, 1),
+	PIN_FIELD_BASE(8, 8, 3, 0x0030, 0x10, 12, 1),
+	PIN_FIELD_BASE(9, 9, 2, 0x0030, 0x10, 16, 1),
+	PIN_FIELD_BASE(10, 10, 2, 0x0030, 0x10, 8, 1),
+	PIN_FIELD_BASE(11, 11, 2, 0x0030, 0x10, 9, 1),
+	PIN_FIELD_BASE(12, 12, 5, 0x0020, 0x10, 9, 1),
+	PIN_FIELD_BASE(13, 13, 6, 0x0020, 0x10, 26, 1),
+	PIN_FIELD_BASE(14, 14, 6, 0x0020, 0x10, 25, 1),
+	PIN_FIELD_BASE(15, 15, 6, 0x0020, 0x10, 27, 1),
+	PIN_FIELD_BASE(16, 16, 6, 0x0020, 0x10, 24, 1),
+	PIN_FIELD_BASE(17, 17, 6, 0x0020, 0x10, 19, 1),
+	PIN_FIELD_BASE(18, 18, 6, 0x0020, 0x10, 16, 1),
+	PIN_FIELD_BASE(19, 19, 6, 0x0020, 0x10, 18, 1),
+	PIN_FIELD_BASE(20, 20, 6, 0x0020, 0x10, 17, 1),
+	PIN_FIELD_BASE(21, 21, 6, 0x0020, 0x10, 22, 1),
+	PIN_FIELD_BASE(22, 22, 6, 0x0020, 0x10, 21, 1),
+	PIN_FIELD_BASE(23, 23, 6, 0x0020, 0x10, 23, 1),
+	PIN_FIELD_BASE(24, 24, 6, 0x0020, 0x10, 20, 1),
+	PIN_FIELD_BASE(25, 25, 6, 0x0020, 0x10, 14, 1),
+	PIN_FIELD_BASE(26, 26, 6, 0x0020, 0x10, 13, 1),
+	PIN_FIELD_BASE(27, 27, 6, 0x0020, 0x10, 15, 1),
+	PIN_FIELD_BASE(28, 28, 6, 0x0020, 0x10, 12, 1),
+	PIN_FIELD_BASE(29, 29, 6, 0x0020, 0x10, 0, 1),
+	PIN_FIELD_BASE(30, 30, 6, 0x0020, 0x10, 1, 1),
+	PIN_FIELD_BASE(31, 31, 6, 0x0020, 0x10, 5, 1),
+	PIN_FIELD_BASE(32, 32, 6, 0x0020, 0x10, 2, 1),
+	PIN_FIELD_BASE(33, 33, 6, 0x0020, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, 6, 0x0020, 0x10, 3, 1),
+	PIN_FIELD_BASE(35, 35, 6, 0x0020, 0x10, 10, 1),
+	PIN_FIELD_BASE(36, 36, 6, 0x0020, 0x10, 11, 1),
+	PIN_FIELD_BASE(37, 37, 6, 0x0020, 0x10, 9, 1),
+	PIN_FIELD_BASE(38, 38, 6, 0x0020, 0x10, 6, 1),
+	PIN_FIELD_BASE(39, 39, 6, 0x0020, 0x10, 8, 1),
+	PIN_FIELD_BASE(40, 40, 6, 0x0020, 0x10, 7, 1),
+	PIN_FIELD_BASE(41, 41, 7, 0x0040, 0x10, 19, 1),
+	PIN_FIELD_BASE(42, 42, 7, 0x0040, 0x10, 9, 1),
+	PIN_FIELD_BASE(43, 43, 7, 0x0040, 0x10, 8, 1),
+	PIN_FIELD_BASE(44, 44, 7, 0x0040, 0x10, 10, 1),
+	PIN_FIELD_BASE(45, 45, 7, 0x0040, 0x10, 22, 1),
+	PIN_FIELD_BASE(46, 46, 7, 0x0040, 0x10, 21, 1),
+	PIN_FIELD_BASE(47, 47, 7, 0x0040, 0x10, 20, 1),
+	PIN_FIELD_BASE(48, 48, 7, 0x0050, 0x10, 3, 1),
+	PIN_FIELD_BASE(49, 49, 7, 0x0050, 0x10, 5, 1),
+	PIN_FIELD_BASE(50, 50, 7, 0x0050, 0x10, 2, 1),
+	PIN_FIELD_BASE(51, 51, 7, 0x0050, 0x10, 4, 1),
+	PIN_FIELD_BASE(52, 52, 7, 0x0040, 0x10, 1, 1),
+	PIN_FIELD_BASE(53, 53, 7, 0x0040, 0x10, 0, 1),
+	PIN_FIELD_BASE(54, 54, 7, 0x0040, 0x10, 5, 1),
+	PIN_FIELD_BASE(55, 55, 7, 0x0040, 0x10, 3, 1),
+	PIN_FIELD_BASE(56, 56, 7, 0x0040, 0x10, 4, 1),
+	PIN_FIELD_BASE(57, 57, 7, 0x0040, 0x10, 2, 1),
+	PIN_FIELD_BASE(58, 58, 7, 0x0050, 0x10, 0, 1),
+	PIN_FIELD_BASE(59, 59, 7, 0x0040, 0x10, 31, 1),
+	PIN_FIELD_BASE(60, 60, 7, 0x0040, 0x10, 30, 1),
+	PIN_FIELD_BASE(61, 61, 3, 0x0030, 0x10, 18, 1),
+	PIN_FIELD_BASE(62, 62, 3, 0x0030, 0x10, 14, 1),
+	PIN_FIELD_BASE(63, 63, 3, 0x0030, 0x10, 17, 1),
+	PIN_FIELD_BASE(64, 64, 3, 0x0030, 0x10, 13, 1),
+	PIN_FIELD_BASE(65, 65, 3, 0x0030, 0x10, 20, 1),
+	PIN_FIELD_BASE(66, 66, 3, 0x0030, 0x10, 16, 1),
+	PIN_FIELD_BASE(67, 67, 3, 0x0030, 0x10, 19, 1),
+	PIN_FIELD_BASE(68, 68, 3, 0x0030, 0x10, 15, 1),
+	PIN_FIELD_BASE(69, 69, 3, 0x0030, 0x10, 8, 1),
+	PIN_FIELD_BASE(70, 70, 3, 0x0030, 0x10, 7, 1),
+	PIN_FIELD_BASE(71, 71, 3, 0x0030, 0x10, 6, 1),
+	PIN_FIELD_BASE(72, 72, 3, 0x0030, 0x10, 5, 1),
+	PIN_FIELD_BASE(73, 73, 3, 0x0030, 0x10, 4, 1),
+	PIN_FIELD_BASE(74, 74, 3, 0x0030, 0x10, 3, 1),
+	PIN_FIELD_BASE(75, 75, 3, 0x0030, 0x10, 2, 1),
+	PIN_FIELD_BASE(76, 76, 3, 0x0030, 0x10, 1, 1),
+	PIN_FIELD_BASE(77, 77, 3, 0x0030, 0x10, 0, 1),
+	PIN_FIELD_BASE(78, 78, 3, 0x0030, 0x10, 9, 1),
+	PIN_FIELD_BASE(79, 79, 3, 0x0030, 0x10, 11, 1),
+	PIN_FIELD_BASE(80, 80, 3, 0x0030, 0x10, 10, 1),
+	PIN_FIELD_BASE(81, 81, 3, 0x0030, 0x10, 25, 1),
+	PIN_FIELD_BASE(82, 82, 3, 0x0030, 0x10, 24, 1),
+	PIN_FIELD_BASE(83, 83, 3, 0x0030, 0x10, 22, 1),
+	PIN_FIELD_BASE(84, 84, 3, 0x0030, 0x10, 23, 1),
+	PIN_FIELD_BASE(85, 85, 7, 0x0050, 0x10, 1, 1),
+	PIN_FIELD_BASE(86, 86, 7, 0x0040, 0x10, 29, 1),
+	PIN_FIELD_BASE(87, 87, 7, 0x0040, 0x10, 7, 1),
+	PIN_FIELD_BASE(88, 88, 7, 0x0040, 0x10, 6, 1),
+	PIN_FIELD_BASE(89, 89, 2, 0x0030, 0x10, 25, 1),
+	PIN_FIELD_BASE(90, 90, 3, 0x0030, 0x10, 21, 1),
+	PIN_FIELD_BASE(91, 91, 2, 0x0030, 0x10, 20, 1),
+	PIN_FIELD_BASE(92, 92, 2, 0x0030, 0x10, 19, 1),
+	PIN_FIELD_BASE(93, 93, 2, 0x0030, 0x10, 17, 1),
+	PIN_FIELD_BASE(94, 94, 2, 0x0030, 0x10, 18, 1),
+	PIN_FIELD_BASE(95, 95, 2, 0x0030, 0x10, 26, 1),
+	PIN_FIELD_BASE(96, 96, 2, 0x0030, 0x10, 27, 1),
+	PIN_FIELD_BASE(97, 97, 2, 0x0030, 0x10, 2, 1),
+	PIN_FIELD_BASE(98, 98, 2, 0x0030, 0x10, 3, 1),
+	PIN_FIELD_BASE(99, 99, 2, 0x0030, 0x10, 0, 1),
+	PIN_FIELD_BASE(100, 100, 2, 0x0030, 0x10, 1, 1),
+	PIN_FIELD_BASE(101, 101, 2, 0x0030, 0x10, 4, 1),
+	PIN_FIELD_BASE(102, 102, 2, 0x0030, 0x10, 5, 1),
+	PIN_FIELD_BASE(103, 103, 2, 0x0030, 0x10, 21, 1),
+	PIN_FIELD_BASE(104, 104, 2, 0x0030, 0x10, 23, 1),
+	PIN_FIELD_BASE(105, 105, 2, 0x0030, 0x10, 22, 1),
+	PIN_FIELD_BASE(106, 106, 2, 0x0030, 0x10, 24, 1),
+	PIN_FIELD_BASE(107, 107, 1, 0x0030, 0x10, 4, 1),
+	PIN_FIELD_BASE(108, 108, 1, 0x0030, 0x10, 3, 1),
+	PIN_FIELD_BASE(109, 109, 1, 0x0030, 0x10, 5, 1),
+	PIN_FIELD_BASE(110, 110, 1, 0x0030, 0x10, 0, 1),
+	PIN_FIELD_BASE(111, 111, 1, 0x0030, 0x10, 1, 1),
+	PIN_FIELD_BASE(112, 112, 1, 0x0030, 0x10, 2, 1),
+	PIN_FIELD_BASE(113, 113, 1, 0x0030, 0x10, 9, 1),
+	PIN_FIELD_BASE(114, 114, 1, 0x0030, 0x10, 10, 1),
+	PIN_FIELD_BASE(115, 115, 1, 0x0030, 0x10, 6, 1),
+	PIN_FIELD_BASE(116, 116, 1, 0x0030, 0x10, 7, 1),
+	PIN_FIELD_BASE(117, 117, 1, 0x0030, 0x10, 12, 1),
+	PIN_FIELD_BASE(118, 118, 1, 0x0030, 0x10, 13, 1),
+	PIN_FIELD_BASE(119, 119, 1, 0x0030, 0x10, 14, 1),
+	PIN_FIELD_BASE(120, 120, 1, 0x0030, 0x10, 11, 1),
+	PIN_FIELD_BASE(121, 121, 1, 0x0030, 0x10, 8, 1),
+	PIN_FIELD_BASE(122, 122, 4, 0x0010, 0x10, 9, 1),
+	PIN_FIELD_BASE(123, 123, 4, 0x0010, 0x10, 10, 1),
+	PIN_FIELD_BASE(124, 124, 4, 0x0010, 0x10, 8, 1),
+	PIN_FIELD_BASE(125, 125, 4, 0x0010, 0x10, 12, 1),
+	PIN_FIELD_BASE(126, 126, 4, 0x0010, 0x10, 14, 1),
+	PIN_FIELD_BASE(127, 127, 4, 0x0010, 0x10, 16, 1),
+	PIN_FIELD_BASE(128, 128, 4, 0x0010, 0x10, 11, 1),
+	PIN_FIELD_BASE(129, 129, 4, 0x0010, 0x10, 15, 1),
+	PIN_FIELD_BASE(130, 130, 4, 0x0010, 0x10, 17, 1),
+	PIN_FIELD_BASE(131, 131, 4, 0x0010, 0x10, 18, 1),
+	PIN_FIELD_BASE(132, 132, 4, 0x0010, 0x10, 13, 1),
+	PIN_FIELD_BASE(133, 133, 4, 0x0010, 0x10, 19, 1),
+	PIN_FIELD_BASE(134, 134, 5, 0x0020, 0x10, 14, 1),
+	PIN_FIELD_BASE(135, 135, 5, 0x0020, 0x10, 17, 1),
+	PIN_FIELD_BASE(136, 136, 5, 0x0020, 0x10, 1, 1),
+	PIN_FIELD_BASE(137, 137, 5, 0x0020, 0x10, 7, 1),
+	PIN_FIELD_BASE(138, 138, 5, 0x0020, 0x10, 4, 1),
+	PIN_FIELD_BASE(139, 139, 5, 0x0020, 0x10, 5, 1),
+	PIN_FIELD_BASE(140, 140, 5, 0x0020, 0x10, 0, 1),
+	PIN_FIELD_BASE(141, 141, 5, 0x0020, 0x10, 6, 1),
+	PIN_FIELD_BASE(142, 142, 5, 0x0020, 0x10, 2, 1),
+	PIN_FIELD_BASE(143, 143, 5, 0x0020, 0x10, 3, 1),
+	PIN_FIELD_BASE(144, 144, 5, 0x0020, 0x10, 12, 1),
+	PIN_FIELD_BASE(145, 145, 5, 0x0020, 0x10, 11, 1),
+	PIN_FIELD_BASE(146, 146, 5, 0x0020, 0x10, 13, 1),
+	PIN_FIELD_BASE(147, 147, 5, 0x0020, 0x10, 10, 1),
+	PIN_FIELD_BASE(148, 148, 5, 0x0020, 0x10, 15, 1),
+	PIN_FIELD_BASE(149, 149, 5, 0x0020, 0x10, 16, 1),
+	PIN_FIELD_BASE(150, 150, 7, 0x0040, 0x10, 23, 1),
+	PIN_FIELD_BASE(151, 151, 7, 0x0040, 0x10, 24, 1),
+	PIN_FIELD_BASE(152, 152, 7, 0x0040, 0x10, 25, 1),
+	PIN_FIELD_BASE(153, 153, 7, 0x0040, 0x10, 26, 1),
+	PIN_FIELD_BASE(154, 154, 7, 0x0040, 0x10, 28, 1),
+	PIN_FIELD_BASE(155, 155, 3, 0x0030, 0x10, 28, 1),
+	PIN_FIELD_BASE(156, 156, 3, 0x0030, 0x10, 27, 1),
+	PIN_FIELD_BASE(157, 157, 3, 0x0030, 0x10, 29, 1),
+	PIN_FIELD_BASE(158, 158, 3, 0x0030, 0x10, 26, 1),
+	PIN_FIELD_BASE(159, 159, 7, 0x0040, 0x10, 27, 1),
+	PIN_FIELD_BASE(160, 160, 5, 0x0020, 0x10, 8, 1),
+	PIN_FIELD_BASE(161, 161, 1, 0x0030, 0x10, 15, 1),
+	PIN_FIELD_BASE(162, 162, 1, 0x0030, 0x10, 16, 1),
+	PIN_FIELD_BASE(163, 163, 4, 0x0010, 0x10, 0, 1),
+	PIN_FIELD_BASE(164, 164, 4, 0x0010, 0x10, 1, 1),
+	PIN_FIELD_BASE(165, 165, 4, 0x0010, 0x10, 2, 1),
+	PIN_FIELD_BASE(166, 166, 4, 0x0010, 0x10, 3, 1),
+	PIN_FIELD_BASE(167, 167, 4, 0x0010, 0x10, 4, 1),
+	PIN_FIELD_BASE(168, 168, 4, 0x0010, 0x10, 5, 1),
+	PIN_FIELD_BASE(169, 169, 4, 0x0010, 0x10, 6, 1),
+	PIN_FIELD_BASE(170, 170, 4, 0x0010, 0x10, 7, 1),
+	PIN_FIELD_BASE(171, 171, 7, 0x0040, 0x10, 17, 1),
+	PIN_FIELD_BASE(172, 172, 7, 0x0040, 0x10, 18, 1),
+	PIN_FIELD_BASE(173, 173, 7, 0x0040, 0x10, 11, 1),
+	PIN_FIELD_BASE(174, 174, 7, 0x0040, 0x10, 12, 1),
+	PIN_FIELD_BASE(175, 175, 7, 0x0040, 0x10, 13, 1),
+	PIN_FIELD_BASE(176, 176, 7, 0x0040, 0x10, 14, 1),
+	PIN_FIELD_BASE(177, 177, 7, 0x0040, 0x10, 15, 1),
+	PINS_FIELD_BASE(178, 179, 7, 0x0040, 0x10, 16, 1),
+};
+
+static const struct mtk_pin_reg_calc mt6765_reg_cals[PINCTRL_PIN_REG_MAX] = {
+	[PINCTRL_PIN_REG_MODE] = MTK_RANGE(mt6765_pin_mode_range),
+	[PINCTRL_PIN_REG_DIR] = MTK_RANGE(mt6765_pin_dir_range),
+	[PINCTRL_PIN_REG_DI] = MTK_RANGE(mt6765_pin_di_range),
+	[PINCTRL_PIN_REG_DO] = MTK_RANGE(mt6765_pin_do_range),
+	[PINCTRL_PIN_REG_SMT] = MTK_RANGE(mt6765_pin_smt_range),
+	[PINCTRL_PIN_REG_PD] = MTK_RANGE(mt6765_pin_pd_range),
+	[PINCTRL_PIN_REG_PU] = MTK_RANGE(mt6765_pin_pu_range),
+	[PINCTRL_PIN_REG_TDSEL] = MTK_RANGE(mt6765_pin_tdsel_range),
+	[PINCTRL_PIN_REG_RDSEL] = MTK_RANGE(mt6765_pin_rdsel_range),
+	[PINCTRL_PIN_REG_DRV] = MTK_RANGE(mt6765_pin_drv_range),
+	[PINCTRL_PIN_REG_PUPD] = MTK_RANGE(mt6765_pin_pupd_range),
+	[PINCTRL_PIN_REG_R0] = MTK_RANGE(mt6765_pin_r0_range),
+	[PINCTRL_PIN_REG_R1] = MTK_RANGE(mt6765_pin_r1_range),
+	[PINCTRL_PIN_REG_IES] = MTK_RANGE(mt6765_pin_ies_range),
+};
+
+static const char * const mt6765_pinctrl_register_base_names[] = {
+	"iocfg0", "iocfg1", "iocfg2", "iocfg3", "iocfg4", "iocfg5",
+	"iocfg6", "iocfg7",
+};
+
+static const struct mtk_eint_hw mt6765_eint_hw = {
+	.port_mask = 7,
+	.ports     = 6,
+	.ap_num    = 160,
+	.db_cnt    = 13,
+};
+
+static const struct mtk_pin_soc mt6765_data = {
+	.reg_cal = mt6765_reg_cals,
+	.pins = mtk_pins_mt6765,
+	.npins = ARRAY_SIZE(mtk_pins_mt6765),
+	.ngrps = ARRAY_SIZE(mtk_pins_mt6765),
+	.eint_hw = &mt6765_eint_hw,
+	.gpio_m = 0,
+	.ies_present = true,
+	.base_names = mt6765_pinctrl_register_base_names,
+	.nbase_names = ARRAY_SIZE(mt6765_pinctrl_register_base_names),
+	.bias_disable_set = mtk_pinconf_bias_disable_set,
+	.bias_disable_get = mtk_pinconf_bias_disable_get,
+	.bias_set = mtk_pinconf_bias_set,
+	.bias_get = mtk_pinconf_bias_get,
+	.drive_set = mtk_pinconf_drive_set_rev1,
+	.drive_get = mtk_pinconf_drive_get_rev1,
+	.adv_pull_get = mtk_pinconf_adv_pull_get,
+	.adv_pull_set = mtk_pinconf_adv_pull_set,
+};
+
+static const struct of_device_id mt6765_pinctrl_of_match[] = {
+	{ .compatible = "mediatek,mt6765-pinctrl", },
+	{ }
+};
+
+static int mt6765_pinctrl_probe(struct platform_device *pdev)
+{
+	return mtk_paris_pinctrl_probe(pdev, &mt6765_data);
+}
+
+static struct platform_driver mt6765_pinctrl_driver = {
+	.driver = {
+		.name = "mt6765-pinctrl",
+		.of_match_table = mt6765_pinctrl_of_match,
+	},
+	.probe = mt6765_pinctrl_probe,
+};
+
+static int __init mt6765_pinctrl_init(void)
+{
+	return platform_driver_register(&mt6765_pinctrl_driver);
+}
+arch_initcall(mt6765_pinctrl_init);
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mt6797.c
@@ -0,0 +1,82 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Based on pinctrl-mt6765.c
+ *
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: ZH Chen <zh.chen@mediatek.com>
+ *
+ * Copyright (C) Manivannan Sadhasivam <manivannan.sadhasivam@linaro.org>
+ *
+ */
+
+#include "pinctrl-mtk-mt6797.h"
+#include "pinctrl-paris.h"
+
+/*
+ * MT6797 have multiple bases to program pin configuration listed as the below:
+ * gpio:0x10005000, iocfg[l]:0x10002000, iocfg[b]:0x10002400,
+ * iocfg[r]:0x10002800, iocfg[t]:0x10002C00.
+ * _i_base could be used to indicate what base the pin should be mapped into.
+ */
+
+static const struct mtk_pin_field_calc mt6797_pin_mode_range[] = {
+	PIN_FIELD(0, 261, 0x300, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_field_calc mt6797_pin_dir_range[] = {
+	PIN_FIELD(0, 261, 0x0, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt6797_pin_di_range[] = {
+	PIN_FIELD(0, 261, 0x200, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt6797_pin_do_range[] = {
+	PIN_FIELD(0, 261, 0x100, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_reg_calc mt6797_reg_cals[PINCTRL_PIN_REG_MAX] = {
+	[PINCTRL_PIN_REG_MODE] = MTK_RANGE(mt6797_pin_mode_range),
+	[PINCTRL_PIN_REG_DIR] = MTK_RANGE(mt6797_pin_dir_range),
+	[PINCTRL_PIN_REG_DI] = MTK_RANGE(mt6797_pin_di_range),
+	[PINCTRL_PIN_REG_DO] = MTK_RANGE(mt6797_pin_do_range),
+};
+
+static const char * const mt6797_pinctrl_register_base_names[] = {
+	"gpio", "iocfgl", "iocfgb", "iocfgr", "iocfgt",
+};
+
+static const struct mtk_pin_soc mt6797_data = {
+	.reg_cal = mt6797_reg_cals,
+	.pins = mtk_pins_mt6797,
+	.npins = ARRAY_SIZE(mtk_pins_mt6797),
+	.ngrps = ARRAY_SIZE(mtk_pins_mt6797),
+	.gpio_m = 0,
+	.base_names = mt6797_pinctrl_register_base_names,
+	.nbase_names = ARRAY_SIZE(mt6797_pinctrl_register_base_names),
+};
+
+static const struct of_device_id mt6797_pinctrl_of_match[] = {
+	{ .compatible = "mediatek,mt6797-pinctrl", },
+	{ }
+};
+
+static int mt6797_pinctrl_probe(struct platform_device *pdev)
+{
+	return mtk_paris_pinctrl_probe(pdev, &mt6797_data);
+}
+
+static struct platform_driver mt6797_pinctrl_driver = {
+	.driver = {
+		.name = "mt6797-pinctrl",
+		.of_match_table = mt6797_pinctrl_of_match,
+	},
+	.probe = mt6797_pinctrl_probe,
+};
+
+static int __init mt6797_pinctrl_init(void)
+{
+	return platform_driver_register(&mt6797_pinctrl_driver);
+}
+arch_initcall(mt6797_pinctrl_init);
--- a/drivers/pinctrl/mediatek/pinctrl-mt7622.c
+++ b/drivers/pinctrl/mediatek/pinctrl-mt7622.c
@@ -1,297 +1,140 @@
+// SPDX-License-Identifier: GPL-2.0
 /*
- * MediaTek MT7622 Pinctrl Driver
+ * Copyright (C) 2017-2018 MediaTek Inc.
  *
- * Copyright (C) 2017 Sean Wang <sean.wang@mediatek.com>
+ * Author: Sean Wang <sean.wang@mediatek.com>
  *
- * This program is free software; you can redistribute it and/or modify
- * it under the terms of the GNU General Public License version 2 as
- * published by the Free Software Foundation.
- *
- * This program is distributed in the hope that it will be useful,
- * but WITHOUT ANY WARRANTY; without even the implied warranty of
- * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
- * GNU General Public License for more details.
- */
-
-#include <linux/gpio.h>
-#include <linux/gpio/driver.h>
-#include <linux/io.h>
-#include <linux/init.h>
-#include <linux/mfd/syscon.h>
-#include <linux/of.h>
-#include <linux/of_irq.h>
-#include <linux/of_platform.h>
-#include <linux/platform_device.h>
-#include <linux/pinctrl/pinctrl.h>
-#include <linux/pinctrl/pinmux.h>
-#include <linux/pinctrl/pinconf.h>
-#include <linux/pinctrl/pinconf-generic.h>
-#include <linux/regmap.h>
-
-#include "../core.h"
-#include "../pinconf.h"
-#include "../pinmux.h"
-#include "mtk-eint.h"
-
-#define PINCTRL_PINCTRL_DEV		KBUILD_MODNAME
-#define MTK_RANGE(_a)		{ .range = (_a), .nranges = ARRAY_SIZE(_a), }
-#define PINCTRL_PIN_GROUP(name, id)			\
-	{						\
-		name,					\
-		id##_pins,				\
-		ARRAY_SIZE(id##_pins),			\
-		id##_funcs,				\
-	}
-
-#define MTK_GPIO_MODE	1
-#define MTK_INPUT	0
-#define MTK_OUTPUT	1
-#define MTK_DISABLE	0
-#define MTK_ENABLE	1
-
-/* Custom pinconf parameters */
-#define MTK_PIN_CONFIG_TDSEL	(PIN_CONFIG_END + 1)
-#define MTK_PIN_CONFIG_RDSEL	(PIN_CONFIG_END + 2)
-
-/* List these attributes which could be modified for the pin */
-enum {
-	PINCTRL_PIN_REG_MODE,
-	PINCTRL_PIN_REG_DIR,
-	PINCTRL_PIN_REG_DI,
-	PINCTRL_PIN_REG_DO,
-	PINCTRL_PIN_REG_SR,
-	PINCTRL_PIN_REG_SMT,
-	PINCTRL_PIN_REG_PD,
-	PINCTRL_PIN_REG_PU,
-	PINCTRL_PIN_REG_E4,
-	PINCTRL_PIN_REG_E8,
-	PINCTRL_PIN_REG_TDSEL,
-	PINCTRL_PIN_REG_RDSEL,
-	PINCTRL_PIN_REG_MAX,
-};
-
-/* struct mtk_pin_field - the structure that holds the information of the field
- *			  used to describe the attribute for the pin
- * @offset:		the register offset relative to the base address
- * @mask:		the mask used to filter out the field from the register
- * @bitpos:		the start bit relative to the register
- * @next:		the indication that the field would be extended to the
-			next register
- */
-struct mtk_pin_field {
-	u32 offset;
-	u32 mask;
-	u8  bitpos;
-	u8  next;
-};
-
-/* struct mtk_pin_field_calc - the structure that holds the range providing
- *			       the guide used to look up the relevant field
- * @s_pin:		the start pin within the range
- * @e_pin:		the end pin within the range
- * @s_addr:		the start address for the range
- * @x_addrs:		the address distance between two consecutive registers
- *			within the range
- * @s_bit:		the start bit for the first register within the range
- * @x_bits:		the bit distance between two consecutive pins within
- *			the range
- */
-struct mtk_pin_field_calc {
-	u16 s_pin;
-	u16 e_pin;
-	u32 s_addr;
-	u8  x_addrs;
-	u8  s_bit;
-	u8  x_bits;
-};
-
-/* struct mtk_pin_reg_calc - the structure that holds all ranges used to
- *			     determine which register the pin would make use of
- *			     for certain pin attribute.
- * @range:		     the start address for the range
- * @nranges:		     the number of items in the range
  */
-struct mtk_pin_reg_calc {
-	const struct mtk_pin_field_calc *range;
-	unsigned int nranges;
-};
 
-/* struct mtk_pin_soc - the structure that holds SoC-specific data */
-struct mtk_pin_soc {
-	const struct mtk_pin_reg_calc	*reg_cal;
-	const struct pinctrl_pin_desc	*pins;
-	unsigned int			npins;
-	const struct group_desc		*grps;
-	unsigned int			ngrps;
-	const struct function_desc	*funcs;
-	unsigned int			nfuncs;
-	const struct mtk_eint_regs	*eint_regs;
-	const struct mtk_eint_hw	*eint_hw;
-};
+#include "pinctrl-moore.h"
 
-struct mtk_pinctrl {
-	struct pinctrl_dev		*pctrl;
-	void __iomem			*base;
-	struct device			*dev;
-	struct gpio_chip		chip;
-	const struct mtk_pin_soc	*soc;
-	struct mtk_eint			*eint;
-};
+#define MT7622_PIN(_number, _name)					\
+	MTK_PIN(_number, _name, 1, _number, DRV_GRP0)
 
 static const struct mtk_pin_field_calc mt7622_pin_mode_range[] = {
-	{0, 0, 0x320, 0x10, 16, 4},
-	{1, 4, 0x3a0, 0x10,  16, 4},
-	{5, 5, 0x320, 0x10,  0, 4},
-	{6, 6, 0x300, 0x10,  4, 4},
-	{7, 7, 0x300, 0x10,  4, 4},
-	{8, 9, 0x350, 0x10,  20, 4},
-	{10, 10, 0x300, 0x10, 8, 4},
-	{11, 11, 0x300, 0x10, 8, 4},
-	{12, 12, 0x300, 0x10, 8, 4},
-	{13, 13, 0x300, 0x10, 8, 4},
-	{14, 15, 0x320, 0x10, 4, 4},
-	{16, 17, 0x320, 0x10, 20, 4},
-	{18, 21, 0x310, 0x10, 16, 4},
-	{22, 22, 0x380, 0x10, 16, 4},
-	{23, 23, 0x300,	0x10, 24, 4},
-	{24, 24, 0x300, 0x10, 24, 4},
-	{25, 25, 0x300, 0x10, 12, 4},
-	{25, 25, 0x300, 0x10, 12, 4},
-	{26, 26, 0x300, 0x10, 12, 4},
-	{27, 27, 0x300, 0x10, 12, 4},
-	{28, 28, 0x300, 0x10, 12, 4},
-	{29, 29, 0x300, 0x10, 12, 4},
-	{30, 30, 0x300, 0x10, 12, 4},
-	{31, 31, 0x300, 0x10, 12, 4},
-	{32, 32, 0x300, 0x10, 12, 4},
-	{33, 33, 0x300,	0x10, 12, 4},
-	{34, 34, 0x300,	0x10, 12, 4},
-	{35, 35, 0x300,	0x10, 12, 4},
-	{36, 36, 0x300, 0x10, 12, 4},
-	{37, 37, 0x300, 0x10, 20, 4},
-	{38, 38, 0x300, 0x10, 20, 4},
-	{39, 39, 0x300, 0x10, 20, 4},
-	{40, 40, 0x300, 0x10, 20, 4},
-	{41, 41, 0x300,	0x10, 20, 4},
-	{42, 42, 0x300, 0x10, 20, 4},
-	{43, 43, 0x300,	0x10, 20, 4},
-	{44, 44, 0x300, 0x10, 20, 4},
-	{45, 46, 0x300, 0x10, 20, 4},
-	{47, 47, 0x300,	0x10, 20, 4},
-	{48, 48, 0x300, 0x10, 20, 4},
-	{49, 49, 0x300, 0x10, 20, 4},
-	{50, 50, 0x300, 0x10, 20, 4},
-	{51, 70, 0x330, 0x10, 4, 4},
-	{71, 71, 0x300, 0x10, 16, 4},
-	{72, 72, 0x300, 0x10, 16, 4},
-	{73, 76, 0x310, 0x10, 0, 4},
-	{77, 77, 0x320, 0x10, 28, 4},
-	{78, 78, 0x320, 0x10, 12, 4},
-	{79, 82, 0x3a0, 0x10, 0, 4},
-	{83, 83, 0x350,	0x10, 28, 4},
-	{84, 84, 0x330, 0x10, 0, 4},
-	{85, 90, 0x360, 0x10, 4, 4},
-	{91, 94, 0x390, 0x10, 16, 4},
-	{95, 97, 0x380, 0x10, 20, 4},
-	{98, 101, 0x390, 0x10, 0, 4},
-	{102, 102, 0x360, 0x10, 0, 4},
+	PIN_FIELD(0, 0, 0x320, 0x10, 16, 4),
+	PIN_FIELD(1, 4, 0x3a0, 0x10, 16, 4),
+	PIN_FIELD(5, 5, 0x320, 0x10, 0, 4),
+	PINS_FIELD(6, 7, 0x300, 0x10, 4, 4),
+	PIN_FIELD(8, 9, 0x350, 0x10, 20, 4),
+	PINS_FIELD(10, 13, 0x300, 0x10, 8, 4),
+	PIN_FIELD(14, 15, 0x320, 0x10, 4, 4),
+	PIN_FIELD(16, 17, 0x320, 0x10, 20, 4),
+	PIN_FIELD(18, 21, 0x310, 0x10, 16, 4),
+	PIN_FIELD(22, 22, 0x380, 0x10, 16, 4),
+	PINS_FIELD(23, 24, 0x300, 0x10, 24, 4),
+	PINS_FIELD(25, 36, 0x300, 0x10, 12, 4),
+	PINS_FIELD(37, 50, 0x300, 0x10, 20, 4),
+	PIN_FIELD(51, 70, 0x330, 0x10, 4, 4),
+	PINS_FIELD(71, 72, 0x300, 0x10, 16, 4),
+	PIN_FIELD(73, 76, 0x310, 0x10, 0, 4),
+	PIN_FIELD(77, 77, 0x320, 0x10, 28, 4),
+	PIN_FIELD(78, 78, 0x320, 0x10, 12, 4),
+	PIN_FIELD(79, 82, 0x3a0, 0x10, 0, 4),
+	PIN_FIELD(83, 83, 0x350, 0x10, 28, 4),
+	PIN_FIELD(84, 84, 0x330, 0x10, 0, 4),
+	PIN_FIELD(85, 90, 0x360, 0x10, 4, 4),
+	PIN_FIELD(91, 94, 0x390, 0x10, 16, 4),
+	PIN_FIELD(95, 97, 0x380, 0x10, 20, 4),
+	PIN_FIELD(98, 101, 0x390, 0x10, 0, 4),
+	PIN_FIELD(102, 102, 0x360, 0x10, 0, 4),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_dir_range[] = {
-	{0, 102, 0x0, 0x10, 0, 1},
+	PIN_FIELD(0, 102, 0x0, 0x10, 0, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_di_range[] = {
-	{0, 102, 0x200, 0x10, 0, 1},
+	PIN_FIELD(0, 102, 0x200, 0x10, 0, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_do_range[] = {
-	{0, 102, 0x100, 0x10, 0, 1},
+	PIN_FIELD(0, 102, 0x100, 0x10, 0, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_sr_range[] = {
-	{0, 31, 0x910, 0x10, 0, 1},
-	{32, 50, 0xa10, 0x10, 0, 1},
-	{51, 70, 0x810, 0x10, 0, 1},
-	{71, 72, 0xb10, 0x10, 0, 1},
-	{73, 86, 0xb10, 0x10, 4, 1},
-	{87, 90, 0xc10, 0x10, 0, 1},
-	{91, 102, 0xb10, 0x10, 18, 1},
+	PIN_FIELD(0, 31, 0x910, 0x10, 0, 1),
+	PIN_FIELD(32, 50, 0xa10, 0x10, 0, 1),
+	PIN_FIELD(51, 70, 0x810, 0x10, 0, 1),
+	PIN_FIELD(71, 72, 0xb10, 0x10, 0, 1),
+	PIN_FIELD(73, 86, 0xb10, 0x10, 4, 1),
+	PIN_FIELD(87, 90, 0xc10, 0x10, 0, 1),
+	PIN_FIELD(91, 102, 0xb10, 0x10, 18, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_smt_range[] = {
-	{0, 31, 0x920, 0x10, 0, 1},
-	{32, 50, 0xa20, 0x10, 0, 1},
-	{51, 70, 0x820, 0x10, 0, 1},
-	{71, 72, 0xb20, 0x10, 0, 1},
-	{73, 86, 0xb20, 0x10, 4, 1},
-	{87, 90, 0xc20, 0x10, 0, 1},
-	{91, 102, 0xb20, 0x10, 18, 1},
+	PIN_FIELD(0, 31, 0x920, 0x10, 0, 1),
+	PIN_FIELD(32, 50, 0xa20, 0x10, 0, 1),
+	PIN_FIELD(51, 70, 0x820, 0x10, 0, 1),
+	PIN_FIELD(71, 72, 0xb20, 0x10, 0, 1),
+	PIN_FIELD(73, 86, 0xb20, 0x10, 4, 1),
+	PIN_FIELD(87, 90, 0xc20, 0x10, 0, 1),
+	PIN_FIELD(91, 102, 0xb20, 0x10, 18, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_pu_range[] = {
-	{0, 31, 0x930, 0x10, 0, 1},
-	{32, 50, 0xa30, 0x10, 0, 1},
-	{51, 70, 0x830, 0x10, 0, 1},
-	{71, 72, 0xb30, 0x10, 0, 1},
-	{73, 86, 0xb30, 0x10, 4, 1},
-	{87, 90, 0xc30, 0x10, 0, 1},
-	{91, 102, 0xb30, 0x10, 18, 1},
+	PIN_FIELD(0, 31, 0x930, 0x10, 0, 1),
+	PIN_FIELD(32, 50, 0xa30, 0x10, 0, 1),
+	PIN_FIELD(51, 70, 0x830, 0x10, 0, 1),
+	PIN_FIELD(71, 72, 0xb30, 0x10, 0, 1),
+	PIN_FIELD(73, 86, 0xb30, 0x10, 4, 1),
+	PIN_FIELD(87, 90, 0xc30, 0x10, 0, 1),
+	PIN_FIELD(91, 102, 0xb30, 0x10, 18, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_pd_range[] = {
-	{0, 31, 0x940, 0x10, 0, 1},
-	{32, 50, 0xa40, 0x10, 0, 1},
-	{51, 70, 0x840, 0x10, 0, 1},
-	{71, 72, 0xb40, 0x10, 0, 1},
-	{73, 86, 0xb40, 0x10, 4, 1},
-	{87, 90, 0xc40, 0x10, 0, 1},
-	{91, 102, 0xb40, 0x10, 18, 1},
+	PIN_FIELD(0, 31, 0x940, 0x10, 0, 1),
+	PIN_FIELD(32, 50, 0xa40, 0x10, 0, 1),
+	PIN_FIELD(51, 70, 0x840, 0x10, 0, 1),
+	PIN_FIELD(71, 72, 0xb40, 0x10, 0, 1),
+	PIN_FIELD(73, 86, 0xb40, 0x10, 4, 1),
+	PIN_FIELD(87, 90, 0xc40, 0x10, 0, 1),
+	PIN_FIELD(91, 102, 0xb40, 0x10, 18, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_e4_range[] = {
-	{0, 31, 0x960, 0x10, 0, 1},
-	{32, 50, 0xa60, 0x10, 0, 1},
-	{51, 70, 0x860, 0x10, 0, 1},
-	{71, 72, 0xb60, 0x10, 0, 1},
-	{73, 86, 0xb60, 0x10, 4, 1},
-	{87, 90, 0xc60, 0x10, 0, 1},
-	{91, 102, 0xb60, 0x10, 18, 1},
+	PIN_FIELD(0, 31, 0x960, 0x10, 0, 1),
+	PIN_FIELD(32, 50, 0xa60, 0x10, 0, 1),
+	PIN_FIELD(51, 70, 0x860, 0x10, 0, 1),
+	PIN_FIELD(71, 72, 0xb60, 0x10, 0, 1),
+	PIN_FIELD(73, 86, 0xb60, 0x10, 4, 1),
+	PIN_FIELD(87, 90, 0xc60, 0x10, 0, 1),
+	PIN_FIELD(91, 102, 0xb60, 0x10, 18, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_e8_range[] = {
-	{0, 31, 0x970, 0x10, 0, 1},
-	{32, 50, 0xa70, 0x10, 0, 1},
-	{51, 70, 0x870, 0x10, 0, 1},
-	{71, 72, 0xb70, 0x10, 0, 1},
-	{73, 86, 0xb70, 0x10, 4, 1},
-	{87, 90, 0xc70, 0x10, 0, 1},
-	{91, 102, 0xb70, 0x10, 18, 1},
+	PIN_FIELD(0, 31, 0x970, 0x10, 0, 1),
+	PIN_FIELD(32, 50, 0xa70, 0x10, 0, 1),
+	PIN_FIELD(51, 70, 0x870, 0x10, 0, 1),
+	PIN_FIELD(71, 72, 0xb70, 0x10, 0, 1),
+	PIN_FIELD(73, 86, 0xb70, 0x10, 4, 1),
+	PIN_FIELD(87, 90, 0xc70, 0x10, 0, 1),
+	PIN_FIELD(91, 102, 0xb70, 0x10, 18, 1),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_tdsel_range[] = {
-	{0, 31, 0x980, 0x4, 0, 4},
-	{32, 50, 0xa80, 0x4, 0, 4},
-	{51, 70, 0x880, 0x4, 0, 4},
-	{71, 72, 0xb80, 0x4, 0, 4},
-	{73, 86, 0xb80, 0x4, 16, 4},
-	{87, 90, 0xc80, 0x4, 0, 4},
-	{91, 102, 0xb88, 0x4, 8, 4},
+	PIN_FIELD(0, 31, 0x980, 0x4, 0, 4),
+	PIN_FIELD(32, 50, 0xa80, 0x4, 0, 4),
+	PIN_FIELD(51, 70, 0x880, 0x4, 0, 4),
+	PIN_FIELD(71, 72, 0xb80, 0x4, 0, 4),
+	PIN_FIELD(73, 86, 0xb80, 0x4, 16, 4),
+	PIN_FIELD(87, 90, 0xc80, 0x4, 0, 4),
+	PIN_FIELD(91, 102, 0xb88, 0x4, 8, 4),
 };
 
 static const struct mtk_pin_field_calc mt7622_pin_rdsel_range[] = {
-	{0, 31, 0x990, 0x4, 0, 6},
-	{32, 50, 0xa90, 0x4, 0, 6},
-	{51, 58, 0x890, 0x4, 0, 6},
-	{59, 60, 0x894, 0x4, 28, 6},
-	{61, 62, 0x894, 0x4, 16, 6},
-	{63, 66, 0x898, 0x4, 8, 6},
-	{67, 68, 0x89c, 0x4, 12, 6},
-	{69, 70, 0x89c, 0x4, 0, 6},
-	{71, 72, 0xb90, 0x4, 0, 6},
-	{73, 86, 0xb90, 0x4, 24, 6},
-	{87, 90, 0xc90, 0x4, 0, 6},
-	{91, 102, 0xb9c, 0x4, 12, 6},
+	PIN_FIELD(0, 31, 0x990, 0x4, 0, 6),
+	PIN_FIELD(32, 50, 0xa90, 0x4, 0, 6),
+	PIN_FIELD(51, 58, 0x890, 0x4, 0, 6),
+	PIN_FIELD(59, 60, 0x894, 0x4, 28, 6),
+	PIN_FIELD(61, 62, 0x894, 0x4, 16, 6),
+	PIN_FIELD(63, 66, 0x898, 0x4, 8, 6),
+	PIN_FIELD(67, 68, 0x89c, 0x4, 12, 6),
+	PIN_FIELD(69, 70, 0x89c, 0x4, 0, 6),
+	PIN_FIELD(71, 72, 0xb90, 0x4, 0, 6),
+	PIN_FIELD(73, 86, 0xb90, 0x4, 24, 6),
+	PIN_FIELD(87, 90, 0xc90, 0x4, 0, 6),
+	PIN_FIELD(91, 102, 0xb9c, 0x4, 12, 6),
 };
 
 static const struct mtk_pin_reg_calc mt7622_reg_cals[PINCTRL_PIN_REG_MAX] = {
@@ -309,110 +152,110 @@ static const struct mtk_pin_reg_calc mt7
 	[PINCTRL_PIN_REG_RDSEL] = MTK_RANGE(mt7622_pin_rdsel_range),
 };
 
-static const struct pinctrl_pin_desc mt7622_pins[] = {
-	PINCTRL_PIN(0, "GPIO_A"),
-	PINCTRL_PIN(1, "I2S1_IN"),
-	PINCTRL_PIN(2, "I2S1_OUT"),
-	PINCTRL_PIN(3, "I2S_BCLK"),
-	PINCTRL_PIN(4, "I2S_WS"),
-	PINCTRL_PIN(5, "I2S_MCLK"),
-	PINCTRL_PIN(6, "TXD0"),
-	PINCTRL_PIN(7, "RXD0"),
-	PINCTRL_PIN(8, "SPI_WP"),
-	PINCTRL_PIN(9, "SPI_HOLD"),
-	PINCTRL_PIN(10, "SPI_CLK"),
-	PINCTRL_PIN(11, "SPI_MOSI"),
-	PINCTRL_PIN(12, "SPI_MISO"),
-	PINCTRL_PIN(13, "SPI_CS"),
-	PINCTRL_PIN(14, "I2C_SDA"),
-	PINCTRL_PIN(15, "I2C_SCL"),
-	PINCTRL_PIN(16, "I2S2_IN"),
-	PINCTRL_PIN(17, "I2S3_IN"),
-	PINCTRL_PIN(18, "I2S4_IN"),
-	PINCTRL_PIN(19, "I2S2_OUT"),
-	PINCTRL_PIN(20, "I2S3_OUT"),
-	PINCTRL_PIN(21, "I2S4_OUT"),
-	PINCTRL_PIN(22, "GPIO_B"),
-	PINCTRL_PIN(23, "MDC"),
-	PINCTRL_PIN(24, "MDIO"),
-	PINCTRL_PIN(25, "G2_TXD0"),
-	PINCTRL_PIN(26, "G2_TXD1"),
-	PINCTRL_PIN(27, "G2_TXD2"),
-	PINCTRL_PIN(28, "G2_TXD3"),
-	PINCTRL_PIN(29, "G2_TXEN"),
-	PINCTRL_PIN(30, "G2_TXC"),
-	PINCTRL_PIN(31, "G2_RXD0"),
-	PINCTRL_PIN(32, "G2_RXD1"),
-	PINCTRL_PIN(33, "G2_RXD2"),
-	PINCTRL_PIN(34, "G2_RXD3"),
-	PINCTRL_PIN(35, "G2_RXDV"),
-	PINCTRL_PIN(36, "G2_RXC"),
-	PINCTRL_PIN(37, "NCEB"),
-	PINCTRL_PIN(38, "NWEB"),
-	PINCTRL_PIN(39, "NREB"),
-	PINCTRL_PIN(40, "NDL4"),
-	PINCTRL_PIN(41, "NDL5"),
-	PINCTRL_PIN(42, "NDL6"),
-	PINCTRL_PIN(43, "NDL7"),
-	PINCTRL_PIN(44, "NRB"),
-	PINCTRL_PIN(45, "NCLE"),
-	PINCTRL_PIN(46, "NALE"),
-	PINCTRL_PIN(47, "NDL0"),
-	PINCTRL_PIN(48, "NDL1"),
-	PINCTRL_PIN(49, "NDL2"),
-	PINCTRL_PIN(50, "NDL3"),
-	PINCTRL_PIN(51, "MDI_TP_P0"),
-	PINCTRL_PIN(52, "MDI_TN_P0"),
-	PINCTRL_PIN(53, "MDI_RP_P0"),
-	PINCTRL_PIN(54, "MDI_RN_P0"),
-	PINCTRL_PIN(55, "MDI_TP_P1"),
-	PINCTRL_PIN(56, "MDI_TN_P1"),
-	PINCTRL_PIN(57, "MDI_RP_P1"),
-	PINCTRL_PIN(58, "MDI_RN_P1"),
-	PINCTRL_PIN(59, "MDI_RP_P2"),
-	PINCTRL_PIN(60, "MDI_RN_P2"),
-	PINCTRL_PIN(61, "MDI_TP_P2"),
-	PINCTRL_PIN(62, "MDI_TN_P2"),
-	PINCTRL_PIN(63, "MDI_TP_P3"),
-	PINCTRL_PIN(64, "MDI_TN_P3"),
-	PINCTRL_PIN(65, "MDI_RP_P3"),
-	PINCTRL_PIN(66, "MDI_RN_P3"),
-	PINCTRL_PIN(67, "MDI_RP_P4"),
-	PINCTRL_PIN(68, "MDI_RN_P4"),
-	PINCTRL_PIN(69, "MDI_TP_P4"),
-	PINCTRL_PIN(70, "MDI_TN_P4"),
-	PINCTRL_PIN(71, "PMIC_SCL"),
-	PINCTRL_PIN(72, "PMIC_SDA"),
-	PINCTRL_PIN(73, "SPIC1_CLK"),
-	PINCTRL_PIN(74, "SPIC1_MOSI"),
-	PINCTRL_PIN(75, "SPIC1_MISO"),
-	PINCTRL_PIN(76, "SPIC1_CS"),
-	PINCTRL_PIN(77, "GPIO_D"),
-	PINCTRL_PIN(78, "WATCHDOG"),
-	PINCTRL_PIN(79, "RTS3_N"),
-	PINCTRL_PIN(80, "CTS3_N"),
-	PINCTRL_PIN(81, "TXD3"),
-	PINCTRL_PIN(82, "RXD3"),
-	PINCTRL_PIN(83, "PERST0_N"),
-	PINCTRL_PIN(84, "PERST1_N"),
-	PINCTRL_PIN(85, "WLED_N"),
-	PINCTRL_PIN(86, "EPHY_LED0_N"),
-	PINCTRL_PIN(87, "AUXIN0"),
-	PINCTRL_PIN(88, "AUXIN1"),
-	PINCTRL_PIN(89, "AUXIN2"),
-	PINCTRL_PIN(90, "AUXIN3"),
-	PINCTRL_PIN(91, "TXD4"),
-	PINCTRL_PIN(92, "RXD4"),
-	PINCTRL_PIN(93, "RTS4_N"),
-	PINCTRL_PIN(94, "CTS4_N"),
-	PINCTRL_PIN(95, "PWM1"),
-	PINCTRL_PIN(96, "PWM2"),
-	PINCTRL_PIN(97, "PWM3"),
-	PINCTRL_PIN(98, "PWM4"),
-	PINCTRL_PIN(99, "PWM5"),
-	PINCTRL_PIN(100, "PWM6"),
-	PINCTRL_PIN(101, "PWM7"),
-	PINCTRL_PIN(102, "GPIO_E"),
+static const struct mtk_pin_desc mt7622_pins[] = {
+	MT7622_PIN(0, "GPIO_A"),
+	MT7622_PIN(1, "I2S1_IN"),
+	MT7622_PIN(2, "I2S1_OUT"),
+	MT7622_PIN(3, "I2S_BCLK"),
+	MT7622_PIN(4, "I2S_WS"),
+	MT7622_PIN(5, "I2S_MCLK"),
+	MT7622_PIN(6, "TXD0"),
+	MT7622_PIN(7, "RXD0"),
+	MT7622_PIN(8, "SPI_WP"),
+	MT7622_PIN(9, "SPI_HOLD"),
+	MT7622_PIN(10, "SPI_CLK"),
+	MT7622_PIN(11, "SPI_MOSI"),
+	MT7622_PIN(12, "SPI_MISO"),
+	MT7622_PIN(13, "SPI_CS"),
+	MT7622_PIN(14, "I2C_SDA"),
+	MT7622_PIN(15, "I2C_SCL"),
+	MT7622_PIN(16, "I2S2_IN"),
+	MT7622_PIN(17, "I2S3_IN"),
+	MT7622_PIN(18, "I2S4_IN"),
+	MT7622_PIN(19, "I2S2_OUT"),
+	MT7622_PIN(20, "I2S3_OUT"),
+	MT7622_PIN(21, "I2S4_OUT"),
+	MT7622_PIN(22, "GPIO_B"),
+	MT7622_PIN(23, "MDC"),
+	MT7622_PIN(24, "MDIO"),
+	MT7622_PIN(25, "G2_TXD0"),
+	MT7622_PIN(26, "G2_TXD1"),
+	MT7622_PIN(27, "G2_TXD2"),
+	MT7622_PIN(28, "G2_TXD3"),
+	MT7622_PIN(29, "G2_TXEN"),
+	MT7622_PIN(30, "G2_TXC"),
+	MT7622_PIN(31, "G2_RXD0"),
+	MT7622_PIN(32, "G2_RXD1"),
+	MT7622_PIN(33, "G2_RXD2"),
+	MT7622_PIN(34, "G2_RXD3"),
+	MT7622_PIN(35, "G2_RXDV"),
+	MT7622_PIN(36, "G2_RXC"),
+	MT7622_PIN(37, "NCEB"),
+	MT7622_PIN(38, "NWEB"),
+	MT7622_PIN(39, "NREB"),
+	MT7622_PIN(40, "NDL4"),
+	MT7622_PIN(41, "NDL5"),
+	MT7622_PIN(42, "NDL6"),
+	MT7622_PIN(43, "NDL7"),
+	MT7622_PIN(44, "NRB"),
+	MT7622_PIN(45, "NCLE"),
+	MT7622_PIN(46, "NALE"),
+	MT7622_PIN(47, "NDL0"),
+	MT7622_PIN(48, "NDL1"),
+	MT7622_PIN(49, "NDL2"),
+	MT7622_PIN(50, "NDL3"),
+	MT7622_PIN(51, "MDI_TP_P0"),
+	MT7622_PIN(52, "MDI_TN_P0"),
+	MT7622_PIN(53, "MDI_RP_P0"),
+	MT7622_PIN(54, "MDI_RN_P0"),
+	MT7622_PIN(55, "MDI_TP_P1"),
+	MT7622_PIN(56, "MDI_TN_P1"),
+	MT7622_PIN(57, "MDI_RP_P1"),
+	MT7622_PIN(58, "MDI_RN_P1"),
+	MT7622_PIN(59, "MDI_RP_P2"),
+	MT7622_PIN(60, "MDI_RN_P2"),
+	MT7622_PIN(61, "MDI_TP_P2"),
+	MT7622_PIN(62, "MDI_TN_P2"),
+	MT7622_PIN(63, "MDI_TP_P3"),
+	MT7622_PIN(64, "MDI_TN_P3"),
+	MT7622_PIN(65, "MDI_RP_P3"),
+	MT7622_PIN(66, "MDI_RN_P3"),
+	MT7622_PIN(67, "MDI_RP_P4"),
+	MT7622_PIN(68, "MDI_RN_P4"),
+	MT7622_PIN(69, "MDI_TP_P4"),
+	MT7622_PIN(70, "MDI_TN_P4"),
+	MT7622_PIN(71, "PMIC_SCL"),
+	MT7622_PIN(72, "PMIC_SDA"),
+	MT7622_PIN(73, "SPIC1_CLK"),
+	MT7622_PIN(74, "SPIC1_MOSI"),
+	MT7622_PIN(75, "SPIC1_MISO"),
+	MT7622_PIN(76, "SPIC1_CS"),
+	MT7622_PIN(77, "GPIO_D"),
+	MT7622_PIN(78, "WATCHDOG"),
+	MT7622_PIN(79, "RTS3_N"),
+	MT7622_PIN(80, "CTS3_N"),
+	MT7622_PIN(81, "TXD3"),
+	MT7622_PIN(82, "RXD3"),
+	MT7622_PIN(83, "PERST0_N"),
+	MT7622_PIN(84, "PERST1_N"),
+	MT7622_PIN(85, "WLED_N"),
+	MT7622_PIN(86, "EPHY_LED0_N"),
+	MT7622_PIN(87, "AUXIN0"),
+	MT7622_PIN(88, "AUXIN1"),
+	MT7622_PIN(89, "AUXIN2"),
+	MT7622_PIN(90, "AUXIN3"),
+	MT7622_PIN(91, "TXD4"),
+	MT7622_PIN(92, "RXD4"),
+	MT7622_PIN(93, "RTS4_N"),
+	MT7622_PIN(94, "CTS4_N"),
+	MT7622_PIN(95, "PWM1"),
+	MT7622_PIN(96, "PWM2"),
+	MT7622_PIN(97, "PWM3"),
+	MT7622_PIN(98, "PWM4"),
+	MT7622_PIN(99, "PWM5"),
+	MT7622_PIN(100, "PWM6"),
+	MT7622_PIN(101, "PWM7"),
+	MT7622_PIN(102, "GPIO_E"),
 };
 
 /* List all groups consisting of these pins dedicated to the enablement of
@@ -906,18 +749,6 @@ static const struct function_desc mt7622
 	{"watchdog", mt7622_wdt_groups, ARRAY_SIZE(mt7622_wdt_groups)},
 };
 
-static const struct pinconf_generic_params mtk_custom_bindings[] = {
-	{"mediatek,tdsel",	MTK_PIN_CONFIG_TDSEL,		0},
-	{"mediatek,rdsel",	MTK_PIN_CONFIG_RDSEL,		0},
-};
-
-#ifdef CONFIG_DEBUG_FS
-static const struct pin_config_item mtk_conf_items[] = {
-	PCONFDUMP(MTK_PIN_CONFIG_TDSEL, "tdsel", NULL, true),
-	PCONFDUMP(MTK_PIN_CONFIG_RDSEL, "rdsel", NULL, true),
-};
-#endif
-
 static const struct mtk_eint_hw mt7622_eint_hw = {
 	.port_mask = 7,
 	.ports     = 7,
@@ -934,830 +765,38 @@ static const struct mtk_pin_soc mt7622_d
 	.funcs = mt7622_functions,
 	.nfuncs = ARRAY_SIZE(mt7622_functions),
 	.eint_hw = &mt7622_eint_hw,
+	.gpio_m	= 1,
+	.ies_present = false,
+	.base_names = mtk_default_register_base_names,
+	.nbase_names = ARRAY_SIZE(mtk_default_register_base_names),
+	.bias_disable_set = mtk_pinconf_bias_disable_set,
+	.bias_disable_get = mtk_pinconf_bias_disable_get,
+	.bias_set = mtk_pinconf_bias_set,
+	.bias_get = mtk_pinconf_bias_get,
+	.drive_set = mtk_pinconf_drive_set,
+	.drive_get = mtk_pinconf_drive_get,
 };
 
-static void mtk_w32(struct mtk_pinctrl *pctl, u32 reg, u32 val)
-{
-	writel_relaxed(val, pctl->base + reg);
-}
-
-static u32 mtk_r32(struct mtk_pinctrl *pctl, u32 reg)
-{
-	return readl_relaxed(pctl->base + reg);
-}
-
-static void mtk_rmw(struct mtk_pinctrl *pctl, u32 reg, u32 mask, u32 set)
-{
-	u32 val;
-
-	val = mtk_r32(pctl, reg);
-	val &= ~mask;
-	val |= set;
-	mtk_w32(pctl, reg, val);
-}
-
-static int mtk_hw_pin_field_lookup(struct mtk_pinctrl *hw, int pin,
-				   const struct mtk_pin_reg_calc *rc,
-				   struct mtk_pin_field *pfd)
-{
-	const struct mtk_pin_field_calc *c, *e;
-	u32 bits;
-
-	c = rc->range;
-	e = c + rc->nranges;
-
-	while (c < e) {
-		if (pin >= c->s_pin && pin <= c->e_pin)
-			break;
-		c++;
-	}
-
-	if (c >= e) {
-		dev_err(hw->dev, "Out of range for pin = %d\n", pin);
-		return -EINVAL;
-	}
-
-	/* Caculated bits as the overall offset the pin is located at */
-	bits = c->s_bit + (pin - c->s_pin) * (c->x_bits);
-
-	/* Fill pfd from bits and 32-bit register applied is assumed */
-	pfd->offset = c->s_addr + c->x_addrs * (bits / 32);
-	pfd->bitpos = bits % 32;
-	pfd->mask = (1 << c->x_bits) - 1;
-
-	/* pfd->next is used for indicating that bit wrapping-around happens
-	 * which requires the manipulation for bit 0 starting in the next
-	 * register to form the complete field read/write.
-	 */
-	pfd->next = pfd->bitpos + c->x_bits - 1 > 31 ? c->x_addrs : 0;
-
-	return 0;
-}
-
-static int mtk_hw_pin_field_get(struct mtk_pinctrl *hw, int pin,
-				int field, struct mtk_pin_field *pfd)
-{
-	const struct mtk_pin_reg_calc *rc;
-
-	if (field < 0 || field >= PINCTRL_PIN_REG_MAX) {
-		dev_err(hw->dev, "Invalid Field %d\n", field);
-		return -EINVAL;
-	}
-
-	if (hw->soc->reg_cal && hw->soc->reg_cal[field].range) {
-		rc = &hw->soc->reg_cal[field];
-	} else {
-		dev_err(hw->dev, "Undefined range for field %d\n", field);
-		return -EINVAL;
-	}
-
-	return mtk_hw_pin_field_lookup(hw, pin, rc, pfd);
-}
-
-static void mtk_hw_bits_part(struct mtk_pin_field *pf, int *h, int *l)
-{
-	*l = 32 - pf->bitpos;
-	*h = get_count_order(pf->mask) - *l;
-}
-
-static void mtk_hw_write_cross_field(struct mtk_pinctrl *hw,
-				     struct mtk_pin_field *pf, int value)
-{
-	int nbits_l, nbits_h;
-
-	mtk_hw_bits_part(pf, &nbits_h, &nbits_l);
-
-	mtk_rmw(hw, pf->offset, pf->mask << pf->bitpos,
-		(value & pf->mask) << pf->bitpos);
-
-	mtk_rmw(hw, pf->offset + pf->next, BIT(nbits_h) - 1,
-		(value & pf->mask) >> nbits_l);
-}
-
-static void mtk_hw_read_cross_field(struct mtk_pinctrl *hw,
-				    struct mtk_pin_field *pf, int *value)
-{
-	int nbits_l, nbits_h, h, l;
-
-	mtk_hw_bits_part(pf, &nbits_h, &nbits_l);
-
-	l  = (mtk_r32(hw, pf->offset) >> pf->bitpos) & (BIT(nbits_l) - 1);
-	h  = (mtk_r32(hw, pf->offset + pf->next)) & (BIT(nbits_h) - 1);
-
-	*value = (h << nbits_l) | l;
-}
-
-static int mtk_hw_set_value(struct mtk_pinctrl *hw, int pin, int field,
-			    int value)
-{
-	struct mtk_pin_field pf;
-	int err;
-
-	err = mtk_hw_pin_field_get(hw, pin, field, &pf);
-	if (err)
-		return err;
-
-	if (!pf.next)
-		mtk_rmw(hw, pf.offset, pf.mask << pf.bitpos,
-			(value & pf.mask) << pf.bitpos);
-	else
-		mtk_hw_write_cross_field(hw, &pf, value);
-
-	return 0;
-}
-
-static int mtk_hw_get_value(struct mtk_pinctrl *hw, int pin, int field,
-			    int *value)
-{
-	struct mtk_pin_field pf;
-	int err;
-
-	err = mtk_hw_pin_field_get(hw, pin, field, &pf);
-	if (err)
-		return err;
-
-	if (!pf.next)
-		*value = (mtk_r32(hw, pf.offset) >> pf.bitpos) & pf.mask;
-	else
-		mtk_hw_read_cross_field(hw, &pf, value);
-
-	return 0;
-}
-
-static int mtk_pinmux_set_mux(struct pinctrl_dev *pctldev,
-			      unsigned int selector, unsigned int group)
-{
-	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
-	struct function_desc *func;
-	struct group_desc *grp;
-	int i;
-
-	func = pinmux_generic_get_function(pctldev, selector);
-	if (!func)
-		return -EINVAL;
-
-	grp = pinctrl_generic_get_group(pctldev, group);
-	if (!grp)
-		return -EINVAL;
-
-	dev_dbg(pctldev->dev, "enable function %s group %s\n",
-		func->name, grp->name);
-
-	for (i = 0; i < grp->num_pins; i++) {
-		int *pin_modes = grp->data;
-
-		mtk_hw_set_value(hw, grp->pins[i], PINCTRL_PIN_REG_MODE,
-				 pin_modes[i]);
-	}
-
-	return 0;
-}
-
-static int mtk_pinmux_gpio_request_enable(struct pinctrl_dev *pctldev,
-					  struct pinctrl_gpio_range *range,
-					  unsigned int pin)
-{
-	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
-
-	return mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_MODE, MTK_GPIO_MODE);
-}
-
-static int mtk_pinmux_gpio_set_direction(struct pinctrl_dev *pctldev,
-					 struct pinctrl_gpio_range *range,
-					 unsigned int pin, bool input)
-{
-	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
-
-	/* hardware would take 0 as input direction */
-	return mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_DIR, !input);
-}
-
-static int mtk_pinconf_get(struct pinctrl_dev *pctldev,
-			   unsigned int pin, unsigned long *config)
-{
-	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
-	u32 param = pinconf_to_config_param(*config);
-	int val, val2, err, reg, ret = 1;
-
-	switch (param) {
-	case PIN_CONFIG_BIAS_DISABLE:
-		err = mtk_hw_get_value(hw, pin, PINCTRL_PIN_REG_PU, &val);
-		if (err)
-			return err;
-
-		err = mtk_hw_get_value(hw, pin, PINCTRL_PIN_REG_PD, &val2);
-		if (err)
-			return err;
-
-		if (val || val2)
-			return -EINVAL;
-
-		break;
-	case PIN_CONFIG_BIAS_PULL_UP:
-	case PIN_CONFIG_BIAS_PULL_DOWN:
-	case PIN_CONFIG_SLEW_RATE:
-		reg = (param == PIN_CONFIG_BIAS_PULL_UP) ?
-		      PINCTRL_PIN_REG_PU :
-		      (param == PIN_CONFIG_BIAS_PULL_DOWN) ?
-		      PINCTRL_PIN_REG_PD : PINCTRL_PIN_REG_SR;
-
-		err = mtk_hw_get_value(hw, pin, reg, &val);
-		if (err)
-			return err;
-
-		if (!val)
-			return -EINVAL;
-
-		break;
-	case PIN_CONFIG_INPUT_ENABLE:
-	case PIN_CONFIG_OUTPUT_ENABLE:
-		err = mtk_hw_get_value(hw, pin, PINCTRL_PIN_REG_DIR, &val);
-		if (err)
-			return err;
-
-		/* HW takes input mode as zero; output mode as non-zero */
-		if ((val && param == PIN_CONFIG_INPUT_ENABLE) ||
-		    (!val && param == PIN_CONFIG_OUTPUT_ENABLE))
-			return -EINVAL;
-
-		break;
-	case PIN_CONFIG_INPUT_SCHMITT_ENABLE:
-		err = mtk_hw_get_value(hw, pin, PINCTRL_PIN_REG_DIR, &val);
-		if (err)
-			return err;
-
-		err = mtk_hw_get_value(hw, pin, PINCTRL_PIN_REG_SMT, &val2);
-		if (err)
-			return err;
-
-		if (val || !val2)
-			return -EINVAL;
-
-		break;
-	case PIN_CONFIG_DRIVE_STRENGTH:
-		err = mtk_hw_get_value(hw, pin, PINCTRL_PIN_REG_E4, &val);
-		if (err)
-			return err;
-
-		err = mtk_hw_get_value(hw, pin, PINCTRL_PIN_REG_E8, &val2);
-		if (err)
-			return err;
-
-		/* 4mA when (e8, e4) = (0, 0); 8mA when (e8, e4) = (0, 1)
-		 * 12mA when (e8, e4) = (1, 0); 16mA when (e8, e4) = (1, 1)
-		 */
-		ret = ((val2 << 1) + val + 1) * 4;
-
-		break;
-	case MTK_PIN_CONFIG_TDSEL:
-	case MTK_PIN_CONFIG_RDSEL:
-		reg = (param == MTK_PIN_CONFIG_TDSEL) ?
-		       PINCTRL_PIN_REG_TDSEL : PINCTRL_PIN_REG_RDSEL;
-
-		err = mtk_hw_get_value(hw, pin, reg, &val);
-		if (err)
-			return err;
-
-		ret = val;
-
-		break;
-	default:
-		return -ENOTSUPP;
-	}
-
-	*config = pinconf_to_config_packed(param, ret);
-
-	return 0;
-}
-
-static int mtk_pinconf_set(struct pinctrl_dev *pctldev, unsigned int pin,
-			   unsigned long *configs, unsigned int num_configs)
-{
-	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
-	u32 reg, param, arg;
-	int cfg, err = 0;
-
-	for (cfg = 0; cfg < num_configs; cfg++) {
-		param = pinconf_to_config_param(configs[cfg]);
-		arg = pinconf_to_config_argument(configs[cfg]);
-
-		switch (param) {
-		case PIN_CONFIG_BIAS_DISABLE:
-		case PIN_CONFIG_BIAS_PULL_UP:
-		case PIN_CONFIG_BIAS_PULL_DOWN:
-			arg = (param == PIN_CONFIG_BIAS_DISABLE) ? 0 :
-			       (param == PIN_CONFIG_BIAS_PULL_UP) ? 1 : 2;
-
-			err = mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_PU,
-					       arg & 1);
-			if (err)
-				goto err;
-
-			err = mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_PD,
-					       !!(arg & 2));
-			if (err)
-				goto err;
-			break;
-		case PIN_CONFIG_OUTPUT_ENABLE:
-			err = mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_SMT,
-					       MTK_DISABLE);
-			if (err)
-				goto err;
-			/* else: fall through */
-		case PIN_CONFIG_INPUT_ENABLE:
-		case PIN_CONFIG_SLEW_RATE:
-			reg = (param == PIN_CONFIG_SLEW_RATE) ?
-			       PINCTRL_PIN_REG_SR : PINCTRL_PIN_REG_DIR;
-
-			arg = (param == PIN_CONFIG_INPUT_ENABLE) ? 0 :
-			      (param == PIN_CONFIG_OUTPUT_ENABLE) ? 1 : arg;
-			err = mtk_hw_set_value(hw, pin, reg, arg);
-			if (err)
-				goto err;
-
-			break;
-		case PIN_CONFIG_OUTPUT:
-			err = mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_DIR,
-					       MTK_OUTPUT);
-			if (err)
-				goto err;
-
-			err = mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_DO,
-					       arg);
-			if (err)
-				goto err;
-			break;
-		case PIN_CONFIG_INPUT_SCHMITT_ENABLE:
-			/* arg = 1: Input mode & SMT enable ;
-			 * arg = 0: Output mode & SMT disable
-			 */
-			arg = arg ? 2 : 1;
-			err = mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_DIR,
-					       arg & 1);
-			if (err)
-				goto err;
-
-			err = mtk_hw_set_value(hw, pin, PINCTRL_PIN_REG_SMT,
-					       !!(arg & 2));
-			if (err)
-				goto err;
-			break;
-		case PIN_CONFIG_DRIVE_STRENGTH:
-			/* 4mA when (e8, e4) = (0, 0);
-			 * 8mA when (e8, e4) = (0, 1);
-			 * 12mA when (e8, e4) = (1, 0);
-			 * 16mA when (e8, e4) = (1, 1)
-			 */
-			if (!(arg % 4) && (arg >= 4 && arg <= 16)) {
-				arg = arg / 4 - 1;
-				err = mtk_hw_set_value(hw, pin,
-						       PINCTRL_PIN_REG_E4,
-						       arg & 0x1);
-				if (err)
-					goto err;
-
-				err = mtk_hw_set_value(hw, pin,
-						       PINCTRL_PIN_REG_E8,
-						       (arg & 0x2) >> 1);
-				if (err)
-					goto err;
-			} else {
-				err = -ENOTSUPP;
-			}
-			break;
-		case MTK_PIN_CONFIG_TDSEL:
-		case MTK_PIN_CONFIG_RDSEL:
-			reg = (param == MTK_PIN_CONFIG_TDSEL) ?
-			       PINCTRL_PIN_REG_TDSEL : PINCTRL_PIN_REG_RDSEL;
-
-			err = mtk_hw_set_value(hw, pin, reg, arg);
-			if (err)
-				goto err;
-			break;
-		default:
-			err = -ENOTSUPP;
-		}
-	}
-err:
-	return err;
-}
-
-static int mtk_pinconf_group_get(struct pinctrl_dev *pctldev,
-				 unsigned int group, unsigned long *config)
-{
-	const unsigned int *pins;
-	unsigned int i, npins, old = 0;
-	int ret;
-
-	ret = pinctrl_generic_get_group_pins(pctldev, group, &pins, &npins);
-	if (ret)
-		return ret;
-
-	for (i = 0; i < npins; i++) {
-		if (mtk_pinconf_get(pctldev, pins[i], config))
-			return -ENOTSUPP;
-
-		/* configs do not match between two pins */
-		if (i && old != *config)
-			return -ENOTSUPP;
-
-		old = *config;
-	}
-
-	return 0;
-}
-
-static int mtk_pinconf_group_set(struct pinctrl_dev *pctldev,
-				 unsigned int group, unsigned long *configs,
-				 unsigned int num_configs)
-{
-	const unsigned int *pins;
-	unsigned int i, npins;
-	int ret;
-
-	ret = pinctrl_generic_get_group_pins(pctldev, group, &pins, &npins);
-	if (ret)
-		return ret;
-
-	for (i = 0; i < npins; i++) {
-		ret = mtk_pinconf_set(pctldev, pins[i], configs, num_configs);
-		if (ret)
-			return ret;
-	}
-
-	return 0;
-}
-
-static const struct pinctrl_ops mtk_pctlops = {
-	.get_groups_count = pinctrl_generic_get_group_count,
-	.get_group_name = pinctrl_generic_get_group_name,
-	.get_group_pins = pinctrl_generic_get_group_pins,
-	.dt_node_to_map = pinconf_generic_dt_node_to_map_all,
-	.dt_free_map = pinconf_generic_dt_free_map,
-};
-
-static const struct pinmux_ops mtk_pmxops = {
-	.get_functions_count = pinmux_generic_get_function_count,
-	.get_function_name = pinmux_generic_get_function_name,
-	.get_function_groups = pinmux_generic_get_function_groups,
-	.set_mux = mtk_pinmux_set_mux,
-	.gpio_request_enable = mtk_pinmux_gpio_request_enable,
-	.gpio_set_direction = mtk_pinmux_gpio_set_direction,
-	.strict = true,
-};
-
-static const struct pinconf_ops mtk_confops = {
-	.is_generic = true,
-	.pin_config_get = mtk_pinconf_get,
-	.pin_config_set = mtk_pinconf_set,
-	.pin_config_group_get = mtk_pinconf_group_get,
-	.pin_config_group_set = mtk_pinconf_group_set,
-	.pin_config_config_dbg_show = pinconf_generic_dump_config,
-};
-
-static struct pinctrl_desc mtk_desc = {
-	.name = PINCTRL_PINCTRL_DEV,
-	.pctlops = &mtk_pctlops,
-	.pmxops = &mtk_pmxops,
-	.confops = &mtk_confops,
-	.owner = THIS_MODULE,
-};
-
-static int mtk_gpio_get(struct gpio_chip *chip, unsigned int gpio)
-{
-	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
-	int value, err;
-
-	err = mtk_hw_get_value(hw, gpio, PINCTRL_PIN_REG_DI, &value);
-	if (err)
-		return err;
-
-	return !!value;
-}
-
-static void mtk_gpio_set(struct gpio_chip *chip, unsigned int gpio, int value)
-{
-	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
-
-	mtk_hw_set_value(hw, gpio, PINCTRL_PIN_REG_DO, !!value);
-}
-
-static int mtk_gpio_direction_input(struct gpio_chip *chip, unsigned int gpio)
-{
-	return pinctrl_gpio_direction_input(chip->base + gpio);
-}
-
-static int mtk_gpio_direction_output(struct gpio_chip *chip, unsigned int gpio,
-				     int value)
-{
-	mtk_gpio_set(chip, gpio, value);
-
-	return pinctrl_gpio_direction_output(chip->base + gpio);
-}
-
-static int mtk_gpio_to_irq(struct gpio_chip *chip, unsigned int offset)
-{
-	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
-	unsigned long eint_n;
-
-	if (!hw->eint)
-		return -ENOTSUPP;
-
-	eint_n = offset;
-
-	return mtk_eint_find_irq(hw->eint, eint_n);
-}
-
-static int mtk_gpio_set_config(struct gpio_chip *chip, unsigned int offset,
-			       unsigned long config)
-{
-	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
-	unsigned long eint_n;
-	u32 debounce;
-
-	if (!hw->eint ||
-	    pinconf_to_config_param(config) != PIN_CONFIG_INPUT_DEBOUNCE)
-		return -ENOTSUPP;
-
-	debounce = pinconf_to_config_argument(config);
-	eint_n = offset;
-
-	return mtk_eint_set_debounce(hw->eint, eint_n, debounce);
-}
-
-static int mtk_build_gpiochip(struct mtk_pinctrl *hw, struct device_node *np)
-{
-	struct gpio_chip *chip = &hw->chip;
-	int ret;
-
-	chip->label		= PINCTRL_PINCTRL_DEV;
-	chip->parent		= hw->dev;
-	chip->request		= gpiochip_generic_request;
-	chip->free		= gpiochip_generic_free;
-	chip->direction_input	= mtk_gpio_direction_input;
-	chip->direction_output	= mtk_gpio_direction_output;
-	chip->get		= mtk_gpio_get;
-	chip->set		= mtk_gpio_set;
-	chip->to_irq		= mtk_gpio_to_irq,
-	chip->set_config	= mtk_gpio_set_config,
-	chip->base		= -1;
-	chip->ngpio		= hw->soc->npins;
-	chip->of_node		= np;
-	chip->of_gpio_n_cells	= 2;
-
-	ret = gpiochip_add_data(chip, hw);
-	if (ret < 0)
-		return ret;
-
-	/* Just for backward compatible for these old pinctrl nodes without
-	 * "gpio-ranges" property. Otherwise, called directly from a
-	 * DeviceTree-supported pinctrl driver is DEPRECATED.
-	 * Please see Section 2.1 of
-	 * Documentation/devicetree/bindings/gpio/gpio.txt on how to
-	 * bind pinctrl and gpio drivers via the "gpio-ranges" property.
-	 */
-	if (!of_find_property(np, "gpio-ranges", NULL)) {
-		ret = gpiochip_add_pin_range(chip, dev_name(hw->dev), 0, 0,
-					     chip->ngpio);
-		if (ret < 0) {
-			gpiochip_remove(chip);
-			return ret;
-		}
-	}
-
-	return 0;
-}
-
-static int mtk_build_groups(struct mtk_pinctrl *hw)
-{
-	int err, i;
-
-	for (i = 0; i < hw->soc->ngrps; i++) {
-		const struct group_desc *group = hw->soc->grps + i;
-
-		err = pinctrl_generic_add_group(hw->pctrl, group->name,
-						group->pins, group->num_pins,
-						group->data);
-		if (err < 0) {
-			dev_err(hw->dev, "Failed to register group %s\n",
-				group->name);
-			return err;
-		}
-	}
-
-	return 0;
-}
-
-static int mtk_build_functions(struct mtk_pinctrl *hw)
-{
-	int i, err;
-
-	for (i = 0; i < hw->soc->nfuncs ; i++) {
-		const struct function_desc *func = hw->soc->funcs + i;
-
-		err = pinmux_generic_add_function(hw->pctrl, func->name,
-						  func->group_names,
-						  func->num_group_names,
-						  func->data);
-		if (err < 0) {
-			dev_err(hw->dev, "Failed to register function %s\n",
-				func->name);
-			return err;
-		}
-	}
-
-	return 0;
-}
-
-static int mtk_xt_get_gpio_n(void *data, unsigned long eint_n,
-			     unsigned int *gpio_n,
-			     struct gpio_chip **gpio_chip)
-{
-	struct mtk_pinctrl *hw = (struct mtk_pinctrl *)data;
-
-	*gpio_chip = &hw->chip;
-	*gpio_n = eint_n;
-
-	return 0;
-}
-
-static int mtk_xt_get_gpio_state(void *data, unsigned long eint_n)
-{
-	struct mtk_pinctrl *hw = (struct mtk_pinctrl *)data;
-	struct gpio_chip *gpio_chip;
-	unsigned int gpio_n;
-	int err;
-
-	err = mtk_xt_get_gpio_n(hw, eint_n, &gpio_n, &gpio_chip);
-	if (err)
-		return err;
-
-	return mtk_gpio_get(gpio_chip, gpio_n);
-}
-
-static int mtk_xt_set_gpio_as_eint(void *data, unsigned long eint_n)
-{
-	struct mtk_pinctrl *hw = (struct mtk_pinctrl *)data;
-	struct gpio_chip *gpio_chip;
-	unsigned int gpio_n;
-	int err;
-
-	err = mtk_xt_get_gpio_n(hw, eint_n, &gpio_n, &gpio_chip);
-	if (err)
-		return err;
-
-	err = mtk_hw_set_value(hw, gpio_n, PINCTRL_PIN_REG_MODE,
-			       MTK_GPIO_MODE);
-	if (err)
-		return err;
-
-	err = mtk_hw_set_value(hw, gpio_n, PINCTRL_PIN_REG_DIR, MTK_INPUT);
-	if (err)
-		return err;
-
-	err = mtk_hw_set_value(hw, gpio_n, PINCTRL_PIN_REG_SMT, MTK_ENABLE);
-	if (err)
-		return err;
-
-	return 0;
-}
-
-static const struct mtk_eint_xt mtk_eint_xt = {
-	.get_gpio_n = mtk_xt_get_gpio_n,
-	.get_gpio_state = mtk_xt_get_gpio_state,
-	.set_gpio_as_eint = mtk_xt_set_gpio_as_eint,
-};
-
-static int
-mtk_build_eint(struct mtk_pinctrl *hw, struct platform_device *pdev)
-{
-	struct device_node *np = pdev->dev.of_node;
-	struct resource *res;
-
-	if (!IS_ENABLED(CONFIG_EINT_MTK))
-		return 0;
-
-	if (!of_property_read_bool(np, "interrupt-controller"))
-		return -ENODEV;
-
-	hw->eint = devm_kzalloc(hw->dev, sizeof(*hw->eint), GFP_KERNEL);
-	if (!hw->eint)
-		return -ENOMEM;
-
-	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "eint");
-	if (!res) {
-		dev_err(&pdev->dev, "Unable to get eint resource\n");
-		return -ENODEV;
-	}
-
-	hw->eint->base = devm_ioremap_resource(&pdev->dev, res);
-	if (IS_ERR(hw->eint->base))
-		return PTR_ERR(hw->eint->base);
-
-	hw->eint->irq = irq_of_parse_and_map(np, 0);
-	if (!hw->eint->irq)
-		return -EINVAL;
-
-	hw->eint->dev = &pdev->dev;
-	hw->eint->hw = hw->soc->eint_hw;
-	hw->eint->pctl = hw;
-	hw->eint->gpio_xlate = &mtk_eint_xt;
-
-	return mtk_eint_do_init(hw->eint);
-}
-
-static const struct of_device_id mtk_pinctrl_of_match[] = {
-	{ .compatible = "mediatek,mt7622-pinctrl", .data = &mt7622_data},
+static const struct of_device_id mt7622_pinctrl_of_match[] = {
+	{ .compatible = "mediatek,mt7622-pinctrl", },
 	{ }
 };
 
-static int mtk_pinctrl_probe(struct platform_device *pdev)
+static int mt7622_pinctrl_probe(struct platform_device *pdev)
 {
-	struct resource *res;
-	struct mtk_pinctrl *hw;
-	const struct of_device_id *of_id =
-		of_match_device(mtk_pinctrl_of_match, &pdev->dev);
-	int err;
-
-	hw = devm_kzalloc(&pdev->dev, sizeof(*hw), GFP_KERNEL);
-	if (!hw)
-		return -ENOMEM;
-
-	hw->soc = of_id->data;
-
-	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
-	if (!res) {
-		dev_err(&pdev->dev, "missing IO resource\n");
-		return -ENXIO;
-	}
-
-	hw->dev = &pdev->dev;
-	hw->base = devm_ioremap_resource(&pdev->dev, res);
-	if (IS_ERR(hw->base))
-		return PTR_ERR(hw->base);
-
-	/* Setup pins descriptions per SoC types */
-	mtk_desc.pins = hw->soc->pins;
-	mtk_desc.npins = hw->soc->npins;
-	mtk_desc.num_custom_params = ARRAY_SIZE(mtk_custom_bindings);
-	mtk_desc.custom_params = mtk_custom_bindings;
-#ifdef CONFIG_DEBUG_FS
-	mtk_desc.custom_conf_items = mtk_conf_items;
-#endif
-
-	err = devm_pinctrl_register_and_init(&pdev->dev, &mtk_desc, hw,
-					     &hw->pctrl);
-	if (err)
-		return err;
-
-	/* Setup groups descriptions per SoC types */
-	err = mtk_build_groups(hw);
-	if (err) {
-		dev_err(&pdev->dev, "Failed to build groups\n");
-		return err;
-	}
-
-	/* Setup functions descriptions per SoC types */
-	err = mtk_build_functions(hw);
-	if (err) {
-		dev_err(&pdev->dev, "Failed to build functions\n");
-		return err;
-	}
-
-	/* For able to make pinctrl_claim_hogs, we must not enable pinctrl
-	 * until all groups and functions are being added one.
-	 */
-	err = pinctrl_enable(hw->pctrl);
-	if (err)
-		return err;
-
-	err = mtk_build_eint(hw, pdev);
-	if (err)
-		dev_warn(&pdev->dev,
-			 "Failed to add EINT, but pinctrl still can work\n");
-
-	/* Build gpiochip should be after pinctrl_enable is done */
-	err = mtk_build_gpiochip(hw, pdev->dev.of_node);
-	if (err) {
-		dev_err(&pdev->dev, "Failed to add gpio_chip\n");
-		return err;
-	}
-
-	platform_set_drvdata(pdev, hw);
-
-	return 0;
+	return mtk_moore_pinctrl_probe(pdev, &mt7622_data);
 }
 
-static struct platform_driver mtk_pinctrl_driver = {
+static struct platform_driver mt7622_pinctrl_driver = {
 	.driver = {
-		.name = "mtk-pinctrl",
-		.of_match_table = mtk_pinctrl_of_match,
+		.name = "mt7622-pinctrl",
+		.of_match_table = mt7622_pinctrl_of_match,
 	},
-	.probe = mtk_pinctrl_probe,
+	.probe = mt7622_pinctrl_probe,
 };
 
-static int __init mtk_pinctrl_init(void)
+static int __init mt7622_pinctrl_init(void)
 {
-	return platform_driver_register(&mtk_pinctrl_driver);
+	return platform_driver_register(&mt7622_pinctrl_driver);
 }
-arch_initcall(mtk_pinctrl_init);
+arch_initcall(mt7622_pinctrl_init);
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mt7623.c
@@ -0,0 +1,1441 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * The MT7623 driver based on Linux generic pinctrl binding.
+ *
+ * Copyright (C) 2015 - 2018 MediaTek Inc.
+ * Author: Biao Huang <biao.huang@mediatek.com>
+ *	   Ryder Lee <ryder.lee@mediatek.com>
+ *	   Sean Wang <sean.wang@mediatek.com>
+ */
+
+#include "pinctrl-moore.h"
+
+#define PIN_BOND_REG0		0xb10
+#define PIN_BOND_REG1		0xf20
+#define PIN_BOND_REG2		0xef0
+#define BOND_PCIE_CLR		(0x77 << 3)
+#define BOND_I2S_CLR		0x3
+#define BOND_MSDC0E_CLR		0x1
+
+#define PIN_FIELD15(_s_pin, _e_pin, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, 0, _s_addr, _x_addrs, _s_bit,	\
+		       _x_bits, 15, false)
+
+#define PIN_FIELD16(_s_pin, _e_pin, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, 0, _s_addr, _x_addrs, _s_bit,	\
+		       _x_bits, 16, 0)
+
+#define PINS_FIELD16(_s_pin, _e_pin, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, 0, _s_addr, _x_addrs, _s_bit,	\
+		       _x_bits, 16, 1)
+
+#define MT7623_PIN(_number, _name, _eint_n, _drv_grp)			\
+	MTK_PIN(_number, _name, 0, _eint_n, _drv_grp)
+
+static const struct mtk_pin_field_calc mt7623_pin_mode_range[] = {
+	PIN_FIELD15(0, 278, 0x760, 0x10, 0, 3),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_dir_range[] = {
+	PIN_FIELD16(0, 175, 0x0, 0x10, 0, 1),
+	PIN_FIELD16(176, 278, 0xc0, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_di_range[] = {
+	PIN_FIELD16(0, 278, 0x630, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_do_range[] = {
+	PIN_FIELD16(0, 278, 0x500, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_ies_range[] = {
+	PINS_FIELD16(0, 6, 0xb20, 0x10, 0, 1),
+	PINS_FIELD16(7, 9, 0xb20, 0x10, 1, 1),
+	PINS_FIELD16(10, 13, 0xb30, 0x10, 3, 1),
+	PINS_FIELD16(14, 15, 0xb30, 0x10, 13, 1),
+	PINS_FIELD16(16, 17, 0xb40, 0x10, 7, 1),
+	PINS_FIELD16(18, 29, 0xb40, 0x10, 13, 1),
+	PINS_FIELD16(30, 32, 0xb40, 0x10, 7, 1),
+	PINS_FIELD16(33, 37, 0xb40, 0x10, 13, 1),
+	PIN_FIELD16(38, 38, 0xb20, 0x10, 13, 1),
+	PINS_FIELD16(39, 42, 0xb40, 0x10, 13, 1),
+	PINS_FIELD16(43, 45, 0xb20, 0x10, 10, 1),
+	PINS_FIELD16(47, 48, 0xb20, 0x10, 11, 1),
+	PIN_FIELD16(49, 49, 0xb20, 0x10, 12, 1),
+	PINS_FIELD16(50, 52, 0xb20, 0x10, 13, 1),
+	PINS_FIELD16(53, 56, 0xb20, 0x10, 14, 1),
+	PINS_FIELD16(57, 58, 0xb20, 0x10, 15, 1),
+	PIN_FIELD16(59, 59, 0xb30, 0x10, 10, 1),
+	PINS_FIELD16(60, 62, 0xb30, 0x10, 0, 1),
+	PINS_FIELD16(63, 65, 0xb30, 0x10, 1, 1),
+	PINS_FIELD16(66, 71, 0xb30, 0x10, 2, 1),
+	PINS_FIELD16(72, 74, 0xb20, 0x10, 12, 1),
+	PINS_FIELD16(75, 76, 0xb30, 0x10, 3, 1),
+	PINS_FIELD16(77, 78, 0xb30, 0x10, 4, 1),
+	PINS_FIELD16(79, 82, 0xb30, 0x10, 5, 1),
+	PINS_FIELD16(83, 84, 0xb30, 0x10, 2, 1),
+	PIN_FIELD16(85, 85, 0xda0, 0x10, 4, 1),
+	PIN_FIELD16(86, 86, 0xd90, 0x10, 4, 1),
+	PINS_FIELD16(87, 90, 0xdb0, 0x10, 4, 1),
+	PINS_FIELD16(101, 104, 0xb30, 0x10, 6, 1),
+	PIN_FIELD16(105, 105, 0xd40, 0x10, 4, 1),
+	PIN_FIELD16(106, 106, 0xd30, 0x10, 4, 1),
+	PINS_FIELD16(107, 110, 0xd50, 0x10, 4, 1),
+	PINS_FIELD16(111, 115, 0xce0, 0x10, 4, 1),
+	PIN_FIELD16(116, 116, 0xcd0, 0x10, 4, 1),
+	PIN_FIELD16(117, 117, 0xcc0, 0x10, 4, 1),
+	PINS_FIELD16(118, 121, 0xce0, 0x10, 4, 1),
+	PINS_FIELD16(122, 125, 0xb30, 0x10, 7, 1),
+	PIN_FIELD16(126, 126, 0xb20, 0x10, 12, 1),
+	PINS_FIELD16(127, 142, 0xb30, 0x10, 9, 1),
+	PINS_FIELD16(143, 160, 0xb30, 0x10, 10, 1),
+	PINS_FIELD16(161, 168, 0xb30, 0x10, 12, 1),
+	PINS_FIELD16(169, 183, 0xb30, 0x10, 10, 1),
+	PINS_FIELD16(184, 186, 0xb30, 0x10, 9, 1),
+	PIN_FIELD16(187, 187, 0xb30, 0x10, 14, 1),
+	PIN_FIELD16(188, 188, 0xb20, 0x10, 13, 1),
+	PINS_FIELD16(189, 193, 0xb30, 0x10, 15, 1),
+	PINS_FIELD16(194, 198, 0xb40, 0x10, 0, 1),
+	PIN_FIELD16(199, 199, 0xb20, 0x10, 1, 1),
+	PINS_FIELD16(200, 202, 0xb40, 0x10, 1, 1),
+	PINS_FIELD16(203, 207, 0xb40, 0x10, 2, 1),
+	PINS_FIELD16(208, 209, 0xb40, 0x10, 3, 1),
+	PIN_FIELD16(210, 210, 0xb40, 0x10, 4, 1),
+	PINS_FIELD16(211, 235, 0xb40, 0x10, 5, 1),
+	PINS_FIELD16(236, 241, 0xb40, 0x10, 6, 1),
+	PINS_FIELD16(242, 243, 0xb40, 0x10, 7, 1),
+	PINS_FIELD16(244, 247, 0xb40, 0x10, 8, 1),
+	PIN_FIELD16(248, 248, 0xb40, 0x10, 9, 1),
+	PINS_FIELD16(249, 257, 0xfc0, 0x10, 4, 1),
+	PIN_FIELD16(258, 258, 0xcb0, 0x10, 4, 1),
+	PIN_FIELD16(259, 259, 0xc90, 0x10, 4, 1),
+	PIN_FIELD16(260, 260, 0x3a0, 0x10, 4, 1),
+	PIN_FIELD16(261, 261, 0xd50, 0x10, 4, 1),
+	PINS_FIELD16(262, 277, 0xb40, 0x10, 12, 1),
+	PIN_FIELD16(278, 278, 0xb40, 0x10, 13, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_smt_range[] = {
+	PINS_FIELD16(0, 6, 0xb50, 0x10, 0, 1),
+	PINS_FIELD16(7, 9, 0xb50, 0x10, 1, 1),
+	PINS_FIELD16(10, 13, 0xb60, 0x10, 3, 1),
+	PINS_FIELD16(14, 15, 0xb60, 0x10, 13, 1),
+	PINS_FIELD16(16, 17, 0xb70, 0x10, 7, 1),
+	PINS_FIELD16(18, 29, 0xb70, 0x10, 13, 1),
+	PINS_FIELD16(30, 32, 0xb70, 0x10, 7, 1),
+	PINS_FIELD16(33, 37, 0xb70, 0x10, 13, 1),
+	PIN_FIELD16(38, 38, 0xb50, 0x10, 13, 1),
+	PINS_FIELD16(39, 42, 0xb70, 0x10, 13, 1),
+	PINS_FIELD16(43, 45, 0xb50, 0x10, 10, 1),
+	PINS_FIELD16(47, 48, 0xb50, 0x10, 11, 1),
+	PIN_FIELD16(49, 49, 0xb50, 0x10, 12, 1),
+	PINS_FIELD16(50, 52, 0xb50, 0x10, 13, 1),
+	PINS_FIELD16(53, 56, 0xb50, 0x10, 14, 1),
+	PINS_FIELD16(57, 58, 0xb50, 0x10, 15, 1),
+	PIN_FIELD16(59, 59, 0xb60, 0x10, 10, 1),
+	PINS_FIELD16(60, 62, 0xb60, 0x10, 0, 1),
+	PINS_FIELD16(63, 65, 0xb60, 0x10, 1, 1),
+	PINS_FIELD16(66, 71, 0xb60, 0x10, 2, 1),
+	PINS_FIELD16(72, 74, 0xb50, 0x10, 12, 1),
+	PINS_FIELD16(75, 76, 0xb60, 0x10, 3, 1),
+	PINS_FIELD16(77, 78, 0xb60, 0x10, 4, 1),
+	PINS_FIELD16(79, 82, 0xb60, 0x10, 5, 1),
+	PINS_FIELD16(83, 84, 0xb60, 0x10, 2, 1),
+	PIN_FIELD16(85, 85, 0xda0, 0x10, 11, 1),
+	PIN_FIELD16(86, 86, 0xd90, 0x10, 11, 1),
+	PIN_FIELD16(87, 87, 0xdc0, 0x10, 3, 1),
+	PIN_FIELD16(88, 88, 0xdc0, 0x10, 7, 1),
+	PIN_FIELD16(89, 89, 0xdc0, 0x10, 11, 1),
+	PIN_FIELD16(90, 90, 0xdc0, 0x10, 15, 1),
+	PINS_FIELD16(101, 104, 0xb60, 0x10, 6, 1),
+	PIN_FIELD16(105, 105, 0xd40, 0x10, 11, 1),
+	PIN_FIELD16(106, 106, 0xd30, 0x10, 11, 1),
+	PIN_FIELD16(107, 107, 0xd60, 0x10, 3, 1),
+	PIN_FIELD16(108, 108, 0xd60, 0x10, 7, 1),
+	PIN_FIELD16(109, 109, 0xd60, 0x10, 11, 1),
+	PIN_FIELD16(110, 110, 0xd60, 0x10, 15, 1),
+	PIN_FIELD16(111, 111, 0xd00, 0x10, 15, 1),
+	PIN_FIELD16(112, 112, 0xd00, 0x10, 11, 1),
+	PIN_FIELD16(113, 113, 0xd00, 0x10, 7, 1),
+	PIN_FIELD16(114, 114, 0xd00, 0x10, 3, 1),
+	PIN_FIELD16(115, 115, 0xd10, 0x10, 3, 1),
+	PIN_FIELD16(116, 116, 0xcd0, 0x10, 11, 1),
+	PIN_FIELD16(117, 117, 0xcc0, 0x10, 11, 1),
+	PIN_FIELD16(118, 118, 0xcf0, 0x10, 15, 1),
+	PIN_FIELD16(119, 119, 0xcf0, 0x10, 7, 1),
+	PIN_FIELD16(120, 120, 0xcf0, 0x10, 3, 1),
+	PIN_FIELD16(121, 121, 0xcf0, 0x10, 7, 1),
+	PINS_FIELD16(122, 125, 0xb60, 0x10, 7, 1),
+	PIN_FIELD16(126, 126, 0xb50, 0x10, 12, 1),
+	PINS_FIELD16(127, 142, 0xb60, 0x10, 9, 1),
+	PINS_FIELD16(143, 160, 0xb60, 0x10, 10, 1),
+	PINS_FIELD16(161, 168, 0xb60, 0x10, 12, 1),
+	PINS_FIELD16(169, 183, 0xb60, 0x10, 10, 1),
+	PINS_FIELD16(184, 186, 0xb60, 0x10, 9, 1),
+	PIN_FIELD16(187, 187, 0xb60, 0x10, 14, 1),
+	PIN_FIELD16(188, 188, 0xb50, 0x10, 13, 1),
+	PINS_FIELD16(189, 193, 0xb60, 0x10, 15, 1),
+	PINS_FIELD16(194, 198, 0xb70, 0x10, 0, 1),
+	PIN_FIELD16(199, 199, 0xb50, 0x10, 1, 1),
+	PINS_FIELD16(200, 202, 0xb70, 0x10, 1, 1),
+	PINS_FIELD16(203, 207, 0xb70, 0x10, 2, 1),
+	PINS_FIELD16(208, 209, 0xb70, 0x10, 3, 1),
+	PIN_FIELD16(210, 210, 0xb70, 0x10, 4, 1),
+	PINS_FIELD16(211, 235, 0xb70, 0x10, 5, 1),
+	PINS_FIELD16(236, 241, 0xb70, 0x10, 6, 1),
+	PINS_FIELD16(242, 243, 0xb70, 0x10, 7, 1),
+	PINS_FIELD16(244, 247, 0xb70, 0x10, 8, 1),
+	PIN_FIELD16(248, 248, 0xb70, 0x10, 9, 10),
+	PIN_FIELD16(249, 249, 0x140, 0x10, 3, 1),
+	PIN_FIELD16(250, 250, 0x130, 0x10, 15, 1),
+	PIN_FIELD16(251, 251, 0x130, 0x10, 11, 1),
+	PIN_FIELD16(252, 252, 0x130, 0x10, 7, 1),
+	PIN_FIELD16(253, 253, 0x130, 0x10, 3, 1),
+	PIN_FIELD16(254, 254, 0xf40, 0x10, 15, 1),
+	PIN_FIELD16(255, 255, 0xf40, 0x10, 11, 1),
+	PIN_FIELD16(256, 256, 0xf40, 0x10, 7, 1),
+	PIN_FIELD16(257, 257, 0xf40, 0x10, 3, 1),
+	PIN_FIELD16(258, 258, 0xcb0, 0x10, 11, 1),
+	PIN_FIELD16(259, 259, 0xc90, 0x10, 11, 1),
+	PIN_FIELD16(260, 260, 0x3a0, 0x10, 11, 1),
+	PIN_FIELD16(261, 261, 0x0b0, 0x10, 3, 1),
+	PINS_FIELD16(262, 277, 0xb70, 0x10, 12, 1),
+	PIN_FIELD16(278, 278, 0xb70, 0x10, 13, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_pullen_range[] = {
+	PIN_FIELD16(0, 278, 0x150, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_pullsel_range[] = {
+	PIN_FIELD16(0, 278, 0x280, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_drv_range[] = {
+	PINS_FIELD16(0, 6, 0xf50, 0x10, 0, 4),
+	PINS_FIELD16(7, 9, 0xf50, 0x10, 4, 4),
+	PINS_FIELD16(10, 13, 0xf50, 0x10, 4, 4),
+	PINS_FIELD16(14, 15, 0xf50, 0x10, 12, 4),
+	PINS_FIELD16(16, 17, 0xf60, 0x10, 0, 4),
+	PINS_FIELD16(18, 21, 0xf60, 0x10, 0, 4),
+	PINS_FIELD16(22, 26, 0xf60, 0x10, 8, 4),
+	PINS_FIELD16(27, 29, 0xf60, 0x10, 12, 4),
+	PINS_FIELD16(30, 32, 0xf60, 0x10, 0, 4),
+	PINS_FIELD16(33, 37, 0xf70, 0x10, 0, 4),
+	PIN_FIELD16(38, 38, 0xf70, 0x10, 4, 4),
+	PINS_FIELD16(39, 42, 0xf70, 0x10, 8, 4),
+	PINS_FIELD16(43, 45, 0xf70, 0x10, 12, 4),
+	PINS_FIELD16(47, 48, 0xf80, 0x10, 0, 4),
+	PIN_FIELD16(49, 49, 0xf80, 0x10, 4, 4),
+	PINS_FIELD16(50, 52, 0xf70, 0x10, 4, 4),
+	PINS_FIELD16(53, 56, 0xf80, 0x10, 12, 4),
+	PINS_FIELD16(60, 62, 0xf90, 0x10, 8, 4),
+	PINS_FIELD16(63, 65, 0xf90, 0x10, 12, 4),
+	PINS_FIELD16(66, 71, 0xfa0, 0x10, 0, 4),
+	PINS_FIELD16(72, 74, 0xf80, 0x10, 4, 4),
+	PIN_FIELD16(85, 85, 0xda0, 0x10, 0, 4),
+	PIN_FIELD16(86, 86, 0xd90, 0x10, 0, 4),
+	PINS_FIELD16(87, 90, 0xdb0, 0x10, 0, 4),
+	PIN_FIELD16(105, 105, 0xd40, 0x10, 0, 4),
+	PIN_FIELD16(106, 106, 0xd30, 0x10, 0, 4),
+	PINS_FIELD16(107, 110, 0xd50, 0x10, 0, 4),
+	PINS_FIELD16(111, 115, 0xce0, 0x10, 0, 4),
+	PIN_FIELD16(116, 116, 0xcd0, 0x10, 0, 4),
+	PIN_FIELD16(117, 117, 0xcc0, 0x10, 0, 4),
+	PINS_FIELD16(118, 121, 0xce0, 0x10, 0, 4),
+	PIN_FIELD16(126, 126, 0xf80, 0x10, 4, 4),
+	PIN_FIELD16(188, 188, 0xf70, 0x10, 4, 4),
+	PINS_FIELD16(189, 193, 0xfe0, 0x10, 8, 4),
+	PINS_FIELD16(194, 198, 0xfe0, 0x10, 12, 4),
+	PIN_FIELD16(199, 199, 0xf50, 0x10, 4, 4),
+	PINS_FIELD16(200, 202, 0xfd0, 0x10, 0, 4),
+	PINS_FIELD16(203, 207, 0xfd0, 0x10, 4, 4),
+	PINS_FIELD16(208, 209, 0xfd0, 0x10, 8, 4),
+	PIN_FIELD16(210, 210, 0xfd0, 0x10, 12, 4),
+	PINS_FIELD16(211, 235, 0xff0, 0x10, 0, 4),
+	PINS_FIELD16(236, 241, 0xff0, 0x10, 4, 4),
+	PINS_FIELD16(242, 243, 0xff0, 0x10, 8, 4),
+	PIN_FIELD16(248, 248, 0xf00, 0x10, 0, 4),
+	PINS_FIELD16(249, 256, 0xfc0, 0x10, 0, 4),
+	PIN_FIELD16(257, 257, 0xce0, 0x10, 0, 4),
+	PIN_FIELD16(258, 258, 0xcb0, 0x10, 0, 4),
+	PIN_FIELD16(259, 259, 0xc90, 0x10, 0, 4),
+	PIN_FIELD16(260, 260, 0x3a0, 0x10, 0, 4),
+	PIN_FIELD16(261, 261, 0xd50, 0x10, 0, 4),
+	PINS_FIELD16(262, 277, 0xf00, 0x10, 8, 4),
+	PIN_FIELD16(278, 278, 0xf70, 0x10, 8, 4),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_tdsel_range[] = {
+	PINS_FIELD16(262, 276, 0x4c0, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_pupd_range[] = {
+	/* MSDC0 */
+	PIN_FIELD16(111, 111, 0xd00, 0x10, 12, 1),
+	PIN_FIELD16(112, 112, 0xd00, 0x10, 8, 1),
+	PIN_FIELD16(113, 113, 0xd00, 0x10, 4, 1),
+	PIN_FIELD16(114, 114, 0xd00, 0x10, 0, 1),
+	PIN_FIELD16(115, 115, 0xd10, 0x10, 0, 1),
+	PIN_FIELD16(116, 116, 0xcd0, 0x10, 8, 1),
+	PIN_FIELD16(117, 117, 0xcc0, 0x10, 8, 1),
+	PIN_FIELD16(118, 118, 0xcf0, 0x10, 12, 1),
+	PIN_FIELD16(119, 119, 0xcf0, 0x10, 8, 1),
+	PIN_FIELD16(120, 120, 0xcf0, 0x10, 4, 1),
+	PIN_FIELD16(121, 121, 0xcf0, 0x10, 0, 1),
+	/* MSDC1 */
+	PIN_FIELD16(105, 105, 0xd40, 0x10, 8, 1),
+	PIN_FIELD16(106, 106, 0xd30, 0x10, 8, 1),
+	PIN_FIELD16(107, 107, 0xd60, 0x10, 0, 1),
+	PIN_FIELD16(108, 108, 0xd60, 0x10, 10, 1),
+	PIN_FIELD16(109, 109, 0xd60, 0x10, 4, 1),
+	PIN_FIELD16(110, 110, 0xc60, 0x10, 12, 1),
+	/* MSDC1 */
+	PIN_FIELD16(85, 85, 0xda0, 0x10, 8, 1),
+	PIN_FIELD16(86, 86, 0xd90, 0x10, 8, 1),
+	PIN_FIELD16(87, 87, 0xdc0, 0x10, 0, 1),
+	PIN_FIELD16(88, 88, 0xdc0, 0x10, 10, 1),
+	PIN_FIELD16(89, 89, 0xdc0, 0x10, 4, 1),
+	PIN_FIELD16(90, 90, 0xdc0, 0x10, 12, 1),
+	/* MSDC0E */
+	PIN_FIELD16(249, 249, 0x140, 0x10, 0, 1),
+	PIN_FIELD16(250, 250, 0x130, 0x10, 12, 1),
+	PIN_FIELD16(251, 251, 0x130, 0x10, 8, 1),
+	PIN_FIELD16(252, 252, 0x130, 0x10, 4, 1),
+	PIN_FIELD16(253, 253, 0x130, 0x10, 0, 1),
+	PIN_FIELD16(254, 254, 0xf40, 0x10, 12, 1),
+	PIN_FIELD16(255, 255, 0xf40, 0x10, 8, 1),
+	PIN_FIELD16(256, 256, 0xf40, 0x10, 4, 1),
+	PIN_FIELD16(257, 257, 0xf40, 0x10, 0, 1),
+	PIN_FIELD16(258, 258, 0xcb0, 0x10, 8, 1),
+	PIN_FIELD16(259, 259, 0xc90, 0x10, 8, 1),
+	PIN_FIELD16(261, 261, 0x140, 0x10, 8, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_r1_range[] = {
+	/* MSDC0 */
+	PIN_FIELD16(111, 111, 0xd00, 0x10, 13, 1),
+	PIN_FIELD16(112, 112, 0xd00, 0x10, 9, 1),
+	PIN_FIELD16(113, 113, 0xd00, 0x10, 5, 1),
+	PIN_FIELD16(114, 114, 0xd00, 0x10, 1, 1),
+	PIN_FIELD16(115, 115, 0xd10, 0x10, 1, 1),
+	PIN_FIELD16(116, 116, 0xcd0, 0x10, 9, 1),
+	PIN_FIELD16(117, 117, 0xcc0, 0x10, 9, 1),
+	PIN_FIELD16(118, 118, 0xcf0, 0x10, 13, 1),
+	PIN_FIELD16(119, 119, 0xcf0, 0x10, 9, 1),
+	PIN_FIELD16(120, 120, 0xcf0, 0x10, 5, 1),
+	PIN_FIELD16(121, 121, 0xcf0, 0x10, 1, 1),
+	/* MSDC1 */
+	PIN_FIELD16(105, 105, 0xd40, 0x10, 9, 1),
+	PIN_FIELD16(106, 106, 0xd30, 0x10, 9, 1),
+	PIN_FIELD16(107, 107, 0xd60, 0x10, 1, 1),
+	PIN_FIELD16(108, 108, 0xd60, 0x10, 9, 1),
+	PIN_FIELD16(109, 109, 0xd60, 0x10, 5, 1),
+	PIN_FIELD16(110, 110, 0xc60, 0x10, 13, 1),
+	/* MSDC2 */
+	PIN_FIELD16(85, 85, 0xda0, 0x10, 9, 1),
+	PIN_FIELD16(86, 86, 0xd90, 0x10, 9, 1),
+	PIN_FIELD16(87, 87, 0xdc0, 0x10, 1, 1),
+	PIN_FIELD16(88, 88, 0xdc0, 0x10, 9, 1),
+	PIN_FIELD16(89, 89, 0xdc0, 0x10, 5, 1),
+	PIN_FIELD16(90, 90, 0xdc0, 0x10, 13, 1),
+	/* MSDC0E */
+	PIN_FIELD16(249, 249, 0x140, 0x10, 1, 1),
+	PIN_FIELD16(250, 250, 0x130, 0x10, 13, 1),
+	PIN_FIELD16(251, 251, 0x130, 0x10, 9, 1),
+	PIN_FIELD16(252, 252, 0x130, 0x10, 5, 1),
+	PIN_FIELD16(253, 253, 0x130, 0x10, 1, 1),
+	PIN_FIELD16(254, 254, 0xf40, 0x10, 13, 1),
+	PIN_FIELD16(255, 255, 0xf40, 0x10, 9, 1),
+	PIN_FIELD16(256, 256, 0xf40, 0x10, 5, 1),
+	PIN_FIELD16(257, 257, 0xf40, 0x10, 1, 1),
+	PIN_FIELD16(258, 258, 0xcb0, 0x10, 9, 1),
+	PIN_FIELD16(259, 259, 0xc90, 0x10, 9, 1),
+	PIN_FIELD16(261, 261, 0x140, 0x10, 9, 1),
+};
+
+static const struct mtk_pin_field_calc mt7623_pin_r0_range[] = {
+	/* MSDC0 */
+	PIN_FIELD16(111, 111, 0xd00, 0x10, 14, 1),
+	PIN_FIELD16(112, 112, 0xd00, 0x10, 10, 1),
+	PIN_FIELD16(113, 113, 0xd00, 0x10, 6, 1),
+	PIN_FIELD16(114, 114, 0xd00, 0x10, 2, 1),
+	PIN_FIELD16(115, 115, 0xd10, 0x10, 2, 1),
+	PIN_FIELD16(116, 116, 0xcd0, 0x10, 10, 1),
+	PIN_FIELD16(117, 117, 0xcc0, 0x10, 10, 1),
+	PIN_FIELD16(118, 118, 0xcf0, 0x10, 14, 1),
+	PIN_FIELD16(119, 119, 0xcf0, 0x10, 10, 1),
+	PIN_FIELD16(120, 120, 0xcf0, 0x10, 6, 1),
+	PIN_FIELD16(121, 121, 0xcf0, 0x10, 2, 1),
+	/* MSDC1 */
+	PIN_FIELD16(105, 105, 0xd40, 0x10, 10, 1),
+	PIN_FIELD16(106, 106, 0xd30, 0x10, 10, 1),
+	PIN_FIELD16(107, 107, 0xd60, 0x10, 2, 1),
+	PIN_FIELD16(108, 108, 0xd60, 0x10, 8, 1),
+	PIN_FIELD16(109, 109, 0xd60, 0x10, 6, 1),
+	PIN_FIELD16(110, 110, 0xc60, 0x10, 14, 1),
+	/* MSDC2 */
+	PIN_FIELD16(85, 85, 0xda0, 0x10, 10, 1),
+	PIN_FIELD16(86, 86, 0xd90, 0x10, 10, 1),
+	PIN_FIELD16(87, 87, 0xdc0, 0x10, 2, 1),
+	PIN_FIELD16(88, 88, 0xdc0, 0x10, 8, 1),
+	PIN_FIELD16(89, 89, 0xdc0, 0x10, 6, 1),
+	PIN_FIELD16(90, 90, 0xdc0, 0x10, 14, 1),
+	/* MSDC0E */
+	PIN_FIELD16(249, 249, 0x140, 0x10, 2, 1),
+	PIN_FIELD16(250, 250, 0x130, 0x10, 14, 1),
+	PIN_FIELD16(251, 251, 0x130, 0x10, 10, 1),
+	PIN_FIELD16(252, 252, 0x130, 0x10, 6, 1),
+	PIN_FIELD16(253, 253, 0x130, 0x10, 2, 1),
+	PIN_FIELD16(254, 254, 0xf40, 0x10, 14, 1),
+	PIN_FIELD16(255, 255, 0xf40, 0x10, 10, 1),
+	PIN_FIELD16(256, 256, 0xf40, 0x10, 6, 1),
+	PIN_FIELD16(257, 257, 0xf40, 0x10, 5, 1),
+	PIN_FIELD16(258, 258, 0xcb0, 0x10, 10, 1),
+	PIN_FIELD16(259, 259, 0xc90, 0x10, 10, 1),
+	PIN_FIELD16(261, 261, 0x140, 0x10, 10, 1),
+};
+
+static const struct mtk_pin_reg_calc mt7623_reg_cals[] = {
+	[PINCTRL_PIN_REG_MODE] = MTK_RANGE(mt7623_pin_mode_range),
+	[PINCTRL_PIN_REG_DIR] = MTK_RANGE(mt7623_pin_dir_range),
+	[PINCTRL_PIN_REG_DI] = MTK_RANGE(mt7623_pin_di_range),
+	[PINCTRL_PIN_REG_DO] = MTK_RANGE(mt7623_pin_do_range),
+	[PINCTRL_PIN_REG_SMT] = MTK_RANGE(mt7623_pin_smt_range),
+	[PINCTRL_PIN_REG_PULLSEL] = MTK_RANGE(mt7623_pin_pullsel_range),
+	[PINCTRL_PIN_REG_PULLEN] = MTK_RANGE(mt7623_pin_pullen_range),
+	[PINCTRL_PIN_REG_DRV] = MTK_RANGE(mt7623_pin_drv_range),
+	[PINCTRL_PIN_REG_TDSEL] = MTK_RANGE(mt7623_pin_tdsel_range),
+	[PINCTRL_PIN_REG_IES] = MTK_RANGE(mt7623_pin_ies_range),
+	[PINCTRL_PIN_REG_PUPD] = MTK_RANGE(mt7623_pin_pupd_range),
+	[PINCTRL_PIN_REG_R0] = MTK_RANGE(mt7623_pin_r0_range),
+	[PINCTRL_PIN_REG_R1] = MTK_RANGE(mt7623_pin_r1_range),
+};
+
+static const struct mtk_pin_desc mt7623_pins[] = {
+	MT7623_PIN(0, "PWRAP_SPI0_MI", 148, DRV_GRP3),
+	MT7623_PIN(1, "PWRAP_SPI0_MO", 149, DRV_GRP3),
+	MT7623_PIN(2, "PWRAP_INT", 150, DRV_GRP3),
+	MT7623_PIN(3, "PWRAP_SPI0_CK", 151, DRV_GRP3),
+	MT7623_PIN(4, "PWRAP_SPI0_CSN", 152, DRV_GRP3),
+	MT7623_PIN(5, "PWRAP_SPI0_CK2", 153, DRV_GRP3),
+	MT7623_PIN(6, "PWRAP_SPI0_CSN2", 154, DRV_GRP3),
+	MT7623_PIN(7, "SPI1_CSN", 155, DRV_GRP3),
+	MT7623_PIN(8, "SPI1_MI", 156, DRV_GRP3),
+	MT7623_PIN(9, "SPI1_MO", 157, DRV_GRP3),
+	MT7623_PIN(10, "RTC32K_CK", 158, DRV_GRP3),
+	MT7623_PIN(11, "WATCHDOG", 159, DRV_GRP3),
+	MT7623_PIN(12, "SRCLKENA", 160, DRV_GRP3),
+	MT7623_PIN(13, "SRCLKENAI", 161, DRV_GRP3),
+	MT7623_PIN(14, "URXD2", 162, DRV_GRP1),
+	MT7623_PIN(15, "UTXD2", 163, DRV_GRP1),
+	MT7623_PIN(16, "I2S5_DATA_IN", 164, DRV_GRP1),
+	MT7623_PIN(17, "I2S5_BCK", 165, DRV_GRP1),
+	MT7623_PIN(18, "PCM_CLK", 166, DRV_GRP1),
+	MT7623_PIN(19, "PCM_SYNC", 167, DRV_GRP1),
+	MT7623_PIN(20, "PCM_RX", EINT_NA, DRV_GRP1),
+	MT7623_PIN(21, "PCM_TX", EINT_NA, DRV_GRP1),
+	MT7623_PIN(22, "EINT0", 0, DRV_GRP1),
+	MT7623_PIN(23, "EINT1", 1, DRV_GRP1),
+	MT7623_PIN(24, "EINT2", 2, DRV_GRP1),
+	MT7623_PIN(25, "EINT3", 3, DRV_GRP1),
+	MT7623_PIN(26, "EINT4", 4, DRV_GRP1),
+	MT7623_PIN(27, "EINT5", 5, DRV_GRP1),
+	MT7623_PIN(28, "EINT6", 6, DRV_GRP1),
+	MT7623_PIN(29, "EINT7", 7, DRV_GRP1),
+	MT7623_PIN(30, "I2S5_LRCK", 12, DRV_GRP1),
+	MT7623_PIN(31, "I2S5_MCLK", 13, DRV_GRP1),
+	MT7623_PIN(32, "I2S5_DATA", 14, DRV_GRP1),
+	MT7623_PIN(33, "I2S1_DATA", 15, DRV_GRP1),
+	MT7623_PIN(34, "I2S1_DATA_IN", 16, DRV_GRP1),
+	MT7623_PIN(35, "I2S1_BCK", 17, DRV_GRP1),
+	MT7623_PIN(36, "I2S1_LRCK", 18, DRV_GRP1),
+	MT7623_PIN(37, "I2S1_MCLK", 19, DRV_GRP1),
+	MT7623_PIN(38, "I2S2_DATA", 20, DRV_GRP1),
+	MT7623_PIN(39, "JTMS", 21, DRV_GRP3),
+	MT7623_PIN(40, "JTCK", 22, DRV_GRP3),
+	MT7623_PIN(41, "JTDI", 23, DRV_GRP3),
+	MT7623_PIN(42, "JTDO", 24, DRV_GRP3),
+	MT7623_PIN(43, "NCLE", 25, DRV_GRP1),
+	MT7623_PIN(44, "NCEB1", 26, DRV_GRP1),
+	MT7623_PIN(45, "NCEB0", 27, DRV_GRP1),
+	MT7623_PIN(46, "IR", 28, DRV_FIXED),
+	MT7623_PIN(47, "NREB", 29, DRV_GRP1),
+	MT7623_PIN(48, "NRNB", 30, DRV_GRP1),
+	MT7623_PIN(49, "I2S0_DATA", 31, DRV_GRP1),
+	MT7623_PIN(50, "I2S2_BCK", 32, DRV_GRP1),
+	MT7623_PIN(51, "I2S2_DATA_IN", 33, DRV_GRP1),
+	MT7623_PIN(52, "I2S2_LRCK", 34, DRV_GRP1),
+	MT7623_PIN(53, "SPI0_CSN", 35, DRV_GRP1),
+	MT7623_PIN(54, "SPI0_CK", 36, DRV_GRP1),
+	MT7623_PIN(55, "SPI0_MI", 37, DRV_GRP1),
+	MT7623_PIN(56, "SPI0_MO", 38, DRV_GRP1),
+	MT7623_PIN(57, "SDA1", 39, DRV_FIXED),
+	MT7623_PIN(58, "SCL1", 40, DRV_FIXED),
+	MT7623_PIN(59, "RAMBUF_I_CLK", EINT_NA, DRV_FIXED),
+	MT7623_PIN(60, "WB_RSTB", 41, DRV_GRP3),
+	MT7623_PIN(61, "F2W_DATA", 42, DRV_GRP3),
+	MT7623_PIN(62, "F2W_CLK", 43, DRV_GRP3),
+	MT7623_PIN(63, "WB_SCLK", 44, DRV_GRP3),
+	MT7623_PIN(64, "WB_SDATA", 45, DRV_GRP3),
+	MT7623_PIN(65, "WB_SEN", 46, DRV_GRP3),
+	MT7623_PIN(66, "WB_CRTL0", 47, DRV_GRP3),
+	MT7623_PIN(67, "WB_CRTL1", 48, DRV_GRP3),
+	MT7623_PIN(68, "WB_CRTL2", 49, DRV_GRP3),
+	MT7623_PIN(69, "WB_CRTL3", 50, DRV_GRP3),
+	MT7623_PIN(70, "WB_CRTL4", 51, DRV_GRP3),
+	MT7623_PIN(71, "WB_CRTL5", 52, DRV_GRP3),
+	MT7623_PIN(72, "I2S0_DATA_IN", 53, DRV_GRP1),
+	MT7623_PIN(73, "I2S0_LRCK", 54, DRV_GRP1),
+	MT7623_PIN(74, "I2S0_BCK", 55, DRV_GRP1),
+	MT7623_PIN(75, "SDA0", 56, DRV_FIXED),
+	MT7623_PIN(76, "SCL0", 57, DRV_FIXED),
+	MT7623_PIN(77, "SDA2", 58, DRV_FIXED),
+	MT7623_PIN(78, "SCL2", 59, DRV_FIXED),
+	MT7623_PIN(79, "URXD0", 60, DRV_FIXED),
+	MT7623_PIN(80, "UTXD0", 61, DRV_FIXED),
+	MT7623_PIN(81, "URXD1", 62, DRV_FIXED),
+	MT7623_PIN(82, "UTXD1", 63, DRV_FIXED),
+	MT7623_PIN(83, "LCM_RST", 64, DRV_FIXED),
+	MT7623_PIN(84, "DSI_TE", 65, DRV_FIXED),
+	MT7623_PIN(85, "MSDC2_CMD", 66, DRV_GRP4),
+	MT7623_PIN(86, "MSDC2_CLK", 67, DRV_GRP4),
+	MT7623_PIN(87, "MSDC2_DAT0", 68, DRV_GRP4),
+	MT7623_PIN(88, "MSDC2_DAT1", 69, DRV_GRP4),
+	MT7623_PIN(89, "MSDC2_DAT2", 70, DRV_GRP4),
+	MT7623_PIN(90, "MSDC2_DAT3", 71, DRV_GRP4),
+	MT7623_PIN(91, "TDN3", EINT_NA, DRV_FIXED),
+	MT7623_PIN(92, "TDP3", EINT_NA, DRV_FIXED),
+	MT7623_PIN(93, "TDN2", EINT_NA, DRV_FIXED),
+	MT7623_PIN(94, "TDP2", EINT_NA, DRV_FIXED),
+	MT7623_PIN(95, "TCN", EINT_NA, DRV_FIXED),
+	MT7623_PIN(96, "TCP", EINT_NA, DRV_FIXED),
+	MT7623_PIN(97, "TDN1", EINT_NA, DRV_FIXED),
+	MT7623_PIN(98, "TDP1", EINT_NA, DRV_FIXED),
+	MT7623_PIN(99, "TDN0", EINT_NA, DRV_FIXED),
+	MT7623_PIN(100, "TDP0", EINT_NA, DRV_FIXED),
+	MT7623_PIN(101, "SPI2_CSN", 74, DRV_FIXED),
+	MT7623_PIN(102, "SPI2_MI", 75, DRV_FIXED),
+	MT7623_PIN(103, "SPI2_MO", 76, DRV_FIXED),
+	MT7623_PIN(104, "SPI2_CLK", 77, DRV_FIXED),
+	MT7623_PIN(105, "MSDC1_CMD", 78, DRV_GRP4),
+	MT7623_PIN(106, "MSDC1_CLK", 79, DRV_GRP4),
+	MT7623_PIN(107, "MSDC1_DAT0", 80, DRV_GRP4),
+	MT7623_PIN(108, "MSDC1_DAT1", 81, DRV_GRP4),
+	MT7623_PIN(109, "MSDC1_DAT2", 82, DRV_GRP4),
+	MT7623_PIN(110, "MSDC1_DAT3", 83, DRV_GRP4),
+	MT7623_PIN(111, "MSDC0_DAT7", 84, DRV_GRP4),
+	MT7623_PIN(112, "MSDC0_DAT6", 85, DRV_GRP4),
+	MT7623_PIN(113, "MSDC0_DAT5", 86, DRV_GRP4),
+	MT7623_PIN(114, "MSDC0_DAT4", 87, DRV_GRP4),
+	MT7623_PIN(115, "MSDC0_RSTB", 88, DRV_GRP4),
+	MT7623_PIN(116, "MSDC0_CMD", 89, DRV_GRP4),
+	MT7623_PIN(117, "MSDC0_CLK", 90, DRV_GRP4),
+	MT7623_PIN(118, "MSDC0_DAT3", 91, DRV_GRP4),
+	MT7623_PIN(119, "MSDC0_DAT2", 92, DRV_GRP4),
+	MT7623_PIN(120, "MSDC0_DAT1", 93, DRV_GRP4),
+	MT7623_PIN(121, "MSDC0_DAT0", 94, DRV_GRP4),
+	MT7623_PIN(122, "CEC", 95, DRV_FIXED),
+	MT7623_PIN(123, "HTPLG", 96, DRV_FIXED),
+	MT7623_PIN(124, "HDMISCK", 97, DRV_FIXED),
+	MT7623_PIN(125, "HDMISD", 98, DRV_FIXED),
+	MT7623_PIN(126, "I2S0_MCLK", 99, DRV_GRP1),
+	MT7623_PIN(127, "RAMBUF_IDATA0", EINT_NA, DRV_FIXED),
+	MT7623_PIN(128, "RAMBUF_IDATA1", EINT_NA, DRV_FIXED),
+	MT7623_PIN(129, "RAMBUF_IDATA2", EINT_NA, DRV_FIXED),
+	MT7623_PIN(130, "RAMBUF_IDATA3", EINT_NA, DRV_FIXED),
+	MT7623_PIN(131, "RAMBUF_IDATA4", EINT_NA, DRV_FIXED),
+	MT7623_PIN(132, "RAMBUF_IDATA5", EINT_NA, DRV_FIXED),
+	MT7623_PIN(133, "RAMBUF_IDATA6", EINT_NA, DRV_FIXED),
+	MT7623_PIN(134, "RAMBUF_IDATA7", EINT_NA, DRV_FIXED),
+	MT7623_PIN(135, "RAMBUF_IDATA8", EINT_NA, DRV_FIXED),
+	MT7623_PIN(136, "RAMBUF_IDATA9", EINT_NA, DRV_FIXED),
+	MT7623_PIN(137, "RAMBUF_IDATA10", EINT_NA, DRV_FIXED),
+	MT7623_PIN(138, "RAMBUF_IDATA11", EINT_NA, DRV_FIXED),
+	MT7623_PIN(139, "RAMBUF_IDATA12", EINT_NA, DRV_FIXED),
+	MT7623_PIN(140, "RAMBUF_IDATA13", EINT_NA, DRV_FIXED),
+	MT7623_PIN(141, "RAMBUF_IDATA14", EINT_NA, DRV_FIXED),
+	MT7623_PIN(142, "RAMBUF_IDATA15", EINT_NA, DRV_FIXED),
+	MT7623_PIN(143, "RAMBUF_ODATA0", EINT_NA, DRV_FIXED),
+	MT7623_PIN(144, "RAMBUF_ODATA1", EINT_NA, DRV_FIXED),
+	MT7623_PIN(145, "RAMBUF_ODATA2", EINT_NA, DRV_FIXED),
+	MT7623_PIN(146, "RAMBUF_ODATA3", EINT_NA, DRV_FIXED),
+	MT7623_PIN(147, "RAMBUF_ODATA4", EINT_NA, DRV_FIXED),
+	MT7623_PIN(148, "RAMBUF_ODATA5", EINT_NA, DRV_FIXED),
+	MT7623_PIN(149, "RAMBUF_ODATA6", EINT_NA, DRV_FIXED),
+	MT7623_PIN(150, "RAMBUF_ODATA7", EINT_NA, DRV_FIXED),
+	MT7623_PIN(151, "RAMBUF_ODATA8", EINT_NA, DRV_FIXED),
+	MT7623_PIN(152, "RAMBUF_ODATA9", EINT_NA, DRV_FIXED),
+	MT7623_PIN(153, "RAMBUF_ODATA10", EINT_NA, DRV_FIXED),
+	MT7623_PIN(154, "RAMBUF_ODATA11", EINT_NA, DRV_FIXED),
+	MT7623_PIN(155, "RAMBUF_ODATA12", EINT_NA, DRV_FIXED),
+	MT7623_PIN(156, "RAMBUF_ODATA13", EINT_NA, DRV_FIXED),
+	MT7623_PIN(157, "RAMBUF_ODATA14", EINT_NA, DRV_FIXED),
+	MT7623_PIN(158, "RAMBUF_ODATA15", EINT_NA, DRV_FIXED),
+	MT7623_PIN(159, "RAMBUF_BE0", EINT_NA, DRV_FIXED),
+	MT7623_PIN(160, "RAMBUF_BE1", EINT_NA, DRV_FIXED),
+	MT7623_PIN(161, "AP2PT_INT", EINT_NA, DRV_FIXED),
+	MT7623_PIN(162, "AP2PT_INT_CLR", EINT_NA, DRV_FIXED),
+	MT7623_PIN(163, "PT2AP_INT", EINT_NA, DRV_FIXED),
+	MT7623_PIN(164, "PT2AP_INT_CLR", EINT_NA, DRV_FIXED),
+	MT7623_PIN(165, "AP2UP_INT", EINT_NA, DRV_FIXED),
+	MT7623_PIN(166, "AP2UP_INT_CLR", EINT_NA, DRV_FIXED),
+	MT7623_PIN(167, "UP2AP_INT", EINT_NA, DRV_FIXED),
+	MT7623_PIN(168, "UP2AP_INT_CLR", EINT_NA, DRV_FIXED),
+	MT7623_PIN(169, "RAMBUF_ADDR0", EINT_NA, DRV_FIXED),
+	MT7623_PIN(170, "RAMBUF_ADDR1", EINT_NA, DRV_FIXED),
+	MT7623_PIN(171, "RAMBUF_ADDR2", EINT_NA, DRV_FIXED),
+	MT7623_PIN(172, "RAMBUF_ADDR3", EINT_NA, DRV_FIXED),
+	MT7623_PIN(173, "RAMBUF_ADDR4", EINT_NA, DRV_FIXED),
+	MT7623_PIN(174, "RAMBUF_ADDR5", EINT_NA, DRV_FIXED),
+	MT7623_PIN(175, "RAMBUF_ADDR6", EINT_NA, DRV_FIXED),
+	MT7623_PIN(176, "RAMBUF_ADDR7", EINT_NA, DRV_FIXED),
+	MT7623_PIN(177, "RAMBUF_ADDR8", EINT_NA, DRV_FIXED),
+	MT7623_PIN(178, "RAMBUF_ADDR9", EINT_NA, DRV_FIXED),
+	MT7623_PIN(179, "RAMBUF_ADDR10", EINT_NA, DRV_FIXED),
+	MT7623_PIN(180, "RAMBUF_RW", EINT_NA, DRV_FIXED),
+	MT7623_PIN(181, "RAMBUF_LAST", EINT_NA, DRV_FIXED),
+	MT7623_PIN(182, "RAMBUF_HP", EINT_NA, DRV_FIXED),
+	MT7623_PIN(183, "RAMBUF_REQ", EINT_NA, DRV_FIXED),
+	MT7623_PIN(184, "RAMBUF_ALE", EINT_NA, DRV_FIXED),
+	MT7623_PIN(185, "RAMBUF_DLE", EINT_NA, DRV_FIXED),
+	MT7623_PIN(186, "RAMBUF_WDLE", EINT_NA, DRV_FIXED),
+	MT7623_PIN(187, "RAMBUF_O_CLK", EINT_NA, DRV_FIXED),
+	MT7623_PIN(188, "I2S2_MCLK", 100, DRV_GRP1),
+	MT7623_PIN(189, "I2S3_DATA", 101, DRV_GRP1),
+	MT7623_PIN(190, "I2S3_DATA_IN", 102, DRV_GRP1),
+	MT7623_PIN(191, "I2S3_BCK", 103, DRV_GRP1),
+	MT7623_PIN(192, "I2S3_LRCK", 104, DRV_GRP1),
+	MT7623_PIN(193, "I2S3_MCLK", 105, DRV_GRP1),
+	MT7623_PIN(194, "I2S4_DATA", 106, DRV_GRP1),
+	MT7623_PIN(195, "I2S4_DATA_IN", 107, DRV_GRP1),
+	MT7623_PIN(196, "I2S4_BCK", 108, DRV_GRP1),
+	MT7623_PIN(197, "I2S4_LRCK", 109, DRV_GRP1),
+	MT7623_PIN(198, "I2S4_MCLK", 110, DRV_GRP1),
+	MT7623_PIN(199, "SPI1_CLK", 111, DRV_GRP3),
+	MT7623_PIN(200, "SPDIF_OUT", 112, DRV_GRP1),
+	MT7623_PIN(201, "SPDIF_IN0", 113, DRV_GRP1),
+	MT7623_PIN(202, "SPDIF_IN1", 114, DRV_GRP1),
+	MT7623_PIN(203, "PWM0", 115, DRV_GRP1),
+	MT7623_PIN(204, "PWM1", 116, DRV_GRP1),
+	MT7623_PIN(205, "PWM2", 117, DRV_GRP1),
+	MT7623_PIN(206, "PWM3", 118, DRV_GRP1),
+	MT7623_PIN(207, "PWM4", 119, DRV_GRP1),
+	MT7623_PIN(208, "AUD_EXT_CK1", 120, DRV_GRP1),
+	MT7623_PIN(209, "AUD_EXT_CK2", 121, DRV_GRP1),
+	MT7623_PIN(210, "AUD_CLOCK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(211, "DVP_RESET", EINT_NA, DRV_GRP3),
+	MT7623_PIN(212, "DVP_CLOCK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(213, "DVP_CS", EINT_NA, DRV_GRP3),
+	MT7623_PIN(214, "DVP_CK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(215, "DVP_DI", EINT_NA, DRV_GRP3),
+	MT7623_PIN(216, "DVP_DO", EINT_NA, DRV_GRP3),
+	MT7623_PIN(217, "AP_CS", EINT_NA, DRV_GRP3),
+	MT7623_PIN(218, "AP_CK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(219, "AP_DI", EINT_NA, DRV_GRP3),
+	MT7623_PIN(220, "AP_DO", EINT_NA, DRV_GRP3),
+	MT7623_PIN(221, "DVD_BCLK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(222, "T8032_CLK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(223, "AP_BCLK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(224, "HOST_CS", EINT_NA, DRV_GRP3),
+	MT7623_PIN(225, "HOST_CK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(226, "HOST_DO0", EINT_NA, DRV_GRP3),
+	MT7623_PIN(227, "HOST_DO1", EINT_NA, DRV_GRP3),
+	MT7623_PIN(228, "SLV_CS", EINT_NA, DRV_GRP3),
+	MT7623_PIN(229, "SLV_CK", EINT_NA, DRV_GRP3),
+	MT7623_PIN(230, "SLV_DI0", EINT_NA, DRV_GRP3),
+	MT7623_PIN(231, "SLV_DI1", EINT_NA, DRV_GRP3),
+	MT7623_PIN(232, "AP2DSP_INT", EINT_NA, DRV_GRP3),
+	MT7623_PIN(233, "AP2DSP_INT_CLR", EINT_NA, DRV_GRP3),
+	MT7623_PIN(234, "DSP2AP_INT", EINT_NA, DRV_GRP3),
+	MT7623_PIN(235, "DSP2AP_INT_CLR", EINT_NA, DRV_GRP3),
+	MT7623_PIN(236, "EXT_SDIO3", 122, DRV_GRP1),
+	MT7623_PIN(237, "EXT_SDIO2", 123, DRV_GRP1),
+	MT7623_PIN(238, "EXT_SDIO1", 124, DRV_GRP1),
+	MT7623_PIN(239, "EXT_SDIO0", 125, DRV_GRP1),
+	MT7623_PIN(240, "EXT_XCS", 126, DRV_GRP1),
+	MT7623_PIN(241, "EXT_SCK", 127, DRV_GRP1),
+	MT7623_PIN(242, "URTS2", 128, DRV_GRP1),
+	MT7623_PIN(243, "UCTS2", 129, DRV_GRP1),
+	MT7623_PIN(244, "HDMI_SDA_RX", 130, DRV_FIXED),
+	MT7623_PIN(245, "HDMI_SCL_RX", 131, DRV_FIXED),
+	MT7623_PIN(246, "MHL_SENCE", 132, DRV_FIXED),
+	MT7623_PIN(247, "HDMI_HPD_CBUS_RX", 69, DRV_FIXED),
+	MT7623_PIN(248, "HDMI_TESTOUTP_RX", 133, DRV_GRP1),
+	MT7623_PIN(249, "MSDC0E_RSTB", 134, DRV_GRP4),
+	MT7623_PIN(250, "MSDC0E_DAT7", 135, DRV_GRP4),
+	MT7623_PIN(251, "MSDC0E_DAT6", 136, DRV_GRP4),
+	MT7623_PIN(252, "MSDC0E_DAT5", 137, DRV_GRP4),
+	MT7623_PIN(253, "MSDC0E_DAT4", 138, DRV_GRP4),
+	MT7623_PIN(254, "MSDC0E_DAT3", 139, DRV_GRP4),
+	MT7623_PIN(255, "MSDC0E_DAT2", 140, DRV_GRP4),
+	MT7623_PIN(256, "MSDC0E_DAT1", 141, DRV_GRP4),
+	MT7623_PIN(257, "MSDC0E_DAT0", 142, DRV_GRP4),
+	MT7623_PIN(258, "MSDC0E_CMD", 143, DRV_GRP4),
+	MT7623_PIN(259, "MSDC0E_CLK", 144, DRV_GRP4),
+	MT7623_PIN(260, "MSDC0E_DSL", 145, DRV_GRP4),
+	MT7623_PIN(261, "MSDC1_INS", 146, DRV_GRP4),
+	MT7623_PIN(262, "G2_TXEN", 8, DRV_GRP1),
+	MT7623_PIN(263, "G2_TXD3", 9, DRV_GRP1),
+	MT7623_PIN(264, "G2_TXD2", 10, DRV_GRP1),
+	MT7623_PIN(265, "G2_TXD1", 11, DRV_GRP1),
+	MT7623_PIN(266, "G2_TXD0", EINT_NA, DRV_GRP1),
+	MT7623_PIN(267, "G2_TXC", EINT_NA, DRV_GRP1),
+	MT7623_PIN(268, "G2_RXC", EINT_NA, DRV_GRP1),
+	MT7623_PIN(269, "G2_RXD0", EINT_NA, DRV_GRP1),
+	MT7623_PIN(270, "G2_RXD1", EINT_NA, DRV_GRP1),
+	MT7623_PIN(271, "G2_RXD2", EINT_NA, DRV_GRP1),
+	MT7623_PIN(272, "G2_RXD3", EINT_NA, DRV_GRP1),
+	MT7623_PIN(273, "ESW_INT", 168, DRV_GRP1),
+	MT7623_PIN(274, "G2_RXDV", EINT_NA, DRV_GRP1),
+	MT7623_PIN(275, "MDC", EINT_NA, DRV_GRP1),
+	MT7623_PIN(276, "MDIO", EINT_NA, DRV_GRP1),
+	MT7623_PIN(277, "ESW_RST", EINT_NA, DRV_GRP1),
+	MT7623_PIN(278, "JTAG_RESET", 147, DRV_GRP3),
+	MT7623_PIN(279, "USB3_RES_BOND", EINT_NA, DRV_GRP1),
+};
+
+/* List all groups consisting of these pins dedicated to the enablement of
+ * certain hardware block and the corresponding mode for all of the pins.
+ * The hardware probably has multiple combinations of these pinouts.
+ */
+
+/* AUDIO EXT CLK */
+static int mt7623_aud_ext_clk0_pins[] = { 208, };
+static int mt7623_aud_ext_clk0_funcs[] = { 1, };
+static int mt7623_aud_ext_clk1_pins[] = { 209, };
+static int mt7623_aud_ext_clk1_funcs[] = { 1, };
+
+/* DISP PWM */
+static int mt7623_disp_pwm_0_pins[] = { 72, };
+static int mt7623_disp_pwm_0_funcs[] = { 5, };
+static int mt7623_disp_pwm_1_pins[] = { 203, };
+static int mt7623_disp_pwm_1_funcs[] = { 2, };
+static int mt7623_disp_pwm_2_pins[] = { 208, };
+static int mt7623_disp_pwm_2_funcs[] = { 5, };
+
+/* ESW */
+static int mt7623_esw_int_pins[] = { 273, };
+static int mt7623_esw_int_funcs[] = { 1, };
+static int mt7623_esw_rst_pins[] = { 277, };
+static int mt7623_esw_rst_funcs[] = { 1, };
+
+/* EPHY */
+static int mt7623_ephy_pins[] = { 262, 263, 264, 265, 266, 267, 268,
+				  269, 270, 271, 272, 274, };
+static int mt7623_ephy_funcs[] = { 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, };
+
+/* EXT_SDIO */
+static int mt7623_ext_sdio_pins[] = { 236, 237, 238, 239, 240, 241, };
+static int mt7623_ext_sdio_funcs[] = { 1, 1, 1, 1, 1, 1, };
+
+/* HDMI RX */
+static int mt7623_hdmi_rx_pins[] = { 247, 248, };
+static int mt7623_hdmi_rx_funcs[] = { 1, 1 };
+static int mt7623_hdmi_rx_i2c_pins[] = { 244, 245, };
+static int mt7623_hdmi_rx_i2c_funcs[] = { 1, 1 };
+
+/* HDMI TX */
+static int mt7623_hdmi_cec_pins[] = { 122, };
+static int mt7623_hdmi_cec_funcs[] = { 1, };
+static int mt7623_hdmi_htplg_pins[] = { 123, };
+static int mt7623_hdmi_htplg_funcs[] = { 1, };
+static int mt7623_hdmi_i2c_pins[] = { 124, 125, };
+static int mt7623_hdmi_i2c_funcs[] = { 1, 1 };
+
+/* I2C */
+static int mt7623_i2c0_pins[] = { 75, 76, };
+static int mt7623_i2c0_funcs[] = { 1, 1, };
+static int mt7623_i2c1_0_pins[] = { 57, 58, };
+static int mt7623_i2c1_0_funcs[] = { 1, 1, };
+static int mt7623_i2c1_1_pins[] = { 242, 243, };
+static int mt7623_i2c1_1_funcs[] = { 4, 4, };
+static int mt7623_i2c1_2_pins[] = { 85, 86, };
+static int mt7623_i2c1_2_funcs[] = { 3, 3, };
+static int mt7623_i2c1_3_pins[] = { 105, 106, };
+static int mt7623_i2c1_3_funcs[] = { 3, 3, };
+static int mt7623_i2c1_4_pins[] = { 124, 125, };
+static int mt7623_i2c1_4_funcs[] = { 4, 4, };
+static int mt7623_i2c2_0_pins[] = { 77, 78, };
+static int mt7623_i2c2_0_funcs[] = { 1, 1, };
+static int mt7623_i2c2_1_pins[] = { 89, 90, };
+static int mt7623_i2c2_1_funcs[] = { 3, 3, };
+static int mt7623_i2c2_2_pins[] = { 109, 110, };
+static int mt7623_i2c2_2_funcs[] = { 3, 3, };
+static int mt7623_i2c2_3_pins[] = { 122, 123, };
+static int mt7623_i2c2_3_funcs[] = { 4, 4, };
+
+/* I2S */
+static int mt7623_i2s0_pins[] = { 49, 72, 73, 74, 126, };
+static int mt7623_i2s0_funcs[] = { 1, 1, 1, 1, 1, };
+static int mt7623_i2s1_pins[] = { 33, 34, 35, 36, 37, };
+static int mt7623_i2s1_funcs[] = { 1, 1, 1, 1, 1, };
+static int mt7623_i2s2_bclk_lrclk_mclk_pins[] = { 50, 52, 188, };
+static int mt7623_i2s2_bclk_lrclk_mclk_funcs[] = { 1, 1, 1, };
+static int mt7623_i2s2_data_in_pins[] = { 51, };
+static int mt7623_i2s2_data_in_funcs[] = { 1, };
+static int mt7623_i2s2_data_0_pins[] = { 203, };
+static int mt7623_i2s2_data_0_funcs[] = { 9, };
+static int mt7623_i2s2_data_1_pins[] = { 38,  };
+static int mt7623_i2s2_data_1_funcs[] = { 4, };
+static int mt7623_i2s3_bclk_lrclk_mclk_pins[] = { 191, 192, 193, };
+static int mt7623_i2s3_bclk_lrclk_mclk_funcs[] = { 1, 1, 1, };
+static int mt7623_i2s3_data_in_pins[] = { 190, };
+static int mt7623_i2s3_data_in_funcs[] = { 1, };
+static int mt7623_i2s3_data_0_pins[] = { 204, };
+static int mt7623_i2s3_data_0_funcs[] = { 9, };
+static int mt7623_i2s3_data_1_pins[] = { 2, };
+static int mt7623_i2s3_data_1_funcs[] = { 0, };
+static int mt7623_i2s4_pins[] = { 194, 195, 196, 197, 198, };
+static int mt7623_i2s4_funcs[] = { 1, 1, 1, 1, 1, };
+static int mt7623_i2s5_pins[] = { 16, 17, 30, 31, 32, };
+static int mt7623_i2s5_funcs[] = { 1, 1, 1, 1, 1, };
+
+/* IR */
+static int mt7623_ir_pins[] = { 46, };
+static int mt7623_ir_funcs[] = { 1, };
+
+/* LCD */
+static int mt7623_mipi_tx_pins[] = { 91, 92, 93, 94, 95, 96, 97, 98,
+				     99, 100, };
+static int mt7623_mipi_tx_funcs[] = { 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, };
+static int mt7623_dsi_te_pins[] = { 84, };
+static int mt7623_dsi_te_funcs[] = { 1, };
+static int mt7623_lcm_rst_pins[] = { 83, };
+static int mt7623_lcm_rst_funcs[] = { 1, };
+
+/* MDC/MDIO */
+static int mt7623_mdc_mdio_pins[] = { 275, 276, };
+static int mt7623_mdc_mdio_funcs[] = { 1, 1, };
+
+/* MSDC */
+static int mt7623_msdc0_pins[] = { 111, 112, 113, 114, 115, 116, 117, 118,
+				   119, 120, 121, };
+static int mt7623_msdc0_funcs[] = { 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, };
+static int mt7623_msdc1_pins[] = { 105, 106, 107, 108, 109, 110, };
+static int mt7623_msdc1_funcs[] = { 1, 1, 1, 1, 1, 1, };
+static int mt7623_msdc1_ins_pins[] = { 261, };
+static int mt7623_msdc1_ins_funcs[] = { 1, };
+static int mt7623_msdc1_wp_0_pins[] = { 29, };
+static int mt7623_msdc1_wp_0_funcs[] = { 1, };
+static int mt7623_msdc1_wp_1_pins[] = { 55, };
+static int mt7623_msdc1_wp_1_funcs[] = { 3, };
+static int mt7623_msdc1_wp_2_pins[] = { 209, };
+static int mt7623_msdc1_wp_2_funcs[] = { 2, };
+static int mt7623_msdc2_pins[] = { 85, 86, 87, 88, 89, 90, };
+static int mt7623_msdc2_funcs[] = { 1, 1, 1, 1, 1, 1, };
+static int mt7623_msdc3_pins[] = { 249, 250, 251, 252, 253, 254, 255, 256,
+				   257, 258, 259, 260, };
+static int mt7623_msdc3_funcs[] = { 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, };
+
+/* NAND */
+static int mt7623_nandc_pins[] = { 43, 47, 48, 111, 112, 113, 114, 115,
+				   116, 117, 118, 119, 120, 121, };
+static int mt7623_nandc_funcs[] = { 1, 1, 1, 4, 4, 4, 4, 4, 4, 4, 4, 4,
+				   4, 4, };
+static int mt7623_nandc_ceb0_pins[] = { 45, };
+static int mt7623_nandc_ceb0_funcs[] = { 1, };
+static int mt7623_nandc_ceb1_pins[] = { 44, };
+static int mt7623_nandc_ceb1_funcs[] = { 1, };
+
+/* RTC */
+static int mt7623_rtc_pins[] = { 10, };
+static int mt7623_rtc_funcs[] = { 1, };
+
+/* OTG */
+static int mt7623_otg_iddig0_0_pins[] = { 29, };
+static int mt7623_otg_iddig0_0_funcs[] = { 1, };
+static int mt7623_otg_iddig0_1_pins[] = { 44, };
+static int mt7623_otg_iddig0_1_funcs[] = { 2, };
+static int mt7623_otg_iddig0_2_pins[] = { 236, };
+static int mt7623_otg_iddig0_2_funcs[] = { 2, };
+static int mt7623_otg_iddig1_0_pins[] = { 27, };
+static int mt7623_otg_iddig1_0_funcs[] = { 2, };
+static int mt7623_otg_iddig1_1_pins[] = { 47, };
+static int mt7623_otg_iddig1_1_funcs[] = { 2, };
+static int mt7623_otg_iddig1_2_pins[] = { 238, };
+static int mt7623_otg_iddig1_2_funcs[] = { 2, };
+static int mt7623_otg_drv_vbus0_0_pins[] = { 28, };
+static int mt7623_otg_drv_vbus0_0_funcs[] = { 1, };
+static int mt7623_otg_drv_vbus0_1_pins[] = { 45, };
+static int mt7623_otg_drv_vbus0_1_funcs[] = { 2, };
+static int mt7623_otg_drv_vbus0_2_pins[] = { 237, };
+static int mt7623_otg_drv_vbus0_2_funcs[] = { 2, };
+static int mt7623_otg_drv_vbus1_0_pins[] = { 26, };
+static int mt7623_otg_drv_vbus1_0_funcs[] = { 2, };
+static int mt7623_otg_drv_vbus1_1_pins[] = { 48, };
+static int mt7623_otg_drv_vbus1_1_funcs[] = { 2, };
+static int mt7623_otg_drv_vbus1_2_pins[] = { 239, };
+static int mt7623_otg_drv_vbus1_2_funcs[] = { 2, };
+
+/* PCIE */
+static int mt7623_pcie0_0_perst_pins[] = { 208, };
+static int mt7623_pcie0_0_perst_funcs[] = { 3, };
+static int mt7623_pcie0_1_perst_pins[] = { 22, };
+static int mt7623_pcie0_1_perst_funcs[] = { 2, };
+static int mt7623_pcie1_0_perst_pins[] = { 209, };
+static int mt7623_pcie1_0_perst_funcs[] = { 3, };
+static int mt7623_pcie1_1_perst_pins[] = { 23, };
+static int mt7623_pcie1_1_perst_funcs[] = { 2, };
+static int mt7623_pcie2_0_perst_pins[] = { 24, };
+static int mt7623_pcie2_0_perst_funcs[] = { 2, };
+static int mt7623_pcie2_1_perst_pins[] = { 29, };
+static int mt7623_pcie2_1_perst_funcs[] = { 6, };
+static int mt7623_pcie0_0_wake_pins[] = { 28, };
+static int mt7623_pcie0_0_wake_funcs[] = { 6, };
+static int mt7623_pcie0_1_wake_pins[] = { 251, };
+static int mt7623_pcie0_1_wake_funcs[] = { 6, };
+static int mt7623_pcie1_0_wake_pins[] = { 27, };
+static int mt7623_pcie1_0_wake_funcs[] = { 6, };
+static int mt7623_pcie1_1_wake_pins[] = { 253, };
+static int mt7623_pcie1_1_wake_funcs[] = { 6, };
+static int mt7623_pcie2_0_wake_pins[] = { 26, };
+static int mt7623_pcie2_0_wake_funcs[] = { 6, };
+static int mt7623_pcie2_1_wake_pins[] = { 255, };
+static int mt7623_pcie2_1_wake_funcs[] = { 6, };
+static int mt7623_pcie0_clkreq_pins[] = { 250, };
+static int mt7623_pcie0_clkreq_funcs[] = { 6, };
+static int mt7623_pcie1_clkreq_pins[] = { 252, };
+static int mt7623_pcie1_clkreq_funcs[] = { 6, };
+static int mt7623_pcie2_clkreq_pins[] = { 254, };
+static int mt7623_pcie2_clkreq_funcs[] = { 6, };
+
+/* the pcie_*_rev are only used for MT7623 */
+static int mt7623_pcie0_0_rev_perst_pins[] = { 208, };
+static int mt7623_pcie0_0_rev_perst_funcs[] = { 11, };
+static int mt7623_pcie0_1_rev_perst_pins[] = { 22, };
+static int mt7623_pcie0_1_rev_perst_funcs[] = { 10, };
+static int mt7623_pcie1_0_rev_perst_pins[] = { 209, };
+static int mt7623_pcie1_0_rev_perst_funcs[] = { 11, };
+static int mt7623_pcie1_1_rev_perst_pins[] = { 23, };
+static int mt7623_pcie1_1_rev_perst_funcs[] = { 10, };
+static int mt7623_pcie2_0_rev_perst_pins[] = { 24, };
+static int mt7623_pcie2_0_rev_perst_funcs[] = { 11, };
+static int mt7623_pcie2_1_rev_perst_pins[] = { 29, };
+static int mt7623_pcie2_1_rev_perst_funcs[] = { 14, };
+
+/* PCM */
+static int mt7623_pcm_clk_0_pins[] = { 18, };
+static int mt7623_pcm_clk_0_funcs[] = { 1, };
+static int mt7623_pcm_clk_1_pins[] = { 17, };
+static int mt7623_pcm_clk_1_funcs[] = { 3, };
+static int mt7623_pcm_clk_2_pins[] = { 35, };
+static int mt7623_pcm_clk_2_funcs[] = { 3, };
+static int mt7623_pcm_clk_3_pins[] = { 50, };
+static int mt7623_pcm_clk_3_funcs[] = { 3, };
+static int mt7623_pcm_clk_4_pins[] = { 74, };
+static int mt7623_pcm_clk_4_funcs[] = { 3, };
+static int mt7623_pcm_clk_5_pins[] = { 191, };
+static int mt7623_pcm_clk_5_funcs[] = { 3, };
+static int mt7623_pcm_clk_6_pins[] = { 196, };
+static int mt7623_pcm_clk_6_funcs[] = { 3, };
+static int mt7623_pcm_sync_0_pins[] = { 19, };
+static int mt7623_pcm_sync_0_funcs[] = { 1, };
+static int mt7623_pcm_sync_1_pins[] = { 30, };
+static int mt7623_pcm_sync_1_funcs[] = { 3, };
+static int mt7623_pcm_sync_2_pins[] = { 36, };
+static int mt7623_pcm_sync_2_funcs[] = { 3, };
+static int mt7623_pcm_sync_3_pins[] = { 52, };
+static int mt7623_pcm_sync_3_funcs[] = { 31, };
+static int mt7623_pcm_sync_4_pins[] = { 73, };
+static int mt7623_pcm_sync_4_funcs[] = { 3, };
+static int mt7623_pcm_sync_5_pins[] = { 192, };
+static int mt7623_pcm_sync_5_funcs[] = { 3, };
+static int mt7623_pcm_sync_6_pins[] = { 197, };
+static int mt7623_pcm_sync_6_funcs[] = { 3, };
+static int mt7623_pcm_rx_0_pins[] = { 20, };
+static int mt7623_pcm_rx_0_funcs[] = { 1, };
+static int mt7623_pcm_rx_1_pins[] = { 16, };
+static int mt7623_pcm_rx_1_funcs[] = { 3, };
+static int mt7623_pcm_rx_2_pins[] = { 34, };
+static int mt7623_pcm_rx_2_funcs[] = { 3, };
+static int mt7623_pcm_rx_3_pins[] = { 51, };
+static int mt7623_pcm_rx_3_funcs[] = { 3, };
+static int mt7623_pcm_rx_4_pins[] = { 72, };
+static int mt7623_pcm_rx_4_funcs[] = { 3, };
+static int mt7623_pcm_rx_5_pins[] = { 190, };
+static int mt7623_pcm_rx_5_funcs[] = { 3, };
+static int mt7623_pcm_rx_6_pins[] = { 195, };
+static int mt7623_pcm_rx_6_funcs[] = { 3, };
+static int mt7623_pcm_tx_0_pins[] = { 21, };
+static int mt7623_pcm_tx_0_funcs[] = { 1, };
+static int mt7623_pcm_tx_1_pins[] = { 32, };
+static int mt7623_pcm_tx_1_funcs[] = { 3, };
+static int mt7623_pcm_tx_2_pins[] = { 33, };
+static int mt7623_pcm_tx_2_funcs[] = { 3, };
+static int mt7623_pcm_tx_3_pins[] = { 38, };
+static int mt7623_pcm_tx_3_funcs[] = { 3, };
+static int mt7623_pcm_tx_4_pins[] = { 49, };
+static int mt7623_pcm_tx_4_funcs[] = { 3, };
+static int mt7623_pcm_tx_5_pins[] = { 189, };
+static int mt7623_pcm_tx_5_funcs[] = { 3, };
+static int mt7623_pcm_tx_6_pins[] = { 194, };
+static int mt7623_pcm_tx_6_funcs[] = { 3, };
+
+/* PWM */
+static int mt7623_pwm_ch1_0_pins[] = { 203, };
+static int mt7623_pwm_ch1_0_funcs[] = { 1, };
+static int mt7623_pwm_ch1_1_pins[] = { 208, };
+static int mt7623_pwm_ch1_1_funcs[] = { 2, };
+static int mt7623_pwm_ch1_2_pins[] = { 72, };
+static int mt7623_pwm_ch1_2_funcs[] = { 4, };
+static int mt7623_pwm_ch1_3_pins[] = { 88, };
+static int mt7623_pwm_ch1_3_funcs[] = { 3, };
+static int mt7623_pwm_ch1_4_pins[] = { 108, };
+static int mt7623_pwm_ch1_4_funcs[] = { 3, };
+static int mt7623_pwm_ch2_0_pins[] = { 204, };
+static int mt7623_pwm_ch2_0_funcs[] = { 1, };
+static int mt7623_pwm_ch2_1_pins[] = { 53, };
+static int mt7623_pwm_ch2_1_funcs[] = { 5, };
+static int mt7623_pwm_ch2_2_pins[] = { 88, };
+static int mt7623_pwm_ch2_2_funcs[] = { 6, };
+static int mt7623_pwm_ch2_3_pins[] = { 108, };
+static int mt7623_pwm_ch2_3_funcs[] = { 6, };
+static int mt7623_pwm_ch2_4_pins[] = { 209, };
+static int mt7623_pwm_ch2_4_funcs[] = { 5, };
+static int mt7623_pwm_ch3_0_pins[] = { 205, };
+static int mt7623_pwm_ch3_0_funcs[] = { 1, };
+static int mt7623_pwm_ch3_1_pins[] = { 55, };
+static int mt7623_pwm_ch3_1_funcs[] = { 5, };
+static int mt7623_pwm_ch3_2_pins[] = { 89, };
+static int mt7623_pwm_ch3_2_funcs[] = { 6, };
+static int mt7623_pwm_ch3_3_pins[] = { 109, };
+static int mt7623_pwm_ch3_3_funcs[] = { 6, };
+static int mt7623_pwm_ch4_0_pins[] = { 206, };
+static int mt7623_pwm_ch4_0_funcs[] = { 1, };
+static int mt7623_pwm_ch4_1_pins[] = { 90, };
+static int mt7623_pwm_ch4_1_funcs[] = { 6, };
+static int mt7623_pwm_ch4_2_pins[] = { 110, };
+static int mt7623_pwm_ch4_2_funcs[] = { 6, };
+static int mt7623_pwm_ch4_3_pins[] = { 124, };
+static int mt7623_pwm_ch4_3_funcs[] = { 5, };
+static int mt7623_pwm_ch5_0_pins[] = { 207, };
+static int mt7623_pwm_ch5_0_funcs[] = { 1, };
+static int mt7623_pwm_ch5_1_pins[] = { 125, };
+static int mt7623_pwm_ch5_1_funcs[] = { 5, };
+
+/* PWRAP */
+static int mt7623_pwrap_pins[] = { 0, 1, 2, 3, 4, 5, 6, };
+static int mt7623_pwrap_funcs[] = { 1, 1, 1, 1, 1, 1, 1, };
+
+/* SPDIF */
+static int mt7623_spdif_in0_0_pins[] = { 56, };
+static int mt7623_spdif_in0_0_funcs[] = { 3, };
+static int mt7623_spdif_in0_1_pins[] = { 201, };
+static int mt7623_spdif_in0_1_funcs[] = { 1, };
+static int mt7623_spdif_in1_0_pins[] = { 54, };
+static int mt7623_spdif_in1_0_funcs[] = { 3, };
+static int mt7623_spdif_in1_1_pins[] = { 202, };
+static int mt7623_spdif_in1_1_funcs[] = { 1, };
+static int mt7623_spdif_out_pins[] = { 202, };
+static int mt7623_spdif_out_funcs[] = { 1, };
+
+/* SPI */
+static int mt7623_spi0_pins[] = { 53, 54, 55, 56, };
+static int mt7623_spi0_funcs[] = { 1, 1, 1, 1, };
+static int mt7623_spi1_pins[] = { 7, 199, 8, 9, };
+static int mt7623_spi1_funcs[] = { 1, 1, 1, 1, };
+static int mt7623_spi2_pins[] = { 101, 104, 102, 103, };
+static int mt7623_spi2_funcs[] = { 1, 1, 1, 1, };
+
+/* UART */
+static int mt7623_uart0_0_txd_rxd_pins[] = { 79, 80, };
+static int mt7623_uart0_0_txd_rxd_funcs[] = { 1, 1, };
+static int mt7623_uart0_1_txd_rxd_pins[] = { 87, 88, };
+static int mt7623_uart0_1_txd_rxd_funcs[] = { 5, 5, };
+static int mt7623_uart0_2_txd_rxd_pins[] = { 107, 108, };
+static int mt7623_uart0_2_txd_rxd_funcs[] = { 5, 5, };
+static int mt7623_uart0_3_txd_rxd_pins[] = { 123, 122, };
+static int mt7623_uart0_3_txd_rxd_funcs[] = { 5, 5, };
+static int mt7623_uart0_rts_cts_pins[] = { 22, 23, };
+static int mt7623_uart0_rts_cts_funcs[] = { 1, 1, };
+static int mt7623_uart1_0_txd_rxd_pins[] = { 81, 82, };
+static int mt7623_uart1_0_txd_rxd_funcs[] = { 1, 1, };
+static int mt7623_uart1_1_txd_rxd_pins[] = { 89, 90, };
+static int mt7623_uart1_1_txd_rxd_funcs[] = { 5, 5, };
+static int mt7623_uart1_2_txd_rxd_pins[] = { 109, 110, };
+static int mt7623_uart1_2_txd_rxd_funcs[] = { 5, 5, };
+static int mt7623_uart1_rts_cts_pins[] = { 24, 25, };
+static int mt7623_uart1_rts_cts_funcs[] = { 1, 1, };
+static int mt7623_uart2_0_txd_rxd_pins[] = { 14, 15, };
+static int mt7623_uart2_0_txd_rxd_funcs[] = { 1, 1, };
+static int mt7623_uart2_1_txd_rxd_pins[] = { 200, 201, };
+static int mt7623_uart2_1_txd_rxd_funcs[] = { 6, 6, };
+static int mt7623_uart2_rts_cts_pins[] = { 242, 243, };
+static int mt7623_uart2_rts_cts_funcs[] = { 1, 1, };
+static int mt7623_uart3_txd_rxd_pins[] = { 242, 243, };
+static int mt7623_uart3_txd_rxd_funcs[] = { 2, 2, };
+static int mt7623_uart3_rts_cts_pins[] = { 26, 27, };
+static int mt7623_uart3_rts_cts_funcs[] = { 1, 1, };
+
+/* Watchdog */
+static int mt7623_watchdog_0_pins[] = { 11, };
+static int mt7623_watchdog_0_funcs[] = { 1, };
+static int mt7623_watchdog_1_pins[] = { 121, };
+static int mt7623_watchdog_1_funcs[] = { 5, };
+
+static const struct group_desc mt7623_groups[] = {
+	PINCTRL_PIN_GROUP("aud_ext_clk0", mt7623_aud_ext_clk0),
+	PINCTRL_PIN_GROUP("aud_ext_clk1", mt7623_aud_ext_clk1),
+	PINCTRL_PIN_GROUP("dsi_te", mt7623_dsi_te),
+	PINCTRL_PIN_GROUP("disp_pwm_0", mt7623_disp_pwm_0),
+	PINCTRL_PIN_GROUP("disp_pwm_1", mt7623_disp_pwm_1),
+	PINCTRL_PIN_GROUP("disp_pwm_2", mt7623_disp_pwm_2),
+	PINCTRL_PIN_GROUP("ephy", mt7623_ephy),
+	PINCTRL_PIN_GROUP("esw_int", mt7623_esw_int),
+	PINCTRL_PIN_GROUP("esw_rst", mt7623_esw_rst),
+	PINCTRL_PIN_GROUP("ext_sdio", mt7623_ext_sdio),
+	PINCTRL_PIN_GROUP("hdmi_cec", mt7623_hdmi_cec),
+	PINCTRL_PIN_GROUP("hdmi_htplg", mt7623_hdmi_htplg),
+	PINCTRL_PIN_GROUP("hdmi_i2c", mt7623_hdmi_i2c),
+	PINCTRL_PIN_GROUP("hdmi_rx", mt7623_hdmi_rx),
+	PINCTRL_PIN_GROUP("hdmi_rx_i2c", mt7623_hdmi_rx_i2c),
+	PINCTRL_PIN_GROUP("i2c0", mt7623_i2c0),
+	PINCTRL_PIN_GROUP("i2c1_0", mt7623_i2c1_0),
+	PINCTRL_PIN_GROUP("i2c1_1", mt7623_i2c1_1),
+	PINCTRL_PIN_GROUP("i2c1_2", mt7623_i2c1_2),
+	PINCTRL_PIN_GROUP("i2c1_3", mt7623_i2c1_3),
+	PINCTRL_PIN_GROUP("i2c1_4", mt7623_i2c1_4),
+	PINCTRL_PIN_GROUP("i2c2_0", mt7623_i2c2_0),
+	PINCTRL_PIN_GROUP("i2c2_1", mt7623_i2c2_1),
+	PINCTRL_PIN_GROUP("i2c2_2", mt7623_i2c2_2),
+	PINCTRL_PIN_GROUP("i2c2_3", mt7623_i2c2_3),
+	PINCTRL_PIN_GROUP("i2s0", mt7623_i2s0),
+	PINCTRL_PIN_GROUP("i2s1", mt7623_i2s1),
+	PINCTRL_PIN_GROUP("i2s4", mt7623_i2s4),
+	PINCTRL_PIN_GROUP("i2s5", mt7623_i2s5),
+	PINCTRL_PIN_GROUP("i2s2_bclk_lrclk_mclk", mt7623_i2s2_bclk_lrclk_mclk),
+	PINCTRL_PIN_GROUP("i2s3_bclk_lrclk_mclk", mt7623_i2s3_bclk_lrclk_mclk),
+	PINCTRL_PIN_GROUP("i2s2_data_in", mt7623_i2s2_data_in),
+	PINCTRL_PIN_GROUP("i2s3_data_in", mt7623_i2s3_data_in),
+	PINCTRL_PIN_GROUP("i2s2_data_0", mt7623_i2s2_data_0),
+	PINCTRL_PIN_GROUP("i2s2_data_1", mt7623_i2s2_data_1),
+	PINCTRL_PIN_GROUP("i2s3_data_0", mt7623_i2s3_data_0),
+	PINCTRL_PIN_GROUP("i2s3_data_1", mt7623_i2s3_data_1),
+	PINCTRL_PIN_GROUP("ir", mt7623_ir),
+	PINCTRL_PIN_GROUP("lcm_rst", mt7623_lcm_rst),
+	PINCTRL_PIN_GROUP("mdc_mdio", mt7623_mdc_mdio),
+	PINCTRL_PIN_GROUP("mipi_tx", mt7623_mipi_tx),
+	PINCTRL_PIN_GROUP("msdc0", mt7623_msdc0),
+	PINCTRL_PIN_GROUP("msdc1", mt7623_msdc1),
+	PINCTRL_PIN_GROUP("msdc1_ins", mt7623_msdc1_ins),
+	PINCTRL_PIN_GROUP("msdc1_wp_0", mt7623_msdc1_wp_0),
+	PINCTRL_PIN_GROUP("msdc1_wp_1", mt7623_msdc1_wp_1),
+	PINCTRL_PIN_GROUP("msdc1_wp_2", mt7623_msdc1_wp_2),
+	PINCTRL_PIN_GROUP("msdc2", mt7623_msdc2),
+	PINCTRL_PIN_GROUP("msdc3", mt7623_msdc3),
+	PINCTRL_PIN_GROUP("nandc", mt7623_nandc),
+	PINCTRL_PIN_GROUP("nandc_ceb0", mt7623_nandc_ceb0),
+	PINCTRL_PIN_GROUP("nandc_ceb1", mt7623_nandc_ceb1),
+	PINCTRL_PIN_GROUP("otg_iddig0_0", mt7623_otg_iddig0_0),
+	PINCTRL_PIN_GROUP("otg_iddig0_1", mt7623_otg_iddig0_1),
+	PINCTRL_PIN_GROUP("otg_iddig0_2", mt7623_otg_iddig0_2),
+	PINCTRL_PIN_GROUP("otg_iddig1_0", mt7623_otg_iddig1_0),
+	PINCTRL_PIN_GROUP("otg_iddig1_1", mt7623_otg_iddig1_1),
+	PINCTRL_PIN_GROUP("otg_iddig1_2", mt7623_otg_iddig1_2),
+	PINCTRL_PIN_GROUP("otg_drv_vbus0_0", mt7623_otg_drv_vbus0_0),
+	PINCTRL_PIN_GROUP("otg_drv_vbus0_1", mt7623_otg_drv_vbus0_1),
+	PINCTRL_PIN_GROUP("otg_drv_vbus0_2", mt7623_otg_drv_vbus0_2),
+	PINCTRL_PIN_GROUP("otg_drv_vbus1_0", mt7623_otg_drv_vbus1_0),
+	PINCTRL_PIN_GROUP("otg_drv_vbus1_1", mt7623_otg_drv_vbus1_1),
+	PINCTRL_PIN_GROUP("otg_drv_vbus1_2", mt7623_otg_drv_vbus1_2),
+	PINCTRL_PIN_GROUP("pcie0_0_perst", mt7623_pcie0_0_perst),
+	PINCTRL_PIN_GROUP("pcie0_1_perst", mt7623_pcie0_1_perst),
+	PINCTRL_PIN_GROUP("pcie1_0_perst", mt7623_pcie1_0_perst),
+	PINCTRL_PIN_GROUP("pcie1_1_perst", mt7623_pcie1_1_perst),
+	PINCTRL_PIN_GROUP("pcie1_1_perst", mt7623_pcie1_1_perst),
+	PINCTRL_PIN_GROUP("pcie0_0_rev_perst", mt7623_pcie0_0_rev_perst),
+	PINCTRL_PIN_GROUP("pcie0_1_rev_perst", mt7623_pcie0_1_rev_perst),
+	PINCTRL_PIN_GROUP("pcie1_0_rev_perst", mt7623_pcie1_0_rev_perst),
+	PINCTRL_PIN_GROUP("pcie1_1_rev_perst", mt7623_pcie1_1_rev_perst),
+	PINCTRL_PIN_GROUP("pcie2_0_rev_perst", mt7623_pcie2_0_rev_perst),
+	PINCTRL_PIN_GROUP("pcie2_1_rev_perst", mt7623_pcie2_1_rev_perst),
+	PINCTRL_PIN_GROUP("pcie2_0_perst", mt7623_pcie2_0_perst),
+	PINCTRL_PIN_GROUP("pcie2_1_perst", mt7623_pcie2_1_perst),
+	PINCTRL_PIN_GROUP("pcie0_0_wake", mt7623_pcie0_0_wake),
+	PINCTRL_PIN_GROUP("pcie0_1_wake", mt7623_pcie0_1_wake),
+	PINCTRL_PIN_GROUP("pcie1_0_wake", mt7623_pcie1_0_wake),
+	PINCTRL_PIN_GROUP("pcie1_1_wake", mt7623_pcie1_1_wake),
+	PINCTRL_PIN_GROUP("pcie2_0_wake", mt7623_pcie2_0_wake),
+	PINCTRL_PIN_GROUP("pcie2_1_wake", mt7623_pcie2_1_wake),
+	PINCTRL_PIN_GROUP("pcie0_clkreq", mt7623_pcie0_clkreq),
+	PINCTRL_PIN_GROUP("pcie1_clkreq", mt7623_pcie1_clkreq),
+	PINCTRL_PIN_GROUP("pcie2_clkreq", mt7623_pcie2_clkreq),
+	PINCTRL_PIN_GROUP("pcm_clk_0", mt7623_pcm_clk_0),
+	PINCTRL_PIN_GROUP("pcm_clk_1", mt7623_pcm_clk_1),
+	PINCTRL_PIN_GROUP("pcm_clk_2", mt7623_pcm_clk_2),
+	PINCTRL_PIN_GROUP("pcm_clk_3", mt7623_pcm_clk_3),
+	PINCTRL_PIN_GROUP("pcm_clk_4", mt7623_pcm_clk_4),
+	PINCTRL_PIN_GROUP("pcm_clk_5", mt7623_pcm_clk_5),
+	PINCTRL_PIN_GROUP("pcm_clk_6", mt7623_pcm_clk_6),
+	PINCTRL_PIN_GROUP("pcm_sync_0", mt7623_pcm_sync_0),
+	PINCTRL_PIN_GROUP("pcm_sync_1", mt7623_pcm_sync_1),
+	PINCTRL_PIN_GROUP("pcm_sync_2", mt7623_pcm_sync_2),
+	PINCTRL_PIN_GROUP("pcm_sync_3", mt7623_pcm_sync_3),
+	PINCTRL_PIN_GROUP("pcm_sync_4", mt7623_pcm_sync_4),
+	PINCTRL_PIN_GROUP("pcm_sync_5", mt7623_pcm_sync_5),
+	PINCTRL_PIN_GROUP("pcm_sync_6", mt7623_pcm_sync_6),
+	PINCTRL_PIN_GROUP("pcm_rx_0", mt7623_pcm_rx_0),
+	PINCTRL_PIN_GROUP("pcm_rx_1", mt7623_pcm_rx_1),
+	PINCTRL_PIN_GROUP("pcm_rx_2", mt7623_pcm_rx_2),
+	PINCTRL_PIN_GROUP("pcm_rx_3", mt7623_pcm_rx_3),
+	PINCTRL_PIN_GROUP("pcm_rx_4", mt7623_pcm_rx_4),
+	PINCTRL_PIN_GROUP("pcm_rx_5", mt7623_pcm_rx_5),
+	PINCTRL_PIN_GROUP("pcm_rx_6", mt7623_pcm_rx_6),
+	PINCTRL_PIN_GROUP("pcm_tx_0", mt7623_pcm_tx_0),
+	PINCTRL_PIN_GROUP("pcm_tx_1", mt7623_pcm_tx_1),
+	PINCTRL_PIN_GROUP("pcm_tx_2", mt7623_pcm_tx_2),
+	PINCTRL_PIN_GROUP("pcm_tx_3", mt7623_pcm_tx_3),
+	PINCTRL_PIN_GROUP("pcm_tx_4", mt7623_pcm_tx_4),
+	PINCTRL_PIN_GROUP("pcm_tx_5", mt7623_pcm_tx_5),
+	PINCTRL_PIN_GROUP("pcm_tx_6", mt7623_pcm_tx_6),
+	PINCTRL_PIN_GROUP("pwm_ch1_0", mt7623_pwm_ch1_0),
+	PINCTRL_PIN_GROUP("pwm_ch1_1", mt7623_pwm_ch1_1),
+	PINCTRL_PIN_GROUP("pwm_ch1_2", mt7623_pwm_ch1_2),
+	PINCTRL_PIN_GROUP("pwm_ch1_3", mt7623_pwm_ch1_3),
+	PINCTRL_PIN_GROUP("pwm_ch1_4", mt7623_pwm_ch1_4),
+	PINCTRL_PIN_GROUP("pwm_ch2_0", mt7623_pwm_ch2_0),
+	PINCTRL_PIN_GROUP("pwm_ch2_1", mt7623_pwm_ch2_1),
+	PINCTRL_PIN_GROUP("pwm_ch2_2", mt7623_pwm_ch2_2),
+	PINCTRL_PIN_GROUP("pwm_ch2_3", mt7623_pwm_ch2_3),
+	PINCTRL_PIN_GROUP("pwm_ch2_4", mt7623_pwm_ch2_4),
+	PINCTRL_PIN_GROUP("pwm_ch3_0", mt7623_pwm_ch3_0),
+	PINCTRL_PIN_GROUP("pwm_ch3_1", mt7623_pwm_ch3_1),
+	PINCTRL_PIN_GROUP("pwm_ch3_2", mt7623_pwm_ch3_2),
+	PINCTRL_PIN_GROUP("pwm_ch3_3", mt7623_pwm_ch3_3),
+	PINCTRL_PIN_GROUP("pwm_ch4_0", mt7623_pwm_ch4_0),
+	PINCTRL_PIN_GROUP("pwm_ch4_1", mt7623_pwm_ch4_1),
+	PINCTRL_PIN_GROUP("pwm_ch4_2", mt7623_pwm_ch4_2),
+	PINCTRL_PIN_GROUP("pwm_ch4_3", mt7623_pwm_ch4_3),
+	PINCTRL_PIN_GROUP("pwm_ch5_0", mt7623_pwm_ch5_0),
+	PINCTRL_PIN_GROUP("pwm_ch5_1", mt7623_pwm_ch5_1),
+	PINCTRL_PIN_GROUP("pwrap", mt7623_pwrap),
+	PINCTRL_PIN_GROUP("rtc", mt7623_rtc),
+	PINCTRL_PIN_GROUP("spdif_in0_0", mt7623_spdif_in0_0),
+	PINCTRL_PIN_GROUP("spdif_in0_1", mt7623_spdif_in0_1),
+	PINCTRL_PIN_GROUP("spdif_in1_0", mt7623_spdif_in1_0),
+	PINCTRL_PIN_GROUP("spdif_in1_1", mt7623_spdif_in1_1),
+	PINCTRL_PIN_GROUP("spdif_out", mt7623_spdif_out),
+	PINCTRL_PIN_GROUP("spi0", mt7623_spi0),
+	PINCTRL_PIN_GROUP("spi1", mt7623_spi1),
+	PINCTRL_PIN_GROUP("spi2", mt7623_spi2),
+	PINCTRL_PIN_GROUP("uart0_0_txd_rxd",  mt7623_uart0_0_txd_rxd),
+	PINCTRL_PIN_GROUP("uart0_1_txd_rxd",  mt7623_uart0_1_txd_rxd),
+	PINCTRL_PIN_GROUP("uart0_2_txd_rxd",  mt7623_uart0_2_txd_rxd),
+	PINCTRL_PIN_GROUP("uart0_3_txd_rxd",  mt7623_uart0_3_txd_rxd),
+	PINCTRL_PIN_GROUP("uart1_0_txd_rxd",  mt7623_uart1_0_txd_rxd),
+	PINCTRL_PIN_GROUP("uart1_1_txd_rxd",  mt7623_uart1_1_txd_rxd),
+	PINCTRL_PIN_GROUP("uart1_2_txd_rxd",  mt7623_uart1_2_txd_rxd),
+	PINCTRL_PIN_GROUP("uart2_0_txd_rxd",  mt7623_uart2_0_txd_rxd),
+	PINCTRL_PIN_GROUP("uart2_1_txd_rxd",  mt7623_uart2_1_txd_rxd),
+	PINCTRL_PIN_GROUP("uart3_txd_rxd",  mt7623_uart3_txd_rxd),
+	PINCTRL_PIN_GROUP("uart0_rts_cts",  mt7623_uart0_rts_cts),
+	PINCTRL_PIN_GROUP("uart1_rts_cts",  mt7623_uart1_rts_cts),
+	PINCTRL_PIN_GROUP("uart2_rts_cts",  mt7623_uart2_rts_cts),
+	PINCTRL_PIN_GROUP("uart3_rts_cts",  mt7623_uart3_rts_cts),
+	PINCTRL_PIN_GROUP("watchdog_0", mt7623_watchdog_0),
+	PINCTRL_PIN_GROUP("watchdog_1", mt7623_watchdog_1),
+};
+
+/* Joint those groups owning the same capability in user point of view which
+ * allows that people tend to use through the device tree.
+ */
+static const char *mt7623_aud_clk_groups[] = { "aud_ext_clk0",
+					       "aud_ext_clk1", };
+static const char *mt7623_disp_pwm_groups[] = { "disp_pwm_0", "disp_pwm_1",
+						"disp_pwm_2", };
+static const char *mt7623_ethernet_groups[] = { "esw_int", "esw_rst",
+						"ephy", "mdc_mdio", };
+static const char *mt7623_ext_sdio_groups[] = { "ext_sdio", };
+static const char *mt7623_hdmi_groups[] = { "hdmi_cec", "hdmi_htplg",
+					    "hdmi_i2c", "hdmi_rx",
+					    "hdmi_rx_i2c", };
+static const char *mt7623_i2c_groups[] = { "i2c0", "i2c1_0", "i2c1_1",
+					   "i2c1_2", "i2c1_3", "i2c1_4",
+					   "i2c2_0", "i2c2_1", "i2c2_2",
+					   "i2c2_3", };
+static const char *mt7623_i2s_groups[] = { "i2s0", "i2s1",
+					   "i2s2_bclk_lrclk_mclk",
+					   "i2s3_bclk_lrclk_mclk",
+					   "i2s4", "i2s5",
+					   "i2s2_data_in", "i2s3_data_in",
+					   "i2s2_data_0", "i2s2_data_1",
+					   "i2s3_data_0", "i2s3_data_1", };
+static const char *mt7623_ir_groups[] = { "ir", };
+static const char *mt7623_lcd_groups[] = { "dsi_te", "lcm_rst", "mipi_tx", };
+static const char *mt7623_msdc_groups[] = { "msdc0", "msdc1", "msdc1_ins",
+					    "msdc1_wp_0", "msdc1_wp_1",
+					    "msdc1_wp_2", "msdc2",
+						"msdc3", };
+static const char *mt7623_nandc_groups[] = { "nandc", "nandc_ceb0",
+					     "nandc_ceb1", };
+static const char *mt7623_otg_groups[] = { "otg_iddig0_0", "otg_iddig0_1",
+					    "otg_iddig0_2", "otg_iddig1_0",
+					    "otg_iddig1_1", "otg_iddig1_2",
+					    "otg_drv_vbus0_0",
+					    "otg_drv_vbus0_1",
+					    "otg_drv_vbus0_2",
+					    "otg_drv_vbus1_0",
+					    "otg_drv_vbus1_1",
+					    "otg_drv_vbus1_2", };
+static const char *mt7623_pcie_groups[] = { "pcie0_0_perst", "pcie0_1_perst",
+					    "pcie1_0_perst", "pcie1_1_perst",
+					    "pcie2_0_perst", "pcie2_1_perst",
+					    "pcie0_0_rev_perst",
+					    "pcie0_1_rev_perst",
+					    "pcie1_0_rev_perst",
+					    "pcie1_1_rev_perst",
+					    "pcie2_0_rev_perst",
+					    "pcie2_1_rev_perst",
+					    "pcie0_0_wake", "pcie0_1_wake",
+					    "pcie2_0_wake", "pcie2_1_wake",
+					    "pcie0_clkreq", "pcie1_clkreq",
+					    "pcie2_clkreq", };
+static const char *mt7623_pcm_groups[] = { "pcm_clk_0", "pcm_clk_1",
+					   "pcm_clk_2", "pcm_clk_3",
+					   "pcm_clk_4", "pcm_clk_5",
+					   "pcm_clk_6", "pcm_sync_0",
+					   "pcm_sync_1", "pcm_sync_2",
+					   "pcm_sync_3", "pcm_sync_4",
+					   "pcm_sync_5", "pcm_sync_6",
+					   "pcm_rx_0", "pcm_rx_1",
+					   "pcm_rx_2", "pcm_rx_3",
+					   "pcm_rx_4", "pcm_rx_5",
+					   "pcm_rx_6", "pcm_tx_0",
+					   "pcm_tx_1", "pcm_tx_2",
+					   "pcm_tx_3", "pcm_tx_4",
+					   "pcm_tx_5", "pcm_tx_6", };
+static const char *mt7623_pwm_groups[] = { "pwm_ch1_0", "pwm_ch1_1",
+					   "pwm_ch1_2", "pwm_ch2_0",
+					   "pwm_ch2_1", "pwm_ch2_2",
+					   "pwm_ch3_0", "pwm_ch3_1",
+					   "pwm_ch3_2", "pwm_ch4_0",
+					   "pwm_ch4_1", "pwm_ch4_2",
+					   "pwm_ch4_3", "pwm_ch5_0",
+					   "pwm_ch5_1", "pwm_ch5_2",
+					   "pwm_ch6_0", "pwm_ch6_1",
+					   "pwm_ch6_2", "pwm_ch6_3",
+					   "pwm_ch7_0", "pwm_ch7_1",
+					   "pwm_ch7_2", };
+static const char *mt7623_pwrap_groups[] = { "pwrap", };
+static const char *mt7623_rtc_groups[] = { "rtc", };
+static const char *mt7623_spi_groups[] = { "spi0", "spi2", "spi2", };
+static const char *mt7623_spdif_groups[] = { "spdif_in0_0", "spdif_in0_1",
+					     "spdif_in1_0", "spdif_in1_1",
+					     "spdif_out", };
+static const char *mt7623_uart_groups[] = { "uart0_0_txd_rxd",
+					    "uart0_1_txd_rxd",
+					    "uart0_2_txd_rxd",
+					    "uart0_3_txd_rxd",
+					    "uart1_0_txd_rxd",
+					    "uart1_1_txd_rxd",
+					    "uart1_2_txd_rxd",
+					    "uart2_0_txd_rxd",
+					    "uart2_1_txd_rxd",
+					    "uart3_txd_rxd",
+					    "uart0_rts_cts",
+					    "uart1_rts_cts",
+					    "uart2_rts_cts",
+					    "uart3_rts_cts", };
+static const char *mt7623_wdt_groups[] = { "watchdog_0", "watchdog_1", };
+
+static const struct function_desc mt7623_functions[] = {
+	{"audck", mt7623_aud_clk_groups, ARRAY_SIZE(mt7623_aud_clk_groups)},
+	{"disp", mt7623_disp_pwm_groups, ARRAY_SIZE(mt7623_disp_pwm_groups)},
+	{"eth",	mt7623_ethernet_groups, ARRAY_SIZE(mt7623_ethernet_groups)},
+	{"sdio", mt7623_ext_sdio_groups, ARRAY_SIZE(mt7623_ext_sdio_groups)},
+	{"hdmi", mt7623_hdmi_groups, ARRAY_SIZE(mt7623_hdmi_groups)},
+	{"i2c", mt7623_i2c_groups, ARRAY_SIZE(mt7623_i2c_groups)},
+	{"i2s",	mt7623_i2s_groups, ARRAY_SIZE(mt7623_i2s_groups)},
+	{"ir",	mt7623_ir_groups, ARRAY_SIZE(mt7623_ir_groups)},
+	{"lcd", mt7623_lcd_groups, ARRAY_SIZE(mt7623_lcd_groups)},
+	{"msdc", mt7623_msdc_groups, ARRAY_SIZE(mt7623_msdc_groups)},
+	{"nand", mt7623_nandc_groups, ARRAY_SIZE(mt7623_nandc_groups)},
+	{"otg", mt7623_otg_groups, ARRAY_SIZE(mt7623_otg_groups)},
+	{"pcie", mt7623_pcie_groups, ARRAY_SIZE(mt7623_pcie_groups)},
+	{"pcm",	mt7623_pcm_groups, ARRAY_SIZE(mt7623_pcm_groups)},
+	{"pwm",	mt7623_pwm_groups, ARRAY_SIZE(mt7623_pwm_groups)},
+	{"pwrap", mt7623_pwrap_groups, ARRAY_SIZE(mt7623_pwrap_groups)},
+	{"rtc", mt7623_rtc_groups, ARRAY_SIZE(mt7623_rtc_groups)},
+	{"spi",	mt7623_spi_groups, ARRAY_SIZE(mt7623_spi_groups)},
+	{"spdif", mt7623_spdif_groups, ARRAY_SIZE(mt7623_spdif_groups)},
+	{"uart", mt7623_uart_groups, ARRAY_SIZE(mt7623_uart_groups)},
+	{"watchdog", mt7623_wdt_groups, ARRAY_SIZE(mt7623_wdt_groups)},
+};
+
+static const struct mtk_eint_hw mt7623_eint_hw = {
+	.port_mask = 6,
+	.ports     = 6,
+	.ap_num    = 169,
+	.db_cnt    = 20,
+};
+
+static struct mtk_pin_soc mt7623_data = {
+	.reg_cal = mt7623_reg_cals,
+	.pins = mt7623_pins,
+	.npins = ARRAY_SIZE(mt7623_pins),
+	.grps = mt7623_groups,
+	.ngrps = ARRAY_SIZE(mt7623_groups),
+	.funcs = mt7623_functions,
+	.nfuncs = ARRAY_SIZE(mt7623_functions),
+	.eint_hw = &mt7623_eint_hw,
+	.gpio_m = 0,
+	.ies_present = true,
+	.base_names = mtk_default_register_base_names,
+	.nbase_names = ARRAY_SIZE(mtk_default_register_base_names),
+	.bias_disable_set = mtk_pinconf_bias_disable_set_rev1,
+	.bias_disable_get = mtk_pinconf_bias_disable_get_rev1,
+	.bias_set = mtk_pinconf_bias_set_rev1,
+	.bias_get = mtk_pinconf_bias_get_rev1,
+	.drive_set = mtk_pinconf_drive_set_rev1,
+	.drive_get = mtk_pinconf_drive_get_rev1,
+	.adv_pull_get = mtk_pinconf_adv_pull_get,
+	.adv_pull_set = mtk_pinconf_adv_pull_set,
+};
+
+/*
+ * There are some specific pins have mux functions greater than 8,
+ * and if we want to switch thees high modes we need to disable
+ * bonding constraints firstly.
+ */
+static void mt7623_bonding_disable(struct platform_device *pdev)
+{
+	struct mtk_pinctrl *hw = platform_get_drvdata(pdev);
+
+	mtk_rmw(hw, 0, PIN_BOND_REG0, BOND_PCIE_CLR, BOND_PCIE_CLR);
+	mtk_rmw(hw, 0, PIN_BOND_REG1, BOND_I2S_CLR, BOND_I2S_CLR);
+	mtk_rmw(hw, 0, PIN_BOND_REG2, BOND_MSDC0E_CLR, BOND_MSDC0E_CLR);
+}
+
+static const struct of_device_id mt7623_pctrl_match[] = {
+	{ .compatible = "mediatek,mt7623-moore-pinctrl", },
+	{}
+};
+
+static int mt7623_pinctrl_probe(struct platform_device *pdev)
+{
+	int err;
+
+	err = mtk_moore_pinctrl_probe(pdev, &mt7623_data);
+	if (err)
+		return err;
+
+	mt7623_bonding_disable(pdev);
+
+	return 0;
+}
+
+static struct platform_driver mtk_pinctrl_driver = {
+	.probe = mt7623_pinctrl_probe,
+	.driver = {
+		.name = "mt7623-moore-pinctrl",
+		.of_match_table = mt7623_pctrl_match,
+	},
+};
+
+static int __init mtk_pinctrl_init(void)
+{
+	return platform_driver_register(&mtk_pinctrl_driver);
+}
+arch_initcall(mtk_pinctrl_init);
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mt7629.c
@@ -0,0 +1,450 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * The MT7629 driver based on Linux generic pinctrl binding.
+ *
+ * Copyright (C) 2018 MediaTek Inc.
+ * Author: Ryder Lee <ryder.lee@mediatek.com>
+ */
+
+#include "pinctrl-moore.h"
+
+#define MT7629_PIN(_number, _name, _eint_n)				\
+	MTK_PIN(_number, _name, 0, _eint_n, DRV_GRP1)
+
+static const struct mtk_pin_field_calc mt7629_pin_mode_range[] = {
+	PIN_FIELD(0, 78, 0x300, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_dir_range[] = {
+	PIN_FIELD(0, 78, 0x0, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_di_range[] = {
+	PIN_FIELD(0, 78, 0x200, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_do_range[] = {
+	PIN_FIELD(0, 78, 0x100, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_ies_range[] = {
+	PIN_FIELD(0, 10, 0x1000, 0x10, 0, 1),
+	PIN_FIELD(11, 18, 0x2000, 0x10, 0, 1),
+	PIN_FIELD(19, 32, 0x3000, 0x10, 0, 1),
+	PIN_FIELD(33, 48, 0x4000, 0x10, 0, 1),
+	PIN_FIELD(49, 50, 0x5000, 0x10, 0, 1),
+	PIN_FIELD(51, 69, 0x6000, 0x10, 0, 1),
+	PIN_FIELD(70, 78, 0x7000, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_smt_range[] = {
+	PIN_FIELD(0, 10, 0x1100, 0x10, 0, 1),
+	PIN_FIELD(11, 18, 0x2100, 0x10, 0, 1),
+	PIN_FIELD(19, 32, 0x3100, 0x10, 0, 1),
+	PIN_FIELD(33, 48, 0x4100, 0x10, 0, 1),
+	PIN_FIELD(49, 50, 0x5100, 0x10, 0, 1),
+	PIN_FIELD(51, 69, 0x6100, 0x10, 0, 1),
+	PIN_FIELD(70, 78, 0x7100, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_pullen_range[] = {
+	PIN_FIELD(0, 10, 0x1400, 0x10, 0, 1),
+	PIN_FIELD(11, 18, 0x2400, 0x10, 0, 1),
+	PIN_FIELD(19, 32, 0x3400, 0x10, 0, 1),
+	PIN_FIELD(33, 48, 0x4400, 0x10, 0, 1),
+	PIN_FIELD(49, 50, 0x5400, 0x10, 0, 1),
+	PIN_FIELD(51, 69, 0x6400, 0x10, 0, 1),
+	PIN_FIELD(70, 78, 0x7400, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_pullsel_range[] = {
+	PIN_FIELD(0, 10, 0x1500, 0x10, 0, 1),
+	PIN_FIELD(11, 18, 0x2500, 0x10, 0, 1),
+	PIN_FIELD(19, 32, 0x3500, 0x10, 0, 1),
+	PIN_FIELD(33, 48, 0x4500, 0x10, 0, 1),
+	PIN_FIELD(49, 50, 0x5500, 0x10, 0, 1),
+	PIN_FIELD(51, 69, 0x6500, 0x10, 0, 1),
+	PIN_FIELD(70, 78, 0x7500, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_drv_range[] = {
+	PIN_FIELD(0, 10, 0x1600, 0x10, 0, 4),
+	PIN_FIELD(11, 18, 0x2600, 0x10, 0, 4),
+	PIN_FIELD(19, 32, 0x3600, 0x10, 0, 4),
+	PIN_FIELD(33, 48, 0x4600, 0x10, 0, 4),
+	PIN_FIELD(49, 50, 0x5600, 0x10, 0, 4),
+	PIN_FIELD(51, 69, 0x6600, 0x10, 0, 4),
+	PIN_FIELD(70, 78, 0x7600, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_tdsel_range[] = {
+	PIN_FIELD(0, 10, 0x1200, 0x10, 0, 4),
+	PIN_FIELD(11, 18, 0x2200, 0x10, 0, 4),
+	PIN_FIELD(19, 32, 0x3200, 0x10, 0, 4),
+	PIN_FIELD(33, 48, 0x4200, 0x10, 0, 4),
+	PIN_FIELD(49, 50, 0x5200, 0x10, 0, 4),
+	PIN_FIELD(51, 69, 0x6200, 0x10, 0, 4),
+	PIN_FIELD(70, 78, 0x7200, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_field_calc mt7629_pin_rdsel_range[] = {
+	PIN_FIELD(0, 10, 0x1300, 0x10, 0, 4),
+	PIN_FIELD(11, 18, 0x2300, 0x10, 0, 4),
+	PIN_FIELD(19, 32, 0x3300, 0x10, 0, 4),
+	PIN_FIELD(33, 48, 0x4300, 0x10, 0, 4),
+	PIN_FIELD(49, 50, 0x5300, 0x10, 0, 4),
+	PIN_FIELD(51, 69, 0x6300, 0x10, 0, 4),
+	PIN_FIELD(70, 78, 0x7300, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_reg_calc mt7629_reg_cals[] = {
+	[PINCTRL_PIN_REG_MODE] = MTK_RANGE(mt7629_pin_mode_range),
+	[PINCTRL_PIN_REG_DIR] = MTK_RANGE(mt7629_pin_dir_range),
+	[PINCTRL_PIN_REG_DI] = MTK_RANGE(mt7629_pin_di_range),
+	[PINCTRL_PIN_REG_DO] = MTK_RANGE(mt7629_pin_do_range),
+	[PINCTRL_PIN_REG_IES] = MTK_RANGE(mt7629_pin_ies_range),
+	[PINCTRL_PIN_REG_SMT] = MTK_RANGE(mt7629_pin_smt_range),
+	[PINCTRL_PIN_REG_PULLSEL] = MTK_RANGE(mt7629_pin_pullsel_range),
+	[PINCTRL_PIN_REG_PULLEN] = MTK_RANGE(mt7629_pin_pullen_range),
+	[PINCTRL_PIN_REG_DRV] = MTK_RANGE(mt7629_pin_drv_range),
+	[PINCTRL_PIN_REG_TDSEL] = MTK_RANGE(mt7629_pin_tdsel_range),
+	[PINCTRL_PIN_REG_RDSEL] = MTK_RANGE(mt7629_pin_rdsel_range),
+};
+
+static const struct mtk_pin_desc mt7629_pins[] = {
+	MT7629_PIN(0, "TOP_5G_CLK", 53),
+	MT7629_PIN(1, "TOP_5G_DATA", 54),
+	MT7629_PIN(2, "WF0_5G_HB0", 55),
+	MT7629_PIN(3, "WF0_5G_HB1", 56),
+	MT7629_PIN(4, "WF0_5G_HB2", 57),
+	MT7629_PIN(5, "WF0_5G_HB3", 58),
+	MT7629_PIN(6, "WF0_5G_HB4", 59),
+	MT7629_PIN(7, "WF0_5G_HB5", 60),
+	MT7629_PIN(8, "WF0_5G_HB6", 61),
+	MT7629_PIN(9, "XO_REQ", 9),
+	MT7629_PIN(10, "TOP_RST_N", 10),
+	MT7629_PIN(11, "SYS_WATCHDOG", 11),
+	MT7629_PIN(12, "EPHY_LED0_N_JTDO", 12),
+	MT7629_PIN(13, "EPHY_LED1_N_JTDI", 13),
+	MT7629_PIN(14, "EPHY_LED2_N_JTMS", 14),
+	MT7629_PIN(15, "EPHY_LED3_N_JTCLK", 15),
+	MT7629_PIN(16, "EPHY_LED4_N_JTRST_N", 16),
+	MT7629_PIN(17, "WF2G_LED_N", 17),
+	MT7629_PIN(18, "WF5G_LED_N", 18),
+	MT7629_PIN(19, "I2C_SDA", 19),
+	MT7629_PIN(20, "I2C_SCL", 20),
+	MT7629_PIN(21, "GPIO_9", 21),
+	MT7629_PIN(22, "GPIO_10", 22),
+	MT7629_PIN(23, "GPIO_11", 23),
+	MT7629_PIN(24, "GPIO_12", 24),
+	MT7629_PIN(25, "UART1_TXD", 25),
+	MT7629_PIN(26, "UART1_RXD", 26),
+	MT7629_PIN(27, "UART1_CTS", 27),
+	MT7629_PIN(28, "UART1_RTS", 28),
+	MT7629_PIN(29, "UART2_TXD", 29),
+	MT7629_PIN(30, "UART2_RXD", 30),
+	MT7629_PIN(31, "UART2_CTS", 31),
+	MT7629_PIN(32, "UART2_RTS", 32),
+	MT7629_PIN(33, "MDI_TP_P1", 33),
+	MT7629_PIN(34, "MDI_TN_P1", 34),
+	MT7629_PIN(35, "MDI_RP_P1", 35),
+	MT7629_PIN(36, "MDI_RN_P1", 36),
+	MT7629_PIN(37, "MDI_RP_P2", 37),
+	MT7629_PIN(38, "MDI_RN_P2", 38),
+	MT7629_PIN(39, "MDI_TP_P2", 39),
+	MT7629_PIN(40, "MDI_TN_P2", 40),
+	MT7629_PIN(41, "MDI_TP_P3", 41),
+	MT7629_PIN(42, "MDI_TN_P3", 42),
+	MT7629_PIN(43, "MDI_RP_P3", 43),
+	MT7629_PIN(44, "MDI_RN_P3", 44),
+	MT7629_PIN(45, "MDI_RP_P4", 45),
+	MT7629_PIN(46, "MDI_RN_P4", 46),
+	MT7629_PIN(47, "MDI_TP_P4", 47),
+	MT7629_PIN(48, "MDI_TN_P4", 48),
+	MT7629_PIN(49, "SMI_MDC", 49),
+	MT7629_PIN(50, "SMI_MDIO", 50),
+	MT7629_PIN(51, "PCIE_PERESET_N", 51),
+	MT7629_PIN(52, "PWM_0", 52),
+	MT7629_PIN(53, "GPIO_0", 0),
+	MT7629_PIN(54, "GPIO_1", 1),
+	MT7629_PIN(55, "GPIO_2", 2),
+	MT7629_PIN(56, "GPIO_3", 3),
+	MT7629_PIN(57, "GPIO_4", 4),
+	MT7629_PIN(58, "GPIO_5", 5),
+	MT7629_PIN(59, "GPIO_6", 6),
+	MT7629_PIN(60, "GPIO_7", 7),
+	MT7629_PIN(61, "GPIO_8", 8),
+	MT7629_PIN(62, "SPI_CLK", 62),
+	MT7629_PIN(63, "SPI_CS", 63),
+	MT7629_PIN(64, "SPI_MOSI", 64),
+	MT7629_PIN(65, "SPI_MISO", 65),
+	MT7629_PIN(66, "SPI_WP", 66),
+	MT7629_PIN(67, "SPI_HOLD", 67),
+	MT7629_PIN(68, "UART0_TXD", 68),
+	MT7629_PIN(69, "UART0_RXD", 69),
+	MT7629_PIN(70, "TOP_2G_CLK", 70),
+	MT7629_PIN(71, "TOP_2G_DATA", 71),
+	MT7629_PIN(72, "WF0_2G_HB0", 72),
+	MT7629_PIN(73, "WF0_2G_HB1", 73),
+	MT7629_PIN(74, "WF0_2G_HB2", 74),
+	MT7629_PIN(75, "WF0_2G_HB3", 75),
+	MT7629_PIN(76, "WF0_2G_HB4", 76),
+	MT7629_PIN(77, "WF0_2G_HB5", 77),
+	MT7629_PIN(78, "WF0_2G_HB6", 78),
+};
+
+/* List all groups consisting of these pins dedicated to the enablement of
+ * certain hardware block and the corresponding mode for all of the pins.
+ * The hardware probably has multiple combinations of these pinouts.
+ */
+
+/* LED for EPHY */
+static int mt7629_ephy_leds_pins[] = { 12, 13, 14, 15, 16, 17, 18, };
+static int mt7629_ephy_leds_funcs[] = { 1, 1, 1, 1, 1, 1, 1, };
+static int mt7629_ephy_led0_pins[] = { 12, };
+static int mt7629_ephy_led0_funcs[] = { 1, };
+static int mt7629_ephy_led1_pins[] = { 13, };
+static int mt7629_ephy_led1_funcs[] = { 1, };
+static int mt7629_ephy_led2_pins[] = { 14, };
+static int mt7629_ephy_led2_funcs[] = { 1, };
+static int mt7629_ephy_led3_pins[] = { 15, };
+static int mt7629_ephy_led3_funcs[] = { 1, };
+static int mt7629_ephy_led4_pins[] = { 16, };
+static int mt7629_ephy_led4_funcs[] = { 1, };
+static int mt7629_wf2g_led_pins[] = { 17, };
+static int mt7629_wf2g_led_funcs[] = { 1, };
+static int mt7629_wf5g_led_pins[] = { 18, };
+static int mt7629_wf5g_led_funcs[] = { 1, };
+
+/* Watchdog */
+static int mt7629_watchdog_pins[] = { 11, };
+static int mt7629_watchdog_funcs[] = { 1, };
+
+/* LED for GPHY */
+static int mt7629_gphy_leds_0_pins[] = { 21, 22, 23, };
+static int mt7629_gphy_leds_0_funcs[] = { 2, 2, 2, };
+static int mt7629_gphy_led1_0_pins[] = { 21, };
+static int mt7629_gphy_led1_0_funcs[] = { 2, };
+static int mt7629_gphy_led2_0_pins[] = { 22, };
+static int mt7629_gphy_led2_0_funcs[] = { 2, };
+static int mt7629_gphy_led3_0_pins[] = { 23, };
+static int mt7629_gphy_led3_0_funcs[] = { 2, };
+static int mt7629_gphy_leds_1_pins[] = { 57, 58, 59, };
+static int mt7629_gphy_leds_1_funcs[] = { 1, 1, 1, };
+static int mt7629_gphy_led1_1_pins[] = { 57, };
+static int mt7629_gphy_led1_1_funcs[] = { 1, };
+static int mt7629_gphy_led2_1_pins[] = { 58, };
+static int mt7629_gphy_led2_1_funcs[] = { 1, };
+static int mt7629_gphy_led3_1_pins[] = { 59, };
+static int mt7629_gphy_led3_1_funcs[] = { 1, };
+
+/* I2C */
+static int mt7629_i2c_0_pins[] = { 19, 20, };
+static int mt7629_i2c_0_funcs[] = { 1, 1, };
+static int mt7629_i2c_1_pins[] = { 53, 54, };
+static int mt7629_i2c_1_funcs[] = { 1, 1, };
+
+/* SPI */
+static int mt7629_spi_0_pins[] = { 21, 22, 23, 24, };
+static int mt7629_spi_0_funcs[] = { 1, 1, 1, 1, };
+static int mt7629_spi_1_pins[] = { 62, 63, 64, 65, };
+static int mt7629_spi_1_funcs[] = { 1, 1, 1, 1, };
+static int mt7629_spi_wp_pins[] = { 66, };
+static int mt7629_spi_wp_funcs[] = { 1, };
+static int mt7629_spi_hold_pins[] = { 67, };
+static int mt7629_spi_hold_funcs[] = { 1, };
+
+/* UART */
+static int mt7629_uart1_0_txd_rxd_pins[] = { 25, 26, };
+static int mt7629_uart1_0_txd_rxd_funcs[] = { 1, 1, };
+static int mt7629_uart1_1_txd_rxd_pins[] = { 53, 54, };
+static int mt7629_uart1_1_txd_rxd_funcs[] = { 2, 2, };
+static int mt7629_uart2_0_txd_rxd_pins[] = { 29, 30, };
+static int mt7629_uart2_0_txd_rxd_funcs[] = { 1, 1, };
+static int mt7629_uart2_1_txd_rxd_pins[] = { 57, 58, };
+static int mt7629_uart2_1_txd_rxd_funcs[] = { 2, 2, };
+static int mt7629_uart1_0_cts_rts_pins[] = { 27, 28, };
+static int mt7629_uart1_0_cts_rts_funcs[] = { 1, 1, };
+static int mt7629_uart1_1_cts_rts_pins[] = { 55, 56, };
+static int mt7629_uart1_1_cts_rts_funcs[] = { 2, 2, };
+static int mt7629_uart2_0_cts_rts_pins[] = { 31, 32, };
+static int mt7629_uart2_0_cts_rts_funcs[] = { 1, 1, };
+static int mt7629_uart2_1_cts_rts_pins[] = { 59, 60, };
+static int mt7629_uart2_1_cts_rts_funcs[] = { 2, 2, };
+static int mt7629_uart0_txd_rxd_pins[] = { 68, 69, };
+static int mt7629_uart0_txd_rxd_funcs[] = { 1, 1, };
+
+/* MDC/MDIO */
+static int mt7629_mdc_mdio_pins[] = { 49, 50, };
+static int mt7629_mdc_mdio_funcs[] = { 1, 1, };
+
+/* PCIE */
+static int mt7629_pcie_pereset_pins[] = { 51, };
+static int mt7629_pcie_pereset_funcs[] = { 1, };
+static int mt7629_pcie_wake_pins[] = { 55, };
+static int mt7629_pcie_wake_funcs[] = { 1, };
+static int mt7629_pcie_clkreq_pins[] = { 56, };
+static int mt7629_pcie_clkreq_funcs[] = { 1, };
+
+/* PWM */
+static int mt7629_pwm_0_pins[] = { 52, };
+static int mt7629_pwm_0_funcs[] = { 1, };
+static int mt7629_pwm_1_pins[] = { 61, };
+static int mt7629_pwm_1_funcs[] = { 2, };
+
+/* WF 2G */
+static int mt7629_wf0_2g_pins[] = { 70, 71, 72, 73, 74, 75, 76, 77, 78, };
+static int mt7629_wf0_2g_funcs[] = { 1, 1, 1, 1, 1, 1, 1, 1, };
+
+/* WF 5G */
+static int mt7629_wf0_5g_pins[] = { 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, };
+static int mt7629_wf0_5g_funcs[] = { 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, };
+
+/* SNFI */
+static int mt7629_snfi_pins[] = { 62, 63, 64, 65, 66, 67 };
+static int mt7629_snfi_funcs[] = { 2, 2, 2, 2, 2, 2 };
+
+/* SPI NOR */
+static int mt7629_snor_pins[] = { 62, 63, 64, 65, 66, 67 };
+static int mt7629_snor_funcs[] = { 1, 1, 1, 1, 1, 1 };
+
+static const struct group_desc mt7629_groups[] = {
+	PINCTRL_PIN_GROUP("ephy_leds", mt7629_ephy_leds),
+	PINCTRL_PIN_GROUP("ephy_led0", mt7629_ephy_led0),
+	PINCTRL_PIN_GROUP("ephy_led1", mt7629_ephy_led1),
+	PINCTRL_PIN_GROUP("ephy_led2", mt7629_ephy_led2),
+	PINCTRL_PIN_GROUP("ephy_led3", mt7629_ephy_led3),
+	PINCTRL_PIN_GROUP("ephy_led4", mt7629_ephy_led4),
+	PINCTRL_PIN_GROUP("wf2g_led", mt7629_wf2g_led),
+	PINCTRL_PIN_GROUP("wf5g_led", mt7629_wf5g_led),
+	PINCTRL_PIN_GROUP("watchdog", mt7629_watchdog),
+	PINCTRL_PIN_GROUP("gphy_leds_0", mt7629_gphy_leds_0),
+	PINCTRL_PIN_GROUP("gphy_led1_0", mt7629_gphy_led1_0),
+	PINCTRL_PIN_GROUP("gphy_led2_0", mt7629_gphy_led2_0),
+	PINCTRL_PIN_GROUP("gphy_led3_0", mt7629_gphy_led3_0),
+	PINCTRL_PIN_GROUP("gphy_leds_1", mt7629_gphy_leds_1),
+	PINCTRL_PIN_GROUP("gphy_led1_1", mt7629_gphy_led1_1),
+	PINCTRL_PIN_GROUP("gphy_led2_1", mt7629_gphy_led2_1),
+	PINCTRL_PIN_GROUP("gphy_led3_1", mt7629_gphy_led3_1),
+	PINCTRL_PIN_GROUP("i2c_0", mt7629_i2c_0),
+	PINCTRL_PIN_GROUP("i2c_1", mt7629_i2c_1),
+	PINCTRL_PIN_GROUP("spi_0", mt7629_spi_0),
+	PINCTRL_PIN_GROUP("spi_1", mt7629_spi_1),
+	PINCTRL_PIN_GROUP("spi_wp", mt7629_spi_wp),
+	PINCTRL_PIN_GROUP("spi_hold", mt7629_spi_hold),
+	PINCTRL_PIN_GROUP("uart1_0_txd_rxd", mt7629_uart1_0_txd_rxd),
+	PINCTRL_PIN_GROUP("uart1_1_txd_rxd", mt7629_uart1_1_txd_rxd),
+	PINCTRL_PIN_GROUP("uart2_0_txd_rxd", mt7629_uart2_0_txd_rxd),
+	PINCTRL_PIN_GROUP("uart2_1_txd_rxd", mt7629_uart2_1_txd_rxd),
+	PINCTRL_PIN_GROUP("uart1_0_cts_rts", mt7629_uart1_0_cts_rts),
+	PINCTRL_PIN_GROUP("uart1_1_cts_rts", mt7629_uart1_1_cts_rts),
+	PINCTRL_PIN_GROUP("uart2_0_cts_rts", mt7629_uart2_0_cts_rts),
+	PINCTRL_PIN_GROUP("uart2_1_cts_rts", mt7629_uart2_1_cts_rts),
+	PINCTRL_PIN_GROUP("uart0_txd_rxd", mt7629_uart0_txd_rxd),
+	PINCTRL_PIN_GROUP("mdc_mdio", mt7629_mdc_mdio),
+	PINCTRL_PIN_GROUP("pcie_pereset", mt7629_pcie_pereset),
+	PINCTRL_PIN_GROUP("pcie_wake", mt7629_pcie_wake),
+	PINCTRL_PIN_GROUP("pcie_clkreq", mt7629_pcie_clkreq),
+	PINCTRL_PIN_GROUP("pwm_0", mt7629_pwm_0),
+	PINCTRL_PIN_GROUP("pwm_1", mt7629_pwm_1),
+	PINCTRL_PIN_GROUP("wf0_5g", mt7629_wf0_5g),
+	PINCTRL_PIN_GROUP("wf0_2g", mt7629_wf0_2g),
+	PINCTRL_PIN_GROUP("snfi", mt7629_snfi),
+	PINCTRL_PIN_GROUP("spi_nor", mt7629_snor),
+};
+
+/* Joint those groups owning the same capability in user point of view which
+ * allows that people tend to use through the device tree.
+ */
+static const char *mt7629_ethernet_groups[] = { "mdc_mdio", };
+static const char *mt7629_i2c_groups[] = { "i2c_0", "i2c_1", };
+static const char *mt7629_led_groups[] = { "ephy_leds", "ephy_led0",
+					   "ephy_led1", "ephy_led2",
+					   "ephy_led3", "ephy_led4",
+					   "wf2g_led", "wf5g_led",
+					   "gphy_leds_0", "gphy_led1_0",
+					   "gphy_led2_0", "gphy_led3_0",
+					   "gphy_leds_1", "gphy_led1_1",
+					   "gphy_led2_1", "gphy_led3_1",};
+static const char *mt7629_pcie_groups[] = { "pcie_pereset", "pcie_wake",
+					    "pcie_clkreq", };
+static const char *mt7629_pwm_groups[] = { "pwm_0", "pwm_1", };
+static const char *mt7629_spi_groups[] = { "spi_0", "spi_1", "spi_wp",
+					   "spi_hold", };
+static const char *mt7629_uart_groups[] = { "uart1_0_txd_rxd",
+					    "uart1_1_txd_rxd",
+					    "uart2_0_txd_rxd",
+					    "uart2_1_txd_rxd",
+					    "uart1_0_cts_rts",
+					    "uart1_1_cts_rts",
+					    "uart2_0_cts_rts",
+					    "uart2_1_cts_rts",
+					    "uart0_txd_rxd", };
+static const char *mt7629_wdt_groups[] = { "watchdog", };
+static const char *mt7629_wifi_groups[] = { "wf0_5g", "wf0_2g", };
+static const char *mt7629_flash_groups[] = { "snfi", "spi_nor" };
+
+static const struct function_desc mt7629_functions[] = {
+	{"eth",	mt7629_ethernet_groups, ARRAY_SIZE(mt7629_ethernet_groups)},
+	{"i2c", mt7629_i2c_groups, ARRAY_SIZE(mt7629_i2c_groups)},
+	{"led",	mt7629_led_groups, ARRAY_SIZE(mt7629_led_groups)},
+	{"pcie", mt7629_pcie_groups, ARRAY_SIZE(mt7629_pcie_groups)},
+	{"pwm",	mt7629_pwm_groups, ARRAY_SIZE(mt7629_pwm_groups)},
+	{"spi",	mt7629_spi_groups, ARRAY_SIZE(mt7629_spi_groups)},
+	{"uart", mt7629_uart_groups, ARRAY_SIZE(mt7629_uart_groups)},
+	{"watchdog", mt7629_wdt_groups, ARRAY_SIZE(mt7629_wdt_groups)},
+	{"wifi", mt7629_wifi_groups, ARRAY_SIZE(mt7629_wifi_groups)},
+	{"flash", mt7629_flash_groups, ARRAY_SIZE(mt7629_flash_groups)},
+};
+
+static const struct mtk_eint_hw mt7629_eint_hw = {
+	.port_mask = 7,
+	.ports     = 7,
+	.ap_num    = ARRAY_SIZE(mt7629_pins),
+	.db_cnt    = 16,
+};
+
+static struct mtk_pin_soc mt7629_data = {
+	.reg_cal = mt7629_reg_cals,
+	.pins = mt7629_pins,
+	.npins = ARRAY_SIZE(mt7629_pins),
+	.grps = mt7629_groups,
+	.ngrps = ARRAY_SIZE(mt7629_groups),
+	.funcs = mt7629_functions,
+	.nfuncs = ARRAY_SIZE(mt7629_functions),
+	.eint_hw = &mt7629_eint_hw,
+	.gpio_m = 0,
+	.ies_present = true,
+	.base_names = mtk_default_register_base_names,
+	.nbase_names = ARRAY_SIZE(mtk_default_register_base_names),
+	.bias_disable_set = mtk_pinconf_bias_disable_set_rev1,
+	.bias_disable_get = mtk_pinconf_bias_disable_get_rev1,
+	.bias_set = mtk_pinconf_bias_set_rev1,
+	.bias_get = mtk_pinconf_bias_get_rev1,
+	.drive_set = mtk_pinconf_drive_set_rev1,
+	.drive_get = mtk_pinconf_drive_get_rev1,
+};
+
+static const struct of_device_id mt7629_pinctrl_of_match[] = {
+	{ .compatible = "mediatek,mt7629-pinctrl", },
+	{}
+};
+
+static int mt7629_pinctrl_probe(struct platform_device *pdev)
+{
+	return mtk_moore_pinctrl_probe(pdev, &mt7629_data);
+}
+
+static struct platform_driver mt7629_pinctrl_driver = {
+	.driver = {
+		.name = "mt7629-pinctrl",
+		.of_match_table = mt7629_pinctrl_of_match,
+	},
+	.probe = mt7629_pinctrl_probe,
+};
+
+static int __init mt7629_pinctrl_init(void)
+{
+	return platform_driver_register(&mt7629_pinctrl_driver);
+}
+arch_initcall(mt7629_pinctrl_init);
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mt8183.c
@@ -0,0 +1,595 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: Zhiyong Tao <zhiyong.tao@mediatek.com>
+ *
+ */
+
+#include "pinctrl-mtk-mt8183.h"
+#include "pinctrl-paris.h"
+
+/* MT8183 have multiple bases to program pin configuration listed as the below:
+ * iocfg[0]:0x10005000, iocfg[1]:0x11F20000, iocfg[2]:0x11E80000,
+ * iocfg[3]:0x11E70000, iocfg[4]:0x11E90000, iocfg[5]:0x11D30000,
+ * iocfg[6]:0x11D20000, iocfg[7]:0x11C50000, iocfg[8]:0x11F30000.
+ * _i_based could be used to indicate what base the pin should be mapped into.
+ */
+
+#define PIN_FIELD_BASE(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit,	\
+		       _x_bits, 32, 0)
+
+#define PINS_FIELD_BASE(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit,	\
+		      _x_bits, 32, 1)
+
+static const struct mtk_pin_field_calc mt8183_pin_mode_range[] = {
+	PIN_FIELD(0, 192, 0x300, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_dir_range[] = {
+	PIN_FIELD(0, 192, 0x0, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_di_range[] = {
+	PIN_FIELD(0, 192, 0x200, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_do_range[] = {
+	PIN_FIELD(0, 192, 0x100, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_ies_range[] = {
+	PINS_FIELD_BASE(0, 3, 6, 0x000, 0x10, 3, 1),
+	PINS_FIELD_BASE(4, 7, 6, 0x000, 0x10, 5, 1),
+	PIN_FIELD_BASE(8, 8, 6, 0x000, 0x10, 0, 1),
+	PINS_FIELD_BASE(9, 10, 6, 0x000, 0x10, 12, 1),
+	PIN_FIELD_BASE(11, 11, 1, 0x000, 0x10, 3, 1),
+	PIN_FIELD_BASE(12, 12, 1, 0x000, 0x10, 7, 1),
+	PINS_FIELD_BASE(13, 16, 2, 0x000, 0x10, 2, 1),
+	PINS_FIELD_BASE(17, 20, 2, 0x000, 0x10, 3, 1),
+	PINS_FIELD_BASE(21, 24, 2, 0x000, 0x10, 4, 1),
+	PINS_FIELD_BASE(25, 28, 2, 0x000, 0x10, 5, 1),
+	PIN_FIELD_BASE(29, 29, 2, 0x000, 0x10, 6, 1),
+	PIN_FIELD_BASE(30, 30, 2, 0x000, 0x10, 7, 1),
+	PINS_FIELD_BASE(31, 31, 2, 0x000, 0x10, 8, 1),
+	PINS_FIELD_BASE(32, 34, 2, 0x000, 0x10, 7, 1),
+	PINS_FIELD_BASE(35, 37, 3, 0x000, 0x10, 0, 1),
+	PINS_FIELD_BASE(38, 40, 3, 0x000, 0x10, 1, 1),
+	PINS_FIELD_BASE(41, 42, 3, 0x000, 0x10, 2, 1),
+	PINS_FIELD_BASE(43, 45, 3, 0x000, 0x10, 3, 1),
+	PINS_FIELD_BASE(46, 47, 3, 0x000, 0x10, 4, 1),
+	PINS_FIELD_BASE(48, 49, 3, 0x000, 0x10, 5, 1),
+	PINS_FIELD_BASE(50, 51, 4, 0x000, 0x10, 0, 1),
+	PINS_FIELD_BASE(52, 57, 4, 0x000, 0x10, 1, 1),
+	PINS_FIELD_BASE(58, 60, 4, 0x000, 0x10, 2, 1),
+	PINS_FIELD_BASE(61, 64, 5, 0x000, 0x10, 0, 1),
+	PINS_FIELD_BASE(65, 66, 5, 0x000, 0x10, 1, 1),
+	PINS_FIELD_BASE(67, 68, 5, 0x000, 0x10, 2, 1),
+	PINS_FIELD_BASE(69, 71, 5, 0x000, 0x10, 3, 1),
+	PINS_FIELD_BASE(72, 76, 5, 0x000, 0x10, 4, 1),
+	PINS_FIELD_BASE(77, 80, 5, 0x000, 0x10, 5, 1),
+	PIN_FIELD_BASE(81, 81, 5, 0x000, 0x10, 6, 1),
+	PINS_FIELD_BASE(82, 83, 5, 0x000, 0x10, 7, 1),
+	PIN_FIELD_BASE(84, 84, 5, 0x000, 0x10, 6, 1),
+	PINS_FIELD_BASE(85, 88, 5, 0x000, 0x10, 8, 1),
+	PIN_FIELD_BASE(89, 89, 6, 0x000, 0x10, 11, 1),
+	PIN_FIELD_BASE(90, 90, 6, 0x000, 0x10, 1, 1),
+	PINS_FIELD_BASE(91, 94, 6, 0x000, 0x10, 2, 1),
+	PINS_FIELD_BASE(95, 96, 6, 0x000, 0x10, 6, 1),
+	PINS_FIELD_BASE(97, 98, 6, 0x000, 0x10, 7, 1),
+	PIN_FIELD_BASE(99, 99, 6, 0x000, 0x10, 8, 1),
+	PIN_FIELD_BASE(100, 100, 6, 0x000, 0x10, 9, 1),
+	PINS_FIELD_BASE(101, 102, 6, 0x000, 0x10, 10, 1),
+	PINS_FIELD_BASE(103, 104, 6, 0x000, 0x10, 13, 1),
+	PINS_FIELD_BASE(105, 106, 6, 0x000, 0x10, 14, 1),
+	PIN_FIELD_BASE(107, 107, 7, 0x000, 0x10, 0, 1),
+	PIN_FIELD_BASE(108, 108, 7, 0x000, 0x10, 1, 1),
+	PIN_FIELD_BASE(109, 109, 7, 0x000, 0x10, 2, 1),
+	PIN_FIELD_BASE(110, 110, 7, 0x000, 0x10, 0, 1),
+	PIN_FIELD_BASE(111, 111, 7, 0x000, 0x10, 3, 1),
+	PIN_FIELD_BASE(112, 112, 7, 0x000, 0x10, 2, 1),
+	PIN_FIELD_BASE(113, 113, 7, 0x000, 0x10, 4, 1),
+	PIN_FIELD_BASE(114, 114, 7, 0x000, 0x10, 5, 1),
+	PIN_FIELD_BASE(115, 115, 7, 0x000, 0x10, 6, 1),
+	PIN_FIELD_BASE(116, 116, 7, 0x000, 0x10, 7, 1),
+	PIN_FIELD_BASE(117, 117, 7, 0x000, 0x10, 8, 1),
+	PIN_FIELD_BASE(118, 118, 7, 0x000, 0x10, 9, 1),
+	PIN_FIELD_BASE(119, 119, 7, 0x000, 0x10, 10, 1),
+	PIN_FIELD_BASE(120, 120, 7, 0x000, 0x10, 11, 1),
+	PIN_FIELD_BASE(121, 121, 7, 0x000, 0x10, 12, 1),
+	PIN_FIELD_BASE(122, 122, 8, 0x000, 0x10, 0, 1),
+	PIN_FIELD_BASE(123, 123, 8, 0x000, 0x10, 1, 1),
+	PIN_FIELD_BASE(124, 124, 8, 0x000, 0x10, 2, 1),
+	PINS_FIELD_BASE(125, 130, 8, 0x000, 0x10, 1, 1),
+	PIN_FIELD_BASE(131, 131, 8, 0x000, 0x10, 3, 1),
+	PIN_FIELD_BASE(132, 132, 8, 0x000, 0x10, 1, 1),
+	PIN_FIELD_BASE(133, 133, 8, 0x000, 0x10, 4, 1),
+	PIN_FIELD_BASE(134, 134, 1, 0x000, 0x10, 0, 1),
+	PIN_FIELD_BASE(135, 135, 1, 0x000, 0x10, 1, 1),
+	PINS_FIELD_BASE(136, 143, 1, 0x000, 0x10, 2, 1),
+	PINS_FIELD_BASE(144, 147, 1, 0x000, 0x10, 4, 1),
+	PIN_FIELD_BASE(148, 148, 1, 0x000, 0x10, 5, 1),
+	PIN_FIELD_BASE(149, 149, 1, 0x000, 0x10, 6, 1),
+	PINS_FIELD_BASE(150, 153, 1, 0x000, 0x10, 8, 1),
+	PIN_FIELD_BASE(154, 154, 1, 0x000, 0x10, 9, 1),
+	PINS_FIELD_BASE(155, 157, 1, 0x000, 0x10, 10, 1),
+	PINS_FIELD_BASE(158, 160, 1, 0x000, 0x10, 8, 1),
+	PINS_FIELD_BASE(161, 164, 2, 0x000, 0x10, 0, 1),
+	PINS_FIELD_BASE(165, 166, 2, 0x000, 0x10, 1, 1),
+	PINS_FIELD_BASE(167, 168, 4, 0x000, 0x10, 2, 1),
+	PIN_FIELD_BASE(169, 169, 4, 0x000, 0x10, 3, 1),
+	PINS_FIELD_BASE(170, 174, 4, 0x000, 0x10, 4, 1),
+	PINS_FIELD_BASE(175, 176, 4, 0x000, 0x10, 3, 1),
+	PINS_FIELD_BASE(177, 179, 6, 0x000, 0x10, 4, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_smt_range[] = {
+	PINS_FIELD_BASE(0, 3, 6, 0x010, 0x10, 3, 1),
+	PINS_FIELD_BASE(4, 7, 6, 0x010, 0x10, 5, 1),
+	PIN_FIELD_BASE(8, 8, 6, 0x010, 0x10, 0, 1),
+	PINS_FIELD_BASE(9, 10, 6, 0x010, 0x10, 12, 1),
+	PIN_FIELD_BASE(11, 11, 1, 0x010, 0x10, 3, 1),
+	PIN_FIELD_BASE(12, 12, 1, 0x010, 0x10, 7, 1),
+	PINS_FIELD_BASE(13, 16, 2, 0x010, 0x10, 2, 1),
+	PINS_FIELD_BASE(17, 20, 2, 0x010, 0x10, 3, 1),
+	PINS_FIELD_BASE(21, 24, 2, 0x010, 0x10, 4, 1),
+	PINS_FIELD_BASE(25, 28, 2, 0x010, 0x10, 5, 1),
+	PIN_FIELD_BASE(29, 29, 2, 0x010, 0x10, 6, 1),
+	PIN_FIELD_BASE(30, 30, 2, 0x010, 0x10, 7, 1),
+	PINS_FIELD_BASE(31, 31, 2, 0x010, 0x10, 8, 1),
+	PINS_FIELD_BASE(32, 34, 2, 0x010, 0x10, 7, 1),
+	PINS_FIELD_BASE(35, 37, 3, 0x010, 0x10, 0, 1),
+	PINS_FIELD_BASE(38, 40, 3, 0x010, 0x10, 1, 1),
+	PINS_FIELD_BASE(41, 42, 3, 0x010, 0x10, 2, 1),
+	PINS_FIELD_BASE(43, 45, 3, 0x010, 0x10, 3, 1),
+	PINS_FIELD_BASE(46, 47, 3, 0x010, 0x10, 4, 1),
+	PINS_FIELD_BASE(48, 49, 3, 0x010, 0x10, 5, 1),
+	PINS_FIELD_BASE(50, 51, 4, 0x010, 0x10, 0, 1),
+	PINS_FIELD_BASE(52, 57, 4, 0x010, 0x10, 1, 1),
+	PINS_FIELD_BASE(58, 60, 4, 0x010, 0x10, 2, 1),
+	PINS_FIELD_BASE(61, 64, 5, 0x010, 0x10, 0, 1),
+	PINS_FIELD_BASE(65, 66, 5, 0x010, 0x10, 1, 1),
+	PINS_FIELD_BASE(67, 68, 5, 0x010, 0x10, 2, 1),
+	PINS_FIELD_BASE(69, 71, 5, 0x010, 0x10, 3, 1),
+	PINS_FIELD_BASE(72, 76, 5, 0x010, 0x10, 4, 1),
+	PINS_FIELD_BASE(77, 80, 5, 0x010, 0x10, 5, 1),
+	PIN_FIELD_BASE(81, 81, 5, 0x010, 0x10, 6, 1),
+	PINS_FIELD_BASE(82, 83, 5, 0x010, 0x10, 7, 1),
+	PIN_FIELD_BASE(84, 84, 5, 0x010, 0x10, 6, 1),
+	PINS_FIELD_BASE(85, 88, 5, 0x010, 0x10, 8, 1),
+	PIN_FIELD_BASE(89, 89, 6, 0x010, 0x10, 11, 1),
+	PIN_FIELD_BASE(90, 90, 6, 0x010, 0x10, 1, 1),
+	PINS_FIELD_BASE(91, 94, 6, 0x010, 0x10, 2, 1),
+	PINS_FIELD_BASE(95, 96, 6, 0x010, 0x10, 6, 1),
+	PINS_FIELD_BASE(97, 98, 6, 0x010, 0x10, 7, 1),
+	PIN_FIELD_BASE(99, 99, 6, 0x010, 0x10, 8, 1),
+	PIN_FIELD_BASE(100, 100, 6, 0x010, 0x10, 9, 1),
+	PINS_FIELD_BASE(101, 102, 6, 0x010, 0x10, 10, 1),
+	PINS_FIELD_BASE(103, 104, 6, 0x010, 0x10, 13, 1),
+	PINS_FIELD_BASE(105, 106, 6, 0x010, 0x10, 14, 1),
+	PIN_FIELD_BASE(107, 107, 7, 0x010, 0x10, 0, 1),
+	PIN_FIELD_BASE(108, 108, 7, 0x010, 0x10, 1, 1),
+	PIN_FIELD_BASE(109, 109, 7, 0x010, 0x10, 2, 1),
+	PIN_FIELD_BASE(110, 110, 7, 0x010, 0x10, 0, 1),
+	PIN_FIELD_BASE(111, 111, 7, 0x010, 0x10, 3, 1),
+	PIN_FIELD_BASE(112, 112, 7, 0x010, 0x10, 2, 1),
+	PIN_FIELD_BASE(113, 113, 7, 0x010, 0x10, 4, 1),
+	PIN_FIELD_BASE(114, 114, 7, 0x010, 0x10, 5, 1),
+	PIN_FIELD_BASE(115, 115, 7, 0x010, 0x10, 6, 1),
+	PIN_FIELD_BASE(116, 116, 7, 0x010, 0x10, 7, 1),
+	PIN_FIELD_BASE(117, 117, 7, 0x010, 0x10, 8, 1),
+	PIN_FIELD_BASE(118, 118, 7, 0x010, 0x10, 9, 1),
+	PIN_FIELD_BASE(119, 119, 7, 0x010, 0x10, 10, 1),
+	PIN_FIELD_BASE(120, 120, 7, 0x010, 0x10, 11, 1),
+	PIN_FIELD_BASE(121, 121, 7, 0x010, 0x10, 12, 1),
+	PIN_FIELD_BASE(122, 122, 8, 0x010, 0x10, 0, 1),
+	PIN_FIELD_BASE(123, 123, 8, 0x010, 0x10, 1, 1),
+	PIN_FIELD_BASE(124, 124, 8, 0x010, 0x10, 2, 1),
+	PINS_FIELD_BASE(125, 130, 8, 0x010, 0x10, 1, 1),
+	PIN_FIELD_BASE(131, 131, 8, 0x010, 0x10, 3, 1),
+	PIN_FIELD_BASE(132, 132, 8, 0x010, 0x10, 1, 1),
+	PIN_FIELD_BASE(133, 133, 8, 0x010, 0x10, 4, 1),
+	PIN_FIELD_BASE(134, 134, 1, 0x010, 0x10, 0, 1),
+	PIN_FIELD_BASE(135, 135, 1, 0x010, 0x10, 1, 1),
+	PINS_FIELD_BASE(136, 143, 1, 0x010, 0x10, 2, 1),
+	PINS_FIELD_BASE(144, 147, 1, 0x010, 0x10, 4, 1),
+	PIN_FIELD_BASE(148, 148, 1, 0x010, 0x10, 5, 1),
+	PIN_FIELD_BASE(149, 149, 1, 0x010, 0x10, 6, 1),
+	PINS_FIELD_BASE(150, 153, 1, 0x010, 0x10, 8, 1),
+	PIN_FIELD_BASE(154, 154, 1, 0x010, 0x10, 9, 1),
+	PINS_FIELD_BASE(155, 157, 1, 0x010, 0x10, 10, 1),
+	PINS_FIELD_BASE(158, 160, 1, 0x010, 0x10, 8, 1),
+	PINS_FIELD_BASE(161, 164, 2, 0x010, 0x10, 0, 1),
+	PINS_FIELD_BASE(165, 166, 2, 0x010, 0x10, 1, 1),
+	PINS_FIELD_BASE(167, 168, 4, 0x010, 0x10, 2, 1),
+	PIN_FIELD_BASE(169, 169, 4, 0x010, 0x10, 3, 1),
+	PINS_FIELD_BASE(170, 174, 4, 0x010, 0x10, 4, 1),
+	PINS_FIELD_BASE(175, 176, 4, 0x010, 0x10, 3, 1),
+	PINS_FIELD_BASE(177, 179, 6, 0x010, 0x10, 4, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_pullen_range[] = {
+	PIN_FIELD_BASE(0, 3, 6, 0x060, 0x10, 6, 1),
+	PIN_FIELD_BASE(4, 7, 6, 0x060, 0x10, 11, 1),
+	PIN_FIELD_BASE(8, 8, 6, 0x060, 0x10, 0, 1),
+	PIN_FIELD_BASE(9, 10, 6, 0x060, 0x10, 26, 1),
+	PIN_FIELD_BASE(11, 11, 1, 0x060, 0x10, 10, 1),
+	PIN_FIELD_BASE(12, 12, 1, 0x060, 0x10, 17, 1),
+	PIN_FIELD_BASE(13, 28, 2, 0x060, 0x10, 6, 1),
+	PIN_FIELD_BASE(43, 49, 3, 0x060, 0x10, 8, 1),
+	PIN_FIELD_BASE(50, 60, 4, 0x060, 0x10, 0, 1),
+	PIN_FIELD_BASE(61, 88, 5, 0x060, 0x10, 0, 1),
+	PIN_FIELD_BASE(89, 89, 6, 0x060, 0x10, 24, 1),
+	PIN_FIELD_BASE(90, 90, 6, 0x060, 0x10, 1, 1),
+	PIN_FIELD_BASE(95, 95, 6, 0x060, 0x10, 15, 1),
+	PIN_FIELD_BASE(96, 102, 6, 0x060, 0x10, 17, 1),
+	PIN_FIELD_BASE(103, 106, 6, 0x060, 0x10, 28, 1),
+	PIN_FIELD_BASE(107, 121, 7, 0x060, 0x10, 0, 1),
+	PIN_FIELD_BASE(134, 143, 1, 0x060, 0x10, 0, 1),
+	PIN_FIELD_BASE(144, 149, 1, 0x060, 0x10, 11, 1),
+	PIN_FIELD_BASE(150, 160, 1, 0x060, 0x10, 18, 1),
+	PIN_FIELD_BASE(161, 166, 2, 0x060, 0x10, 0, 1),
+	PIN_FIELD_BASE(167, 176, 4, 0x060, 0x10, 11, 1),
+	PIN_FIELD_BASE(177, 177, 6, 0x060, 0x10, 10, 1),
+	PIN_FIELD_BASE(178, 178, 6, 0x060, 0x10, 16, 1),
+	PIN_FIELD_BASE(179, 179, 6, 0x060, 0x10, 25, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_pullsel_range[] = {
+	PIN_FIELD_BASE(0, 3, 6, 0x080, 0x10, 6, 1),
+	PIN_FIELD_BASE(4, 7, 6, 0x080, 0x10, 11, 1),
+	PIN_FIELD_BASE(8, 8, 6, 0x080, 0x10, 0, 1),
+	PIN_FIELD_BASE(9, 10, 6, 0x080, 0x10, 26, 1),
+	PIN_FIELD_BASE(11, 11, 1, 0x080, 0x10, 10, 1),
+	PIN_FIELD_BASE(12, 12, 1, 0x080, 0x10, 17, 1),
+	PIN_FIELD_BASE(13, 28, 2, 0x080, 0x10, 6, 1),
+	PIN_FIELD_BASE(43, 49, 3, 0x080, 0x10, 8, 1),
+	PIN_FIELD_BASE(50, 60, 4, 0x080, 0x10, 0, 1),
+	PIN_FIELD_BASE(61, 88, 5, 0x080, 0x10, 0, 1),
+	PIN_FIELD_BASE(89, 89, 6, 0x080, 0x10, 24, 1),
+	PIN_FIELD_BASE(90, 90, 6, 0x080, 0x10, 1, 1),
+	PIN_FIELD_BASE(95, 95, 6, 0x080, 0x10, 15, 1),
+	PIN_FIELD_BASE(96, 102, 6, 0x080, 0x10, 17, 1),
+	PIN_FIELD_BASE(103, 106, 6, 0x080, 0x10, 28, 1),
+	PIN_FIELD_BASE(107, 121, 7, 0x080, 0x10, 0, 1),
+	PIN_FIELD_BASE(134, 143, 1, 0x080, 0x10, 0, 1),
+	PIN_FIELD_BASE(144, 149, 1, 0x080, 0x10, 11, 1),
+	PIN_FIELD_BASE(150, 160, 1, 0x080, 0x10, 18, 1),
+	PIN_FIELD_BASE(161, 166, 2, 0x080, 0x10, 0, 1),
+	PIN_FIELD_BASE(167, 176, 4, 0x080, 0x10, 11, 1),
+	PIN_FIELD_BASE(177, 177, 6, 0x080, 0x10, 10, 1),
+	PIN_FIELD_BASE(178, 178, 6, 0x080, 0x10, 16, 1),
+	PIN_FIELD_BASE(179, 179, 6, 0x080, 0x10, 25, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_drv_range[] = {
+	PINS_FIELD_BASE(0, 3, 6, 0x0A0, 0x10, 12, 3),
+	PINS_FIELD_BASE(4, 7, 6, 0x0A0, 0x10, 20, 3),
+	PIN_FIELD_BASE(8, 8, 6, 0x0A0, 0x10, 0, 3),
+	PINS_FIELD_BASE(9, 10, 6, 0x0B0, 0x10, 16, 3),
+	PIN_FIELD_BASE(11, 11, 1, 0x0A0, 0x10, 12, 3),
+	PIN_FIELD_BASE(12, 12, 1, 0x0A0, 0x10, 28, 3),
+	PINS_FIELD_BASE(13, 16, 2, 0x0A0, 0x10, 8, 3),
+	PINS_FIELD_BASE(17, 20, 2, 0x0A0, 0x10, 12, 3),
+	PINS_FIELD_BASE(21, 24, 2, 0x0A0, 0x10, 16, 3),
+	PINS_FIELD_BASE(25, 28, 2, 0x0A0, 0x10, 20, 3),
+	PIN_FIELD_BASE(29, 29, 2, 0x0A0, 0x10, 24, 3),
+	PIN_FIELD_BASE(30, 30, 2, 0x0A0, 0x10, 28, 3),
+	PINS_FIELD_BASE(31, 31, 2, 0x0B0, 0x10, 0, 3),
+	PINS_FIELD_BASE(32, 34, 2, 0x0A0, 0x10, 28, 3),
+	PINS_FIELD_BASE(35, 37, 3, 0x0A0, 0x10, 0, 3),
+	PINS_FIELD_BASE(38, 40, 3, 0x0A0, 0x10, 4, 3),
+	PINS_FIELD_BASE(41, 42, 3, 0x0A0, 0x10, 8, 3),
+	PINS_FIELD_BASE(43, 45, 3, 0x0A0, 0x10, 12, 3),
+	PINS_FIELD_BASE(46, 47, 3, 0x0A0, 0x10, 16, 3),
+	PINS_FIELD_BASE(48, 49, 3, 0x0A0, 0x10, 20, 3),
+	PINS_FIELD_BASE(50, 51, 4, 0x0A0, 0x10, 0, 3),
+	PINS_FIELD_BASE(52, 57, 4, 0x0A0, 0x10, 4, 3),
+	PINS_FIELD_BASE(58, 60, 4, 0x0A0, 0x10, 8, 3),
+	PINS_FIELD_BASE(61, 64, 5, 0x0A0, 0x10, 0, 3),
+	PINS_FIELD_BASE(65, 66, 5, 0x0A0, 0x10, 4, 3),
+	PINS_FIELD_BASE(67, 68, 5, 0x0A0, 0x10, 8, 3),
+	PINS_FIELD_BASE(69, 71, 5, 0x0A0, 0x10, 12, 3),
+	PINS_FIELD_BASE(72, 76, 5, 0x0A0, 0x10, 16, 3),
+	PINS_FIELD_BASE(77, 80, 5, 0x0A0, 0x10, 20, 3),
+	PIN_FIELD_BASE(81, 81, 5, 0x0A0, 0x10, 24, 3),
+	PINS_FIELD_BASE(82, 83, 5, 0x0A0, 0x10, 28, 3),
+	PIN_FIELD_BASE(84, 84, 5, 0x0A0, 0x10, 24, 3),
+	PINS_FIELD_BASE(85, 88, 5, 0x0B0, 0x10, 0, 3),
+	PIN_FIELD_BASE(89, 89, 6, 0x0B0, 0x10, 12, 3),
+	PIN_FIELD_BASE(90, 90, 6, 0x0A0, 0x10, 4, 3),
+	PINS_FIELD_BASE(91, 94, 6, 0x0A0, 0x10, 8, 3),
+	PINS_FIELD_BASE(95, 96, 6, 0x0A0, 0x10, 24, 3),
+	PINS_FIELD_BASE(97, 98, 6, 0x0A0, 0x10, 28, 3),
+	PIN_FIELD_BASE(99, 99, 6, 0x0B0, 0x10, 0, 3),
+	PIN_FIELD_BASE(100, 100, 6, 0x0B0, 0x10, 4, 3),
+	PINS_FIELD_BASE(101, 102, 6, 0x0B0, 0x10, 8, 3),
+	PINS_FIELD_BASE(103, 104, 6, 0x0B0, 0x10, 20, 3),
+	PINS_FIELD_BASE(105, 106, 6, 0x0B0, 0x10, 24, 3),
+	PIN_FIELD_BASE(107, 107, 7, 0x0A0, 0x10, 0, 3),
+	PIN_FIELD_BASE(108, 108, 7, 0x0A0, 0x10, 4, 3),
+	PIN_FIELD_BASE(109, 109, 7, 0x0A0, 0x10, 8, 3),
+	PIN_FIELD_BASE(110, 110, 7, 0x0A0, 0x10, 0, 3),
+	PIN_FIELD_BASE(111, 111, 7, 0x0A0, 0x10, 4, 3),
+	PIN_FIELD_BASE(112, 112, 7, 0x0A0, 0x10, 8, 3),
+	PIN_FIELD_BASE(113, 113, 7, 0x0A0, 0x10, 16, 3),
+	PIN_FIELD_BASE(114, 114, 7, 0x0A0, 0x10, 20, 3),
+	PIN_FIELD_BASE(115, 115, 7, 0x0A0, 0x10, 24, 3),
+	PIN_FIELD_BASE(116, 116, 7, 0x0A0, 0x10, 28, 3),
+	PIN_FIELD_BASE(117, 117, 7, 0x0B0, 0x10, 0, 3),
+	PIN_FIELD_BASE(118, 118, 7, 0x0B0, 0x10, 4, 3),
+	PIN_FIELD_BASE(119, 119, 7, 0x0B0, 0x10, 8, 3),
+	PIN_FIELD_BASE(120, 120, 7, 0x0B0, 0x10, 12, 3),
+	PIN_FIELD_BASE(121, 121, 7, 0x0B0, 0x10, 16, 3),
+	PIN_FIELD_BASE(122, 122, 8, 0x0A0, 0x10, 0, 3),
+	PIN_FIELD_BASE(123, 123, 8, 0x0A0, 0x10, 4, 3),
+	PIN_FIELD_BASE(124, 124, 8, 0x0A0, 0x10, 8, 3),
+	PINS_FIELD_BASE(125, 130, 8, 0x0A0, 0x10, 4, 3),
+	PIN_FIELD_BASE(131, 131, 8, 0x0A0, 0x10, 12, 3),
+	PIN_FIELD_BASE(132, 132, 8, 0x0A0, 0x10, 4, 3),
+	PIN_FIELD_BASE(133, 133, 8, 0x0A0, 0x10, 16, 3),
+	PIN_FIELD_BASE(134, 134, 1, 0x0A0, 0x10, 0, 3),
+	PIN_FIELD_BASE(135, 135, 1, 0x0A0, 0x10, 4, 3),
+	PINS_FIELD_BASE(136, 143, 1, 0x0A0, 0x10, 8, 3),
+	PINS_FIELD_BASE(144, 147, 1, 0x0A0, 0x10, 16, 3),
+	PIN_FIELD_BASE(148, 148, 1, 0x0A0, 0x10, 20, 3),
+	PIN_FIELD_BASE(149, 149, 1, 0x0A0, 0x10, 24, 3),
+	PINS_FIELD_BASE(150, 153, 1, 0x0B0, 0x10, 0, 3),
+	PIN_FIELD_BASE(154, 154, 1, 0x0B0, 0x10, 4, 3),
+	PINS_FIELD_BASE(155, 157, 1, 0x0B0, 0x10, 8, 3),
+	PINS_FIELD_BASE(158, 160, 1, 0x0B0, 0x10, 0, 3),
+	PINS_FIELD_BASE(161, 164, 2, 0x0A0, 0x10, 0, 3),
+	PINS_FIELD_BASE(165, 166, 2, 0x0A0, 0x10, 4, 3),
+	PINS_FIELD_BASE(167, 168, 4, 0x0A0, 0x10, 8, 3),
+	PIN_FIELD_BASE(169, 169, 4, 0x0A0, 0x10, 12, 3),
+	PINS_FIELD_BASE(170, 174, 4, 0x0A0, 0x10, 16, 3),
+	PINS_FIELD_BASE(175, 176, 4, 0x0A0, 0x10, 12, 3),
+	PINS_FIELD_BASE(177, 179, 6, 0x0A0, 0x10, 16, 3),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_pupd_range[] = {
+	PIN_FIELD_BASE(29, 29, 2, 0x0C0, 0x10, 2, 1),
+	PIN_FIELD_BASE(30, 30, 2, 0x0C0, 0x10, 6, 1),
+	PIN_FIELD_BASE(31, 31, 2, 0x0C0, 0x10, 10, 1),
+	PIN_FIELD_BASE(32, 32, 2, 0x0C0, 0x10, 14, 1),
+	PIN_FIELD_BASE(33, 33, 2, 0x0C0, 0x10, 18, 1),
+	PIN_FIELD_BASE(34, 34, 2, 0x0C0, 0x10, 22, 1),
+	PIN_FIELD_BASE(35, 35, 3, 0x0C0, 0x10, 2, 1),
+	PIN_FIELD_BASE(36, 36, 3, 0x0C0, 0x10, 6, 1),
+	PIN_FIELD_BASE(37, 37, 3, 0x0C0, 0x10, 10, 1),
+	PIN_FIELD_BASE(38, 38, 3, 0x0C0, 0x10, 14, 1),
+	PIN_FIELD_BASE(39, 39, 3, 0x0C0, 0x10, 18, 1),
+	PIN_FIELD_BASE(40, 40, 3, 0x0C0, 0x10, 22, 1),
+	PIN_FIELD_BASE(41, 41, 3, 0x0C0, 0x10, 26, 1),
+	PIN_FIELD_BASE(42, 42, 3, 0x0C0, 0x10, 30, 1),
+	PIN_FIELD_BASE(91, 91, 6, 0x0C0, 0x10, 2, 1),
+	PIN_FIELD_BASE(92, 92, 6, 0x0C0, 0x10, 6, 1),
+	PIN_FIELD_BASE(93, 93, 6, 0x0C0, 0x10, 10, 1),
+	PIN_FIELD_BASE(94, 94, 6, 0x0C0, 0x10, 14, 1),
+	PIN_FIELD_BASE(122, 122, 8, 0x0C0, 0x10, 2, 1),
+	PIN_FIELD_BASE(123, 123, 8, 0x0C0, 0x10, 6, 1),
+	PIN_FIELD_BASE(124, 124, 8, 0x0C0, 0x10, 10, 1),
+	PIN_FIELD_BASE(125, 125, 8, 0x0C0, 0x10, 14, 1),
+	PIN_FIELD_BASE(126, 126, 8, 0x0C0, 0x10, 18, 1),
+	PIN_FIELD_BASE(127, 127, 8, 0x0C0, 0x10, 22, 1),
+	PIN_FIELD_BASE(128, 128, 8, 0x0C0, 0x10, 26, 1),
+	PIN_FIELD_BASE(129, 129, 8, 0x0C0, 0x10, 30, 1),
+	PIN_FIELD_BASE(130, 130, 8, 0x0D0, 0x10, 2, 1),
+	PIN_FIELD_BASE(131, 131, 8, 0x0D0, 0x10, 6, 1),
+	PIN_FIELD_BASE(132, 132, 8, 0x0D0, 0x10, 10, 1),
+	PIN_FIELD_BASE(133, 133, 8, 0x0D0, 0x10, 14, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_r0_range[] = {
+	PIN_FIELD_BASE(29, 29, 2, 0x0C0, 0x10, 0, 1),
+	PIN_FIELD_BASE(30, 30, 2, 0x0C0, 0x10, 4, 1),
+	PIN_FIELD_BASE(31, 31, 2, 0x0C0, 0x10, 8, 1),
+	PIN_FIELD_BASE(32, 32, 2, 0x0C0, 0x10, 12, 1),
+	PIN_FIELD_BASE(33, 33, 2, 0x0C0, 0x10, 16, 1),
+	PIN_FIELD_BASE(34, 34, 2, 0x0C0, 0x10, 20, 1),
+	PIN_FIELD_BASE(35, 35, 3, 0x0C0, 0x10, 0, 1),
+	PIN_FIELD_BASE(36, 36, 3, 0x0C0, 0x10, 4, 1),
+	PIN_FIELD_BASE(37, 37, 3, 0x0C0, 0x10, 8, 1),
+	PIN_FIELD_BASE(38, 38, 3, 0x0C0, 0x10, 12, 1),
+	PIN_FIELD_BASE(39, 39, 3, 0x0C0, 0x10, 16, 1),
+	PIN_FIELD_BASE(40, 40, 3, 0x0C0, 0x10, 20, 1),
+	PIN_FIELD_BASE(41, 41, 3, 0x0C0, 0x10, 24, 1),
+	PIN_FIELD_BASE(42, 42, 3, 0x0C0, 0x10, 28, 1),
+	PIN_FIELD_BASE(48, 48, 3, 0x0F0, 0x10, 18, 1),
+	PIN_FIELD_BASE(49, 49, 3, 0x0F0, 0x10, 13, 1),
+	PIN_FIELD_BASE(50, 50, 4, 0x0F0, 0x10, 10, 1),
+	PIN_FIELD_BASE(51, 51, 4, 0x0F0, 0x10, 5, 1),
+	PIN_FIELD_BASE(81, 81, 5, 0x0F0, 0x10, 7, 1),
+	PIN_FIELD_BASE(82, 82, 5, 0x0F0, 0x10, 5, 1),
+	PIN_FIELD_BASE(83, 83, 5, 0x0F0, 0x10, 15, 1),
+	PIN_FIELD_BASE(84, 84, 5, 0x0F0, 0x10, 17, 1),
+	PIN_FIELD_BASE(91, 91, 6, 0x0C0, 0x10, 0, 1),
+	PIN_FIELD_BASE(92, 92, 6, 0x0C0, 0x10, 4, 1),
+	PIN_FIELD_BASE(93, 93, 6, 0x0C0, 0x10, 8, 1),
+	PIN_FIELD_BASE(94, 94, 6, 0x0C0, 0x10, 12, 1),
+	PIN_FIELD_BASE(103, 103, 6, 0x0F0, 0x10, 20, 1),
+	PIN_FIELD_BASE(104, 104, 6, 0x0F0, 0x10, 10, 1),
+	PIN_FIELD_BASE(105, 105, 6, 0x0F0, 0x10, 22, 1),
+	PIN_FIELD_BASE(106, 106, 6, 0x0F0, 0x10, 12, 1),
+	PIN_FIELD_BASE(122, 122, 8, 0x0C0, 0x10, 0, 1),
+	PIN_FIELD_BASE(123, 123, 8, 0x0C0, 0x10, 4, 1),
+	PIN_FIELD_BASE(124, 124, 8, 0x0C0, 0x10, 8, 1),
+	PIN_FIELD_BASE(125, 125, 8, 0x0C0, 0x10, 12, 1),
+	PIN_FIELD_BASE(126, 126, 8, 0x0C0, 0x10, 16, 1),
+	PIN_FIELD_BASE(127, 127, 8, 0x0C0, 0x10, 20, 1),
+	PIN_FIELD_BASE(128, 128, 8, 0x0C0, 0x10, 24, 1),
+	PIN_FIELD_BASE(129, 129, 8, 0x0C0, 0x10, 28, 1),
+	PIN_FIELD_BASE(130, 130, 8, 0x0D0, 0x10, 0, 1),
+	PIN_FIELD_BASE(131, 131, 8, 0x0D0, 0x10, 4, 1),
+	PIN_FIELD_BASE(132, 132, 8, 0x0D0, 0x10, 8, 1),
+	PIN_FIELD_BASE(133, 133, 8, 0x0D0, 0x10, 12, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_r1_range[] = {
+	PIN_FIELD_BASE(29, 29, 2, 0x0C0, 0x10, 1, 1),
+	PIN_FIELD_BASE(30, 30, 2, 0x0C0, 0x10, 5, 1),
+	PIN_FIELD_BASE(31, 31, 2, 0x0C0, 0x10, 9, 1),
+	PIN_FIELD_BASE(32, 32, 2, 0x0C0, 0x10, 13, 1),
+	PIN_FIELD_BASE(33, 33, 2, 0x0C0, 0x10, 17, 1),
+	PIN_FIELD_BASE(34, 34, 2, 0x0C0, 0x10, 21, 1),
+	PIN_FIELD_BASE(35, 35, 3, 0x0C0, 0x10, 1, 1),
+	PIN_FIELD_BASE(36, 36, 3, 0x0C0, 0x10, 5, 1),
+	PIN_FIELD_BASE(37, 37, 3, 0x0C0, 0x10, 9, 1),
+	PIN_FIELD_BASE(38, 38, 3, 0x0C0, 0x10, 13, 1),
+	PIN_FIELD_BASE(39, 39, 3, 0x0C0, 0x10, 17, 1),
+	PIN_FIELD_BASE(40, 40, 3, 0x0C0, 0x10, 21, 1),
+	PIN_FIELD_BASE(41, 41, 3, 0x0C0, 0x10, 25, 1),
+	PIN_FIELD_BASE(42, 42, 3, 0x0C0, 0x10, 29, 1),
+	PIN_FIELD_BASE(48, 48, 3, 0x0F0, 0x10, 19, 1),
+	PIN_FIELD_BASE(49, 49, 3, 0x0F0, 0x10, 14, 1),
+	PIN_FIELD_BASE(50, 50, 4, 0x0F0, 0x10, 11, 1),
+	PIN_FIELD_BASE(51, 51, 4, 0x0F0, 0x10, 6, 1),
+	PIN_FIELD_BASE(81, 81, 5, 0x0F0, 0x10, 8, 1),
+	PIN_FIELD_BASE(82, 82, 5, 0x0F0, 0x10, 6, 1),
+	PIN_FIELD_BASE(83, 83, 5, 0x0F0, 0x10, 16, 1),
+	PIN_FIELD_BASE(84, 84, 5, 0x0F0, 0x10, 18, 1),
+	PIN_FIELD_BASE(91, 91, 6, 0x0C0, 0x10, 1, 1),
+	PIN_FIELD_BASE(92, 92, 6, 0x0C0, 0x10, 5, 1),
+	PIN_FIELD_BASE(93, 93, 6, 0x0C0, 0x10, 9, 1),
+	PIN_FIELD_BASE(94, 94, 6, 0x0C0, 0x10, 13, 1),
+	PIN_FIELD_BASE(103, 103, 6, 0x0F0, 0x10, 21, 1),
+	PIN_FIELD_BASE(104, 104, 6, 0x0F0, 0x10, 11, 1),
+	PIN_FIELD_BASE(105, 105, 6, 0x0F0, 0x10, 23, 1),
+	PIN_FIELD_BASE(106, 106, 6, 0x0F0, 0x10, 13, 1),
+	PIN_FIELD_BASE(122, 122, 8, 0x0C0, 0x10, 1, 1),
+	PIN_FIELD_BASE(123, 123, 8, 0x0C0, 0x10, 5, 1),
+	PIN_FIELD_BASE(124, 124, 8, 0x0C0, 0x10, 9, 1),
+	PIN_FIELD_BASE(125, 125, 8, 0x0C0, 0x10, 13, 1),
+	PIN_FIELD_BASE(126, 126, 8, 0x0C0, 0x10, 17, 1),
+	PIN_FIELD_BASE(127, 127, 8, 0x0C0, 0x10, 21, 1),
+	PIN_FIELD_BASE(128, 128, 8, 0x0C0, 0x10, 25, 1),
+	PIN_FIELD_BASE(129, 129, 8, 0x0C0, 0x10, 29, 1),
+	PIN_FIELD_BASE(130, 130, 8, 0x0D0, 0x10, 1, 1),
+	PIN_FIELD_BASE(131, 131, 8, 0x0D0, 0x10, 5, 1),
+	PIN_FIELD_BASE(132, 132, 8, 0x0D0, 0x10, 9, 1),
+	PIN_FIELD_BASE(133, 133, 8, 0x0D0, 0x10, 13, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_e1e0en_range[] = {
+	PIN_FIELD_BASE(48, 48, 3, 0x0F0, 0x10, 20, 1),
+	PIN_FIELD_BASE(49, 49, 3, 0x0F0, 0x10, 15, 1),
+	PIN_FIELD_BASE(50, 50, 4, 0x0F0, 0x10, 12, 1),
+	PIN_FIELD_BASE(51, 51, 4, 0x0F0, 0x10, 7, 1),
+	PIN_FIELD_BASE(81, 81, 5, 0x0F0, 0x10, 12, 1),
+	PIN_FIELD_BASE(82, 82, 5, 0x0F0, 0x10, 9, 1),
+	PIN_FIELD_BASE(83, 83, 5, 0x0F0, 0x10, 19, 1),
+	PIN_FIELD_BASE(84, 84, 5, 0x0F0, 0x10, 22, 1),
+	PIN_FIELD_BASE(103, 103, 6, 0x0F0, 0x10, 24, 1),
+	PIN_FIELD_BASE(104, 104, 6, 0x0F0, 0x10, 14, 1),
+	PIN_FIELD_BASE(105, 105, 6, 0x0F0, 0x10, 27, 1),
+	PIN_FIELD_BASE(106, 106, 6, 0x0F0, 0x10, 17, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_e0_range[] = {
+	PIN_FIELD_BASE(48, 48, 3, 0x0F0, 0x10, 21, 1),
+	PIN_FIELD_BASE(49, 49, 3, 0x0F0, 0x10, 16, 1),
+	PIN_FIELD_BASE(50, 50, 4, 0x0F0, 0x10, 13, 1),
+	PIN_FIELD_BASE(51, 51, 4, 0x0F0, 0x10, 8, 1),
+	PIN_FIELD_BASE(81, 81, 5, 0x0F0, 0x10, 13, 1),
+	PIN_FIELD_BASE(82, 82, 5, 0x0F0, 0x10, 10, 1),
+	PIN_FIELD_BASE(83, 83, 5, 0x0F0, 0x10, 20, 1),
+	PIN_FIELD_BASE(84, 84, 5, 0x0F0, 0x10, 23, 1),
+	PIN_FIELD_BASE(103, 103, 6, 0x0F0, 0x10, 25, 1),
+	PIN_FIELD_BASE(104, 104, 6, 0x0F0, 0x10, 15, 1),
+	PIN_FIELD_BASE(105, 105, 6, 0x0F0, 0x10, 28, 1),
+	PIN_FIELD_BASE(106, 106, 6, 0x0F0, 0x10, 18, 1),
+};
+
+static const struct mtk_pin_field_calc mt8183_pin_e1_range[] = {
+	PIN_FIELD_BASE(48, 48, 3, 0x0F0, 0x10, 22, 1),
+	PIN_FIELD_BASE(49, 49, 3, 0x0F0, 0x10, 17, 1),
+	PIN_FIELD_BASE(50, 50, 4, 0x0F0, 0x10, 14, 1),
+	PIN_FIELD_BASE(51, 51, 4, 0x0F0, 0x10, 9, 1),
+	PIN_FIELD_BASE(81, 81, 5, 0x0F0, 0x10, 14, 1),
+	PIN_FIELD_BASE(82, 82, 5, 0x0F0, 0x10, 11, 1),
+	PIN_FIELD_BASE(83, 83, 5, 0x0F0, 0x10, 21, 1),
+	PIN_FIELD_BASE(84, 84, 5, 0x0F0, 0x10, 24, 1),
+	PIN_FIELD_BASE(103, 103, 6, 0x0F0, 0x10, 26, 1),
+	PIN_FIELD_BASE(104, 104, 6, 0x0F0, 0x10, 16, 1),
+	PIN_FIELD_BASE(105, 105, 6, 0x0F0, 0x10, 29, 1),
+	PIN_FIELD_BASE(106, 106, 6, 0x0F0, 0x10, 19, 1),
+};
+
+static const struct mtk_pin_reg_calc mt8183_reg_cals[PINCTRL_PIN_REG_MAX] = {
+	[PINCTRL_PIN_REG_MODE] = MTK_RANGE(mt8183_pin_mode_range),
+	[PINCTRL_PIN_REG_DIR] = MTK_RANGE(mt8183_pin_dir_range),
+	[PINCTRL_PIN_REG_DI] = MTK_RANGE(mt8183_pin_di_range),
+	[PINCTRL_PIN_REG_DO] = MTK_RANGE(mt8183_pin_do_range),
+	[PINCTRL_PIN_REG_SMT] = MTK_RANGE(mt8183_pin_smt_range),
+	[PINCTRL_PIN_REG_IES] = MTK_RANGE(mt8183_pin_ies_range),
+	[PINCTRL_PIN_REG_PULLEN] = MTK_RANGE(mt8183_pin_pullen_range),
+	[PINCTRL_PIN_REG_PULLSEL] = MTK_RANGE(mt8183_pin_pullsel_range),
+	[PINCTRL_PIN_REG_DRV] = MTK_RANGE(mt8183_pin_drv_range),
+	[PINCTRL_PIN_REG_PUPD] = MTK_RANGE(mt8183_pin_pupd_range),
+	[PINCTRL_PIN_REG_R0] = MTK_RANGE(mt8183_pin_r0_range),
+	[PINCTRL_PIN_REG_R1] = MTK_RANGE(mt8183_pin_r1_range),
+	[PINCTRL_PIN_REG_DRV_EN] = MTK_RANGE(mt8183_pin_e1e0en_range),
+	[PINCTRL_PIN_REG_DRV_E0] = MTK_RANGE(mt8183_pin_e0_range),
+	[PINCTRL_PIN_REG_DRV_E1] = MTK_RANGE(mt8183_pin_e1_range),
+};
+
+static const char * const mt8183_pinctrl_register_base_names[] = {
+	"iocfg0", "iocfg1", "iocfg2", "iocfg3", "iocfg4", "iocfg5",
+	"iocfg6", "iocfg7", "iocfg8",
+};
+
+static const struct mtk_eint_hw mt8183_eint_hw = {
+	.port_mask = 7,
+	.ports     = 6,
+	.ap_num    = 212,
+	.db_cnt    = 13,
+};
+
+static const struct mtk_pin_soc mt8183_data = {
+	.reg_cal = mt8183_reg_cals,
+	.pins = mtk_pins_mt8183,
+	.npins = ARRAY_SIZE(mtk_pins_mt8183),
+	.ngrps = ARRAY_SIZE(mtk_pins_mt8183),
+	.eint_hw = &mt8183_eint_hw,
+	.gpio_m = 0,
+	.ies_present = true,
+	.base_names = mt8183_pinctrl_register_base_names,
+	.nbase_names = ARRAY_SIZE(mt8183_pinctrl_register_base_names),
+	.bias_disable_set = mtk_pinconf_bias_disable_set_rev1,
+	.bias_disable_get = mtk_pinconf_bias_disable_get_rev1,
+	.bias_set = mtk_pinconf_bias_set_rev1,
+	.bias_get = mtk_pinconf_bias_get_rev1,
+	.drive_set = mtk_pinconf_drive_set_rev1,
+	.drive_get = mtk_pinconf_drive_get_rev1,
+	.adv_pull_get = mtk_pinconf_adv_pull_get,
+	.adv_pull_set = mtk_pinconf_adv_pull_set,
+	.adv_drive_get = mtk_pinconf_adv_drive_get,
+	.adv_drive_set = mtk_pinconf_adv_drive_set,
+};
+
+static const struct of_device_id mt8183_pinctrl_of_match[] = {
+	{ .compatible = "mediatek,mt8183-pinctrl", },
+	{ }
+};
+
+static int mt8183_pinctrl_probe(struct platform_device *pdev)
+{
+	return mtk_paris_pinctrl_probe(pdev, &mt8183_data);
+}
+
+static struct platform_driver mt8183_pinctrl_driver = {
+	.driver = {
+		.name = "mt8183-pinctrl",
+		.of_match_table = mt8183_pinctrl_of_match,
+		.pm = &mtk_paris_pinctrl_pm_ops,
+	},
+	.probe = mt8183_pinctrl_probe,
+};
+
+static int __init mt8183_pinctrl_init(void)
+{
+	return platform_driver_register(&mt8183_pinctrl_driver);
+}
+arch_initcall(mt8183_pinctrl_init);
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mt8516.c
@@ -0,0 +1,362 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (c) 2019 MediaTek Inc.
+ * Author: Min.Guo <min.guo@mediatek.com>
+ */
+
+#include <dt-bindings/pinctrl/mt65xx.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/module.h>
+#include <linux/pinctrl/pinctrl.h>
+#include <linux/platform_device.h>
+#include <linux/regmap.h>
+
+#include "pinctrl-mtk-common.h"
+#include "pinctrl-mtk-mt8516.h"
+
+static const struct mtk_drv_group_desc mt8516_drv_grp[] = {
+	/* 0E4E8SR 4/8/12/16 */
+	MTK_DRV_GRP(4, 16, 1, 2, 4),
+	/* 0E2E4SR  2/4/6/8 */
+	MTK_DRV_GRP(2, 8, 1, 2, 2),
+	/* E8E4E2  2/4/6/8/10/12/14/16 */
+	MTK_DRV_GRP(2, 16, 0, 2, 2)
+};
+
+static const struct mtk_pin_drv_grp mt8516_pin_drv[] = {
+	MTK_PIN_DRV_GRP(0, 0xd00, 0, 0),
+	MTK_PIN_DRV_GRP(1, 0xd00, 0, 0),
+	MTK_PIN_DRV_GRP(2, 0xd00, 0, 0),
+	MTK_PIN_DRV_GRP(3, 0xd00, 0, 0),
+	MTK_PIN_DRV_GRP(4, 0xd00, 0, 0),
+
+	MTK_PIN_DRV_GRP(5, 0xd00, 4, 0),
+	MTK_PIN_DRV_GRP(6, 0xd00, 4, 0),
+	MTK_PIN_DRV_GRP(7, 0xd00, 4, 0),
+	MTK_PIN_DRV_GRP(8, 0xd00, 4, 0),
+	MTK_PIN_DRV_GRP(9, 0xd00, 4, 0),
+	MTK_PIN_DRV_GRP(10, 0xd00, 4, 0),
+
+	MTK_PIN_DRV_GRP(11, 0xd00, 8, 0),
+	MTK_PIN_DRV_GRP(12, 0xd00, 8, 0),
+	MTK_PIN_DRV_GRP(13, 0xd00, 8, 0),
+
+	MTK_PIN_DRV_GRP(14, 0xd00, 12, 2),
+	MTK_PIN_DRV_GRP(15, 0xd00, 12, 2),
+	MTK_PIN_DRV_GRP(16, 0xd00, 12, 2),
+	MTK_PIN_DRV_GRP(17, 0xd00, 12, 2),
+
+	MTK_PIN_DRV_GRP(18, 0xd10, 0, 0),
+	MTK_PIN_DRV_GRP(19, 0xd10, 0, 0),
+	MTK_PIN_DRV_GRP(20, 0xd10, 0, 0),
+
+	MTK_PIN_DRV_GRP(21, 0xd00, 12, 2),
+	MTK_PIN_DRV_GRP(22, 0xd00, 12, 2),
+	MTK_PIN_DRV_GRP(23, 0xd00, 12, 2),
+
+	MTK_PIN_DRV_GRP(24, 0xd00, 8, 0),
+	MTK_PIN_DRV_GRP(25, 0xd00, 8, 0),
+
+	MTK_PIN_DRV_GRP(26, 0xd10, 4, 1),
+	MTK_PIN_DRV_GRP(27, 0xd10, 4, 1),
+	MTK_PIN_DRV_GRP(28, 0xd10, 4, 1),
+	MTK_PIN_DRV_GRP(29, 0xd10, 4, 1),
+	MTK_PIN_DRV_GRP(30, 0xd10, 4, 1),
+
+	MTK_PIN_DRV_GRP(31, 0xd10, 8, 1),
+	MTK_PIN_DRV_GRP(32, 0xd10, 8, 1),
+	MTK_PIN_DRV_GRP(33, 0xd10, 8, 1),
+
+	MTK_PIN_DRV_GRP(34, 0xd10, 12, 0),
+	MTK_PIN_DRV_GRP(35, 0xd10, 12, 0),
+
+	MTK_PIN_DRV_GRP(36, 0xd20, 0, 0),
+	MTK_PIN_DRV_GRP(37, 0xd20, 0, 0),
+	MTK_PIN_DRV_GRP(38, 0xd20, 0, 0),
+	MTK_PIN_DRV_GRP(39, 0xd20, 0, 0),
+
+	MTK_PIN_DRV_GRP(40, 0xd20, 4, 1),
+
+	MTK_PIN_DRV_GRP(41, 0xd20, 8, 1),
+	MTK_PIN_DRV_GRP(42, 0xd20, 8, 1),
+	MTK_PIN_DRV_GRP(43, 0xd20, 8, 1),
+
+	MTK_PIN_DRV_GRP(44, 0xd20, 12, 1),
+	MTK_PIN_DRV_GRP(45, 0xd20, 12, 1),
+	MTK_PIN_DRV_GRP(46, 0xd20, 12, 1),
+	MTK_PIN_DRV_GRP(47, 0xd20, 12, 1),
+
+	MTK_PIN_DRV_GRP(48, 0xd30, 0, 1),
+	MTK_PIN_DRV_GRP(49, 0xd30, 0, 1),
+	MTK_PIN_DRV_GRP(50, 0xd30, 0, 1),
+	MTK_PIN_DRV_GRP(51, 0xd30, 0, 1),
+
+	MTK_PIN_DRV_GRP(54, 0xd30, 8, 1),
+
+	MTK_PIN_DRV_GRP(55, 0xd30, 12, 1),
+	MTK_PIN_DRV_GRP(56, 0xd30, 12, 1),
+	MTK_PIN_DRV_GRP(57, 0xd30, 12, 1),
+
+	MTK_PIN_DRV_GRP(62, 0xd40, 8, 1),
+	MTK_PIN_DRV_GRP(63, 0xd40, 8, 1),
+	MTK_PIN_DRV_GRP(64, 0xd40, 8, 1),
+	MTK_PIN_DRV_GRP(65, 0xd40, 8, 1),
+	MTK_PIN_DRV_GRP(66, 0xd40, 8, 1),
+	MTK_PIN_DRV_GRP(67, 0xd40, 8, 1),
+
+	MTK_PIN_DRV_GRP(68, 0xd40, 12, 2),
+
+	MTK_PIN_DRV_GRP(69, 0xd50, 0, 2),
+
+	MTK_PIN_DRV_GRP(70, 0xd50, 4, 2),
+	MTK_PIN_DRV_GRP(71, 0xd50, 4, 2),
+	MTK_PIN_DRV_GRP(72, 0xd50, 4, 2),
+	MTK_PIN_DRV_GRP(73, 0xd50, 4, 2),
+
+	MTK_PIN_DRV_GRP(100, 0xd50, 8, 1),
+	MTK_PIN_DRV_GRP(101, 0xd50, 8, 1),
+	MTK_PIN_DRV_GRP(102, 0xd50, 8, 1),
+	MTK_PIN_DRV_GRP(103, 0xd50, 8, 1),
+
+	MTK_PIN_DRV_GRP(104, 0xd50, 12, 2),
+
+	MTK_PIN_DRV_GRP(105, 0xd60, 0, 2),
+
+	MTK_PIN_DRV_GRP(106, 0xd60, 4, 2),
+	MTK_PIN_DRV_GRP(107, 0xd60, 4, 2),
+	MTK_PIN_DRV_GRP(108, 0xd60, 4, 2),
+	MTK_PIN_DRV_GRP(109, 0xd60, 4, 2),
+
+	MTK_PIN_DRV_GRP(110, 0xd70, 0, 2),
+	MTK_PIN_DRV_GRP(111, 0xd70, 0, 2),
+	MTK_PIN_DRV_GRP(112, 0xd70, 0, 2),
+	MTK_PIN_DRV_GRP(113, 0xd70, 0, 2),
+
+	MTK_PIN_DRV_GRP(114, 0xd70, 4, 2),
+
+	MTK_PIN_DRV_GRP(115, 0xd60, 12, 2),
+
+	MTK_PIN_DRV_GRP(116, 0xd60, 8, 2),
+
+	MTK_PIN_DRV_GRP(117, 0xd70, 0, 2),
+	MTK_PIN_DRV_GRP(118, 0xd70, 0, 2),
+	MTK_PIN_DRV_GRP(119, 0xd70, 0, 2),
+	MTK_PIN_DRV_GRP(120, 0xd70, 0, 2),
+};
+
+static const struct mtk_pin_spec_pupd_set_samereg mt8516_spec_pupd[] = {
+	MTK_PIN_PUPD_SPEC_SR(14, 0xe50, 14, 13, 12),
+	MTK_PIN_PUPD_SPEC_SR(15, 0xe60, 2, 1, 0),
+	MTK_PIN_PUPD_SPEC_SR(16, 0xe60, 6, 5, 4),
+	MTK_PIN_PUPD_SPEC_SR(17, 0xe60, 10, 9, 8),
+
+	MTK_PIN_PUPD_SPEC_SR(21, 0xe60, 14, 13, 12),
+	MTK_PIN_PUPD_SPEC_SR(22, 0xe70, 2, 1, 0),
+	MTK_PIN_PUPD_SPEC_SR(23, 0xe70, 6, 5, 4),
+
+	MTK_PIN_PUPD_SPEC_SR(40, 0xe80, 2, 1, 0),
+	MTK_PIN_PUPD_SPEC_SR(41, 0xe80, 6, 5, 4),
+	MTK_PIN_PUPD_SPEC_SR(42, 0xe90, 2, 1, 0),
+	MTK_PIN_PUPD_SPEC_SR(43, 0xe90, 6, 5, 4),
+
+	MTK_PIN_PUPD_SPEC_SR(68, 0xe50, 10, 9, 8),
+	MTK_PIN_PUPD_SPEC_SR(69, 0xe50, 6, 5, 4),
+	MTK_PIN_PUPD_SPEC_SR(70, 0xe40, 6, 5, 4),
+	MTK_PIN_PUPD_SPEC_SR(71, 0xe40, 10, 9, 8),
+	MTK_PIN_PUPD_SPEC_SR(72, 0xe40, 14, 13, 12),
+	MTK_PIN_PUPD_SPEC_SR(73, 0xe50, 2, 1, 0),
+
+	MTK_PIN_PUPD_SPEC_SR(104, 0xe40, 2, 1, 0),
+	MTK_PIN_PUPD_SPEC_SR(105, 0xe30, 14, 13, 12),
+	MTK_PIN_PUPD_SPEC_SR(106, 0xe20, 14, 13, 12),
+	MTK_PIN_PUPD_SPEC_SR(107, 0xe30, 2, 1, 0),
+	MTK_PIN_PUPD_SPEC_SR(108, 0xe30, 6, 5, 4),
+	MTK_PIN_PUPD_SPEC_SR(109, 0xe30, 10, 9, 8),
+	MTK_PIN_PUPD_SPEC_SR(110, 0xe10, 14, 13, 12),
+	MTK_PIN_PUPD_SPEC_SR(111, 0xe10, 10, 9, 8),
+	MTK_PIN_PUPD_SPEC_SR(112, 0xe10, 6, 5, 4),
+	MTK_PIN_PUPD_SPEC_SR(113, 0xe10, 2, 1, 0),
+	MTK_PIN_PUPD_SPEC_SR(114, 0xe20, 10, 9, 8),
+	MTK_PIN_PUPD_SPEC_SR(115, 0xe20, 2, 1, 0),
+	MTK_PIN_PUPD_SPEC_SR(116, 0xe20, 6, 5, 4),
+	MTK_PIN_PUPD_SPEC_SR(117, 0xe00, 14, 13, 12),
+	MTK_PIN_PUPD_SPEC_SR(118, 0xe00, 10, 9, 8),
+	MTK_PIN_PUPD_SPEC_SR(119, 0xe00, 6, 5, 4),
+	MTK_PIN_PUPD_SPEC_SR(120, 0xe00, 2, 1, 0),
+};
+
+static int mt8516_spec_pull_set(struct regmap *regmap, unsigned int pin,
+			unsigned char align, bool isup, unsigned int r1r0)
+{
+	return mtk_pctrl_spec_pull_set_samereg(regmap, mt8516_spec_pupd,
+		ARRAY_SIZE(mt8516_spec_pupd), pin, align, isup, r1r0);
+}
+
+static const struct mtk_pin_ies_smt_set mt8516_ies_set[] = {
+	MTK_PIN_IES_SMT_SPEC(0, 6, 0x900, 2),
+	MTK_PIN_IES_SMT_SPEC(7, 10, 0x900, 3),
+	MTK_PIN_IES_SMT_SPEC(11, 13, 0x900, 12),
+	MTK_PIN_IES_SMT_SPEC(14, 17, 0x900, 13),
+	MTK_PIN_IES_SMT_SPEC(18, 20, 0x910, 10),
+	MTK_PIN_IES_SMT_SPEC(21, 23, 0x900, 13),
+	MTK_PIN_IES_SMT_SPEC(24, 25, 0x900, 12),
+	MTK_PIN_IES_SMT_SPEC(26, 30, 0x900, 0),
+	MTK_PIN_IES_SMT_SPEC(31, 33, 0x900, 1),
+	MTK_PIN_IES_SMT_SPEC(34, 39, 0x900, 2),
+	MTK_PIN_IES_SMT_SPEC(40, 40, 0x910, 11),
+	MTK_PIN_IES_SMT_SPEC(41, 43, 0x900, 10),
+	MTK_PIN_IES_SMT_SPEC(44, 47, 0x900, 11),
+	MTK_PIN_IES_SMT_SPEC(48, 51, 0x900, 14),
+	MTK_PIN_IES_SMT_SPEC(52, 53, 0x910, 0),
+	MTK_PIN_IES_SMT_SPEC(54, 54, 0x910, 2),
+	MTK_PIN_IES_SMT_SPEC(55, 57, 0x910, 4),
+	MTK_PIN_IES_SMT_SPEC(58, 59, 0x900, 15),
+	MTK_PIN_IES_SMT_SPEC(60, 61, 0x910, 1),
+	MTK_PIN_IES_SMT_SPEC(62, 65, 0x910, 5),
+	MTK_PIN_IES_SMT_SPEC(66, 67, 0x910, 6),
+	MTK_PIN_IES_SMT_SPEC(68, 68, 0x930, 2),
+	MTK_PIN_IES_SMT_SPEC(69, 69, 0x930, 1),
+	MTK_PIN_IES_SMT_SPEC(70, 70, 0x930, 6),
+	MTK_PIN_IES_SMT_SPEC(71, 71, 0x930, 5),
+	MTK_PIN_IES_SMT_SPEC(72, 72, 0x930, 4),
+	MTK_PIN_IES_SMT_SPEC(73, 73, 0x930, 3),
+	MTK_PIN_IES_SMT_SPEC(100, 103, 0x910, 7),
+	MTK_PIN_IES_SMT_SPEC(104, 104, 0x920, 12),
+	MTK_PIN_IES_SMT_SPEC(105, 105, 0x920, 11),
+	MTK_PIN_IES_SMT_SPEC(106, 106, 0x930, 0),
+	MTK_PIN_IES_SMT_SPEC(107, 107, 0x920, 15),
+	MTK_PIN_IES_SMT_SPEC(108, 108, 0x920, 14),
+	MTK_PIN_IES_SMT_SPEC(109, 109, 0x920, 13),
+	MTK_PIN_IES_SMT_SPEC(110, 110, 0x920, 9),
+	MTK_PIN_IES_SMT_SPEC(111, 111, 0x920, 8),
+	MTK_PIN_IES_SMT_SPEC(112, 112, 0x920, 7),
+	MTK_PIN_IES_SMT_SPEC(113, 113, 0x920, 6),
+	MTK_PIN_IES_SMT_SPEC(114, 114, 0x920, 10),
+	MTK_PIN_IES_SMT_SPEC(115, 115, 0x920, 1),
+	MTK_PIN_IES_SMT_SPEC(116, 116, 0x920, 0),
+	MTK_PIN_IES_SMT_SPEC(117, 117, 0x920, 5),
+	MTK_PIN_IES_SMT_SPEC(118, 118, 0x920, 4),
+	MTK_PIN_IES_SMT_SPEC(119, 119, 0x920, 3),
+	MTK_PIN_IES_SMT_SPEC(120, 120, 0x920, 2),
+	MTK_PIN_IES_SMT_SPEC(121, 124, 0x910, 9),
+};
+
+static const struct mtk_pin_ies_smt_set mt8516_smt_set[] = {
+	MTK_PIN_IES_SMT_SPEC(0, 6, 0xA00, 2),
+	MTK_PIN_IES_SMT_SPEC(7, 10, 0xA00, 3),
+	MTK_PIN_IES_SMT_SPEC(11, 13, 0xA00, 12),
+	MTK_PIN_IES_SMT_SPEC(14, 17, 0xA00, 13),
+	MTK_PIN_IES_SMT_SPEC(18, 20, 0xA10, 10),
+	MTK_PIN_IES_SMT_SPEC(21, 23, 0xA00, 13),
+	MTK_PIN_IES_SMT_SPEC(24, 25, 0xA00, 12),
+	MTK_PIN_IES_SMT_SPEC(26, 30, 0xA00, 0),
+	MTK_PIN_IES_SMT_SPEC(31, 33, 0xA00, 1),
+	MTK_PIN_IES_SMT_SPEC(34, 39, 0xA900, 2),
+	MTK_PIN_IES_SMT_SPEC(40, 40, 0xA10, 11),
+	MTK_PIN_IES_SMT_SPEC(41, 43, 0xA00, 10),
+	MTK_PIN_IES_SMT_SPEC(44, 47, 0xA00, 11),
+	MTK_PIN_IES_SMT_SPEC(48, 51, 0xA00, 14),
+	MTK_PIN_IES_SMT_SPEC(52, 53, 0xA10, 0),
+	MTK_PIN_IES_SMT_SPEC(54, 54, 0xA10, 2),
+	MTK_PIN_IES_SMT_SPEC(55, 57, 0xA10, 4),
+	MTK_PIN_IES_SMT_SPEC(58, 59, 0xA00, 15),
+	MTK_PIN_IES_SMT_SPEC(60, 61, 0xA10, 1),
+	MTK_PIN_IES_SMT_SPEC(62, 65, 0xA10, 5),
+	MTK_PIN_IES_SMT_SPEC(66, 67, 0xA10, 6),
+	MTK_PIN_IES_SMT_SPEC(68, 68, 0xA30, 2),
+	MTK_PIN_IES_SMT_SPEC(69, 69, 0xA30, 1),
+	MTK_PIN_IES_SMT_SPEC(70, 70, 0xA30, 3),
+	MTK_PIN_IES_SMT_SPEC(71, 71, 0xA30, 4),
+	MTK_PIN_IES_SMT_SPEC(72, 72, 0xA30, 5),
+	MTK_PIN_IES_SMT_SPEC(73, 73, 0xA30, 6),
+
+	MTK_PIN_IES_SMT_SPEC(100, 103, 0xA10, 7),
+	MTK_PIN_IES_SMT_SPEC(104, 104, 0xA20, 12),
+	MTK_PIN_IES_SMT_SPEC(105, 105, 0xA20, 11),
+	MTK_PIN_IES_SMT_SPEC(106, 106, 0xA30, 13),
+	MTK_PIN_IES_SMT_SPEC(107, 107, 0xA20, 14),
+	MTK_PIN_IES_SMT_SPEC(108, 108, 0xA20, 15),
+	MTK_PIN_IES_SMT_SPEC(109, 109, 0xA30, 0),
+	MTK_PIN_IES_SMT_SPEC(110, 110, 0xA20, 9),
+	MTK_PIN_IES_SMT_SPEC(111, 111, 0xA20, 8),
+	MTK_PIN_IES_SMT_SPEC(112, 112, 0xA20, 7),
+	MTK_PIN_IES_SMT_SPEC(113, 113, 0xA20, 6),
+	MTK_PIN_IES_SMT_SPEC(114, 114, 0xA20, 10),
+	MTK_PIN_IES_SMT_SPEC(115, 115, 0xA20, 1),
+	MTK_PIN_IES_SMT_SPEC(116, 116, 0xA20, 0),
+	MTK_PIN_IES_SMT_SPEC(117, 117, 0xA20, 5),
+	MTK_PIN_IES_SMT_SPEC(118, 118, 0xA20, 4),
+	MTK_PIN_IES_SMT_SPEC(119, 119, 0xA20, 3),
+	MTK_PIN_IES_SMT_SPEC(120, 120, 0xA20, 2),
+	MTK_PIN_IES_SMT_SPEC(121, 124, 0xA10, 9),
+};
+
+static int mt8516_ies_smt_set(struct regmap *regmap, unsigned int pin,
+		unsigned char align, int value, enum pin_config_param arg)
+{
+	if (arg == PIN_CONFIG_INPUT_ENABLE)
+		return mtk_pconf_spec_set_ies_smt_range(regmap, mt8516_ies_set,
+			ARRAY_SIZE(mt8516_ies_set), pin, align, value);
+	else if (arg == PIN_CONFIG_INPUT_SCHMITT_ENABLE)
+		return mtk_pconf_spec_set_ies_smt_range(regmap, mt8516_smt_set,
+			ARRAY_SIZE(mt8516_smt_set), pin, align, value);
+	return -EINVAL;
+}
+
+static const struct mtk_pinctrl_devdata mt8516_pinctrl_data = {
+	.pins = mtk_pins_mt8516,
+	.npins = ARRAY_SIZE(mtk_pins_mt8516),
+	.grp_desc = mt8516_drv_grp,
+	.n_grp_cls = ARRAY_SIZE(mt8516_drv_grp),
+	.pin_drv_grp = mt8516_pin_drv,
+	.n_pin_drv_grps = ARRAY_SIZE(mt8516_pin_drv),
+	.spec_pull_set = mt8516_spec_pull_set,
+	.spec_ies_smt_set = mt8516_ies_smt_set,
+	.dir_offset = 0x0000,
+	.pullen_offset = 0x0500,
+	.pullsel_offset = 0x0600,
+	.dout_offset = 0x0100,
+	.din_offset = 0x0200,
+	.pinmux_offset = 0x0300,
+	.type1_start = 125,
+	.type1_end = 125,
+	.port_shf = 4,
+	.port_mask = 0xf,
+	.port_align = 4,
+	.eint_hw = {
+		.port_mask = 7,
+		.ports     = 6,
+		.ap_num    = 169,
+		.db_cnt    = 64,
+	},
+};
+
+static int mt8516_pinctrl_probe(struct platform_device *pdev)
+{
+	return mtk_pctrl_init(pdev, &mt8516_pinctrl_data, NULL);
+}
+
+static const struct of_device_id mt8516_pctrl_match[] = {
+	{
+		.compatible = "mediatek,mt8516-pinctrl",
+	},
+	{}
+};
+
+MODULE_DEVICE_TABLE(of, mt8516_pctrl_match);
+
+static struct platform_driver mtk_pinctrl_driver = {
+	.probe = mt8516_pinctrl_probe,
+	.driver = {
+		.name = "mediatek-mt8516-pinctrl",
+		.of_match_table = mt8516_pctrl_match,
+		.pm = &mtk_eint_pm_ops,
+	},
+};
+
+static int __init mtk_pinctrl_init(void)
+{
+	return platform_driver_register(&mtk_pinctrl_driver);
+}
+arch_initcall(mtk_pinctrl_init);
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mtk-common-v2.c
@@ -0,0 +1,725 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: Sean Wang <sean.wang@mediatek.com>
+ *
+ */
+
+#include <linux/device.h>
+#include <linux/err.h>
+#include <linux/gpio/driver.h>
+#include <linux/platform_device.h>
+#include <linux/io.h>
+#include <linux/of_irq.h>
+
+#include "mtk-eint.h"
+#include "pinctrl-mtk-common-v2.h"
+
+/**
+ * struct mtk_drive_desc - the structure that holds the information
+ *			    of the driving current
+ * @min:	the minimum current of this group
+ * @max:	the maximum current of this group
+ * @step:	the step current of this group
+ * @scal:	the weight factor
+ *
+ * formula: output = ((input) / step - 1) * scal
+ */
+struct mtk_drive_desc {
+	u8 min;
+	u8 max;
+	u8 step;
+	u8 scal;
+};
+
+/* The groups of drive strength */
+static const struct mtk_drive_desc mtk_drive[] = {
+	[DRV_GRP0] = { 4, 16, 4, 1 },
+	[DRV_GRP1] = { 4, 16, 4, 2 },
+	[DRV_GRP2] = { 2, 8, 2, 1 },
+	[DRV_GRP3] = { 2, 8, 2, 2 },
+	[DRV_GRP4] = { 2, 16, 2, 1 },
+};
+
+static void mtk_w32(struct mtk_pinctrl *pctl, u8 i, u32 reg, u32 val)
+{
+	writel_relaxed(val, pctl->base[i] + reg);
+}
+
+static u32 mtk_r32(struct mtk_pinctrl *pctl, u8 i, u32 reg)
+{
+	return readl_relaxed(pctl->base[i] + reg);
+}
+
+void mtk_rmw(struct mtk_pinctrl *pctl, u8 i, u32 reg, u32 mask, u32 set)
+{
+	u32 val;
+
+	val = mtk_r32(pctl, i, reg);
+	val &= ~mask;
+	val |= set;
+	mtk_w32(pctl, i, reg, val);
+}
+
+static int mtk_hw_pin_field_lookup(struct mtk_pinctrl *hw,
+				   const struct mtk_pin_desc *desc,
+				   int field, struct mtk_pin_field *pfd)
+{
+	const struct mtk_pin_field_calc *c, *e;
+	const struct mtk_pin_reg_calc *rc;
+	u32 bits;
+
+	if (hw->soc->reg_cal && hw->soc->reg_cal[field].range) {
+		rc = &hw->soc->reg_cal[field];
+	} else {
+		dev_dbg(hw->dev,
+			"Not support field %d for pin %d (%s)\n",
+			field, desc->number, desc->name);
+		return -ENOTSUPP;
+	}
+
+	c = rc->range;
+	e = c + rc->nranges;
+
+	while (c < e) {
+		if (desc->number >= c->s_pin && desc->number <= c->e_pin)
+			break;
+		c++;
+	}
+
+	if (c >= e) {
+		dev_dbg(hw->dev, "Not support field %d for pin = %d (%s)\n",
+			field, desc->number, desc->name);
+		return -ENOTSUPP;
+	}
+
+	if (c->i_base > hw->nbase - 1) {
+		dev_err(hw->dev,
+			"Invalid base for field %d for pin = %d (%s)\n",
+			field, desc->number, desc->name);
+		return -EINVAL;
+	}
+
+	/* Calculated bits as the overall offset the pin is located at,
+	 * if c->fixed is held, that determines the all the pins in the
+	 * range use the same field with the s_pin.
+	 */
+	bits = c->fixed ? c->s_bit : c->s_bit +
+	       (desc->number - c->s_pin) * (c->x_bits);
+
+	/* Fill pfd from bits. For example 32-bit register applied is assumed
+	 * when c->sz_reg is equal to 32.
+	 */
+	pfd->index = c->i_base;
+	pfd->offset = c->s_addr + c->x_addrs * (bits / c->sz_reg);
+	pfd->bitpos = bits % c->sz_reg;
+	pfd->mask = (1 << c->x_bits) - 1;
+
+	/* pfd->next is used for indicating that bit wrapping-around happens
+	 * which requires the manipulation for bit 0 starting in the next
+	 * register to form the complete field read/write.
+	 */
+	pfd->next = pfd->bitpos + c->x_bits > c->sz_reg ? c->x_addrs : 0;
+
+	return 0;
+}
+
+static int mtk_hw_pin_field_get(struct mtk_pinctrl *hw,
+				const struct mtk_pin_desc *desc,
+				int field, struct mtk_pin_field *pfd)
+{
+	if (field < 0 || field >= PINCTRL_PIN_REG_MAX) {
+		dev_err(hw->dev, "Invalid Field %d\n", field);
+		return -EINVAL;
+	}
+
+	return mtk_hw_pin_field_lookup(hw, desc, field, pfd);
+}
+
+static void mtk_hw_bits_part(struct mtk_pin_field *pf, int *h, int *l)
+{
+	*l = 32 - pf->bitpos;
+	*h = get_count_order(pf->mask) - *l;
+}
+
+static void mtk_hw_write_cross_field(struct mtk_pinctrl *hw,
+				     struct mtk_pin_field *pf, int value)
+{
+	int nbits_l, nbits_h;
+
+	mtk_hw_bits_part(pf, &nbits_h, &nbits_l);
+
+	mtk_rmw(hw, pf->index, pf->offset, pf->mask << pf->bitpos,
+		(value & pf->mask) << pf->bitpos);
+
+	mtk_rmw(hw, pf->index, pf->offset + pf->next, BIT(nbits_h) - 1,
+		(value & pf->mask) >> nbits_l);
+}
+
+static void mtk_hw_read_cross_field(struct mtk_pinctrl *hw,
+				    struct mtk_pin_field *pf, int *value)
+{
+	int nbits_l, nbits_h, h, l;
+
+	mtk_hw_bits_part(pf, &nbits_h, &nbits_l);
+
+	l  = (mtk_r32(hw, pf->index, pf->offset)
+	      >> pf->bitpos) & (BIT(nbits_l) - 1);
+	h  = (mtk_r32(hw, pf->index, pf->offset + pf->next))
+	      & (BIT(nbits_h) - 1);
+
+	*value = (h << nbits_l) | l;
+}
+
+int mtk_hw_set_value(struct mtk_pinctrl *hw, const struct mtk_pin_desc *desc,
+		     int field, int value)
+{
+	struct mtk_pin_field pf;
+	int err;
+
+	err = mtk_hw_pin_field_get(hw, desc, field, &pf);
+	if (err)
+		return err;
+
+	if (!pf.next)
+		mtk_rmw(hw, pf.index, pf.offset, pf.mask << pf.bitpos,
+			(value & pf.mask) << pf.bitpos);
+	else
+		mtk_hw_write_cross_field(hw, &pf, value);
+
+	return 0;
+}
+
+int mtk_hw_get_value(struct mtk_pinctrl *hw, const struct mtk_pin_desc *desc,
+		     int field, int *value)
+{
+	struct mtk_pin_field pf;
+	int err;
+
+	err = mtk_hw_pin_field_get(hw, desc, field, &pf);
+	if (err)
+		return err;
+
+	if (!pf.next)
+		*value = (mtk_r32(hw, pf.index, pf.offset)
+			  >> pf.bitpos) & pf.mask;
+	else
+		mtk_hw_read_cross_field(hw, &pf, value);
+
+	return 0;
+}
+
+static int mtk_xt_find_eint_num(struct mtk_pinctrl *hw, unsigned long eint_n)
+{
+	const struct mtk_pin_desc *desc;
+	int i = 0;
+
+	desc = (const struct mtk_pin_desc *)hw->soc->pins;
+
+	while (i < hw->soc->npins) {
+		if (desc[i].eint.eint_n == eint_n)
+			return desc[i].number;
+		i++;
+	}
+
+	return EINT_NA;
+}
+
+static int mtk_xt_get_gpio_n(void *data, unsigned long eint_n,
+			     unsigned int *gpio_n,
+			     struct gpio_chip **gpio_chip)
+{
+	struct mtk_pinctrl *hw = (struct mtk_pinctrl *)data;
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)hw->soc->pins;
+	*gpio_chip = &hw->chip;
+
+	/* Be greedy to guess first gpio_n is equal to eint_n */
+	if (desc[eint_n].eint.eint_n == eint_n)
+		*gpio_n = eint_n;
+	else
+		*gpio_n = mtk_xt_find_eint_num(hw, eint_n);
+
+	return *gpio_n == EINT_NA ? -EINVAL : 0;
+}
+
+static int mtk_xt_get_gpio_state(void *data, unsigned long eint_n)
+{
+	struct mtk_pinctrl *hw = (struct mtk_pinctrl *)data;
+	const struct mtk_pin_desc *desc;
+	struct gpio_chip *gpio_chip;
+	unsigned int gpio_n;
+	int value, err;
+
+	err = mtk_xt_get_gpio_n(hw, eint_n, &gpio_n, &gpio_chip);
+	if (err)
+		return err;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[gpio_n];
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DI, &value);
+	if (err)
+		return err;
+
+	return !!value;
+}
+
+static int mtk_xt_set_gpio_as_eint(void *data, unsigned long eint_n)
+{
+	struct mtk_pinctrl *hw = (struct mtk_pinctrl *)data;
+	const struct mtk_pin_desc *desc;
+	struct gpio_chip *gpio_chip;
+	unsigned int gpio_n;
+	int err;
+
+	err = mtk_xt_get_gpio_n(hw, eint_n, &gpio_n, &gpio_chip);
+	if (err)
+		return err;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[gpio_n];
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_MODE,
+			       desc->eint.eint_m);
+	if (err)
+		return err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR, MTK_INPUT);
+	if (err)
+		return err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_SMT, MTK_ENABLE);
+	/* SMT is supposed to be supported by every real GPIO and doesn't
+	 * support virtual GPIOs, so the extra condition err != -ENOTSUPP
+	 * is just for adding EINT support to these virtual GPIOs. It should
+	 * add an extra flag in the pin descriptor when more pins with
+	 * distinctive characteristic come out.
+	 */
+	if (err && err != -ENOTSUPP)
+		return err;
+
+	return 0;
+}
+
+static const struct mtk_eint_xt mtk_eint_xt = {
+	.get_gpio_n = mtk_xt_get_gpio_n,
+	.get_gpio_state = mtk_xt_get_gpio_state,
+	.set_gpio_as_eint = mtk_xt_set_gpio_as_eint,
+};
+
+int mtk_build_eint(struct mtk_pinctrl *hw, struct platform_device *pdev)
+{
+	struct device_node *np = pdev->dev.of_node;
+	struct resource *res;
+
+	if (!IS_ENABLED(CONFIG_EINT_MTK))
+		return 0;
+
+	if (!of_property_read_bool(np, "interrupt-controller"))
+		return -ENODEV;
+
+	hw->eint = devm_kzalloc(hw->dev, sizeof(*hw->eint), GFP_KERNEL);
+	if (!hw->eint)
+		return -ENOMEM;
+
+	res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "eint");
+	if (!res) {
+		dev_err(&pdev->dev, "Unable to get eint resource\n");
+		return -ENODEV;
+	}
+
+	hw->eint->base = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(hw->eint->base))
+		return PTR_ERR(hw->eint->base);
+
+	hw->eint->irq = irq_of_parse_and_map(np, 0);
+	if (!hw->eint->irq)
+		return -EINVAL;
+
+	if (!hw->soc->eint_hw)
+		return -ENODEV;
+
+	hw->eint->dev = &pdev->dev;
+	hw->eint->hw = hw->soc->eint_hw;
+	hw->eint->pctl = hw;
+	hw->eint->gpio_xlate = &mtk_eint_xt;
+
+	return mtk_eint_do_init(hw->eint);
+}
+
+/* Revision 0 */
+int mtk_pinconf_bias_disable_set(struct mtk_pinctrl *hw,
+				 const struct mtk_pin_desc *desc)
+{
+	int err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_PU,
+			       MTK_DISABLE);
+	if (err)
+		return err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_PD,
+			       MTK_DISABLE);
+	if (err)
+		return err;
+
+	return 0;
+}
+
+int mtk_pinconf_bias_disable_get(struct mtk_pinctrl *hw,
+				 const struct mtk_pin_desc *desc, int *res)
+{
+	int v, v2;
+	int err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_PU, &v);
+	if (err)
+		return err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_PD, &v2);
+	if (err)
+		return err;
+
+	if (v == MTK_ENABLE || v2 == MTK_ENABLE)
+		return -EINVAL;
+
+	*res = 1;
+
+	return 0;
+}
+
+int mtk_pinconf_bias_set(struct mtk_pinctrl *hw,
+			 const struct mtk_pin_desc *desc, bool pullup)
+{
+	int err, arg;
+
+	arg = pullup ? 1 : 2;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_PU, arg & 1);
+	if (err)
+		return err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_PD,
+			       !!(arg & 2));
+	if (err)
+		return err;
+
+	return 0;
+}
+
+int mtk_pinconf_bias_get(struct mtk_pinctrl *hw,
+			 const struct mtk_pin_desc *desc, bool pullup, int *res)
+{
+	int reg, err, v;
+
+	reg = pullup ? PINCTRL_PIN_REG_PU : PINCTRL_PIN_REG_PD;
+
+	err = mtk_hw_get_value(hw, desc, reg, &v);
+	if (err)
+		return err;
+
+	if (!v)
+		return -EINVAL;
+
+	*res = 1;
+
+	return 0;
+}
+
+/* Revision 1 */
+int mtk_pinconf_bias_disable_set_rev1(struct mtk_pinctrl *hw,
+				      const struct mtk_pin_desc *desc)
+{
+	int err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_PULLEN,
+			       MTK_DISABLE);
+	if (err)
+		return err;
+
+	return 0;
+}
+
+int mtk_pinconf_bias_disable_get_rev1(struct mtk_pinctrl *hw,
+				      const struct mtk_pin_desc *desc, int *res)
+{
+	int v, err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_PULLEN, &v);
+	if (err)
+		return err;
+
+	if (v == MTK_ENABLE)
+		return -EINVAL;
+
+	*res = 1;
+
+	return 0;
+}
+
+int mtk_pinconf_bias_set_rev1(struct mtk_pinctrl *hw,
+			      const struct mtk_pin_desc *desc, bool pullup)
+{
+	int err, arg;
+
+	arg = pullup ? MTK_PULLUP : MTK_PULLDOWN;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_PULLEN,
+			       MTK_ENABLE);
+	if (err)
+		return err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_PULLSEL, arg);
+	if (err)
+		return err;
+
+	return 0;
+}
+
+int mtk_pinconf_bias_get_rev1(struct mtk_pinctrl *hw,
+			      const struct mtk_pin_desc *desc, bool pullup,
+			      int *res)
+{
+	int err, v;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_PULLEN, &v);
+	if (err)
+		return err;
+
+	if (v == MTK_DISABLE)
+		return -EINVAL;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_PULLSEL, &v);
+	if (err)
+		return err;
+
+	if (pullup ^ (v == MTK_PULLUP))
+		return -EINVAL;
+
+	*res = 1;
+
+	return 0;
+}
+
+/* Revision 0 */
+int mtk_pinconf_drive_set(struct mtk_pinctrl *hw,
+			  const struct mtk_pin_desc *desc, u32 arg)
+{
+	const struct mtk_drive_desc *tb;
+	int err = -ENOTSUPP;
+
+	tb = &mtk_drive[desc->drv_n];
+	/* 4mA when (e8, e4) = (0, 0)
+	 * 8mA when (e8, e4) = (0, 1)
+	 * 12mA when (e8, e4) = (1, 0)
+	 * 16mA when (e8, e4) = (1, 1)
+	 */
+	if ((arg >= tb->min && arg <= tb->max) && !(arg % tb->step)) {
+		arg = (arg / tb->step - 1) * tb->scal;
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_E4,
+				       arg & 0x1);
+		if (err)
+			return err;
+
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_E8,
+				       (arg & 0x2) >> 1);
+		if (err)
+			return err;
+	}
+
+	return err;
+}
+
+int mtk_pinconf_drive_get(struct mtk_pinctrl *hw,
+			  const struct mtk_pin_desc *desc, int *val)
+{
+	const struct mtk_drive_desc *tb;
+	int err, val1, val2;
+
+	tb = &mtk_drive[desc->drv_n];
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_E4, &val1);
+	if (err)
+		return err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_E8, &val2);
+	if (err)
+		return err;
+
+	/* 4mA when (e8, e4) = (0, 0); 8mA when (e8, e4) = (0, 1)
+	 * 12mA when (e8, e4) = (1, 0); 16mA when (e8, e4) = (1, 1)
+	 */
+	*val = (((val2 << 1) + val1) / tb->scal + 1) * tb->step;
+
+	return 0;
+}
+
+/* Revision 1 */
+int mtk_pinconf_drive_set_rev1(struct mtk_pinctrl *hw,
+			       const struct mtk_pin_desc *desc, u32 arg)
+{
+	const struct mtk_drive_desc *tb;
+	int err = -ENOTSUPP;
+
+	tb = &mtk_drive[desc->drv_n];
+
+	if ((arg >= tb->min && arg <= tb->max) && !(arg % tb->step)) {
+		arg = (arg / tb->step - 1) * tb->scal;
+
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DRV,
+				       arg);
+		if (err)
+			return err;
+	}
+
+	return err;
+}
+
+int mtk_pinconf_drive_get_rev1(struct mtk_pinctrl *hw,
+			       const struct mtk_pin_desc *desc, int *val)
+{
+	const struct mtk_drive_desc *tb;
+	int err, val1;
+
+	tb = &mtk_drive[desc->drv_n];
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DRV, &val1);
+	if (err)
+		return err;
+
+	*val = ((val1 & 0x7) / tb->scal + 1) * tb->step;
+
+	return 0;
+}
+
+int mtk_pinconf_adv_pull_set(struct mtk_pinctrl *hw,
+			     const struct mtk_pin_desc *desc, bool pullup,
+			     u32 arg)
+{
+	int err;
+
+	/* 10K off & 50K (75K) off, when (R0, R1) = (0, 0);
+	 * 10K off & 50K (75K) on, when (R0, R1) = (0, 1);
+	 * 10K on & 50K (75K) off, when (R0, R1) = (1, 0);
+	 * 10K on & 50K (75K) on, when (R0, R1) = (1, 1)
+	 */
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_R0, arg & 1);
+	if (err)
+		return 0;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_R1,
+			       !!(arg & 2));
+	if (err)
+		return 0;
+
+	arg = pullup ? 0 : 1;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_PUPD, arg);
+
+	/* If PUPD register is not supported for that pin, let's fallback to
+	 * general bias control.
+	 */
+	if (err == -ENOTSUPP) {
+		if (hw->soc->bias_set) {
+			err = hw->soc->bias_set(hw, desc, pullup);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+	}
+
+	return err;
+}
+
+int mtk_pinconf_adv_pull_get(struct mtk_pinctrl *hw,
+			     const struct mtk_pin_desc *desc, bool pullup,
+			     u32 *val)
+{
+	u32 t, t2;
+	int err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_PUPD, &t);
+
+	/* If PUPD register is not supported for that pin, let's fallback to
+	 * general bias control.
+	 */
+	if (err == -ENOTSUPP) {
+		if (hw->soc->bias_get) {
+			err = hw->soc->bias_get(hw, desc, pullup, val);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+	} else {
+		/* t == 0 supposes PULLUP for the customized PULL setup */
+		if (err)
+			return err;
+
+		if (pullup ^ !t)
+			return -EINVAL;
+	}
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_R0, &t);
+	if (err)
+		return err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_R1, &t2);
+	if (err)
+		return err;
+
+	*val = (t | t2 << 1) & 0x7;
+
+	return 0;
+}
+
+int mtk_pinconf_adv_drive_set(struct mtk_pinctrl *hw,
+			      const struct mtk_pin_desc *desc, u32 arg)
+{
+	int err;
+	int en = arg & 1;
+	int e0 = !!(arg & 2);
+	int e1 = !!(arg & 4);
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DRV_EN, en);
+	if (err)
+		return err;
+
+	if (!en)
+		return err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DRV_E0, e0);
+	if (err)
+		return err;
+
+	err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DRV_E1, e1);
+	if (err)
+		return err;
+
+	return err;
+}
+
+int mtk_pinconf_adv_drive_get(struct mtk_pinctrl *hw,
+			      const struct mtk_pin_desc *desc, u32 *val)
+{
+	u32 en, e0, e1;
+	int err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DRV_EN, &en);
+	if (err)
+		return err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DRV_E0, &e0);
+	if (err)
+		return err;
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DRV_E1, &e1);
+	if (err)
+		return err;
+
+	*val = (en | e0 << 1 | e1 << 2) & 0x7;
+
+	return 0;
+}
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mtk-common-v2.h
@@ -0,0 +1,302 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: Sean Wang <sean.wang@mediatek.com>
+ *
+ */
+
+#ifndef __PINCTRL_MTK_COMMON_V2_H
+#define __PINCTRL_MTK_COMMON_V2_H
+
+#include <linux/gpio/driver.h>
+
+#define MTK_INPUT      0
+#define MTK_OUTPUT     1
+#define MTK_DISABLE    0
+#define MTK_ENABLE     1
+#define MTK_PULLDOWN   0
+#define MTK_PULLUP     1
+
+#define EINT_NA	U16_MAX
+#define NO_EINT_SUPPORT	EINT_NA
+
+#define PIN_FIELD_CALC(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs,      \
+		       _s_bit, _x_bits, _sz_reg, _fixed) {		\
+		.s_pin = _s_pin,					\
+		.e_pin = _e_pin,					\
+		.i_base = _i_base,					\
+		.s_addr = _s_addr,					\
+		.x_addrs = _x_addrs,					\
+		.s_bit = _s_bit,					\
+		.x_bits = _x_bits,					\
+		.sz_reg = _sz_reg,					\
+		.fixed = _fixed,					\
+	}
+
+#define PIN_FIELD(_s_pin, _e_pin, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, 0, _s_addr, _x_addrs, _s_bit,	\
+		       _x_bits, 32, 0)
+
+#define PINS_FIELD(_s_pin, _e_pin, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_CALC(_s_pin, _e_pin, 0, _s_addr, _x_addrs, _s_bit,	\
+		       _x_bits, 32, 1)
+
+/* List these attributes which could be modified for the pin */
+enum {
+	PINCTRL_PIN_REG_MODE,
+	PINCTRL_PIN_REG_DIR,
+	PINCTRL_PIN_REG_DI,
+	PINCTRL_PIN_REG_DO,
+	PINCTRL_PIN_REG_SR,
+	PINCTRL_PIN_REG_SMT,
+	PINCTRL_PIN_REG_PD,
+	PINCTRL_PIN_REG_PU,
+	PINCTRL_PIN_REG_E4,
+	PINCTRL_PIN_REG_E8,
+	PINCTRL_PIN_REG_TDSEL,
+	PINCTRL_PIN_REG_RDSEL,
+	PINCTRL_PIN_REG_DRV,
+	PINCTRL_PIN_REG_PUPD,
+	PINCTRL_PIN_REG_R0,
+	PINCTRL_PIN_REG_R1,
+	PINCTRL_PIN_REG_IES,
+	PINCTRL_PIN_REG_PULLEN,
+	PINCTRL_PIN_REG_PULLSEL,
+	PINCTRL_PIN_REG_DRV_EN,
+	PINCTRL_PIN_REG_DRV_E0,
+	PINCTRL_PIN_REG_DRV_E1,
+	PINCTRL_PIN_REG_MAX,
+};
+
+/* Group the pins by the driving current */
+enum {
+	DRV_FIXED,
+	DRV_GRP0,
+	DRV_GRP1,
+	DRV_GRP2,
+	DRV_GRP3,
+	DRV_GRP4,
+	DRV_GRP_MAX,
+};
+
+static const char * const mtk_default_register_base_names[] = {
+	"base",
+};
+
+/* struct mtk_pin_field - the structure that holds the information of the field
+ *			  used to describe the attribute for the pin
+ * @base:		the index pointing to the entry in base address list
+ * @offset:		the register offset relative to the base address
+ * @mask:		the mask used to filter out the field from the register
+ * @bitpos:		the start bit relative to the register
+ * @next:		the indication that the field would be extended to the
+			next register
+ */
+struct mtk_pin_field {
+	u8  index;
+	u32 offset;
+	u32 mask;
+	u8  bitpos;
+	u8  next;
+};
+
+/* struct mtk_pin_field_calc - the structure that holds the range providing
+ *			       the guide used to look up the relevant field
+ * @s_pin:		the start pin within the range
+ * @e_pin:		the end pin within the range
+ * @i_base:		the index pointing to the entry in base address list
+ * @s_addr:		the start address for the range
+ * @x_addrs:		the address distance between two consecutive registers
+ *			within the range
+ * @s_bit:		the start bit for the first register within the range
+ * @x_bits:		the bit distance between two consecutive pins within
+ *			the range
+ * @sz_reg:		the size of bits in a register
+ * @fixed:		the consecutive pins share the same bits with the 1st
+ *			pin
+ */
+struct mtk_pin_field_calc {
+	u16 s_pin;
+	u16 e_pin;
+	u8  i_base;
+	u32 s_addr;
+	u8  x_addrs;
+	u8  s_bit;
+	u8  x_bits;
+	u8  sz_reg;
+	u8  fixed;
+};
+
+/* struct mtk_pin_reg_calc - the structure that holds all ranges used to
+ *			     determine which register the pin would make use of
+ *			     for certain pin attribute.
+ * @range:		     the start address for the range
+ * @nranges:		     the number of items in the range
+ */
+struct mtk_pin_reg_calc {
+	const struct mtk_pin_field_calc *range;
+	unsigned int nranges;
+};
+
+/**
+ * struct mtk_func_desc - the structure that providing information
+ *			  all the funcs for this pin
+ * @name:		the name of function
+ * @muxval:		the mux to the function
+ */
+struct mtk_func_desc {
+	const char *name;
+	u8 muxval;
+};
+
+/**
+ * struct mtk_eint_desc - the structure that providing information
+ *			       for eint data per pin
+ * @eint_m:		the eint mux for this pin
+ * @eitn_n:		the eint number for this pin
+ */
+struct mtk_eint_desc {
+	u16 eint_m;
+	u16 eint_n;
+};
+
+/**
+ * struct mtk_pin_desc - the structure that providing information
+ *			       for each pin of chips
+ * @number:		unique pin number from the global pin number space
+ * @name:		name for this pin
+ * @eint:		the eint data for this pin
+ * @drv_n:		the index with the driving group
+ * @funcs:		all available functions for this pins (only used in
+ *			those drivers compatible to pinctrl-mtk-common.c-like
+ *			ones)
+ */
+struct mtk_pin_desc {
+	unsigned int number;
+	const char *name;
+	struct mtk_eint_desc eint;
+	u8 drv_n;
+	struct mtk_func_desc *funcs;
+};
+
+struct mtk_pinctrl_group {
+	const char	*name;
+	unsigned long	config;
+	unsigned	pin;
+};
+
+struct mtk_pinctrl;
+
+/* struct mtk_pin_soc - the structure that holds SoC-specific data */
+struct mtk_pin_soc {
+	const struct mtk_pin_reg_calc	*reg_cal;
+	const struct mtk_pin_desc	*pins;
+	unsigned int			npins;
+	const struct group_desc		*grps;
+	unsigned int			ngrps;
+	const struct function_desc	*funcs;
+	unsigned int			nfuncs;
+	const struct mtk_eint_regs	*eint_regs;
+	const struct mtk_eint_hw	*eint_hw;
+
+	/* Specific parameters per SoC */
+	u8				gpio_m;
+	bool				ies_present;
+	const char * const		*base_names;
+	unsigned int			nbase_names;
+
+	/* Specific pinconfig operations */
+	int (*bias_disable_set)(struct mtk_pinctrl *hw,
+				const struct mtk_pin_desc *desc);
+	int (*bias_disable_get)(struct mtk_pinctrl *hw,
+				const struct mtk_pin_desc *desc, int *res);
+	int (*bias_set)(struct mtk_pinctrl *hw,
+			const struct mtk_pin_desc *desc, bool pullup);
+	int (*bias_get)(struct mtk_pinctrl *hw,
+			const struct mtk_pin_desc *desc, bool pullup, int *res);
+
+	int (*drive_set)(struct mtk_pinctrl *hw,
+			 const struct mtk_pin_desc *desc, u32 arg);
+	int (*drive_get)(struct mtk_pinctrl *hw,
+			 const struct mtk_pin_desc *desc, int *val);
+
+	int (*adv_pull_set)(struct mtk_pinctrl *hw,
+			    const struct mtk_pin_desc *desc, bool pullup,
+			    u32 arg);
+	int (*adv_pull_get)(struct mtk_pinctrl *hw,
+			    const struct mtk_pin_desc *desc, bool pullup,
+			    u32 *val);
+	int (*adv_drive_set)(struct mtk_pinctrl *hw,
+			     const struct mtk_pin_desc *desc, u32 arg);
+	int (*adv_drive_get)(struct mtk_pinctrl *hw,
+			     const struct mtk_pin_desc *desc, u32 *val);
+
+	/* Specific driver data */
+	void				*driver_data;
+};
+
+struct mtk_pinctrl {
+	struct pinctrl_dev		*pctrl;
+	void __iomem			**base;
+	u8				nbase;
+	struct device			*dev;
+	struct gpio_chip		chip;
+	const struct mtk_pin_soc        *soc;
+	struct mtk_eint			*eint;
+	struct mtk_pinctrl_group	*groups;
+	const char          **grp_names;
+};
+
+void mtk_rmw(struct mtk_pinctrl *pctl, u8 i, u32 reg, u32 mask, u32 set);
+
+int mtk_hw_set_value(struct mtk_pinctrl *hw, const struct mtk_pin_desc *desc,
+		     int field, int value);
+int mtk_hw_get_value(struct mtk_pinctrl *hw, const struct mtk_pin_desc *desc,
+		     int field, int *value);
+
+int mtk_build_eint(struct mtk_pinctrl *hw, struct platform_device *pdev);
+
+int mtk_pinconf_bias_disable_set(struct mtk_pinctrl *hw,
+				 const struct mtk_pin_desc *desc);
+int mtk_pinconf_bias_disable_get(struct mtk_pinctrl *hw,
+				 const struct mtk_pin_desc *desc, int *res);
+int mtk_pinconf_bias_set(struct mtk_pinctrl *hw,
+			 const struct mtk_pin_desc *desc, bool pullup);
+int mtk_pinconf_bias_get(struct mtk_pinctrl *hw,
+			 const struct mtk_pin_desc *desc, bool pullup,
+			 int *res);
+
+int mtk_pinconf_bias_disable_set_rev1(struct mtk_pinctrl *hw,
+				      const struct mtk_pin_desc *desc);
+int mtk_pinconf_bias_disable_get_rev1(struct mtk_pinctrl *hw,
+				      const struct mtk_pin_desc *desc,
+				      int *res);
+int mtk_pinconf_bias_set_rev1(struct mtk_pinctrl *hw,
+			      const struct mtk_pin_desc *desc, bool pullup);
+int mtk_pinconf_bias_get_rev1(struct mtk_pinctrl *hw,
+			      const struct mtk_pin_desc *desc, bool pullup,
+			      int *res);
+
+int mtk_pinconf_drive_set(struct mtk_pinctrl *hw,
+			  const struct mtk_pin_desc *desc, u32 arg);
+int mtk_pinconf_drive_get(struct mtk_pinctrl *hw,
+			  const struct mtk_pin_desc *desc, int *val);
+
+int mtk_pinconf_drive_set_rev1(struct mtk_pinctrl *hw,
+			       const struct mtk_pin_desc *desc, u32 arg);
+int mtk_pinconf_drive_get_rev1(struct mtk_pinctrl *hw,
+			       const struct mtk_pin_desc *desc, int *val);
+
+int mtk_pinconf_adv_pull_set(struct mtk_pinctrl *hw,
+			     const struct mtk_pin_desc *desc, bool pullup,
+			     u32 arg);
+int mtk_pinconf_adv_pull_get(struct mtk_pinctrl *hw,
+			     const struct mtk_pin_desc *desc, bool pullup,
+			     u32 *val);
+int mtk_pinconf_adv_drive_set(struct mtk_pinctrl *hw,
+			      const struct mtk_pin_desc *desc, u32 arg);
+int mtk_pinconf_adv_drive_get(struct mtk_pinctrl *hw,
+			      const struct mtk_pin_desc *desc, u32 *val);
+
+#endif /* __PINCTRL_MTK_COMMON_V2_H */
--- a/drivers/pinctrl/mediatek/pinctrl-mtk-common.c
+++ b/drivers/pinctrl/mediatek/pinctrl-mtk-common.c
@@ -514,8 +514,8 @@ static int mtk_pctrl_dt_subnode_to_map(s
 
 	pins = of_find_property(node, "pinmux", NULL);
 	if (!pins) {
-		dev_err(pctl->dev, "missing pins property in node %s .\n",
-				node->name);
+		dev_err(pctl->dev, "missing pins property in node %pOFn .\n",
+				node);
 		return -EINVAL;
 	}
 
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mtk-mt6765.h
@@ -0,0 +1,1754 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: ZH Chen <zh.chen@mediatek.com>
+ *
+ */
+
+#ifndef __PINCTRL_MTK_MT6765_H
+#define __PINCTRL_MTK_MT6765_H
+
+#include "pinctrl-paris.h"
+
+static struct mtk_pin_desc mtk_pins_mt6765[] = {
+	MTK_PIN(
+		0, "GPIO0",
+		MTK_EINT_FUNCTION(0, 0),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO0"),
+		MTK_FUNCTION(1, "UTXD1"),
+		MTK_FUNCTION(2, "CLKM0"),
+		MTK_FUNCTION(3, "MD_INT0"),
+		MTK_FUNCTION(4, "I2S0_MCK"),
+		MTK_FUNCTION(5, "MD_UTXD1"),
+		MTK_FUNCTION(6, "TP_GPIO0_AO"),
+		MTK_FUNCTION(7, "DBG_MON_B9")
+	),
+	MTK_PIN(
+		1, "GPIO1",
+		MTK_EINT_FUNCTION(0, 1),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO1"),
+		MTK_FUNCTION(1, "URXD1"),
+		MTK_FUNCTION(2, "CLKM1"),
+		MTK_FUNCTION(4, "I2S0_BCK"),
+		MTK_FUNCTION(5, "MD_URXD1"),
+		MTK_FUNCTION(6, "TP_GPIO1_AO"),
+		MTK_FUNCTION(7, "DBG_MON_B10")
+	),
+	MTK_PIN(
+		2, "GPIO2",
+		MTK_EINT_FUNCTION(0, 2),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO2"),
+		MTK_FUNCTION(1, "UCTS0"),
+		MTK_FUNCTION(2, "CLKM2"),
+		MTK_FUNCTION(3, "UTXD1"),
+		MTK_FUNCTION(4, "I2S0_LRCK"),
+		MTK_FUNCTION(5, "ANT_SEL6"),
+		MTK_FUNCTION(6, "TP_GPIO2_AO"),
+		MTK_FUNCTION(7, "DBG_MON_B11")
+	),
+	MTK_PIN(
+		3, "GPIO3",
+		MTK_EINT_FUNCTION(0, 3),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO3"),
+		MTK_FUNCTION(1, "URTS0"),
+		MTK_FUNCTION(2, "CLKM3"),
+		MTK_FUNCTION(3, "URXD1"),
+		MTK_FUNCTION(4, "I2S0_DI"),
+		MTK_FUNCTION(5, "ANT_SEL7"),
+		MTK_FUNCTION(6, "TP_GPIO3_AO"),
+		MTK_FUNCTION(7, "DBG_MON_B12")
+	),
+	MTK_PIN(
+		4, "GPIO4",
+		MTK_EINT_FUNCTION(0, 4),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO4"),
+		MTK_FUNCTION(1, "SPI1_B_MI"),
+		MTK_FUNCTION(2, "SCP_SPI1_MI"),
+		MTK_FUNCTION(3, "UCTS0"),
+		MTK_FUNCTION(4, "I2S3_MCK"),
+		MTK_FUNCTION(5, "SSPM_URXD_AO"),
+		MTK_FUNCTION(6, "TP_GPIO4_AO")
+	),
+	MTK_PIN(
+		5, "GPIO5",
+		MTK_EINT_FUNCTION(0, 5),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO5"),
+		MTK_FUNCTION(1, "SPI1_B_CSB"),
+		MTK_FUNCTION(2, "SCP_SPI1_CS"),
+		MTK_FUNCTION(3, "URTS0"),
+		MTK_FUNCTION(4, "I2S3_BCK"),
+		MTK_FUNCTION(5, "SSPM_UTXD_AO"),
+		MTK_FUNCTION(6, "TP_GPIO5_AO")
+	),
+	MTK_PIN(
+		6, "GPIO6",
+		MTK_EINT_FUNCTION(0, 6),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO6"),
+		MTK_FUNCTION(1, "SPI1_B_MO"),
+		MTK_FUNCTION(2, "SCP_SPI1_MO"),
+		MTK_FUNCTION(3, "PWM0"),
+		MTK_FUNCTION(4, "I2S3_LRCK"),
+		MTK_FUNCTION(5, "MD_UTXD0"),
+		MTK_FUNCTION(6, "TP_GPIO6_AO")
+	),
+	MTK_PIN(
+		7, "GPIO7",
+		MTK_EINT_FUNCTION(0, 7),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO7"),
+		MTK_FUNCTION(1, "SPI1_B_CLK"),
+		MTK_FUNCTION(2, "SCP_SPI1_CK"),
+		MTK_FUNCTION(3, "PWM1"),
+		MTK_FUNCTION(4, "I2S3_DO"),
+		MTK_FUNCTION(5, "MD_URXD0"),
+		MTK_FUNCTION(6, "TP_GPIO7_AO")
+	),
+	MTK_PIN(
+		8, "GPIO8",
+		MTK_EINT_FUNCTION(0, 8),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO8"),
+		MTK_FUNCTION(1, "UTXD1"),
+		MTK_FUNCTION(2, "SRCLKENAI0"),
+		MTK_FUNCTION(3, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(4, "ANT_SEL3"),
+		MTK_FUNCTION(5, "MFG_JTAG_TRSTN"),
+		MTK_FUNCTION(6, "I2S2_MCK"),
+		MTK_FUNCTION(7, "JTRSTN_SEL1")
+	),
+	MTK_PIN(
+		9, "GPIO9",
+		MTK_EINT_FUNCTION(0, 9),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO9"),
+		MTK_FUNCTION(1, "MD_INT0"),
+		MTK_FUNCTION(2, "CMMCLK2"),
+		MTK_FUNCTION(3, "CONN_MCU_TRST_B"),
+		MTK_FUNCTION(4, "IDDIG"),
+		MTK_FUNCTION(5, "SDA_6306"),
+		MTK_FUNCTION(6, "MCUPM_JTAG_TRSTN"),
+		MTK_FUNCTION(7, "DBG_MON_B22")
+	),
+	MTK_PIN(
+		10, "GPIO10",
+		MTK_EINT_FUNCTION(0, 10),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO10"),
+		MTK_FUNCTION(1, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(3, "CONN_MCU_DBGI_N"),
+		MTK_FUNCTION(4, "SRCLKENAI1"),
+		MTK_FUNCTION(5, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(6, "CMVREF1"),
+		MTK_FUNCTION(7, "DBG_MON_B23")
+	),
+	MTK_PIN(
+		11, "GPIO11",
+		MTK_EINT_FUNCTION(0, 11),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO11"),
+		MTK_FUNCTION(1, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(2, "CLKM3"),
+		MTK_FUNCTION(3, "ANT_SEL6"),
+		MTK_FUNCTION(4, "SRCLKENAI0"),
+		MTK_FUNCTION(5, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(6, "UCTS1"),
+		MTK_FUNCTION(7, "DBG_MON_B24")
+	),
+	MTK_PIN(
+		12, "GPIO12",
+		MTK_EINT_FUNCTION(0, 12),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO12"),
+		MTK_FUNCTION(1, "PWM0"),
+		MTK_FUNCTION(2, "SRCLKENAI1"),
+		MTK_FUNCTION(3, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(4, "MD_INT0"),
+		MTK_FUNCTION(5, "DVFSRC_EXT_REQ"),
+		MTK_FUNCTION(6, "URTS1")
+	),
+	MTK_PIN(
+		13, "GPIO13",
+		MTK_EINT_FUNCTION(0, 13),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO13"),
+		MTK_FUNCTION(1, "ANT_SEL0"),
+		MTK_FUNCTION(2, "SPI4_MI"),
+		MTK_FUNCTION(3, "SCP_SPI0_MI"),
+		MTK_FUNCTION(4, "MD_URXD0"),
+		MTK_FUNCTION(5, "CLKM0"),
+		MTK_FUNCTION(6, "I2S0_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A0")
+	),
+	MTK_PIN(
+		14, "GPIO14",
+		MTK_EINT_FUNCTION(0, 14),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO14"),
+		MTK_FUNCTION(1, "ANT_SEL1"),
+		MTK_FUNCTION(2, "SPI4_CSB"),
+		MTK_FUNCTION(3, "SCP_SPI0_CS"),
+		MTK_FUNCTION(4, "MD_UTXD0"),
+		MTK_FUNCTION(5, "CLKM1"),
+		MTK_FUNCTION(6, "I2S0_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A1")
+	),
+	MTK_PIN(
+		15, "GPIO15",
+		MTK_EINT_FUNCTION(0, 15),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO15"),
+		MTK_FUNCTION(1, "ANT_SEL2"),
+		MTK_FUNCTION(2, "SPI4_MO"),
+		MTK_FUNCTION(3, "SCP_SPI0_MO"),
+		MTK_FUNCTION(4, "MD_URXD1"),
+		MTK_FUNCTION(5, "CLKM2"),
+		MTK_FUNCTION(6, "I2S0_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A2")
+	),
+	MTK_PIN(
+		16, "GPIO16",
+		MTK_EINT_FUNCTION(0, 16),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO16"),
+		MTK_FUNCTION(1, "ANT_SEL3"),
+		MTK_FUNCTION(2, "SPI4_CLK"),
+		MTK_FUNCTION(3, "SCP_SPI0_CK"),
+		MTK_FUNCTION(4, "MD_UTXD1"),
+		MTK_FUNCTION(5, "CLKM3"),
+		MTK_FUNCTION(6, "I2S3_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A3")
+	),
+	MTK_PIN(
+		17, "GPIO17",
+		MTK_EINT_FUNCTION(0, 17),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO17"),
+		MTK_FUNCTION(1, "ANT_SEL4"),
+		MTK_FUNCTION(2, "SPI2_MO"),
+		MTK_FUNCTION(3, "SCP_SPI0_MO"),
+		MTK_FUNCTION(4, "PWM1"),
+		MTK_FUNCTION(5, "IDDIG"),
+		MTK_FUNCTION(6, "I2S0_DI"),
+		MTK_FUNCTION(7, "DBG_MON_A4")
+	),
+	MTK_PIN(
+		18, "GPIO18",
+		MTK_EINT_FUNCTION(0, 18),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO18"),
+		MTK_FUNCTION(1, "ANT_SEL5"),
+		MTK_FUNCTION(2, "SPI2_CLK"),
+		MTK_FUNCTION(3, "SCP_SPI0_CK"),
+		MTK_FUNCTION(4, "MD_INT0"),
+		MTK_FUNCTION(5, "USB_DRVVBUS"),
+		MTK_FUNCTION(6, "I2S3_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A5")
+	),
+	MTK_PIN(
+		19, "GPIO19",
+		MTK_EINT_FUNCTION(0, 19),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO19"),
+		MTK_FUNCTION(1, "ANT_SEL6"),
+		MTK_FUNCTION(2, "SPI2_MI"),
+		MTK_FUNCTION(3, "SCP_SPI0_MI"),
+		MTK_FUNCTION(4, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(6, "I2S3_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A6")
+	),
+	MTK_PIN(
+		20, "GPIO20",
+		MTK_EINT_FUNCTION(0, 20),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO20"),
+		MTK_FUNCTION(1, "ANT_SEL7"),
+		MTK_FUNCTION(2, "SPI2_CSB"),
+		MTK_FUNCTION(3, "SCP_SPI0_CS"),
+		MTK_FUNCTION(4, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(5, "CMMCLK3"),
+		MTK_FUNCTION(6, "I2S3_DO"),
+		MTK_FUNCTION(7, "DBG_MON_A7")
+	),
+	MTK_PIN(
+		21, "GPIO21",
+		MTK_EINT_FUNCTION(0, 21),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO21"),
+		MTK_FUNCTION(1, "SPI3_MI"),
+		MTK_FUNCTION(2, "SRCLKENAI1"),
+		MTK_FUNCTION(3, "DAP_MD32_SWD"),
+		MTK_FUNCTION(4, "CMVREF0"),
+		MTK_FUNCTION(5, "SCP_SPI0_MI"),
+		MTK_FUNCTION(6, "I2S2_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A8")
+	),
+	MTK_PIN(
+		22, "GPIO22",
+		MTK_EINT_FUNCTION(0, 22),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO22"),
+		MTK_FUNCTION(1, "SPI3_CSB"),
+		MTK_FUNCTION(2, "SRCLKENAI0"),
+		MTK_FUNCTION(3, "DAP_MD32_SWCK"),
+		MTK_FUNCTION(4, "CMVREF1"),
+		MTK_FUNCTION(5, "SCP_SPI0_CS"),
+		MTK_FUNCTION(6, "I2S2_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A9")
+	),
+	MTK_PIN(
+		23, "GPIO23",
+		MTK_EINT_FUNCTION(0, 23),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO23"),
+		MTK_FUNCTION(1, "SPI3_MO"),
+		MTK_FUNCTION(2, "PWM0"),
+		MTK_FUNCTION(3, "KPROW7"),
+		MTK_FUNCTION(4, "ANT_SEL3"),
+		MTK_FUNCTION(5, "SCP_SPI0_MO"),
+		MTK_FUNCTION(6, "I2S2_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A10")
+	),
+	MTK_PIN(
+		24, "GPIO24",
+		MTK_EINT_FUNCTION(0, 24),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO24"),
+		MTK_FUNCTION(1, "SPI3_CLK"),
+		MTK_FUNCTION(2, "UDI_TCK"),
+		MTK_FUNCTION(3, "IO_JTAG_TCK"),
+		MTK_FUNCTION(4, "SSPM_JTAG_TCK"),
+		MTK_FUNCTION(5, "SCP_SPI0_CK"),
+		MTK_FUNCTION(6, "I2S2_DI"),
+		MTK_FUNCTION(7, "DBG_MON_A11")
+	),
+	MTK_PIN(
+		25, "GPIO25",
+		MTK_EINT_FUNCTION(0, 25),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO25"),
+		MTK_FUNCTION(1, "SPI1_A_MI"),
+		MTK_FUNCTION(2, "UDI_TMS"),
+		MTK_FUNCTION(3, "IO_JTAG_TMS"),
+		MTK_FUNCTION(4, "SSPM_JTAG_TMS"),
+		MTK_FUNCTION(5, "KPROW3"),
+		MTK_FUNCTION(6, "I2S1_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A12")
+	),
+	MTK_PIN(
+		26, "GPIO26",
+		MTK_EINT_FUNCTION(0, 26),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO26"),
+		MTK_FUNCTION(1, "SPI1_A_CSB"),
+		MTK_FUNCTION(2, "UDI_TDI"),
+		MTK_FUNCTION(3, "IO_JTAG_TDI"),
+		MTK_FUNCTION(4, "SSPM_JTAG_TDI"),
+		MTK_FUNCTION(5, "KPROW4"),
+		MTK_FUNCTION(6, "I2S1_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A13")
+	),
+	MTK_PIN(
+		27, "GPIO27",
+		MTK_EINT_FUNCTION(0, 27),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO27"),
+		MTK_FUNCTION(1, "SPI1_A_MO"),
+		MTK_FUNCTION(2, "UDI_TDO"),
+		MTK_FUNCTION(3, "IO_JTAG_TDO"),
+		MTK_FUNCTION(4, "SSPM_JTAG_TDO"),
+		MTK_FUNCTION(5, "KPROW5"),
+		MTK_FUNCTION(6, "I2S1_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A14")
+	),
+	MTK_PIN(
+		28, "GPIO28",
+		MTK_EINT_FUNCTION(0, 28),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO28"),
+		MTK_FUNCTION(1, "SPI1_A_CLK"),
+		MTK_FUNCTION(2, "UDI_NTRST"),
+		MTK_FUNCTION(3, "IO_JTAG_TRSTN"),
+		MTK_FUNCTION(4, "SSPM_JTAG_TRSTN"),
+		MTK_FUNCTION(5, "KPROW6"),
+		MTK_FUNCTION(6, "I2S1_DO"),
+		MTK_FUNCTION(7, "DBG_MON_A15")
+	),
+	MTK_PIN(
+		29, "GPIO29",
+		MTK_EINT_FUNCTION(0, 29),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO29"),
+		MTK_FUNCTION(1, "MSDC1_CLK"),
+		MTK_FUNCTION(2, "IO_JTAG_TCK"),
+		MTK_FUNCTION(3, "UDI_TCK"),
+		MTK_FUNCTION(4, "CONN_DSP_JCK"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TCK"),
+		MTK_FUNCTION(6, "CONN_MCU_AICE_TCKC"),
+		MTK_FUNCTION(7, "DAP_MD32_SWCK")
+	),
+	MTK_PIN(
+		30, "GPIO30",
+		MTK_EINT_FUNCTION(0, 30),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO30"),
+		MTK_FUNCTION(1, "MSDC1_CMD"),
+		MTK_FUNCTION(2, "IO_JTAG_TMS"),
+		MTK_FUNCTION(3, "UDI_TMS"),
+		MTK_FUNCTION(4, "CONN_DSP_JMS"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TMS"),
+		MTK_FUNCTION(6, "CONN_MCU_AICE_TMSC"),
+		MTK_FUNCTION(7, "DAP_MD32_SWD")
+	),
+	MTK_PIN(
+		31, "GPIO31",
+		MTK_EINT_FUNCTION(0, 31),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO31"),
+		MTK_FUNCTION(1, "MSDC1_DAT3")
+	),
+	MTK_PIN(
+		32, "GPIO32",
+		MTK_EINT_FUNCTION(0, 32),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO32"),
+		MTK_FUNCTION(1, "MSDC1_DAT0"),
+		MTK_FUNCTION(2, "IO_JTAG_TDI"),
+		MTK_FUNCTION(3, "UDI_TDI"),
+		MTK_FUNCTION(4, "CONN_DSP_JDI"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TDI")
+	),
+	MTK_PIN(
+		33, "GPIO33",
+		MTK_EINT_FUNCTION(0, 33),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO33"),
+		MTK_FUNCTION(1, "MSDC1_DAT2"),
+		MTK_FUNCTION(2, "IO_JTAG_TRSTN"),
+		MTK_FUNCTION(3, "UDI_NTRST"),
+		MTK_FUNCTION(4, "CONN_DSP_JINTP"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TRSTN")
+	),
+	MTK_PIN(
+		34, "GPIO34",
+		MTK_EINT_FUNCTION(0, 34),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO34"),
+		MTK_FUNCTION(1, "MSDC1_DAT1"),
+		MTK_FUNCTION(2, "IO_JTAG_TDO"),
+		MTK_FUNCTION(3, "UDI_TDO"),
+		MTK_FUNCTION(4, "CONN_DSP_JDO"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TDO")
+	),
+	MTK_PIN(
+		35, "GPIO35",
+		MTK_EINT_FUNCTION(0, 35),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO35"),
+		MTK_FUNCTION(1, "MD1_SIM2_SIO"),
+		MTK_FUNCTION(2, "CCU_JTAG_TDO"),
+		MTK_FUNCTION(3, "MD1_SIM1_SIO"),
+		MTK_FUNCTION(5, "SCP_JTAG_TDO"),
+		MTK_FUNCTION(6, "CONN_DSP_JDO"),
+		MTK_FUNCTION(7, "DBG_MON_A16")
+	),
+	MTK_PIN(
+		36, "GPIO36",
+		MTK_EINT_FUNCTION(0, 36),
+		DRV_GRP0,
+		MTK_FUNCTION(0, "GPIO36"),
+		MTK_FUNCTION(1, "MD1_SIM2_SRST"),
+		MTK_FUNCTION(2, "CCU_JTAG_TMS"),
+		MTK_FUNCTION(3, "MD1_SIM1_SRST"),
+		MTK_FUNCTION(4, "CONN_MCU_AICE_TMSC"),
+		MTK_FUNCTION(5, "SCP_JTAG_TMS"),
+		MTK_FUNCTION(6, "CONN_DSP_JMS"),
+		MTK_FUNCTION(7, "DBG_MON_A17")
+	),
+	MTK_PIN(
+		37, "GPIO37",
+		MTK_EINT_FUNCTION(0, 37),
+		DRV_GRP0,
+		MTK_FUNCTION(0, "GPIO37"),
+		MTK_FUNCTION(1, "MD1_SIM2_SCLK"),
+		MTK_FUNCTION(2, "CCU_JTAG_TDI"),
+		MTK_FUNCTION(3, "MD1_SIM1_SCLK"),
+		MTK_FUNCTION(5, "SCP_JTAG_TDI"),
+		MTK_FUNCTION(6, "CONN_DSP_JDI"),
+		MTK_FUNCTION(7, "DBG_MON_A18")
+	),
+	MTK_PIN(
+		38, "GPIO38",
+		MTK_EINT_FUNCTION(0, 38),
+		DRV_GRP0,
+		MTK_FUNCTION(0, "GPIO38"),
+		MTK_FUNCTION(1, "MD1_SIM1_SCLK"),
+		MTK_FUNCTION(3, "MD1_SIM2_SCLK"),
+		MTK_FUNCTION(7, "DBG_MON_A19")
+	),
+	MTK_PIN(
+		39, "GPIO39",
+		MTK_EINT_FUNCTION(0, 39),
+		DRV_GRP0,
+		MTK_FUNCTION(0, "GPIO39"),
+		MTK_FUNCTION(1, "MD1_SIM1_SRST"),
+		MTK_FUNCTION(2, "CCU_JTAG_TCK"),
+		MTK_FUNCTION(3, "MD1_SIM2_SRST"),
+		MTK_FUNCTION(4, "CONN_MCU_AICE_TCKC"),
+		MTK_FUNCTION(5, "SCP_JTAG_TCK"),
+		MTK_FUNCTION(6, "CONN_DSP_JCK"),
+		MTK_FUNCTION(7, "DBG_MON_A20")
+	),
+	MTK_PIN(
+		40, "GPIO40",
+		MTK_EINT_FUNCTION(0, 40),
+		DRV_GRP0,
+		MTK_FUNCTION(0, "GPIO40"),
+		MTK_FUNCTION(1, "MD1_SIM1_SIO"),
+		MTK_FUNCTION(2, "CCU_JTAG_TRST"),
+		MTK_FUNCTION(3, "MD1_SIM2_SIO"),
+		MTK_FUNCTION(5, "SCP_JTAG_TRSTN"),
+		MTK_FUNCTION(6, "CONN_DSP_JINTP"),
+		MTK_FUNCTION(7, "DBG_MON_A21")
+	),
+	MTK_PIN(
+		41, "GPIO41",
+		MTK_EINT_FUNCTION(0, 41),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO41"),
+		MTK_FUNCTION(1, "IDDIG"),
+		MTK_FUNCTION(2, "URXD1"),
+		MTK_FUNCTION(3, "UCTS0"),
+		MTK_FUNCTION(4, "KPCOL2"),
+		MTK_FUNCTION(5, "SSPM_UTXD_AO"),
+		MTK_FUNCTION(6, "MD_INT0"),
+		MTK_FUNCTION(7, "DBG_MON_A22")
+	),
+	MTK_PIN(
+		42, "GPIO42",
+		MTK_EINT_FUNCTION(0, 42),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO42"),
+		MTK_FUNCTION(1, "USB_DRVVBUS"),
+		MTK_FUNCTION(2, "UTXD1"),
+		MTK_FUNCTION(3, "URTS0"),
+		MTK_FUNCTION(4, "KPROW2"),
+		MTK_FUNCTION(5, "SSPM_URXD_AO"),
+		MTK_FUNCTION(6, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(7, "DBG_MON_A23")
+	),
+	MTK_PIN(
+		43, "GPIO43",
+		MTK_EINT_FUNCTION(0, 43),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO43"),
+		MTK_FUNCTION(1, "DISP_PWM"),
+		MTK_FUNCTION(7, "DBG_MON_A24")
+	),
+	MTK_PIN(
+		44, "GPIO44",
+		MTK_EINT_FUNCTION(0, 44),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO44"),
+		MTK_FUNCTION(1, "DSI_TE"),
+		MTK_FUNCTION(7, "DBG_MON_A25")
+	),
+	MTK_PIN(
+		45, "GPIO45",
+		MTK_EINT_FUNCTION(0, 45),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO45"),
+		MTK_FUNCTION(1, "LCM_RST"),
+		MTK_FUNCTION(7, "DBG_MON_A26")
+	),
+	MTK_PIN(
+		46, "GPIO46",
+		MTK_EINT_FUNCTION(0, 46),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO46"),
+		MTK_FUNCTION(1, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(2, "UCTS0"),
+		MTK_FUNCTION(3, "UCTS1"),
+		MTK_FUNCTION(4, "IDDIG"),
+		MTK_FUNCTION(5, "SCL_6306"),
+		MTK_FUNCTION(6, "TP_UCTS1_AO"),
+		MTK_FUNCTION(7, "DBG_MON_A27")
+	),
+	MTK_PIN(
+		47, "GPIO47",
+		MTK_EINT_FUNCTION(0, 47),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO47"),
+		MTK_FUNCTION(1, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(2, "URTS0"),
+		MTK_FUNCTION(3, "URTS1"),
+		MTK_FUNCTION(4, "USB_DRVVBUS"),
+		MTK_FUNCTION(5, "SDA_6306"),
+		MTK_FUNCTION(6, "TP_URTS1_AO"),
+		MTK_FUNCTION(7, "DBG_MON_A28")
+	),
+	MTK_PIN(
+		48, "GPIO48",
+		MTK_EINT_FUNCTION(0, 48),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO48"),
+		MTK_FUNCTION(1, "SCL5"),
+		MTK_FUNCTION(7, "DBG_MON_A29")
+	),
+	MTK_PIN(
+		49, "GPIO49",
+		MTK_EINT_FUNCTION(0, 49),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO49"),
+		MTK_FUNCTION(1, "SDA5"),
+		MTK_FUNCTION(7, "DBG_MON_A30")
+	),
+	MTK_PIN(
+		50, "GPIO50",
+		MTK_EINT_FUNCTION(0, 50),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO50"),
+		MTK_FUNCTION(1, "SCL3"),
+		MTK_FUNCTION(2, "URXD1"),
+		MTK_FUNCTION(3, "MD_URXD1"),
+		MTK_FUNCTION(4, "SSPM_URXD_AO"),
+		MTK_FUNCTION(5, "IDDIG"),
+		MTK_FUNCTION(6, "TP_URXD1_AO"),
+		MTK_FUNCTION(7, "DBG_MON_A31")
+	),
+	MTK_PIN(
+		51, "GPIO51",
+		MTK_EINT_FUNCTION(0, 51),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO51"),
+		MTK_FUNCTION(1, "SDA3"),
+		MTK_FUNCTION(2, "UTXD1"),
+		MTK_FUNCTION(3, "MD_UTXD1"),
+		MTK_FUNCTION(4, "SSPM_UTXD_AO"),
+		MTK_FUNCTION(5, "USB_DRVVBUS"),
+		MTK_FUNCTION(6, "TP_UTXD1_AO"),
+		MTK_FUNCTION(7, "DBG_MON_A32")
+	),
+	MTK_PIN(
+		52, "GPIO52",
+		MTK_EINT_FUNCTION(0, 52),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO52"),
+		MTK_FUNCTION(1, "BPI_BUS15")
+	),
+	MTK_PIN(
+		53, "GPIO53",
+		MTK_EINT_FUNCTION(0, 53),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO53"),
+		MTK_FUNCTION(1, "BPI_BUS13")
+	),
+	MTK_PIN(
+		54, "GPIO54",
+		MTK_EINT_FUNCTION(0, 54),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO54"),
+		MTK_FUNCTION(1, "BPI_BUS12")
+	),
+	MTK_PIN(
+		55, "GPIO55",
+		MTK_EINT_FUNCTION(0, 55),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO55"),
+		MTK_FUNCTION(1, "BPI_BUS8")
+	),
+	MTK_PIN(
+		56, "GPIO56",
+		MTK_EINT_FUNCTION(0, 56),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO56"),
+		MTK_FUNCTION(1, "BPI_BUS9"),
+		MTK_FUNCTION(2, "SCL_6306")
+	),
+	MTK_PIN(
+		57, "GPIO57",
+		MTK_EINT_FUNCTION(0, 57),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO57"),
+		MTK_FUNCTION(1, "BPI_BUS10"),
+		MTK_FUNCTION(2, "SDA_6306")
+	),
+	MTK_PIN(
+		58, "GPIO58",
+		MTK_EINT_FUNCTION(0, 58),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO58"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D2")
+	),
+	MTK_PIN(
+		59, "GPIO59",
+		MTK_EINT_FUNCTION(0, 59),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO59"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D1")
+	),
+	MTK_PIN(
+		60, "GPIO60",
+		MTK_EINT_FUNCTION(0, 60),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO60"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D0")
+	),
+	MTK_PIN(
+		61, "GPIO61",
+		MTK_EINT_FUNCTION(0, 61),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO61"),
+		MTK_FUNCTION(1, "MIPI1_SDATA")
+	),
+	MTK_PIN(
+		62, "GPIO62",
+		MTK_EINT_FUNCTION(0, 62),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO62"),
+		MTK_FUNCTION(1, "MIPI1_SCLK")
+	),
+	MTK_PIN(
+		63, "GPIO63",
+		MTK_EINT_FUNCTION(0, 63),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO63"),
+		MTK_FUNCTION(1, "MIPI0_SDATA")
+	),
+	MTK_PIN(
+		64, "GPIO64",
+		MTK_EINT_FUNCTION(0, 64),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO64"),
+		MTK_FUNCTION(1, "MIPI0_SCLK")
+	),
+	MTK_PIN(
+		65, "GPIO65",
+		MTK_EINT_FUNCTION(0, 65),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO65"),
+		MTK_FUNCTION(1, "MIPI3_SDATA"),
+		MTK_FUNCTION(2, "BPI_BUS16")
+	),
+	MTK_PIN(
+		66, "GPIO66",
+		MTK_EINT_FUNCTION(0, 66),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO66"),
+		MTK_FUNCTION(1, "MIPI3_SCLK"),
+		MTK_FUNCTION(2, "BPI_BUS17")
+	),
+	MTK_PIN(
+		67, "GPIO67",
+		MTK_EINT_FUNCTION(0, 67),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO67"),
+		MTK_FUNCTION(1, "MIPI2_SDATA")
+	),
+	MTK_PIN(
+		68, "GPIO68",
+		MTK_EINT_FUNCTION(0, 68),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO68"),
+		MTK_FUNCTION(1, "MIPI2_SCLK")
+	),
+	MTK_PIN(
+		69, "GPIO69",
+		MTK_EINT_FUNCTION(0, 69),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO69"),
+		MTK_FUNCTION(1, "BPI_BUS7")
+	),
+	MTK_PIN(
+		70, "GPIO70",
+		MTK_EINT_FUNCTION(0, 70),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO70"),
+		MTK_FUNCTION(1, "BPI_BUS6")
+	),
+	MTK_PIN(
+		71, "GPIO71",
+		MTK_EINT_FUNCTION(0, 71),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO71"),
+		MTK_FUNCTION(1, "BPI_BUS5")
+	),
+	MTK_PIN(
+		72, "GPIO72",
+		MTK_EINT_FUNCTION(0, 72),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO72"),
+		MTK_FUNCTION(1, "BPI_BUS4")
+	),
+	MTK_PIN(
+		73, "GPIO73",
+		MTK_EINT_FUNCTION(0, 73),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO73"),
+		MTK_FUNCTION(1, "BPI_BUS3")
+	),
+	MTK_PIN(
+		74, "GPIO74",
+		MTK_EINT_FUNCTION(0, 74),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO74"),
+		MTK_FUNCTION(1, "BPI_BUS2")
+	),
+	MTK_PIN(
+		75, "GPIO75",
+		MTK_EINT_FUNCTION(0, 75),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO75"),
+		MTK_FUNCTION(1, "BPI_BUS1")
+	),
+	MTK_PIN(
+		76, "GPIO76",
+		MTK_EINT_FUNCTION(0, 76),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO76"),
+		MTK_FUNCTION(1, "BPI_BUS0")
+	),
+	MTK_PIN(
+		77, "GPIO77",
+		MTK_EINT_FUNCTION(0, 77),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO77"),
+		MTK_FUNCTION(1, "BPI_BUS14")
+	),
+	MTK_PIN(
+		78, "GPIO78",
+		MTK_EINT_FUNCTION(0, 78),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO78"),
+		MTK_FUNCTION(1, "BPI_BUS11")
+	),
+	MTK_PIN(
+		79, "GPIO79",
+		MTK_EINT_FUNCTION(0, 79),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO79"),
+		MTK_FUNCTION(1, "BPI_PA_VM1"),
+		MTK_FUNCTION(2, "MIPI4_SDATA")
+	),
+	MTK_PIN(
+		80, "GPIO80",
+		MTK_EINT_FUNCTION(0, 80),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO80"),
+		MTK_FUNCTION(1, "BPI_PA_VM0"),
+		MTK_FUNCTION(2, "MIPI4_SCLK")
+	),
+	MTK_PIN(
+		81, "GPIO81",
+		MTK_EINT_FUNCTION(0, 81),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO81"),
+		MTK_FUNCTION(1, "SDA1"),
+		MTK_FUNCTION(7, "DBG_MON_B0")
+	),
+	MTK_PIN(
+		82, "GPIO82",
+		MTK_EINT_FUNCTION(0, 82),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO82"),
+		MTK_FUNCTION(1, "SDA0"),
+		MTK_FUNCTION(7, "DBG_MON_B1")
+	),
+	MTK_PIN(
+		83, "GPIO83",
+		MTK_EINT_FUNCTION(0, 83),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO83"),
+		MTK_FUNCTION(1, "SCL0"),
+		MTK_FUNCTION(7, "DBG_MON_B2")
+	),
+	MTK_PIN(
+		84, "GPIO84",
+		MTK_EINT_FUNCTION(0, 84),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO84"),
+		MTK_FUNCTION(1, "SCL1"),
+		MTK_FUNCTION(7, "DBG_MON_B3")
+	),
+	MTK_PIN(
+		85, "GPIO85",
+		MTK_EINT_FUNCTION(0, 85),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO85"),
+		MTK_FUNCTION(1, "RFIC0_BSI_EN")
+	),
+	MTK_PIN(
+		86, "GPIO86",
+		MTK_EINT_FUNCTION(0, 86),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO86"),
+		MTK_FUNCTION(1, "RFIC0_BSI_CK")
+	),
+	MTK_PIN(
+		87, "GPIO87",
+		MTK_EINT_FUNCTION(0, 87),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO87"),
+		MTK_FUNCTION(2, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(3, "CMVREF0"),
+		MTK_FUNCTION(4, "MD_URXD0"),
+		MTK_FUNCTION(5, "AGPS_SYNC"),
+		MTK_FUNCTION(6, "EXT_FRAME_SYNC")
+	),
+	MTK_PIN(
+		88, "GPIO88",
+		MTK_EINT_FUNCTION(0, 88),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO88"),
+		MTK_FUNCTION(1, "CMMCLK3"),
+		MTK_FUNCTION(2, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(3, "CMVREF1"),
+		MTK_FUNCTION(4, "MD_UTXD0"),
+		MTK_FUNCTION(5, "AGPS_SYNC"),
+		MTK_FUNCTION(6, "DVFSRC_EXT_REQ")
+	),
+	MTK_PIN(
+		89, "GPIO89",
+		MTK_EINT_FUNCTION(0, 89),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO89"),
+		MTK_FUNCTION(1, "SRCLKENAI0"),
+		MTK_FUNCTION(2, "PWM2"),
+		MTK_FUNCTION(3, "MD_INT0"),
+		MTK_FUNCTION(4, "USB_DRVVBUS"),
+		MTK_FUNCTION(5, "SCL_6306"),
+		MTK_FUNCTION(6, "TP_GPIO4_AO"),
+		MTK_FUNCTION(7, "DBG_MON_B21")
+	),
+	MTK_PIN(
+		90, "GPIO90",
+		MTK_EINT_FUNCTION(0, 90),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO90"),
+		MTK_FUNCTION(1, "URXD1"),
+		MTK_FUNCTION(2, "PWM0"),
+		MTK_FUNCTION(3, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(4, "ANT_SEL4"),
+		MTK_FUNCTION(5, "USB_DRVVBUS"),
+		MTK_FUNCTION(6, "I2S2_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_B4")
+	),
+	MTK_PIN(
+		91, "GPIO91",
+		MTK_EINT_FUNCTION(0, 91),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO91"),
+		MTK_FUNCTION(1, "KPROW1"),
+		MTK_FUNCTION(2, "PWM2"),
+		MTK_FUNCTION(3, "MD_INT0"),
+		MTK_FUNCTION(4, "ANT_SEL5"),
+		MTK_FUNCTION(5, "IDDIG"),
+		MTK_FUNCTION(6, "I2S2_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_B5")
+	),
+	MTK_PIN(
+		92, "GPIO92",
+		MTK_EINT_FUNCTION(0, 92),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO92"),
+		MTK_FUNCTION(1, "KPROW0"),
+		MTK_FUNCTION(5, "DVFSRC_EXT_REQ"),
+		MTK_FUNCTION(6, "I2S2_DI"),
+		MTK_FUNCTION(7, "DBG_MON_B6")
+	),
+	MTK_PIN(
+		93, "GPIO93",
+		MTK_EINT_FUNCTION(0, 93),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO93"),
+		MTK_FUNCTION(1, "KPCOL0"),
+		MTK_FUNCTION(7, "DBG_MON_B7")
+	),
+	MTK_PIN(
+		94, "GPIO94",
+		MTK_EINT_FUNCTION(0, 94),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO94"),
+		MTK_FUNCTION(1, "KPCOL1"),
+		MTK_FUNCTION(5, "CMFLASH"),
+		MTK_FUNCTION(6, "CMVREF0"),
+		MTK_FUNCTION(7, "DBG_MON_B8")
+	),
+	MTK_PIN(
+		95, "GPIO95",
+		MTK_EINT_FUNCTION(0, 95),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO95"),
+		MTK_FUNCTION(1, "URXD0"),
+		MTK_FUNCTION(2, "UTXD0"),
+		MTK_FUNCTION(3, "MD_URXD0"),
+		MTK_FUNCTION(4, "PTA_RXD"),
+		MTK_FUNCTION(5, "SSPM_URXD_AO"),
+		MTK_FUNCTION(6, "WIFI_RXD")
+	),
+	MTK_PIN(
+		96, "GPIO96",
+		MTK_EINT_FUNCTION(0, 96),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO96"),
+		MTK_FUNCTION(1, "UTXD0"),
+		MTK_FUNCTION(2, "URXD0"),
+		MTK_FUNCTION(3, "MD_UTXD0"),
+		MTK_FUNCTION(4, "PTA_TXD"),
+		MTK_FUNCTION(5, "SSPM_UTXD_AO"),
+		MTK_FUNCTION(6, "WIFI_TXD")
+	),
+	MTK_PIN(
+		97, "GPIO97",
+		MTK_EINT_FUNCTION(0, 97),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO97"),
+		MTK_FUNCTION(1, "UCTS0"),
+		MTK_FUNCTION(2, "I2S1_MCK"),
+		MTK_FUNCTION(3, "CONN_MCU_TDO"),
+		MTK_FUNCTION(4, "SPI5_MI"),
+		MTK_FUNCTION(5, "SCL_6306"),
+		MTK_FUNCTION(6, "MCUPM_JTAG_TDO"),
+		MTK_FUNCTION(7, "DBG_MON_B15")
+	),
+	MTK_PIN(
+		98, "GPIO98",
+		MTK_EINT_FUNCTION(0, 98),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO98"),
+		MTK_FUNCTION(1, "URTS0"),
+		MTK_FUNCTION(2, "I2S1_BCK"),
+		MTK_FUNCTION(3, "CONN_MCU_TMS"),
+		MTK_FUNCTION(4, "SPI5_CSB"),
+		MTK_FUNCTION(6, "MCUPM_JTAG_TMS"),
+		MTK_FUNCTION(7, "DBG_MON_B16")
+	),
+	MTK_PIN(
+		99, "GPIO99",
+		MTK_EINT_FUNCTION(0, 99),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO99"),
+		MTK_FUNCTION(1, "CMMCLK0"),
+		MTK_FUNCTION(4, "AUXIF_CLK"),
+		MTK_FUNCTION(5, "PTA_RXD"),
+		MTK_FUNCTION(6, "CONN_UART0_RXD"),
+		MTK_FUNCTION(7, "DBG_MON_B17")
+	),
+
+	MTK_PIN(
+		100, "GPIO100",
+		MTK_EINT_FUNCTION(0, 100),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO100"),
+		MTK_FUNCTION(1, "CMMCLK1"),
+		MTK_FUNCTION(4, "AUXIF_ST"),
+		MTK_FUNCTION(5, "PTA_TXD"),
+		MTK_FUNCTION(6, "CONN_UART0_TXD"),
+		MTK_FUNCTION(7, "DBG_MON_B18")
+	),
+	MTK_PIN(
+		101, "GPIO101",
+		MTK_EINT_FUNCTION(0, 101),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO101"),
+		MTK_FUNCTION(1, "CMFLASH"),
+		MTK_FUNCTION(2, "I2S1_LRCK"),
+		MTK_FUNCTION(3, "CONN_MCU_TCK"),
+		MTK_FUNCTION(4, "SPI5_MO"),
+		MTK_FUNCTION(6, "MCUPM_JTAG_TCK"),
+		MTK_FUNCTION(7, "DBG_MON_B19")
+	),
+	MTK_PIN(
+		102, "GPIO102",
+		MTK_EINT_FUNCTION(0, 102),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO102"),
+		MTK_FUNCTION(1, "CMVREF0"),
+		MTK_FUNCTION(2, "I2S1_DO"),
+		MTK_FUNCTION(3, "CONN_MCU_TDI"),
+		MTK_FUNCTION(4, "SPI5_CLK"),
+		MTK_FUNCTION(5, "AGPS_SYNC"),
+		MTK_FUNCTION(6, "MCUPM_JTAG_TDI"),
+		MTK_FUNCTION(7, "DBG_MON_B20")
+	),
+	MTK_PIN(
+		103, "GPIO103",
+		MTK_EINT_FUNCTION(0, 103),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO103"),
+		MTK_FUNCTION(1, "SCL2"),
+		MTK_FUNCTION(2, "TP_UTXD1_AO"),
+		MTK_FUNCTION(3, "MD_UTXD0"),
+		MTK_FUNCTION(4, "MD_UTXD1"),
+		MTK_FUNCTION(5, "TP_URTS2_AO"),
+		MTK_FUNCTION(6, "WIFI_TXD"),
+		MTK_FUNCTION(7, "DBG_MON_B25")
+	),
+	MTK_PIN(
+		104, "GPIO104",
+		MTK_EINT_FUNCTION(0, 104),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO104"),
+		MTK_FUNCTION(1, "SDA2"),
+		MTK_FUNCTION(2, "TP_URXD1_AO"),
+		MTK_FUNCTION(3, "MD_URXD0"),
+		MTK_FUNCTION(4, "MD_URXD1"),
+		MTK_FUNCTION(5, "TP_UCTS2_AO"),
+		MTK_FUNCTION(6, "WIFI_RXD"),
+		MTK_FUNCTION(7, "DBG_MON_B26")
+	),
+	MTK_PIN(
+		105, "GPIO105",
+		MTK_EINT_FUNCTION(0, 105),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO105"),
+		MTK_FUNCTION(1, "SCL4"),
+		MTK_FUNCTION(3, "MD_UTXD1"),
+		MTK_FUNCTION(4, "MD_UTXD0"),
+		MTK_FUNCTION(5, "TP_UTXD2_AO"),
+		MTK_FUNCTION(6, "PTA_TXD"),
+		MTK_FUNCTION(7, "DBG_MON_B27")
+	),
+	MTK_PIN(
+		106, "GPIO106",
+		MTK_EINT_FUNCTION(0, 106),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO106"),
+		MTK_FUNCTION(1, "SDA4"),
+		MTK_FUNCTION(3, "MD_URXD1"),
+		MTK_FUNCTION(4, "MD_URXD0"),
+		MTK_FUNCTION(5, "TP_URXD2_AO"),
+		MTK_FUNCTION(6, "PTA_RXD"),
+		MTK_FUNCTION(7, "DBG_MON_B28")
+	),
+	MTK_PIN(
+		107, "GPIO107",
+		MTK_EINT_FUNCTION(0, 107),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO107"),
+		MTK_FUNCTION(1, "UTXD1"),
+		MTK_FUNCTION(2, "MD_UTXD0"),
+		MTK_FUNCTION(3, "SDA_6306"),
+		MTK_FUNCTION(4, "KPCOL3"),
+		MTK_FUNCTION(5, "CMVREF0"),
+		MTK_FUNCTION(6, "URTS0"),
+		MTK_FUNCTION(7, "DBG_MON_B29")
+	),
+	MTK_PIN(
+		108, "GPIO108",
+		MTK_EINT_FUNCTION(0, 108),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO108"),
+		MTK_FUNCTION(1, "CMMCLK2"),
+		MTK_FUNCTION(2, "MD_INT0"),
+		MTK_FUNCTION(3, "CONN_MCU_DBGACK_N"),
+		MTK_FUNCTION(4, "KPCOL4"),
+		MTK_FUNCTION(6, "I2S3_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B30")
+	),
+	MTK_PIN(
+		109, "GPIO109",
+		MTK_EINT_FUNCTION(0, 109),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO109"),
+		MTK_FUNCTION(1, "URXD1"),
+		MTK_FUNCTION(2, "MD_URXD0"),
+		MTK_FUNCTION(3, "ANT_SEL7"),
+		MTK_FUNCTION(4, "KPCOL5"),
+		MTK_FUNCTION(5, "CMVREF1"),
+		MTK_FUNCTION(6, "UCTS0"),
+		MTK_FUNCTION(7, "DBG_MON_B31")
+	),
+	MTK_PIN(
+		110, "GPIO110",
+		MTK_EINT_FUNCTION(0, 110),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO110"),
+		MTK_FUNCTION(1, "ANT_SEL0"),
+		MTK_FUNCTION(2, "CLKM0"),
+		MTK_FUNCTION(3, "PWM3"),
+		MTK_FUNCTION(4, "MD_INT0"),
+		MTK_FUNCTION(5, "IDDIG"),
+		MTK_FUNCTION(6, "I2S3_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_B13")
+	),
+	MTK_PIN(
+		111, "GPIO111",
+		MTK_EINT_FUNCTION(0, 111),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO111"),
+		MTK_FUNCTION(1, "ANT_SEL1"),
+		MTK_FUNCTION(2, "CLKM1"),
+		MTK_FUNCTION(3, "PWM4"),
+		MTK_FUNCTION(4, "PTA_RXD"),
+		MTK_FUNCTION(5, "CMVREF0"),
+		MTK_FUNCTION(6, "I2S3_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_B14")
+	),
+	MTK_PIN(
+		112, "GPIO112",
+		MTK_EINT_FUNCTION(0, 112),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO112"),
+		MTK_FUNCTION(1, "ANT_SEL2"),
+		MTK_FUNCTION(2, "CLKM2"),
+		MTK_FUNCTION(3, "PWM5"),
+		MTK_FUNCTION(4, "PTA_TXD"),
+		MTK_FUNCTION(5, "CMVREF1"),
+		MTK_FUNCTION(6, "I2S3_DO")
+	),
+	MTK_PIN(
+		113, "GPIO113",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO113"),
+		MTK_FUNCTION(1, "CONN_TOP_CLK")
+	),
+	MTK_PIN(
+		114, "GPIO114",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO114"),
+		MTK_FUNCTION(1, "CONN_TOP_DATA")
+	),
+	MTK_PIN(
+		115, "GPIO115",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO115"),
+		MTK_FUNCTION(1, "CONN_BT_CLK")
+	),
+	MTK_PIN(
+		116, "GPIO116",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO116"),
+		MTK_FUNCTION(1, "CONN_BT_DATA")
+	),
+	MTK_PIN(
+		117, "GPIO117",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO117"),
+		MTK_FUNCTION(1, "CONN_WF_CTRL0")
+	),
+	MTK_PIN(
+		118, "GPIO118",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO118"),
+		MTK_FUNCTION(1, "CONN_WF_CTRL1")
+	),
+	MTK_PIN(
+		119, "GPIO119",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO119"),
+		MTK_FUNCTION(1, "CONN_WF_CTRL2")
+	),
+	MTK_PIN(
+		120, "GPIO120",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO120"),
+		MTK_FUNCTION(1, "CONN_WB_PTA")
+	),
+	MTK_PIN(
+		121, "GPIO121",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO121"),
+		MTK_FUNCTION(1, "CONN_HRST_B")
+	),
+	MTK_PIN(
+		122, "GPIO122",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO122"),
+		MTK_FUNCTION(1, "MSDC0_CMD"),
+		MTK_FUNCTION(2, "MSDC0_CMD")
+	),
+	MTK_PIN(
+		123, "GPIO123",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO123"),
+		MTK_FUNCTION(1, "MSDC0_DAT0"),
+		MTK_FUNCTION(2, "MSDC0_DAT4")
+	),
+	MTK_PIN(
+		124, "GPIO124",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO124"),
+		MTK_FUNCTION(1, "MSDC0_CLK"),
+		MTK_FUNCTION(2, "MSDC0_CLK")
+	),
+	MTK_PIN(
+		125, "GPIO125",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO125"),
+		MTK_FUNCTION(1, "MSDC0_DAT2"),
+		MTK_FUNCTION(2, "MSDC0_DAT5")
+	),
+	MTK_PIN(
+		126, "GPIO126",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO126"),
+		MTK_FUNCTION(1, "MSDC0_DAT4"),
+		MTK_FUNCTION(2, "MSDC0_DAT2")
+	),
+	MTK_PIN(
+		127, "GPIO127",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO127"),
+		MTK_FUNCTION(1, "MSDC0_DAT6"),
+		MTK_FUNCTION(2, "MSDC0_DAT1")
+	),
+	MTK_PIN(
+		128, "GPIO128",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO128"),
+		MTK_FUNCTION(1, "MSDC0_DAT1"),
+		MTK_FUNCTION(2, "MSDC0_DAT6")
+	),
+	MTK_PIN(
+		129, "GPIO129",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO129"),
+		MTK_FUNCTION(1, "MSDC0_DAT5"),
+		MTK_FUNCTION(2, "MSDC0_DAT0")
+	),
+	MTK_PIN(
+		130, "GPIO130",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO130"),
+		MTK_FUNCTION(1, "MSDC0_DAT7"),
+		MTK_FUNCTION(2, "MSDC0_DAT7")
+	),
+	MTK_PIN(
+		131, "GPIO131",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO131"),
+		MTK_FUNCTION(1, "MSDC0_DSL"),
+		MTK_FUNCTION(2, "MSDC0_DSL")
+	),
+	MTK_PIN(
+		132, "GPIO132",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO132"),
+		MTK_FUNCTION(1, "MSDC0_DAT3"),
+		MTK_FUNCTION(2, "MSDC0_DAT3")
+	),
+	MTK_PIN(
+		133, "GPIO133",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO133"),
+		MTK_FUNCTION(1, "MSDC0_RSTB"),
+		MTK_FUNCTION(2, "MSDC0_RSTB")
+	),
+	MTK_PIN(
+		134, "GPIO134",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO134"),
+		MTK_FUNCTION(1, "RTC32K_CK")
+	),
+	MTK_PIN(
+		135, "GPIO135",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO135"),
+		MTK_FUNCTION(1, "WATCHDOG")
+	),
+	MTK_PIN(
+		136, "GPIO136",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO136"),
+		MTK_FUNCTION(1, "AUD_CLK_MOSI"),
+		MTK_FUNCTION(2, "AUD_CLK_MISO"),
+		MTK_FUNCTION(3, "I2S1_MCK")
+	),
+	MTK_PIN(
+		137, "GPIO137",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO137"),
+		MTK_FUNCTION(1, "AUD_SYNC_MOSI"),
+		MTK_FUNCTION(2, "AUD_SYNC_MISO"),
+		MTK_FUNCTION(3, "I2S1_BCK")
+	),
+	MTK_PIN(
+		138, "GPIO138",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO138"),
+		MTK_FUNCTION(1, "AUD_DAT_MOSI0"),
+		MTK_FUNCTION(2, "AUD_DAT_MISO0"),
+		MTK_FUNCTION(3, "I2S1_LRCK")
+	),
+	MTK_PIN(
+		139, "GPIO139",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO139"),
+		MTK_FUNCTION(1, "AUD_DAT_MOSI1"),
+		MTK_FUNCTION(2, "AUD_DAT_MISO1"),
+		MTK_FUNCTION(3, "I2S1_DO")
+	),
+	MTK_PIN(
+		140, "GPIO140",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO140"),
+		MTK_FUNCTION(1, "AUD_CLK_MISO"),
+		MTK_FUNCTION(2, "AUD_CLK_MOSI"),
+		MTK_FUNCTION(3, "I2S2_MCK")
+	),
+	MTK_PIN(
+		141, "GPIO141",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO141"),
+		MTK_FUNCTION(1, "AUD_SYNC_MISO"),
+		MTK_FUNCTION(2, "AUD_SYNC_MOSI"),
+		MTK_FUNCTION(3, "I2S2_BCK")
+	),
+	MTK_PIN(
+		142, "GPIO142",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO142"),
+		MTK_FUNCTION(1, "AUD_DAT_MISO0"),
+		MTK_FUNCTION(2, "AUD_DAT_MOSI0"),
+		MTK_FUNCTION(3, "I2S2_LRCK")
+	),
+	MTK_PIN(
+		143, "GPIO143",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO143"),
+		MTK_FUNCTION(1, "AUD_DAT_MISO1"),
+		MTK_FUNCTION(2, "AUD_DAT_MOSI1"),
+		MTK_FUNCTION(3, "I2S2_DI")
+	),
+	MTK_PIN(
+		144, "GPIO144",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO144"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_MI"),
+		MTK_FUNCTION(2, "PWRAP_SPI0_MO")
+	),
+	MTK_PIN(
+		145, "GPIO145",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO145"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_CSN")
+	),
+	MTK_PIN(
+		146, "GPIO146",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO146"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_MO"),
+		MTK_FUNCTION(2, "PWRAP_SPI0_MI")
+	),
+	MTK_PIN(
+		147, "GPIO147",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO147"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_CK")
+	),
+	MTK_PIN(
+		148, "GPIO148",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO148"),
+		MTK_FUNCTION(1, "SRCLKENA0")
+	),
+	MTK_PIN(
+		149, "GPIO149",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO149"),
+		MTK_FUNCTION(1, "SRCLKENA1")
+	),
+	MTK_PIN(
+		150, "GPIO150",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO150"),
+		MTK_FUNCTION(1, "PWM0"),
+		MTK_FUNCTION(2, "CMFLASH"),
+		MTK_FUNCTION(3, "ANT_SEL3"),
+		MTK_FUNCTION(5, "MD_URXD0"),
+		MTK_FUNCTION(6, "TP_URXD2_AO")
+	),
+	MTK_PIN(
+		151, "GPIO151",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO151"),
+		MTK_FUNCTION(1, "PWM1"),
+		MTK_FUNCTION(2, "CMVREF0"),
+		MTK_FUNCTION(3, "ANT_SEL4"),
+		MTK_FUNCTION(5, "MD_UTXD0"),
+		MTK_FUNCTION(6, "TP_UTXD2_AO")
+	),
+	MTK_PIN(
+		152, "GPIO152",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO152"),
+		MTK_FUNCTION(1, "PWM2"),
+		MTK_FUNCTION(2, "CMVREF1"),
+		MTK_FUNCTION(3, "ANT_SEL5"),
+		MTK_FUNCTION(5, "MD_URXD1"),
+		MTK_FUNCTION(6, "TP_UCTS1_AO")
+	),
+	MTK_PIN(
+		153, "GPIO153",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO153"),
+		MTK_FUNCTION(1, "PWM3"),
+		MTK_FUNCTION(2, "CLKM0"),
+		MTK_FUNCTION(3, "ANT_SEL6"),
+		MTK_FUNCTION(5, "MD_UTXD1"),
+		MTK_FUNCTION(6, "TP_URTS1_AO")
+	),
+	MTK_PIN(
+		154, "GPIO154",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO154"),
+		MTK_FUNCTION(1, "PWM5"),
+		MTK_FUNCTION(2, "CLKM2"),
+		MTK_FUNCTION(3, "USB_DRVVBUS"),
+		MTK_FUNCTION(5, "PTA_TXD"),
+		MTK_FUNCTION(6, "CONN_UART0_TXD")
+	),
+	MTK_PIN(
+		155, "GPIO155",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO155"),
+		MTK_FUNCTION(1, "SPI0_MI"),
+		MTK_FUNCTION(2, "IDDIG"),
+		MTK_FUNCTION(3, "AGPS_SYNC"),
+		MTK_FUNCTION(4, "TP_GPIO0_AO"),
+		MTK_FUNCTION(5, "MFG_JTAG_TDO"),
+		MTK_FUNCTION(6, "DFD_TDO"),
+		MTK_FUNCTION(7, "JTDO_SEL1")
+	),
+	MTK_PIN(
+		156, "GPIO156",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO156"),
+		MTK_FUNCTION(1, "SPI0_CSB"),
+		MTK_FUNCTION(2, "USB_DRVVBUS"),
+		MTK_FUNCTION(3, "DVFSRC_EXT_REQ"),
+		MTK_FUNCTION(4, "TP_GPIO1_AO"),
+		MTK_FUNCTION(5, "MFG_JTAG_TMS"),
+		MTK_FUNCTION(6, "DFD_TMS"),
+		MTK_FUNCTION(7, "JTMS_SEL1")
+	),
+	MTK_PIN(
+		157, "GPIO157",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO157"),
+		MTK_FUNCTION(1, "SPI0_MO"),
+		MTK_FUNCTION(2, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(3, "CLKM0"),
+		MTK_FUNCTION(4, "TP_GPIO2_AO"),
+		MTK_FUNCTION(5, "MFG_JTAG_TDI"),
+		MTK_FUNCTION(6, "DFD_TDI"),
+		MTK_FUNCTION(7, "JTDI_SEL1")
+	),
+	MTK_PIN(
+		158, "GPIO158",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO158"),
+		MTK_FUNCTION(1, "SPI0_CLK"),
+		MTK_FUNCTION(2, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(3, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(4, "TP_GPIO3_AO"),
+		MTK_FUNCTION(5, "MFG_JTAG_TCK"),
+		MTK_FUNCTION(6, "DFD_TCK_XI"),
+		MTK_FUNCTION(7, "JTCK_SEL1")
+	),
+	MTK_PIN(
+		159, "GPIO159",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO159"),
+		MTK_FUNCTION(1, "PWM4"),
+		MTK_FUNCTION(2, "CLKM1"),
+		MTK_FUNCTION(3, "ANT_SEL7"),
+		MTK_FUNCTION(5, "PTA_RXD"),
+		MTK_FUNCTION(6, "CONN_UART0_RXD")
+	),
+	MTK_PIN(
+		160, "GPIO160",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO160"),
+		MTK_FUNCTION(1, "CLKM0"),
+		MTK_FUNCTION(2, "PWM2"),
+		MTK_FUNCTION(3, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(4, "TP_GPIO5_AO"),
+		MTK_FUNCTION(5, "AGPS_SYNC"),
+		MTK_FUNCTION(6, "DVFSRC_EXT_REQ")
+	),
+	MTK_PIN(
+		161, "GPIO161",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO161"),
+		MTK_FUNCTION(1, "SCL6"),
+		MTK_FUNCTION(2, "SCL_6306"),
+		MTK_FUNCTION(3, "TP_GPIO6_AO"),
+		MTK_FUNCTION(4, "KPCOL6"),
+		MTK_FUNCTION(5, "PTA_RXD"),
+		MTK_FUNCTION(6, "CONN_UART0_RXD")
+	),
+	MTK_PIN(
+		162, "GPIO162",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO162"),
+		MTK_FUNCTION(1, "SDA6"),
+		MTK_FUNCTION(2, "SDA_6306"),
+		MTK_FUNCTION(3, "TP_GPIO7_AO"),
+		MTK_FUNCTION(4, "KPCOL7"),
+		MTK_FUNCTION(5, "PTA_TXD"),
+		MTK_FUNCTION(6, "CONN_UART0_TXD")
+	),
+	MTK_PIN(
+		163, "GPIO163",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO163")
+	),
+	MTK_PIN(
+		164, "GPIO164",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO164")
+	),
+	MTK_PIN(
+		165, "GPIO165",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO165")
+	),
+	MTK_PIN(
+		166, "GPIO166",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO166")
+	),
+	MTK_PIN(
+		167, "GPIO167",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO167")
+	),
+	MTK_PIN(
+		168, "GPIO168",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO168")
+	),
+	MTK_PIN(
+		169, "GPIO169",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO169")
+	),
+	MTK_PIN(
+		170, "GPIO170",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO170")
+	),
+	MTK_PIN(
+		171, "GPIO171",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO171")
+	),
+	MTK_PIN(
+		172, "GPIO172",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO172")
+	),
+	MTK_PIN(
+		173, "GPIO173",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO173")
+	),
+	MTK_PIN(
+		174, "GPIO174",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO174")
+	),
+	MTK_PIN(
+		175, "GPIO175",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO175")
+	),
+	MTK_PIN(
+		176, "GPIO176",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO176")
+	),
+	MTK_PIN(
+		177, "GPIO177",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO177")
+	),
+	MTK_PIN(
+		178, "GPIO178",
+		MTK_EINT_FUNCTION(0, NO_EINT_SUPPORT),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO178")
+	),
+	MTK_PIN(
+		179, "GPIO179",
+		MTK_EINT_FUNCTION(0, 151),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO179")
+	),
+};
+
+#endif /* __PINCTRL_MTK_MT6765_H */
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mtk-mt6797.h
@@ -0,0 +1,2429 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Based on pinctrl-mtk-mt6765.h
+ *
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: ZH Chen <zh.chen@mediatek.com>
+ *
+ * Copyright (c) 2018 Manivannan Sadhasivam
+ */
+
+#ifndef __PINCTRL_MTK_MT6797_H
+#define __PINCTRL_MTK_MT6797_H
+
+#include "pinctrl-paris.h"
+
+static const struct mtk_pin_desc mtk_pins_mt6797[] = {
+	MTK_PIN(
+		0, "GPIO0",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO0"),
+		MTK_FUNCTION(1, "CSI0A_L0P_T0A")
+	),
+	MTK_PIN(
+		1, "GPIO1",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO1"),
+		MTK_FUNCTION(1, "CSI0A_L0N_T0B")
+	),
+	MTK_PIN(
+		2, "GPIO2",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO2"),
+		MTK_FUNCTION(1, "CSI0A_L1P_T0C")
+	),
+	MTK_PIN(
+		3, "GPIO3",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO3"),
+		MTK_FUNCTION(1, "CSI0A_L1N_T1A")
+	),
+	MTK_PIN(
+		4, "GPIO4",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO4"),
+		MTK_FUNCTION(1, "CSI0A_L2P_T1B")
+	),
+	MTK_PIN(
+		5, "GPIO5",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO5"),
+		MTK_FUNCTION(1, "CSI0A_L2N_T1C")
+	),
+	MTK_PIN(
+		6, "GPIO6",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO6"),
+		MTK_FUNCTION(1, "CSI0B_L0P_T0A")
+	),
+	MTK_PIN(
+		7, "GPIO7",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO7"),
+		MTK_FUNCTION(1, "CSI0B_L0N_T0B")
+	),
+	MTK_PIN(
+		8, "GPIO8",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO8"),
+		MTK_FUNCTION(1, "CSI0B_L1P_T0C")
+	),
+	MTK_PIN(
+		9, "GPIO9",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO9"),
+		MTK_FUNCTION(1, "CSI0B_L1N_T1A")
+	),
+	MTK_PIN(
+		10, "GPIO10",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO10"),
+		MTK_FUNCTION(1, "CSI1A_L0P_T0A")
+	),
+	MTK_PIN(
+		11, "GPIO11",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO11"),
+		MTK_FUNCTION(1, "CSI1A_L0N_T0B")
+	),
+	MTK_PIN(
+		12, "GPIO12",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO12"),
+		MTK_FUNCTION(1, "CSI1A_L1P_T0C")
+	),
+	MTK_PIN(
+		13, "GPIO13",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO13"),
+		MTK_FUNCTION(1, "CSI1A_L1N_T1A")
+	),
+	MTK_PIN(
+		14, "GPIO14",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO14"),
+		MTK_FUNCTION(1, "CSI1A_L2P_T1B")
+	),
+	MTK_PIN(
+		15, "GPIO15",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO15"),
+		MTK_FUNCTION(1, "CSI1A_L2N_T1C")
+	),
+	MTK_PIN(
+		16, "GPIO16",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO16"),
+		MTK_FUNCTION(1, "CSI1B_L0P_T0A")
+	),
+	MTK_PIN(
+		17, "GPIO17",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO17"),
+		MTK_FUNCTION(1, "CSI1B_L0N_T0B")
+	),
+	MTK_PIN(
+		18, "GPIO18",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO18"),
+		MTK_FUNCTION(1, "CSI1B_L1P_T0C")
+	),
+	MTK_PIN(
+		19, "GPIO19",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO19"),
+		MTK_FUNCTION(1, "CSI1B_L1N_T1A")
+	),
+	MTK_PIN(
+		20, "GPIO20",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO20"),
+		MTK_FUNCTION(1, "CSI1B_L2P_T1B")
+	),
+	MTK_PIN(
+		21, "GPIO21",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO21"),
+		MTK_FUNCTION(1, "CSI1B_L2N_T1C")
+	),
+	MTK_PIN(
+		22, "GPIO22",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO22"),
+		MTK_FUNCTION(1, "CSI2_L0P_T0A")
+	),
+	MTK_PIN(
+		23, "GPIO23",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO23"),
+		MTK_FUNCTION(1, "CSI2_L0N_T0B")
+	),
+	MTK_PIN(
+		24, "GPIO24",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO24"),
+		MTK_FUNCTION(1, "CSI2_L1P_T0C")
+	),
+	MTK_PIN(
+		25, "GPIO25",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO25"),
+		MTK_FUNCTION(1, "CSI2_L1N_T1A")
+	),
+	MTK_PIN(
+		26, "GPIO26",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO26"),
+		MTK_FUNCTION(1, "CSI2_L2P_T1B")
+	),
+	MTK_PIN(
+		27, "GPIO27",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO27"),
+		MTK_FUNCTION(1, "CSI2_L2N_T1C")
+	),
+	MTK_PIN(
+		28, "GPIO28",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO28"),
+		MTK_FUNCTION(1, "SPI5_CLK_A"),
+		MTK_FUNCTION(2, "IRTX_OUT"),
+		MTK_FUNCTION(3, "UDI_TDO"),
+		MTK_FUNCTION(4, "SCP_JTAG_TDO"),
+		MTK_FUNCTION(5, "CONN_MCU_TDO"),
+		MTK_FUNCTION(6, "PWM_A"),
+		MTK_FUNCTION(7, "C2K_DM_OTDO")
+	),
+	MTK_PIN(
+		29, "GPIO29",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO29"),
+		MTK_FUNCTION(1, "SPI5_MI_A"),
+		MTK_FUNCTION(2, "DAP_SIB1_SWD"),
+		MTK_FUNCTION(3, "UDI_TMS"),
+		MTK_FUNCTION(4, "SCP_JTAG_TMS"),
+		MTK_FUNCTION(5, "CONN_MCU_TMS"),
+		MTK_FUNCTION(6, "CONN_MCU_AICE_TMSC"),
+		MTK_FUNCTION(7, "C2K_DM_OTMS")
+	),
+	MTK_PIN(
+		30, "GPIO30",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO30"),
+		MTK_FUNCTION(1, "CMMCLK0"),
+		MTK_FUNCTION(7, "MD_CLKM0")
+	),
+	MTK_PIN(
+		31, "GPIO31",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO31"),
+		MTK_FUNCTION(1, "CMMCLK1"),
+		MTK_FUNCTION(7, "MD_CLKM1")
+	),
+	MTK_PIN(
+		32, "GPIO32",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO32"),
+		MTK_FUNCTION(1, "SPI5_CS_A"),
+		MTK_FUNCTION(2, "DAP_SIB1_SWCK"),
+		MTK_FUNCTION(3, "UDI_TCK_XI"),
+		MTK_FUNCTION(4, "SCP_JTAG_TCK"),
+		MTK_FUNCTION(5, "CONN_MCU_TCK"),
+		MTK_FUNCTION(6, "CONN_MCU_AICE_TCKC"),
+		MTK_FUNCTION(7, "C2K_DM_OTCK")
+	),
+	MTK_PIN(
+		33, "GPIO33",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO33"),
+		MTK_FUNCTION(1, "SPI5_MO_A"),
+		MTK_FUNCTION(2, "CMFLASH"),
+		MTK_FUNCTION(3, "UDI_TDI"),
+		MTK_FUNCTION(4, "SCP_JTAG_TDI"),
+		MTK_FUNCTION(5, "CONN_MCU_TDI"),
+		MTK_FUNCTION(6, "MD_URXD0"),
+		MTK_FUNCTION(7, "C2K_DM_OTDI")
+	),
+	MTK_PIN(
+		34, "GPIO34",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO34"),
+		MTK_FUNCTION(1, "CMFLASH"),
+		MTK_FUNCTION(2, "CLKM0"),
+		MTK_FUNCTION(3, "UDI_NTRST"),
+		MTK_FUNCTION(4, "SCP_JTAG_TRSTN"),
+		MTK_FUNCTION(5, "CONN_MCU_TRST_B"),
+		MTK_FUNCTION(6, "MD_UTXD0"),
+		MTK_FUNCTION(7, "C2K_DM_JTINTP")
+	),
+	MTK_PIN(
+		35, "GPIO35",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO35"),
+		MTK_FUNCTION(1, "CMMCLK3"),
+		MTK_FUNCTION(2, "CLKM1"),
+		MTK_FUNCTION(3, "MD_URXD1"),
+		MTK_FUNCTION(4, "PTA_RXD"),
+		MTK_FUNCTION(5, "CONN_MCU_DBGACK_N"),
+		MTK_FUNCTION(6, "PWM_B"),
+		MTK_FUNCTION(7, "PCC_PPC_IO")
+	),
+	MTK_PIN(
+		36, "GPIO36",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO36"),
+		MTK_FUNCTION(1, "CMMCLK2"),
+		MTK_FUNCTION(2, "CLKM2"),
+		MTK_FUNCTION(3, "MD_UTXD1"),
+		MTK_FUNCTION(4, "PTA_TXD"),
+		MTK_FUNCTION(5, "CONN_MCU_DBGI_N"),
+		MTK_FUNCTION(6, "PWM_C"),
+		MTK_FUNCTION(7, "EXT_FRAME_SYNC")
+	),
+	MTK_PIN(
+		37, "GPIO37",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO37"),
+		MTK_FUNCTION(1, "SCL0_0")
+	),
+	MTK_PIN(
+		38, "GPIO38",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO38"),
+		MTK_FUNCTION(1, "SDA0_0")
+	),
+	MTK_PIN(
+		39, "GPIO39",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO39"),
+		MTK_FUNCTION(1, "DPI_D0"),
+		MTK_FUNCTION(2, "SPI1_CLK_A"),
+		MTK_FUNCTION(3, "PCM0_SYNC"),
+		MTK_FUNCTION(4, "I2S0_LRCK"),
+		MTK_FUNCTION(5, "CONN_MCU_TRST_B"),
+		MTK_FUNCTION(6, "URXD3"),
+		MTK_FUNCTION(7, "C2K_NTRST")
+	),
+	MTK_PIN(
+		40, "GPIO40",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO40"),
+		MTK_FUNCTION(1, "DPI_D1"),
+		MTK_FUNCTION(2, "SPI1_MI_A"),
+		MTK_FUNCTION(3, "PCM0_CLK"),
+		MTK_FUNCTION(4, "I2S0_BCK"),
+		MTK_FUNCTION(5, "CONN_MCU_TDO"),
+		MTK_FUNCTION(6, "UTXD3"),
+		MTK_FUNCTION(7, "C2K_TCK")
+	),
+	MTK_PIN(
+		41, "GPIO41",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO41"),
+		MTK_FUNCTION(1, "DPI_D2"),
+		MTK_FUNCTION(2, "SPI1_CS_A"),
+		MTK_FUNCTION(3, "PCM0_DO"),
+		MTK_FUNCTION(4, "I2S3_DO"),
+		MTK_FUNCTION(5, "CONN_MCU_DBGACK_N"),
+		MTK_FUNCTION(6, "URTS3"),
+		MTK_FUNCTION(7, "C2K_TDI")
+	),
+	MTK_PIN(
+		42, "GPIO42",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO42"),
+		MTK_FUNCTION(1, "DPI_D3"),
+		MTK_FUNCTION(2, "SPI1_MO_A"),
+		MTK_FUNCTION(3, "PCM0_DI"),
+		MTK_FUNCTION(4, "I2S0_DI"),
+		MTK_FUNCTION(5, "CONN_MCU_TDI"),
+		MTK_FUNCTION(6, "UCTS3"),
+		MTK_FUNCTION(7, "C2K_TMS")
+	),
+	MTK_PIN(
+		43, "GPIO43",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO43"),
+		MTK_FUNCTION(1, "DPI_D4"),
+		MTK_FUNCTION(2, "SPI2_CLK_A"),
+		MTK_FUNCTION(3, "PCM1_SYNC"),
+		MTK_FUNCTION(4, "I2S2_LRCK"),
+		MTK_FUNCTION(5, "CONN_MCU_TMS"),
+		MTK_FUNCTION(6, "CONN_MCU_AICE_TMSC"),
+		MTK_FUNCTION(7, "C2K_TDO")
+	),
+	MTK_PIN(
+		44, "GPIO44",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO44"),
+		MTK_FUNCTION(1, "DPI_D5"),
+		MTK_FUNCTION(2, "SPI2_MI_A"),
+		MTK_FUNCTION(3, "PCM1_CLK"),
+		MTK_FUNCTION(4, "I2S2_BCK"),
+		MTK_FUNCTION(5, "CONN_MCU_TCK"),
+		MTK_FUNCTION(6, "CONN_MCU_AICE_TCKC"),
+		MTK_FUNCTION(7, "C2K_RTCK")
+	),
+	MTK_PIN(
+		45, "GPIO45",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO45"),
+		MTK_FUNCTION(1, "DPI_D6"),
+		MTK_FUNCTION(2, "SPI2_CS_A"),
+		MTK_FUNCTION(3, "PCM1_DI"),
+		MTK_FUNCTION(4, "I2S2_DI"),
+		MTK_FUNCTION(5, "CONN_MCU_DBGI_N"),
+		MTK_FUNCTION(6, "MD_URXD0")
+	),
+	MTK_PIN(
+		46, "GPIO46",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO46"),
+		MTK_FUNCTION(1, "DPI_D7"),
+		MTK_FUNCTION(2, "SPI2_MO_A"),
+		MTK_FUNCTION(3, "PCM1_DO0"),
+		MTK_FUNCTION(4, "I2S1_DO"),
+		MTK_FUNCTION(5, "ANT_SEL0"),
+		MTK_FUNCTION(6, "MD_UTXD0")
+	),
+	MTK_PIN(
+		47, "GPIO47",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO47"),
+		MTK_FUNCTION(1, "DPI_D8"),
+		MTK_FUNCTION(2, "CLKM0"),
+		MTK_FUNCTION(3, "PCM1_DO1"),
+		MTK_FUNCTION(4, "I2S0_MCK"),
+		MTK_FUNCTION(5, "ANT_SEL1"),
+		MTK_FUNCTION(6, "PTA_RXD"),
+		MTK_FUNCTION(7, "C2K_URXD0")
+	),
+	MTK_PIN(
+		48, "GPIO48",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO48"),
+		MTK_FUNCTION(1, "DPI_D9"),
+		MTK_FUNCTION(2, "CLKM1"),
+		MTK_FUNCTION(3, "CMFLASH"),
+		MTK_FUNCTION(4, "I2S2_MCK"),
+		MTK_FUNCTION(5, "ANT_SEL2"),
+		MTK_FUNCTION(6, "PTA_TXD"),
+		MTK_FUNCTION(7, "C2K_UTXD0")
+	),
+	MTK_PIN(
+		49, "GPIO49",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO49"),
+		MTK_FUNCTION(1, "DPI_D10"),
+		MTK_FUNCTION(2, "MD_INT1_C2K_UIM1_HOT_PLUG_IN"),
+		MTK_FUNCTION(3, "PWM_C"),
+		MTK_FUNCTION(4, "IRTX_OUT"),
+		MTK_FUNCTION(5, "ANT_SEL3"),
+		MTK_FUNCTION(6, "MD_URXD1")
+	),
+	MTK_PIN(
+		50, "GPIO50",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO50"),
+		MTK_FUNCTION(1, "DPI_D11"),
+		MTK_FUNCTION(2, "MD_INT2"),
+		MTK_FUNCTION(3, "PWM_D"),
+		MTK_FUNCTION(4, "CLKM2"),
+		MTK_FUNCTION(5, "ANT_SEL4"),
+		MTK_FUNCTION(6, "MD_UTXD1")
+	),
+	MTK_PIN(
+		51, "GPIO51",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO51"),
+		MTK_FUNCTION(1, "DPI_DE"),
+		MTK_FUNCTION(2, "SPI4_CLK_A"),
+		MTK_FUNCTION(3, "IRTX_OUT"),
+		MTK_FUNCTION(4, "SCL0_1"),
+		MTK_FUNCTION(5, "ANT_SEL5"),
+		MTK_FUNCTION(7, "C2K_UTXD1")
+	),
+	MTK_PIN(
+		52, "GPIO52",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO52"),
+		MTK_FUNCTION(1, "DPI_CK"),
+		MTK_FUNCTION(2, "SPI4_MI_A"),
+		MTK_FUNCTION(3, "SPI4_MO_A"),
+		MTK_FUNCTION(4, "SDA0_1"),
+		MTK_FUNCTION(5, "ANT_SEL6"),
+		MTK_FUNCTION(7, "C2K_URXD1")
+	),
+	MTK_PIN(
+		53, "GPIO53",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO53"),
+		MTK_FUNCTION(1, "DPI_HSYNC"),
+		MTK_FUNCTION(2, "SPI4_CS_A"),
+		MTK_FUNCTION(3, "CMFLASH"),
+		MTK_FUNCTION(4, "SCL1_1"),
+		MTK_FUNCTION(5, "ANT_SEL7"),
+		MTK_FUNCTION(6, "MD_URXD2"),
+		MTK_FUNCTION(7, "PCC_PPC_IO")
+	),
+	MTK_PIN(
+		54, "GPIO54",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO54"),
+		MTK_FUNCTION(1, "DPI_VSYNC"),
+		MTK_FUNCTION(2, "SPI4_MO_A"),
+		MTK_FUNCTION(3, "SPI4_MI_A"),
+		MTK_FUNCTION(4, "SDA1_1"),
+		MTK_FUNCTION(5, "PWM_A"),
+		MTK_FUNCTION(6, "MD_UTXD2"),
+		MTK_FUNCTION(7, "EXT_FRAME_SYNC")
+	),
+	MTK_PIN(
+		55, "GPIO55",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO55"),
+		MTK_FUNCTION(1, "SCL1_0")
+	),
+	MTK_PIN(
+		56, "GPIO56",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO56"),
+		MTK_FUNCTION(1, "SDA1_0")
+	),
+	MTK_PIN(
+		57, "GPIO57",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO57"),
+		MTK_FUNCTION(1, "SPI0_CLK"),
+		MTK_FUNCTION(2, "SCL0_2"),
+		MTK_FUNCTION(3, "PWM_B"),
+		MTK_FUNCTION(4, "UTXD3"),
+		MTK_FUNCTION(5, "PCM0_SYNC")
+	),
+	MTK_PIN(
+		58, "GPIO58",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO58"),
+		MTK_FUNCTION(1, "SPI0_MI"),
+		MTK_FUNCTION(2, "SPI0_MO"),
+		MTK_FUNCTION(3, "SDA1_2"),
+		MTK_FUNCTION(4, "URXD3"),
+		MTK_FUNCTION(5, "PCM0_CLK")
+	),
+	MTK_PIN(
+		59, "GPIO59",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO59"),
+		MTK_FUNCTION(1, "SPI0_MO"),
+		MTK_FUNCTION(2, "SPI0_MI"),
+		MTK_FUNCTION(3, "PWM_C"),
+		MTK_FUNCTION(4, "URTS3"),
+		MTK_FUNCTION(5, "PCM0_DO")
+	),
+	MTK_PIN(
+		60, "GPIO60",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO60"),
+		MTK_FUNCTION(1, "SPI0_CS"),
+		MTK_FUNCTION(2, "SDA0_2"),
+		MTK_FUNCTION(3, "SCL1_2"),
+		MTK_FUNCTION(4, "UCTS3"),
+		MTK_FUNCTION(5, "PCM0_DI")
+	),
+	MTK_PIN(
+		61, "GPIO61",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO61"),
+		MTK_FUNCTION(1, "EINT0"),
+		MTK_FUNCTION(2, "IDDIG"),
+		MTK_FUNCTION(3, "SPI4_CLK_B"),
+		MTK_FUNCTION(4, "I2S0_LRCK"),
+		MTK_FUNCTION(5, "PCM0_SYNC"),
+		MTK_FUNCTION(7, "C2K_EINT0")
+	),
+	MTK_PIN(
+		62, "GPIO62",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO62"),
+		MTK_FUNCTION(1, "EINT1"),
+		MTK_FUNCTION(2, "USB_DRVVBUS"),
+		MTK_FUNCTION(3, "SPI4_MI_B"),
+		MTK_FUNCTION(4, "I2S0_BCK"),
+		MTK_FUNCTION(5, "PCM0_CLK"),
+		MTK_FUNCTION(7, "C2K_EINT1")
+	),
+	MTK_PIN(
+		63, "GPIO63",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO63"),
+		MTK_FUNCTION(1, "EINT2"),
+		MTK_FUNCTION(2, "IRTX_OUT"),
+		MTK_FUNCTION(3, "SPI4_MO_B"),
+		MTK_FUNCTION(4, "I2S0_MCK"),
+		MTK_FUNCTION(5, "PCM0_DI"),
+		MTK_FUNCTION(7, "C2K_DM_EINT0")
+	),
+	MTK_PIN(
+		64, "GPIO64",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO64"),
+		MTK_FUNCTION(1, "EINT3"),
+		MTK_FUNCTION(2, "CMFLASH"),
+		MTK_FUNCTION(3, "SPI4_CS_B"),
+		MTK_FUNCTION(4, "I2S0_DI"),
+		MTK_FUNCTION(5, "PCM0_DO"),
+		MTK_FUNCTION(7, "C2K_DM_EINT1")
+	),
+	MTK_PIN(
+		65, "GPIO65",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO65"),
+		MTK_FUNCTION(1, "EINT4"),
+		MTK_FUNCTION(2, "CLKM0"),
+		MTK_FUNCTION(3, "SPI5_CLK_B"),
+		MTK_FUNCTION(4, "I2S1_LRCK"),
+		MTK_FUNCTION(5, "PWM_A"),
+		MTK_FUNCTION(7, "C2K_DM_EINT2")
+	),
+	MTK_PIN(
+		66, "GPIO66",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO66"),
+		MTK_FUNCTION(1, "EINT5"),
+		MTK_FUNCTION(2, "CLKM1"),
+		MTK_FUNCTION(3, "SPI5_MI_B"),
+		MTK_FUNCTION(4, "I2S1_BCK"),
+		MTK_FUNCTION(5, "PWM_B"),
+		MTK_FUNCTION(7, "C2K_DM_EINT3")
+	),
+	MTK_PIN(
+		67, "GPIO67",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO67"),
+		MTK_FUNCTION(1, "EINT6"),
+		MTK_FUNCTION(2, "CLKM2"),
+		MTK_FUNCTION(3, "SPI5_MO_B"),
+		MTK_FUNCTION(4, "I2S1_MCK"),
+		MTK_FUNCTION(5, "PWM_C"),
+		MTK_FUNCTION(7, "DBG_MON_A0")
+	),
+	MTK_PIN(
+		68, "GPIO68",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO68"),
+		MTK_FUNCTION(1, "EINT7"),
+		MTK_FUNCTION(2, "CLKM3"),
+		MTK_FUNCTION(3, "SPI5_CS_B"),
+		MTK_FUNCTION(4, "I2S1_DO"),
+		MTK_FUNCTION(5, "PWM_D"),
+		MTK_FUNCTION(7, "DBG_MON_A1")
+	),
+	MTK_PIN(
+		69, "GPIO69",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO69"),
+		MTK_FUNCTION(1, "I2S0_LRCK"),
+		MTK_FUNCTION(2, "I2S3_LRCK"),
+		MTK_FUNCTION(3, "I2S1_LRCK"),
+		MTK_FUNCTION(4, "I2S2_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A2")
+	),
+	MTK_PIN(
+		70, "GPIO70",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO70"),
+		MTK_FUNCTION(1, "I2S0_BCK"),
+		MTK_FUNCTION(2, "I2S3_BCK"),
+		MTK_FUNCTION(3, "I2S1_BCK"),
+		MTK_FUNCTION(4, "I2S2_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A3")
+	),
+	MTK_PIN(
+		71, "GPIO71",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO71"),
+		MTK_FUNCTION(1, "I2S0_MCK"),
+		MTK_FUNCTION(2, "I2S3_MCK"),
+		MTK_FUNCTION(3, "I2S1_MCK"),
+		MTK_FUNCTION(4, "I2S2_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A4")
+	),
+	MTK_PIN(
+		72, "GPIO72",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO72"),
+		MTK_FUNCTION(1, "I2S0_DI"),
+		MTK_FUNCTION(2, "I2S0_DI"),
+		MTK_FUNCTION(3, "I2S2_DI"),
+		MTK_FUNCTION(4, "I2S2_DI"),
+		MTK_FUNCTION(7, "DBG_MON_A5")
+	),
+	MTK_PIN(
+		73, "GPIO73",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO73"),
+		MTK_FUNCTION(1, "I2S3_DO"),
+		MTK_FUNCTION(2, "I2S3_DO"),
+		MTK_FUNCTION(3, "I2S1_DO"),
+		MTK_FUNCTION(4, "I2S1_DO"),
+		MTK_FUNCTION(7, "DBG_MON_A6")
+	),
+	MTK_PIN(
+		74, "GPIO74",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO74"),
+		MTK_FUNCTION(1, "SCL3_0"),
+		MTK_FUNCTION(7, "AUXIF_CLK1")
+	),
+	MTK_PIN(
+		75, "GPIO75",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO75"),
+		MTK_FUNCTION(1, "SDA3_0"),
+		MTK_FUNCTION(7, "AUXIF_ST1")
+	),
+	MTK_PIN(
+		76, "GPIO76",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO76"),
+		MTK_FUNCTION(1, "CONN_HRST_B"),
+		MTK_FUNCTION(7, "C2K_DM_EINT0")
+	),
+	MTK_PIN(
+		77, "GPIO77",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO77"),
+		MTK_FUNCTION(1, "CONN_TOP_CLK"),
+		MTK_FUNCTION(7, "C2K_DM_EINT1")
+	),
+	MTK_PIN(
+		78, "GPIO78",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO78"),
+		MTK_FUNCTION(1, "CONN_TOP_DATA"),
+		MTK_FUNCTION(7, "C2K_DM_EINT2")
+	),
+	MTK_PIN(
+		79, "GPIO79",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO79"),
+		MTK_FUNCTION(1, "CONN_WB_PTA"),
+		MTK_FUNCTION(7, "C2K_DM_EINT3")
+	),
+	MTK_PIN(
+		80, "GPIO80",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO80"),
+		MTK_FUNCTION(1, "CONN_WF_HB0"),
+		MTK_FUNCTION(7, "C2K_EINT0")
+	),
+	MTK_PIN(
+		81, "GPIO81",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO81"),
+		MTK_FUNCTION(1, "CONN_WF_HB1"),
+		MTK_FUNCTION(7, "C2K_EINT1")
+	),
+	MTK_PIN(
+		82, "GPIO82",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO82"),
+		MTK_FUNCTION(1, "CONN_WF_HB2"),
+		MTK_FUNCTION(7, "MD_CLKM0")
+	),
+	MTK_PIN(
+		83, "GPIO83",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO83"),
+		MTK_FUNCTION(1, "CONN_BT_CLK"),
+		MTK_FUNCTION(7, "MD_CLKM1")
+	),
+	MTK_PIN(
+		84, "GPIO84",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO84"),
+		MTK_FUNCTION(1, "CONN_BT_DATA")
+	),
+	MTK_PIN(
+		85, "GPIO85",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO85"),
+		MTK_FUNCTION(1, "EINT8"),
+		MTK_FUNCTION(2, "I2S1_LRCK"),
+		MTK_FUNCTION(3, "I2S2_LRCK"),
+		MTK_FUNCTION(4, "URXD1"),
+		MTK_FUNCTION(5, "MD_URXD0"),
+		MTK_FUNCTION(7, "DBG_MON_A7")
+	),
+	MTK_PIN(
+		86, "GPIO86",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO86"),
+		MTK_FUNCTION(1, "EINT9"),
+		MTK_FUNCTION(2, "I2S1_BCK"),
+		MTK_FUNCTION(3, "I2S2_BCK"),
+		MTK_FUNCTION(4, "UTXD1"),
+		MTK_FUNCTION(5, "MD_UTXD0"),
+		MTK_FUNCTION(7, "DBG_MON_A8")
+	),
+	MTK_PIN(
+		87, "GPIO87",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO87"),
+		MTK_FUNCTION(1, "EINT10"),
+		MTK_FUNCTION(2, "I2S1_MCK"),
+		MTK_FUNCTION(3, "I2S2_MCK"),
+		MTK_FUNCTION(4, "URTS1"),
+		MTK_FUNCTION(5, "MD_URXD1"),
+		MTK_FUNCTION(7, "DBG_MON_A9")
+	),
+	MTK_PIN(
+		88, "GPIO88",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO88"),
+		MTK_FUNCTION(1, "EINT11"),
+		MTK_FUNCTION(2, "I2S1_DO"),
+		MTK_FUNCTION(3, "I2S2_DI"),
+		MTK_FUNCTION(4, "UCTS1"),
+		MTK_FUNCTION(5, "MD_UTXD1"),
+		MTK_FUNCTION(7, "DBG_MON_A10")
+	),
+	MTK_PIN(
+		89, "GPIO89",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO89"),
+		MTK_FUNCTION(1, "EINT12"),
+		MTK_FUNCTION(2, "IRTX_OUT"),
+		MTK_FUNCTION(3, "CLKM0"),
+		MTK_FUNCTION(4, "PCM1_SYNC"),
+		MTK_FUNCTION(5, "URTS0"),
+		MTK_FUNCTION(7, "DBG_MON_A11")
+	),
+	MTK_PIN(
+		90, "GPIO90",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO90"),
+		MTK_FUNCTION(1, "EINT13"),
+		MTK_FUNCTION(2, "CMFLASH"),
+		MTK_FUNCTION(3, "CLKM1"),
+		MTK_FUNCTION(4, "PCM1_CLK"),
+		MTK_FUNCTION(5, "UCTS0"),
+		MTK_FUNCTION(7, "C2K_DM_EINT0")
+	),
+	MTK_PIN(
+		91, "GPIO91",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO91"),
+		MTK_FUNCTION(1, "EINT14"),
+		MTK_FUNCTION(2, "PWM_A"),
+		MTK_FUNCTION(3, "CLKM2"),
+		MTK_FUNCTION(4, "PCM1_DI"),
+		MTK_FUNCTION(5, "SDA0_3"),
+		MTK_FUNCTION(7, "C2K_DM_EINT1")
+	),
+	MTK_PIN(
+		92, "GPIO92",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO92"),
+		MTK_FUNCTION(1, "EINT15"),
+		MTK_FUNCTION(2, "PWM_B"),
+		MTK_FUNCTION(3, "CLKM3"),
+		MTK_FUNCTION(4, "PCM1_DO0"),
+		MTK_FUNCTION(5, "SCL0_3")
+	),
+	MTK_PIN(
+		93, "GPIO93",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO93"),
+		MTK_FUNCTION(1, "EINT16"),
+		MTK_FUNCTION(2, "IDDIG"),
+		MTK_FUNCTION(3, "CLKM4"),
+		MTK_FUNCTION(4, "PCM1_DO1"),
+		MTK_FUNCTION(5, "MD_INT2"),
+		MTK_FUNCTION(7, "DROP_ZONE")
+	),
+	MTK_PIN(
+		94, "GPIO94",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO94"),
+		MTK_FUNCTION(1, "USB_DRVVBUS"),
+		MTK_FUNCTION(2, "PWM_C"),
+		MTK_FUNCTION(3, "CLKM5")
+	),
+	MTK_PIN(
+		95, "GPIO95",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO95"),
+		MTK_FUNCTION(1, "SDA2_0"),
+		MTK_FUNCTION(7, "AUXIF_ST0")
+	),
+	MTK_PIN(
+		96, "GPIO96",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO96"),
+		MTK_FUNCTION(1, "SCL2_0"),
+		MTK_FUNCTION(7, "AUXIF_CLK0")
+	),
+	MTK_PIN(
+		97, "GPIO97",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO97"),
+		MTK_FUNCTION(1, "URXD0"),
+		MTK_FUNCTION(2, "UTXD0"),
+		MTK_FUNCTION(3, "MD_URXD0"),
+		MTK_FUNCTION(4, "MD_URXD1"),
+		MTK_FUNCTION(5, "MD_URXD2"),
+		MTK_FUNCTION(6, "C2K_URXD0"),
+		MTK_FUNCTION(7, "C2K_URXD1")
+	),
+	MTK_PIN(
+		98, "GPIO98",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO98"),
+		MTK_FUNCTION(1, "UTXD0"),
+		MTK_FUNCTION(2, "URXD0"),
+		MTK_FUNCTION(3, "MD_UTXD0"),
+		MTK_FUNCTION(4, "MD_UTXD1"),
+		MTK_FUNCTION(5, "MD_UTXD2"),
+		MTK_FUNCTION(6, "C2K_UTXD0"),
+		MTK_FUNCTION(7, "C2K_UTXD1")
+	),
+	MTK_PIN(
+		99, "GPIO99",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO99"),
+		MTK_FUNCTION(1, "RTC32K_CK")
+	),
+	MTK_PIN(
+		100, "GPIO100",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO100"),
+		MTK_FUNCTION(1, "SRCLKENAI0")
+	),
+	MTK_PIN(
+		101, "GPIO101",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO101"),
+		MTK_FUNCTION(1, "SRCLKENAI1")
+	),
+	MTK_PIN(
+		102, "GPIO102",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO102"),
+		MTK_FUNCTION(1, "SRCLKENA0")
+	),
+	MTK_PIN(
+		103, "GPIO103",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO103"),
+		MTK_FUNCTION(1, "SRCLKENA1")
+	),
+	MTK_PIN(
+		104, "GPIO104",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO104"),
+		MTK_FUNCTION(1, "SYSRSTB")
+	),
+	MTK_PIN(
+		105, "GPIO105",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO105"),
+		MTK_FUNCTION(1, "WATCHDOG")
+	),
+	MTK_PIN(
+		106, "GPIO106",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO106"),
+		MTK_FUNCTION(1, "KPROW0"),
+		MTK_FUNCTION(2, "CMFLASH"),
+		MTK_FUNCTION(3, "CLKM4"),
+		MTK_FUNCTION(4, "TP_GPIO0_AO"),
+		MTK_FUNCTION(5, "IRTX_OUT")
+	),
+	MTK_PIN(
+		107, "GPIO107",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO107"),
+		MTK_FUNCTION(1, "KPROW1"),
+		MTK_FUNCTION(2, "IDDIG"),
+		MTK_FUNCTION(3, "CLKM5"),
+		MTK_FUNCTION(4, "TP_GPIO1_AO"),
+		MTK_FUNCTION(5, "I2S1_BCK"),
+		MTK_FUNCTION(7, "DAP_SIB1_SWD")
+	),
+	MTK_PIN(
+		108, "GPIO108",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO108"),
+		MTK_FUNCTION(1, "KPROW2"),
+		MTK_FUNCTION(2, "USB_DRVVBUS"),
+		MTK_FUNCTION(3, "PWM_A"),
+		MTK_FUNCTION(4, "CMFLASH"),
+		MTK_FUNCTION(5, "I2S1_LRCK"),
+		MTK_FUNCTION(7, "DAP_SIB1_SWCK")
+	),
+	MTK_PIN(
+		109, "GPIO109",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO109"),
+		MTK_FUNCTION(1, "KPCOL0")
+	),
+	MTK_PIN(
+		110, "GPIO110",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO110"),
+		MTK_FUNCTION(1, "KPCOL1"),
+		MTK_FUNCTION(2, "SDA1_3"),
+		MTK_FUNCTION(3, "PWM_B"),
+		MTK_FUNCTION(4, "CLKM0"),
+		MTK_FUNCTION(5, "I2S1_DO"),
+		MTK_FUNCTION(7, "C2K_DM_EINT3")
+	),
+	MTK_PIN(
+		111, "GPIO111",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO111"),
+		MTK_FUNCTION(1, "KPCOL2"),
+		MTK_FUNCTION(2, "SCL1_3"),
+		MTK_FUNCTION(3, "PWM_C"),
+		MTK_FUNCTION(4, "DISP_PWM"),
+		MTK_FUNCTION(5, "I2S1_MCK"),
+		MTK_FUNCTION(7, "C2K_DM_EINT2")
+	),
+	MTK_PIN(
+		112, "GPIO112",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO112"),
+		MTK_FUNCTION(1, "MD_INT1_C2K_UIM1_HOT_PLUG_IN"),
+		MTK_FUNCTION(7, "C2K_DM_EINT1")
+	),
+	MTK_PIN(
+		113, "GPIO113",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO113"),
+		MTK_FUNCTION(1, "MD_INT0_C2K_UIM0_HOT_PLUG_IN"),
+		MTK_FUNCTION(7, "C2K_DM_EINT0")
+	),
+	MTK_PIN(
+		114, "GPIO114",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO114"),
+		MTK_FUNCTION(1, "MSDC0_DAT0")
+	),
+	MTK_PIN(
+		115, "GPIO115",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO115"),
+		MTK_FUNCTION(1, "MSDC0_DAT1")
+	),
+	MTK_PIN(
+		116, "GPIO116",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO116"),
+		MTK_FUNCTION(1, "MSDC0_DAT2")
+	),
+	MTK_PIN(
+		117, "GPIO117",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO117"),
+		MTK_FUNCTION(1, "MSDC0_DAT3")
+	),
+	MTK_PIN(
+		118, "GPIO118",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO118"),
+		MTK_FUNCTION(1, "MSDC0_DAT4")
+	),
+	MTK_PIN(
+		119, "GPIO119",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO119"),
+		MTK_FUNCTION(1, "MSDC0_DAT5")
+	),
+	MTK_PIN(
+		120, "GPIO120",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO120"),
+		MTK_FUNCTION(1, "MSDC0_DAT6")
+	),
+	MTK_PIN(
+		121, "GPIO121",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO121"),
+		MTK_FUNCTION(1, "MSDC0_DAT7")
+	),
+	MTK_PIN(
+		122, "GPIO122",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO122"),
+		MTK_FUNCTION(1, "MSDC0_CMD")
+	),
+	MTK_PIN(
+		123, "GPIO123",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO123"),
+		MTK_FUNCTION(1, "MSDC0_CLK")
+	),
+	MTK_PIN(
+		124, "GPIO124",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO124"),
+		MTK_FUNCTION(1, "MSDC0_DSL")
+	),
+	MTK_PIN(
+		125, "GPIO125",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO125"),
+		MTK_FUNCTION(1, "MSDC0_RSTB")
+	),
+	MTK_PIN(
+		126, "GPIO126",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO126"),
+		MTK_FUNCTION(1, "MD1_SIM1_SCLK"),
+		MTK_FUNCTION(2, "MD1_SIM2_SCLK"),
+		MTK_FUNCTION(3, "C2K_UIM0_CLK"),
+		MTK_FUNCTION(4, "C2K_UIM1_CLK")
+	),
+	MTK_PIN(
+		127, "GPIO127",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO127"),
+		MTK_FUNCTION(1, "MD1_SIM1_SRST"),
+		MTK_FUNCTION(2, "MD1_SIM2_SRST"),
+		MTK_FUNCTION(3, "C2K_UIM0_RST"),
+		MTK_FUNCTION(4, "C2K_UIM1_RST")
+	),
+	MTK_PIN(
+		128, "GPIO128",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO128"),
+		MTK_FUNCTION(1, "MD1_SIM1_SIO"),
+		MTK_FUNCTION(2, "MD1_SIM2_SIO"),
+		MTK_FUNCTION(3, "C2K_UIM0_IO"),
+		MTK_FUNCTION(4, "C2K_UIM1_IO")
+	),
+	MTK_PIN(
+		129, "GPIO129",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO129"),
+		MTK_FUNCTION(1, "MSDC1_CMD"),
+		MTK_FUNCTION(2, "CONN_DSP_JMS"),
+		MTK_FUNCTION(3, "LTE_JTAG_TMS"),
+		MTK_FUNCTION(4, "UDI_TMS"),
+		MTK_FUNCTION(5, "C2K_TMS")
+	),
+	MTK_PIN(
+		130, "GPIO130",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO130"),
+		MTK_FUNCTION(1, "MSDC1_DAT0"),
+		MTK_FUNCTION(2, "CONN_DSP_JDI"),
+		MTK_FUNCTION(3, "LTE_JTAG_TDI"),
+		MTK_FUNCTION(4, "UDI_TDI"),
+		MTK_FUNCTION(5, "C2K_TDI")
+	),
+	MTK_PIN(
+		131, "GPIO131",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO131"),
+		MTK_FUNCTION(1, "MSDC1_DAT1"),
+		MTK_FUNCTION(2, "CONN_DSP_JDO"),
+		MTK_FUNCTION(3, "LTE_JTAG_TDO"),
+		MTK_FUNCTION(4, "UDI_TDO"),
+		MTK_FUNCTION(5, "C2K_TDO")
+	),
+	MTK_PIN(
+		132, "GPIO132",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO132"),
+		MTK_FUNCTION(1, "MSDC1_DAT2"),
+		MTK_FUNCTION(5, "C2K_RTCK")
+	),
+	MTK_PIN(
+		133, "GPIO133",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO133"),
+		MTK_FUNCTION(1, "MSDC1_DAT3"),
+		MTK_FUNCTION(2, "CONN_DSP_JINTP"),
+		MTK_FUNCTION(3, "LTE_JTAG_TRSTN"),
+		MTK_FUNCTION(4, "UDI_NTRST"),
+		MTK_FUNCTION(5, "C2K_NTRST")
+	),
+	MTK_PIN(
+		134, "GPIO134",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO134"),
+		MTK_FUNCTION(1, "MSDC1_CLK"),
+		MTK_FUNCTION(2, "CONN_DSP_JCK"),
+		MTK_FUNCTION(3, "LTE_JTAG_TCK"),
+		MTK_FUNCTION(4, "UDI_TCK_XI"),
+		MTK_FUNCTION(5, "C2K_TCK")
+	),
+	MTK_PIN(
+		135, "GPIO135",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO135"),
+		MTK_FUNCTION(1, "TDM_LRCK"),
+		MTK_FUNCTION(2, "I2S0_LRCK"),
+		MTK_FUNCTION(3, "CLKM0"),
+		MTK_FUNCTION(4, "PCM1_SYNC"),
+		MTK_FUNCTION(5, "PWM_A"),
+		MTK_FUNCTION(7, "DBG_MON_A12")
+	),
+	MTK_PIN(
+		136, "GPIO136",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO136"),
+		MTK_FUNCTION(1, "TDM_BCK"),
+		MTK_FUNCTION(2, "I2S0_BCK"),
+		MTK_FUNCTION(3, "CLKM1"),
+		MTK_FUNCTION(4, "PCM1_CLK"),
+		MTK_FUNCTION(5, "PWM_B"),
+		MTK_FUNCTION(7, "DBG_MON_A13")
+	),
+	MTK_PIN(
+		137, "GPIO137",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO137"),
+		MTK_FUNCTION(1, "TDM_MCK"),
+		MTK_FUNCTION(2, "I2S0_MCK"),
+		MTK_FUNCTION(3, "CLKM2"),
+		MTK_FUNCTION(4, "PCM1_DI"),
+		MTK_FUNCTION(5, "IRTX_OUT"),
+		MTK_FUNCTION(7, "DBG_MON_A14")
+	),
+	MTK_PIN(
+		138, "GPIO138",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO138"),
+		MTK_FUNCTION(1, "TDM_DATA0"),
+		MTK_FUNCTION(2, "I2S0_DI"),
+		MTK_FUNCTION(3, "CLKM3"),
+		MTK_FUNCTION(4, "PCM1_DO0"),
+		MTK_FUNCTION(5, "PWM_C"),
+		MTK_FUNCTION(6, "SDA3_1"),
+		MTK_FUNCTION(7, "DBG_MON_A15")
+	),
+	MTK_PIN(
+		139, "GPIO139",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO139"),
+		MTK_FUNCTION(1, "TDM_DATA1"),
+		MTK_FUNCTION(2, "I2S3_DO"),
+		MTK_FUNCTION(3, "CLKM4"),
+		MTK_FUNCTION(4, "PCM1_DO1"),
+		MTK_FUNCTION(5, "ANT_SEL2"),
+		MTK_FUNCTION(6, "SCL3_1"),
+		MTK_FUNCTION(7, "DBG_MON_A16")
+	),
+	MTK_PIN(
+		140, "GPIO140",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO140"),
+		MTK_FUNCTION(1, "TDM_DATA2"),
+		MTK_FUNCTION(2, "DISP_PWM"),
+		MTK_FUNCTION(3, "CLKM5"),
+		MTK_FUNCTION(4, "SDA1_4"),
+		MTK_FUNCTION(5, "ANT_SEL1"),
+		MTK_FUNCTION(6, "URXD3"),
+		MTK_FUNCTION(7, "DBG_MON_A17")
+	),
+	MTK_PIN(
+		141, "GPIO141",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO141"),
+		MTK_FUNCTION(1, "TDM_DATA3"),
+		MTK_FUNCTION(2, "CMFLASH"),
+		MTK_FUNCTION(3, "IRTX_OUT"),
+		MTK_FUNCTION(4, "SCL1_4"),
+		MTK_FUNCTION(5, "ANT_SEL0"),
+		MTK_FUNCTION(6, "UTXD3"),
+		MTK_FUNCTION(7, "DBG_MON_A18")
+	),
+	MTK_PIN(
+		142, "GPIO142",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO142"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_MI"),
+		MTK_FUNCTION(2, "PWRAP_SPI0_MO")
+	),
+	MTK_PIN(
+		143, "GPIO143",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO143"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_MO"),
+		MTK_FUNCTION(2, "PWRAP_SPI0_MI")
+	),
+	MTK_PIN(
+		144, "GPIO144",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO144"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_CK")
+	),
+	MTK_PIN(
+		145, "GPIO145",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO145"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_CSN")
+	),
+	MTK_PIN(
+		146, "GPIO146",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO146"),
+		MTK_FUNCTION(1, "AUD_CLK_MOSI")
+	),
+	MTK_PIN(
+		147, "GPIO147",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO147"),
+		MTK_FUNCTION(1, "AUD_DAT_MISO"),
+		MTK_FUNCTION(2, "AUD_DAT_MOSI"),
+		MTK_FUNCTION(3, "VOW_DAT_MISO")
+	),
+	MTK_PIN(
+		148, "GPIO148",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO148"),
+		MTK_FUNCTION(1, "AUD_DAT_MOSI"),
+		MTK_FUNCTION(2, "AUD_DAT_MISO")
+	),
+	MTK_PIN(
+		149, "GPIO149",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO149"),
+		MTK_FUNCTION(1, "VOW_CLK_MISO")
+	),
+	MTK_PIN(
+		150, "GPIO150",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO150"),
+		MTK_FUNCTION(1, "ANC_DAT_MOSI")
+	),
+	MTK_PIN(
+		151, "GPIO151",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO151"),
+		MTK_FUNCTION(1, "SCL6_0")
+	),
+	MTK_PIN(
+		152, "GPIO152",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO152"),
+		MTK_FUNCTION(1, "SDA6_0")
+	),
+	MTK_PIN(
+		153, "GPIO153",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO153"),
+		MTK_FUNCTION(1, "SCL7_0")
+	),
+	MTK_PIN(
+		154, "GPIO154",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO154"),
+		MTK_FUNCTION(1, "SDA7_0")
+	),
+	MTK_PIN(
+		155, "GPIO155",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO155"),
+		MTK_FUNCTION(1, "MD1_SIM2_SCLK"),
+		MTK_FUNCTION(2, "MD1_SIM1_SCLK"),
+		MTK_FUNCTION(3, "C2K_UIM0_CLK"),
+		MTK_FUNCTION(4, "C2K_UIM1_CLK")
+	),
+	MTK_PIN(
+		156, "GPIO156",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO156"),
+		MTK_FUNCTION(1, "MD1_SIM2_SRST"),
+		MTK_FUNCTION(2, "MD1_SIM1_SRST"),
+		MTK_FUNCTION(3, "C2K_UIM0_RST"),
+		MTK_FUNCTION(4, "C2K_UIM1_RST")
+	),
+	MTK_PIN(
+		157, "GPIO157",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO157"),
+		MTK_FUNCTION(1, "MD1_SIM2_SIO"),
+		MTK_FUNCTION(2, "MD1_SIM1_SIO"),
+		MTK_FUNCTION(3, "C2K_UIM0_IO"),
+		MTK_FUNCTION(4, "C2K_UIM1_IO")
+	),
+	MTK_PIN(
+		158, "GPIO158",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO158"),
+		MTK_FUNCTION(1, "MIPI_TDP0")
+	),
+	MTK_PIN(
+		159, "GPIO159",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO159"),
+		MTK_FUNCTION(1, "MIPI_TDN0")
+	),
+	MTK_PIN(
+		160, "GPIO160",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO160"),
+		MTK_FUNCTION(1, "MIPI_TDP1")
+	),
+	MTK_PIN(
+		161, "GPIO161",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO161"),
+		MTK_FUNCTION(1, "MIPI_TDN1")
+	),
+	MTK_PIN(
+		162, "GPIO162",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO162"),
+		MTK_FUNCTION(1, "MIPI_TCP")
+	),
+	MTK_PIN(
+		163, "GPIO163",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO163"),
+		MTK_FUNCTION(1, "MIPI_TCN")
+	),
+	MTK_PIN(
+		164, "GPIO164",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO164"),
+		MTK_FUNCTION(1, "MIPI_TDP2")
+	),
+	MTK_PIN(
+		165, "GPIO165",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO165"),
+		MTK_FUNCTION(1, "MIPI_TDN2")
+	),
+	MTK_PIN(
+		166, "GPIO166",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO166"),
+		MTK_FUNCTION(1, "MIPI_TDP3")
+	),
+	MTK_PIN(
+		167, "GPIO167",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO167"),
+		MTK_FUNCTION(1, "MIPI_TDN3")
+	),
+	MTK_PIN(
+		168, "GPIO168",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO168"),
+		MTK_FUNCTION(1, "MIPI_TDP0_A")
+	),
+	MTK_PIN(
+		169, "GPIO169",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO169"),
+		MTK_FUNCTION(1, "MIPI_TDN0_A")
+	),
+	MTK_PIN(
+		170, "GPIO170",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO170"),
+		MTK_FUNCTION(1, "MIPI_TDP1_A")
+	),
+	MTK_PIN(
+		171, "GPIO171",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO171"),
+		MTK_FUNCTION(1, "MIPI_TDN1_A")
+	),
+	MTK_PIN(
+		172, "GPIO172",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO172"),
+		MTK_FUNCTION(1, "MIPI_TCP_A")
+	),
+	MTK_PIN(
+		173, "GPIO173",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO173"),
+		MTK_FUNCTION(1, "MIPI_TCN_A")
+	),
+	MTK_PIN(
+		174, "GPIO174",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO174"),
+		MTK_FUNCTION(1, "MIPI_TDP2_A")
+	),
+	MTK_PIN(
+		175, "GPIO175",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO175"),
+		MTK_FUNCTION(1, "MIPI_TDN2_A")
+	),
+	MTK_PIN(
+		176, "GPIO176",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO176"),
+		MTK_FUNCTION(1, "MIPI_TDP3_A")
+	),
+	MTK_PIN(
+		177, "GPIO177",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO177"),
+		MTK_FUNCTION(1, "MIPI_TDN3_A")
+	),
+	MTK_PIN(
+		178, "GPIO178",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO178"),
+		MTK_FUNCTION(1, "DISP_PWM"),
+		MTK_FUNCTION(2, "PWM_D"),
+		MTK_FUNCTION(3, "CLKM5"),
+		MTK_FUNCTION(7, "DBG_MON_A19")
+	),
+	MTK_PIN(
+		179, "GPIO179",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO179"),
+		MTK_FUNCTION(1, "DSI_TE0"),
+		MTK_FUNCTION(7, "DBG_MON_A20")
+	),
+	MTK_PIN(
+		180, "GPIO180",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO180"),
+		MTK_FUNCTION(1, "LCM_RST"),
+		MTK_FUNCTION(2, "DSI_TE1"),
+		MTK_FUNCTION(7, "DBG_MON_A21")
+	),
+	MTK_PIN(
+		181, "GPIO181",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO181"),
+		MTK_FUNCTION(1, "IDDIG"),
+		MTK_FUNCTION(2, "DSI_TE1"),
+		MTK_FUNCTION(7, "DBG_MON_A22")
+	),
+	MTK_PIN(
+		182, "GPIO182",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO182"),
+		MTK_FUNCTION(1, "TESTMODE")
+	),
+	MTK_PIN(
+		183, "GPIO183",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO183"),
+		MTK_FUNCTION(1, "RFIC0_BSI_CK"),
+		MTK_FUNCTION(2, "SPM_BSI_CK"),
+		MTK_FUNCTION(7, "DBG_MON_B27")
+	),
+	MTK_PIN(
+		184, "GPIO184",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO184"),
+		MTK_FUNCTION(1, "RFIC0_BSI_EN"),
+		MTK_FUNCTION(2, "SPM_BSI_EN"),
+		MTK_FUNCTION(7, "DBG_MON_B28")
+	),
+	MTK_PIN(
+		185, "GPIO185",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO185"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D0"),
+		MTK_FUNCTION(2, "SPM_BSI_D0"),
+		MTK_FUNCTION(7, "DBG_MON_B29")
+	),
+	MTK_PIN(
+		186, "GPIO186",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO186"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D1"),
+		MTK_FUNCTION(2, "SPM_BSI_D1"),
+		MTK_FUNCTION(7, "DBG_MON_B30")
+	),
+	MTK_PIN(
+		187, "GPIO187",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO187"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D2"),
+		MTK_FUNCTION(2, "SPM_BSI_D2"),
+		MTK_FUNCTION(7, "DBG_MON_B31")
+	),
+	MTK_PIN(
+		188, "GPIO188",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO188"),
+		MTK_FUNCTION(1, "MIPI0_SCLK"),
+		MTK_FUNCTION(7, "DBG_MON_B32")
+	),
+	MTK_PIN(
+		189, "GPIO189",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO189"),
+		MTK_FUNCTION(1, "MIPI0_SDATA")
+	),
+	MTK_PIN(
+		190, "GPIO190",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO190"),
+		MTK_FUNCTION(1, "MIPI1_SCLK")
+	),
+	MTK_PIN(
+		191, "GPIO191",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO191"),
+		MTK_FUNCTION(1, "MIPI1_SDATA")
+	),
+	MTK_PIN(
+		192, "GPIO192",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO192"),
+		MTK_FUNCTION(1, "BPI_BUS4")
+	),
+	MTK_PIN(
+		193, "GPIO193",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO193"),
+		MTK_FUNCTION(1, "BPI_BUS5"),
+		MTK_FUNCTION(7, "DBG_MON_B0")
+	),
+	MTK_PIN(
+		194, "GPIO194",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO194"),
+		MTK_FUNCTION(1, "BPI_BUS6"),
+		MTK_FUNCTION(7, "DBG_MON_B1")
+	),
+	MTK_PIN(
+		195, "GPIO195",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO195"),
+		MTK_FUNCTION(1, "BPI_BUS7"),
+		MTK_FUNCTION(7, "DBG_MON_B2")
+	),
+	MTK_PIN(
+		196, "GPIO196",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO196"),
+		MTK_FUNCTION(1, "BPI_BUS8"),
+		MTK_FUNCTION(7, "DBG_MON_B3")
+	),
+	MTK_PIN(
+		197, "GPIO197",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO197"),
+		MTK_FUNCTION(1, "BPI_BUS9"),
+		MTK_FUNCTION(7, "DBG_MON_B4")
+	),
+	MTK_PIN(
+		198, "GPIO198",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO198"),
+		MTK_FUNCTION(1, "BPI_BUS10"),
+		MTK_FUNCTION(7, "DBG_MON_B5")
+	),
+	MTK_PIN(
+		199, "GPIO199",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO199"),
+		MTK_FUNCTION(1, "BPI_BUS11"),
+		MTK_FUNCTION(7, "DBG_MON_B6")
+	),
+	MTK_PIN(
+		200, "GPIO200",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO200"),
+		MTK_FUNCTION(1, "BPI_BUS12"),
+		MTK_FUNCTION(7, "DBG_MON_B7")
+	),
+	MTK_PIN(
+		201, "GPIO201",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO201"),
+		MTK_FUNCTION(1, "BPI_BUS13"),
+		MTK_FUNCTION(7, "DBG_MON_B8")
+	),
+	MTK_PIN(
+		202, "GPIO202",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO202"),
+		MTK_FUNCTION(1, "BPI_BUS14"),
+		MTK_FUNCTION(7, "DBG_MON_B9")
+	),
+	MTK_PIN(
+		203, "GPIO203",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO203"),
+		MTK_FUNCTION(1, "BPI_BUS15"),
+		MTK_FUNCTION(7, "DBG_MON_B10")
+	),
+	MTK_PIN(
+		204, "GPIO204",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO204"),
+		MTK_FUNCTION(1, "BPI_BUS16"),
+		MTK_FUNCTION(2, "PA_VM0"),
+		MTK_FUNCTION(7, "DBG_MON_B11")
+	),
+	MTK_PIN(
+		205, "GPIO205",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO205"),
+		MTK_FUNCTION(1, "BPI_BUS17"),
+		MTK_FUNCTION(2, "PA_VM1"),
+		MTK_FUNCTION(7, "DBG_MON_B12")
+	),
+	MTK_PIN(
+		206, "GPIO206",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO206"),
+		MTK_FUNCTION(1, "BPI_BUS18"),
+		MTK_FUNCTION(2, "TX_SWAP0"),
+		MTK_FUNCTION(7, "DBG_MON_B13")
+	),
+	MTK_PIN(
+		207, "GPIO207",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO207"),
+		MTK_FUNCTION(1, "BPI_BUS19"),
+		MTK_FUNCTION(2, "TX_SWAP1"),
+		MTK_FUNCTION(7, "DBG_MON_B14")
+	),
+	MTK_PIN(
+		208, "GPIO208",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO208"),
+		MTK_FUNCTION(1, "BPI_BUS20"),
+		MTK_FUNCTION(2, "TX_SWAP2"),
+		MTK_FUNCTION(7, "DBG_MON_B15")
+	),
+	MTK_PIN(
+		209, "GPIO209",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO209"),
+		MTK_FUNCTION(1, "BPI_BUS21"),
+		MTK_FUNCTION(2, "TX_SWAP3"),
+		MTK_FUNCTION(7, "DBG_MON_B16")
+	),
+	MTK_PIN(
+		210, "GPIO210",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO210"),
+		MTK_FUNCTION(1, "BPI_BUS22"),
+		MTK_FUNCTION(2, "DET_BPI0"),
+		MTK_FUNCTION(7, "DBG_MON_B17")
+	),
+	MTK_PIN(
+		211, "GPIO211",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO211"),
+		MTK_FUNCTION(1, "BPI_BUS23"),
+		MTK_FUNCTION(2, "DET_BPI1"),
+		MTK_FUNCTION(7, "DBG_MON_B18")
+	),
+	MTK_PIN(
+		212, "GPIO212",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO212"),
+		MTK_FUNCTION(1, "BPI_BUS0"),
+		MTK_FUNCTION(7, "DBG_MON_B19")
+	),
+	MTK_PIN(
+		213, "GPIO213",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO213"),
+		MTK_FUNCTION(1, "BPI_BUS1"),
+		MTK_FUNCTION(7, "DBG_MON_B20")
+	),
+	MTK_PIN(
+		214, "GPIO214",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO214"),
+		MTK_FUNCTION(1, "BPI_BUS2"),
+		MTK_FUNCTION(7, "DBG_MON_B21")
+	),
+	MTK_PIN(
+		215, "GPIO215",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO215"),
+		MTK_FUNCTION(1, "BPI_BUS3"),
+		MTK_FUNCTION(7, "DBG_MON_B22")
+	),
+	MTK_PIN(
+		216, "GPIO216",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO216"),
+		MTK_FUNCTION(1, "MIPI2_SCLK"),
+		MTK_FUNCTION(7, "DBG_MON_B23")
+	),
+	MTK_PIN(
+		217, "GPIO217",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO217"),
+		MTK_FUNCTION(1, "MIPI2_SDATA"),
+		MTK_FUNCTION(7, "DBG_MON_B24")
+	),
+	MTK_PIN(
+		218, "GPIO218",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO218"),
+		MTK_FUNCTION(1, "MIPI3_SCLK"),
+		MTK_FUNCTION(7, "DBG_MON_B25")
+	),
+	MTK_PIN(
+		219, "GPIO219",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO219"),
+		MTK_FUNCTION(1, "MIPI3_SDATA"),
+		MTK_FUNCTION(7, "DBG_MON_B26")
+	),
+	MTK_PIN(
+		220, "GPIO220",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO220"),
+		MTK_FUNCTION(1, "CONN_WF_IP")
+	),
+	MTK_PIN(
+		221, "GPIO221",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO221"),
+		MTK_FUNCTION(1, "CONN_WF_IN")
+	),
+	MTK_PIN(
+		222, "GPIO222",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO222"),
+		MTK_FUNCTION(1, "CONN_WF_QP")
+	),
+	MTK_PIN(
+		223, "GPIO223",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO223"),
+		MTK_FUNCTION(1, "CONN_WF_QN")
+	),
+	MTK_PIN(
+		224, "GPIO224",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO224"),
+		MTK_FUNCTION(1, "CONN_BT_IP")
+	),
+	MTK_PIN(
+		225, "GPIO225",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO225"),
+		MTK_FUNCTION(1, "CONN_BT_IN")
+	),
+	MTK_PIN(
+		226, "GPIO226",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO226"),
+		MTK_FUNCTION(1, "CONN_BT_QP")
+	),
+	MTK_PIN(
+		227, "GPIO227",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO227"),
+		MTK_FUNCTION(1, "CONN_BT_QN")
+	),
+	MTK_PIN(
+		228, "GPIO228",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO228"),
+		MTK_FUNCTION(1, "CONN_GPS_IP")
+	),
+	MTK_PIN(
+		229, "GPIO229",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO229"),
+		MTK_FUNCTION(1, "CONN_GPS_IN")
+	),
+	MTK_PIN(
+		230, "GPIO230",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO230"),
+		MTK_FUNCTION(1, "CONN_GPS_QP")
+	),
+	MTK_PIN(
+		231, "GPIO231",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO231"),
+		MTK_FUNCTION(1, "CONN_GPS_QN")
+	),
+	MTK_PIN(
+		232, "GPIO232",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO232"),
+		MTK_FUNCTION(1, "URXD1"),
+		MTK_FUNCTION(2, "UTXD1"),
+		MTK_FUNCTION(3, "MD_URXD0"),
+		MTK_FUNCTION(4, "MD_URXD1"),
+		MTK_FUNCTION(5, "MD_URXD2"),
+		MTK_FUNCTION(6, "C2K_URXD0"),
+		MTK_FUNCTION(7, "C2K_URXD1")
+	),
+	MTK_PIN(
+		233, "GPIO233",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO233"),
+		MTK_FUNCTION(1, "UTXD1"),
+		MTK_FUNCTION(2, "URXD1"),
+		MTK_FUNCTION(3, "MD_UTXD0"),
+		MTK_FUNCTION(4, "MD_UTXD1"),
+		MTK_FUNCTION(5, "MD_UTXD2"),
+		MTK_FUNCTION(6, "C2K_UTXD0"),
+		MTK_FUNCTION(7, "C2K_UTXD1")
+	),
+	MTK_PIN(
+		234, "GPIO234",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO234"),
+		MTK_FUNCTION(1, "SPI1_CLK_B"),
+		MTK_FUNCTION(2, "TP_UTXD1_AO"),
+		MTK_FUNCTION(3, "SCL4_1"),
+		MTK_FUNCTION(4, "UTXD0"),
+		MTK_FUNCTION(6, "PWM_A"),
+		MTK_FUNCTION(7, "DBG_MON_A23")
+	),
+	MTK_PIN(
+		235, "GPIO235",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO235"),
+		MTK_FUNCTION(1, "SPI1_MI_B"),
+		MTK_FUNCTION(2, "SPI1_MO_B"),
+		MTK_FUNCTION(3, "SDA4_1"),
+		MTK_FUNCTION(4, "URXD0"),
+		MTK_FUNCTION(6, "CLKM0"),
+		MTK_FUNCTION(7, "DBG_MON_A24")
+	),
+	MTK_PIN(
+		236, "GPIO236",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO236"),
+		MTK_FUNCTION(1, "SPI1_MO_B"),
+		MTK_FUNCTION(2, "SPI1_MI_B"),
+		MTK_FUNCTION(3, "SCL5_1"),
+		MTK_FUNCTION(4, "URTS0"),
+		MTK_FUNCTION(6, "PWM_B"),
+		MTK_FUNCTION(7, "DBG_MON_A25")
+	),
+	MTK_PIN(
+		237, "GPIO237",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO237"),
+		MTK_FUNCTION(1, "SPI1_CS_B"),
+		MTK_FUNCTION(2, "TP_URXD1_AO"),
+		MTK_FUNCTION(3, "SDA5_1"),
+		MTK_FUNCTION(4, "UCTS0"),
+		MTK_FUNCTION(6, "CLKM1"),
+		MTK_FUNCTION(7, "DBG_MON_A26")
+	),
+	MTK_PIN(
+		238, "GPIO238",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO238"),
+		MTK_FUNCTION(1, "SDA4_0")
+	),
+	MTK_PIN(
+		239, "GPIO239",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO239"),
+		MTK_FUNCTION(1, "SCL4_0")
+	),
+	MTK_PIN(
+		240, "GPIO240",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO240"),
+		MTK_FUNCTION(1, "SDA5_0")
+	),
+	MTK_PIN(
+		241, "GPIO241",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+				MTK_FUNCTION(0, "GPIO241"),
+		MTK_FUNCTION(1, "SCL5_0")
+	),
+	MTK_PIN(
+		242, "GPIO242",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO242"),
+		MTK_FUNCTION(1, "SPI2_CLK_B"),
+		MTK_FUNCTION(2, "TP_UTXD2_AO"),
+		MTK_FUNCTION(3, "SCL4_2"),
+		MTK_FUNCTION(4, "UTXD1"),
+		MTK_FUNCTION(5, "URTS3"),
+		MTK_FUNCTION(6, "PWM_C"),
+		MTK_FUNCTION(7, "DBG_MON_A27")
+	),
+	MTK_PIN(
+		243, "GPIO243",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO243"),
+		MTK_FUNCTION(1, "SPI2_MI_B"),
+		MTK_FUNCTION(2, "SPI2_MO_B"),
+		MTK_FUNCTION(3, "SDA4_2"),
+		MTK_FUNCTION(4, "URXD1"),
+		MTK_FUNCTION(5, "UCTS3"),
+		MTK_FUNCTION(6, "CLKM2"),
+		MTK_FUNCTION(7, "DBG_MON_A28")
+	),
+	MTK_PIN(
+		244, "GPIO244",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO244"),
+		MTK_FUNCTION(1, "SPI2_MO_B"),
+		MTK_FUNCTION(2, "SPI2_MI_B"),
+		MTK_FUNCTION(3, "SCL5_2"),
+		MTK_FUNCTION(4, "URTS1"),
+		MTK_FUNCTION(5, "UTXD3"),
+		MTK_FUNCTION(6, "PWM_D"),
+		MTK_FUNCTION(7, "DBG_MON_A29")
+	),
+	MTK_PIN(
+		245, "GPIO245",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO245"),
+		MTK_FUNCTION(1, "SPI2_CS_B"),
+		MTK_FUNCTION(2, "TP_URXD2_AO"),
+		MTK_FUNCTION(3, "SDA5_2"),
+		MTK_FUNCTION(4, "UCTS1"),
+		MTK_FUNCTION(5, "URXD3"),
+		MTK_FUNCTION(6, "CLKM3"),
+		MTK_FUNCTION(7, "DBG_MON_A30")
+	),
+	MTK_PIN(
+		246, "GPIO246",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO246"),
+		MTK_FUNCTION(1, "I2S1_LRCK"),
+		MTK_FUNCTION(2, "I2S2_LRCK"),
+		MTK_FUNCTION(3, "I2S0_LRCK"),
+		MTK_FUNCTION(4, "I2S3_LRCK"),
+		MTK_FUNCTION(5, "PCM0_SYNC"),
+		MTK_FUNCTION(6, "SPI5_CLK_C"),
+		MTK_FUNCTION(7, "DBG_MON_A31")
+	),
+	MTK_PIN(
+		247, "GPIO247",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO247"),
+		MTK_FUNCTION(1, "I2S1_BCK"),
+		MTK_FUNCTION(2, "I2S2_BCK"),
+		MTK_FUNCTION(3, "I2S0_BCK"),
+		MTK_FUNCTION(4, "I2S3_BCK"),
+		MTK_FUNCTION(5, "PCM0_CLK"),
+		MTK_FUNCTION(6, "SPI5_MI_C"),
+		MTK_FUNCTION(7, "DBG_MON_A32")
+	),
+	MTK_PIN(
+		248, "GPIO248",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO248"),
+		MTK_FUNCTION(1, "I2S2_DI"),
+		MTK_FUNCTION(2, "I2S2_DI"),
+		MTK_FUNCTION(3, "I2S0_DI"),
+		MTK_FUNCTION(4, "I2S0_DI"),
+		MTK_FUNCTION(5, "PCM0_DI"),
+		MTK_FUNCTION(6, "SPI5_CS_C")
+	),
+	MTK_PIN(
+		249, "GPIO249",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO249"),
+		MTK_FUNCTION(1, "I2S1_DO"),
+		MTK_FUNCTION(2, "I2S1_DO"),
+		MTK_FUNCTION(3, "I2S3_DO"),
+		MTK_FUNCTION(4, "I2S3_DO"),
+		MTK_FUNCTION(5, "PCM0_DO"),
+		MTK_FUNCTION(6, "SPI5_MO_C"),
+		MTK_FUNCTION(7, "TRAP_SRAM_PWR_BYPASS")
+	),
+	MTK_PIN(
+		250, "GPIO250",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO250"),
+		MTK_FUNCTION(1, "SPI3_MI"),
+		MTK_FUNCTION(2, "SPI3_MO"),
+		MTK_FUNCTION(3, "IRTX_OUT"),
+		MTK_FUNCTION(6, "TP_URXD1_AO"),
+		MTK_FUNCTION(7, "DROP_ZONE")
+	),
+	MTK_PIN(
+		251, "GPIO251",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO251"),
+		MTK_FUNCTION(1, "SPI3_MO"),
+		MTK_FUNCTION(2, "SPI3_MI"),
+		MTK_FUNCTION(3, "CMFLASH"),
+		MTK_FUNCTION(6, "TP_UTXD1_AO"),
+		MTK_FUNCTION(7, "C2K_RTCK")
+	),
+	MTK_PIN(
+		252, "GPIO252",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO252"),
+		MTK_FUNCTION(1, "SPI3_CLK"),
+		MTK_FUNCTION(2, "SCL0_4"),
+		MTK_FUNCTION(3, "PWM_D"),
+		MTK_FUNCTION(7, "C2K_TMS")
+	),
+	MTK_PIN(
+		253, "GPIO253",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO253"),
+		MTK_FUNCTION(1, "SPI3_CS"),
+		MTK_FUNCTION(2, "SDA0_4"),
+		MTK_FUNCTION(3, "PWM_A"),
+		MTK_FUNCTION(7, "C2K_TCK")
+	),
+	MTK_PIN(
+		254, "GPIO254",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO254"),
+		MTK_FUNCTION(1, "I2S1_MCK"),
+		MTK_FUNCTION(2, "I2S2_MCK"),
+		MTK_FUNCTION(3, "I2S0_MCK"),
+		MTK_FUNCTION(4, "I2S3_MCK"),
+		MTK_FUNCTION(5, "CLKM0"),
+		MTK_FUNCTION(7, "C2K_TDI")
+	),
+	MTK_PIN(
+		255, "GPIO255",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO255"),
+		MTK_FUNCTION(1, "CLKM1"),
+		MTK_FUNCTION(2, "DISP_PWM"),
+		MTK_FUNCTION(3, "PWM_B"),
+		MTK_FUNCTION(6, "TP_GPIO1_AO"),
+		MTK_FUNCTION(7, "C2K_TDO")
+	),
+	MTK_PIN(
+		256, "GPIO256",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO256"),
+		MTK_FUNCTION(1, "CLKM2"),
+		MTK_FUNCTION(2, "IRTX_OUT"),
+		MTK_FUNCTION(3, "PWM_C"),
+		MTK_FUNCTION(6, "TP_GPIO0_AO"),
+		MTK_FUNCTION(7, "C2K_NTRST")
+	),
+	MTK_PIN(
+		257, "GPIO257",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO257"),
+		MTK_FUNCTION(1, "IO_JTAG_TMS"),
+		MTK_FUNCTION(2, "LTE_JTAG_TMS"),
+		MTK_FUNCTION(3, "DFD_TMS"),
+		MTK_FUNCTION(4, "DAP_SIB1_SWD"),
+		MTK_FUNCTION(5, "ANC_JTAG_TMS"),
+		MTK_FUNCTION(6, "SCP_JTAG_TMS"),
+		MTK_FUNCTION(7, "C2K_DM_OTMS")
+	),
+	MTK_PIN(
+		258, "GPIO258",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO258"),
+		MTK_FUNCTION(1, "IO_JTAG_TCK"),
+		MTK_FUNCTION(2, "LTE_JTAG_TCK"),
+		MTK_FUNCTION(3, "DFD_TCK_XI"),
+		MTK_FUNCTION(4, "DAP_SIB1_SWCK"),
+		MTK_FUNCTION(5, "ANC_JTAG_TCK"),
+		MTK_FUNCTION(6, "SCP_JTAG_TCK"),
+		MTK_FUNCTION(7, "C2K_DM_OTCK")
+	),
+	MTK_PIN(
+		259, "GPIO259",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO259"),
+		MTK_FUNCTION(1, "IO_JTAG_TDI"),
+		MTK_FUNCTION(2, "LTE_JTAG_TDI"),
+		MTK_FUNCTION(3, "DFD_TDI"),
+		MTK_FUNCTION(5, "ANC_JTAG_TDI"),
+		MTK_FUNCTION(6, "SCP_JTAG_TDI"),
+		MTK_FUNCTION(7, "C2K_DM_OTDI")
+	),
+	MTK_PIN(
+		260, "GPIO260",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO260"),
+		MTK_FUNCTION(1, "IO_JTAG_TDO"),
+		MTK_FUNCTION(2, "LTE_JTAG_TDO"),
+		MTK_FUNCTION(3, "DFD_TDO"),
+		MTK_FUNCTION(5, "ANC_JTAG_TDO"),
+		MTK_FUNCTION(6, "SCP_JTAG_TDO"),
+		MTK_FUNCTION(7, "C2K_DM_OTDO")
+	),
+	MTK_PIN(
+		261, "GPIO261",
+		MTK_EINT_FUNCTION(NO_EINT_SUPPORT, NO_EINT_SUPPORT),
+		DRV_GRP3,
+		MTK_FUNCTION(0, "GPIO261"),
+		MTK_FUNCTION(2, "LTE_JTAG_TRSTN"),
+		MTK_FUNCTION(3, "DFD_NTRST"),
+		MTK_FUNCTION(5, "ANC_JTAG_TRSTN"),
+		MTK_FUNCTION(6, "SCP_JTAG_TRSTN"),
+		MTK_FUNCTION(7, "C2K_DM_JTINTP")
+	),
+};
+
+#endif /* __PINCTRL_MTK_MT6797_H */
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mtk-mt8183.h
@@ -0,0 +1,1916 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: Zhiyong Tao <zhiyong.tao@mediatek.com>
+ *
+ */
+
+#ifndef __PINCTRL_MTK_MT8183_H
+#define __PINCTRL_MTK_MT8183_H
+
+#include "pinctrl-paris.h"
+
+static struct mtk_pin_desc mtk_pins_mt8183[] = {
+	MTK_PIN(
+		0, "GPIO0",
+		MTK_EINT_FUNCTION(0, 0),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO0"),
+		MTK_FUNCTION(1, "MRG_SYNC"),
+		MTK_FUNCTION(2, "PCM0_SYNC"),
+		MTK_FUNCTION(3, "TP_GPIO0_AO"),
+		MTK_FUNCTION(4, "SRCLKENAI0"),
+		MTK_FUNCTION(5, "SCP_SPI2_CS"),
+		MTK_FUNCTION(6, "I2S3_MCK"),
+		MTK_FUNCTION(7, "SPI2_CSB")
+	),
+	MTK_PIN(
+		1, "GPIO1",
+		MTK_EINT_FUNCTION(0, 1),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO1"),
+		MTK_FUNCTION(1, "MRG_CLK"),
+		MTK_FUNCTION(2, "PCM0_CLK"),
+		MTK_FUNCTION(3, "TP_GPIO1_AO"),
+		MTK_FUNCTION(4, "CLKM3"),
+		MTK_FUNCTION(5, "SCP_SPI2_MO"),
+		MTK_FUNCTION(6, "I2S3_BCK"),
+		MTK_FUNCTION(7, "SPI2_MO")
+	),
+	MTK_PIN(
+		2, "GPIO2",
+		MTK_EINT_FUNCTION(0, 2),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO2"),
+		MTK_FUNCTION(1, "MRG_DO"),
+		MTK_FUNCTION(2, "PCM0_DO"),
+		MTK_FUNCTION(3, "TP_GPIO2_AO"),
+		MTK_FUNCTION(4, "SCL6"),
+		MTK_FUNCTION(5, "SCP_SPI2_CK"),
+		MTK_FUNCTION(6, "I2S3_LRCK"),
+		MTK_FUNCTION(7, "SPI2_CLK")
+	),
+	MTK_PIN(
+		3, "GPIO3",
+		MTK_EINT_FUNCTION(0, 3),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO3"),
+		MTK_FUNCTION(1, "MRG_DI"),
+		MTK_FUNCTION(2, "PCM0_DI"),
+		MTK_FUNCTION(3, "TP_GPIO3_AO"),
+		MTK_FUNCTION(4, "SDA6"),
+		MTK_FUNCTION(5, "TDM_MCK"),
+		MTK_FUNCTION(6, "I2S3_DO"),
+		MTK_FUNCTION(7, "SCP_VREQ_VAO")
+	),
+	MTK_PIN(
+		4, "GPIO4",
+		MTK_EINT_FUNCTION(0, 4),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO4"),
+		MTK_FUNCTION(1, "PWM_B"),
+		MTK_FUNCTION(2, "I2S0_MCK"),
+		MTK_FUNCTION(3, "SSPM_UTXD_AO"),
+		MTK_FUNCTION(4, "MD_URXD1"),
+		MTK_FUNCTION(5, "TDM_BCK"),
+		MTK_FUNCTION(6, "TP_GPIO4_AO"),
+		MTK_FUNCTION(7, "DAP_MD32_SWD")
+	),
+	MTK_PIN(
+		5, "GPIO5",
+		MTK_EINT_FUNCTION(0, 5),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO5"),
+		MTK_FUNCTION(1, "PWM_C"),
+		MTK_FUNCTION(2, "I2S0_BCK"),
+		MTK_FUNCTION(3, "SSPM_URXD_AO"),
+		MTK_FUNCTION(4, "MD_UTXD1"),
+		MTK_FUNCTION(5, "TDM_LRCK"),
+		MTK_FUNCTION(6, "TP_GPIO5_AO"),
+		MTK_FUNCTION(7, "DAP_MD32_SWCK")
+	),
+	MTK_PIN(
+		6, "GPIO6",
+		MTK_EINT_FUNCTION(0, 6),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO6"),
+		MTK_FUNCTION(1, "PWM_A"),
+		MTK_FUNCTION(2, "I2S0_LRCK"),
+		MTK_FUNCTION(3, "IDDIG"),
+		MTK_FUNCTION(4, "MD_URXD0"),
+		MTK_FUNCTION(5, "TDM_DATA0"),
+		MTK_FUNCTION(6, "TP_GPIO6_AO"),
+		MTK_FUNCTION(7, "CMFLASH")
+	),
+	MTK_PIN(
+		7, "GPIO7",
+		MTK_EINT_FUNCTION(0, 7),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO7"),
+		MTK_FUNCTION(1, "SPI1_B_MI"),
+		MTK_FUNCTION(2, "I2S0_DI"),
+		MTK_FUNCTION(3, "USB_DRVVBUS"),
+		MTK_FUNCTION(4, "MD_UTXD0"),
+		MTK_FUNCTION(5, "TDM_DATA1"),
+		MTK_FUNCTION(6, "TP_GPIO7_AO"),
+		MTK_FUNCTION(7, "DVFSRC_EXT_REQ")
+	),
+	MTK_PIN(
+		8, "GPIO8",
+		MTK_EINT_FUNCTION(0, 8),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO8"),
+		MTK_FUNCTION(1, "SPI1_B_CSB"),
+		MTK_FUNCTION(2, "ANT_SEL3"),
+		MTK_FUNCTION(3, "SCL7"),
+		MTK_FUNCTION(4, "CONN_MCU_TRST_B"),
+		MTK_FUNCTION(5, "TDM_DATA2"),
+		MTK_FUNCTION(6, "MD_INT0"),
+		MTK_FUNCTION(7, "JTRSTN_SEL1")
+	),
+	MTK_PIN(
+		9, "GPIO9",
+		MTK_EINT_FUNCTION(0, 9),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO9"),
+		MTK_FUNCTION(1, "SPI1_B_MO"),
+		MTK_FUNCTION(2, "ANT_SEL4"),
+		MTK_FUNCTION(3, "CMMCLK2"),
+		MTK_FUNCTION(4, "CONN_MCU_DBGACK_N"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TRSTN"),
+		MTK_FUNCTION(6, "IO_JTAG_TRSTN"),
+		MTK_FUNCTION(7, "DBG_MON_B10")
+	),
+	MTK_PIN(
+		10, "GPIO10",
+		MTK_EINT_FUNCTION(0, 10),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO10"),
+		MTK_FUNCTION(1, "SPI1_B_CLK"),
+		MTK_FUNCTION(2, "ANT_SEL5"),
+		MTK_FUNCTION(3, "CMMCLK3"),
+		MTK_FUNCTION(4, "CONN_MCU_DBGI_N"),
+		MTK_FUNCTION(5, "TDM_DATA3"),
+		MTK_FUNCTION(6, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(7, "DBG_MON_B11")
+	),
+	MTK_PIN(
+		11, "GPIO11",
+		MTK_EINT_FUNCTION(0, 11),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO11"),
+		MTK_FUNCTION(1, "TP_URXD1_AO"),
+		MTK_FUNCTION(2, "IDDIG"),
+		MTK_FUNCTION(3, "SCL6"),
+		MTK_FUNCTION(4, "UCTS1"),
+		MTK_FUNCTION(5, "UCTS0"),
+		MTK_FUNCTION(6, "SRCLKENAI1"),
+		MTK_FUNCTION(7, "I2S5_MCK")
+	),
+	MTK_PIN(
+		12, "GPIO12",
+		MTK_EINT_FUNCTION(0, 12),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO12"),
+		MTK_FUNCTION(1, "TP_UTXD1_AO"),
+		MTK_FUNCTION(2, "USB_DRVVBUS"),
+		MTK_FUNCTION(3, "SDA6"),
+		MTK_FUNCTION(4, "URTS1"),
+		MTK_FUNCTION(5, "URTS0"),
+		MTK_FUNCTION(6, "I2S2_DI2"),
+		MTK_FUNCTION(7, "I2S5_BCK")
+	),
+	MTK_PIN(
+		13, "GPIO13",
+		MTK_EINT_FUNCTION(0, 13),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO13"),
+		MTK_FUNCTION(1, "DBPI_D0"),
+		MTK_FUNCTION(2, "SPI5_MI"),
+		MTK_FUNCTION(3, "PCM0_SYNC"),
+		MTK_FUNCTION(4, "MD_URXD0"),
+		MTK_FUNCTION(5, "ANT_SEL3"),
+		MTK_FUNCTION(6, "I2S0_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B15")
+	),
+	MTK_PIN(
+		14, "GPIO14",
+		MTK_EINT_FUNCTION(0, 14),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO14"),
+		MTK_FUNCTION(1, "DBPI_D1"),
+		MTK_FUNCTION(2, "SPI5_CSB"),
+		MTK_FUNCTION(3, "PCM0_CLK"),
+		MTK_FUNCTION(4, "MD_UTXD0"),
+		MTK_FUNCTION(5, "ANT_SEL4"),
+		MTK_FUNCTION(6, "I2S0_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_B16")
+	),
+	MTK_PIN(
+		15, "GPIO15",
+		MTK_EINT_FUNCTION(0, 15),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO15"),
+		MTK_FUNCTION(1, "DBPI_D2"),
+		MTK_FUNCTION(2, "SPI5_MO"),
+		MTK_FUNCTION(3, "PCM0_DO"),
+		MTK_FUNCTION(4, "MD_URXD1"),
+		MTK_FUNCTION(5, "ANT_SEL5"),
+		MTK_FUNCTION(6, "I2S0_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_B17")
+	),
+	MTK_PIN(
+		16, "GPIO16",
+		MTK_EINT_FUNCTION(0, 16),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO16"),
+		MTK_FUNCTION(1, "DBPI_D3"),
+		MTK_FUNCTION(2, "SPI5_CLK"),
+		MTK_FUNCTION(3, "PCM0_DI"),
+		MTK_FUNCTION(4, "MD_UTXD1"),
+		MTK_FUNCTION(5, "ANT_SEL6"),
+		MTK_FUNCTION(6, "I2S0_DI"),
+		MTK_FUNCTION(7, "DBG_MON_B23")
+	),
+	MTK_PIN(
+		17, "GPIO17",
+		MTK_EINT_FUNCTION(0, 17),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO17"),
+		MTK_FUNCTION(1, "DBPI_D4"),
+		MTK_FUNCTION(2, "SPI4_MI"),
+		MTK_FUNCTION(3, "CONN_MCU_TRST_B"),
+		MTK_FUNCTION(4, "MD_INT0"),
+		MTK_FUNCTION(5, "ANT_SEL7"),
+		MTK_FUNCTION(6, "I2S3_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A1")
+	),
+	MTK_PIN(
+		18, "GPIO18",
+		MTK_EINT_FUNCTION(0, 18),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO18"),
+		MTK_FUNCTION(1, "DBPI_D5"),
+		MTK_FUNCTION(2, "SPI4_CSB"),
+		MTK_FUNCTION(3, "CONN_MCU_DBGI_N"),
+		MTK_FUNCTION(4, "MD_INT0"),
+		MTK_FUNCTION(5, "SCP_VREQ_VAO"),
+		MTK_FUNCTION(6, "I2S3_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A2")
+	),
+	MTK_PIN(
+		19, "GPIO19",
+		MTK_EINT_FUNCTION(0, 19),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO19"),
+		MTK_FUNCTION(1, "DBPI_D6"),
+		MTK_FUNCTION(2, "SPI4_MO"),
+		MTK_FUNCTION(3, "CONN_MCU_TDO"),
+		MTK_FUNCTION(4, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(5, "URXD1"),
+		MTK_FUNCTION(6, "I2S3_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A3")
+	),
+	MTK_PIN(
+		20, "GPIO20",
+		MTK_EINT_FUNCTION(0, 20),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO20"),
+		MTK_FUNCTION(1, "DBPI_D7"),
+		MTK_FUNCTION(2, "SPI4_CLK"),
+		MTK_FUNCTION(3, "CONN_MCU_DBGACK_N"),
+		MTK_FUNCTION(4, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(5, "UTXD1"),
+		MTK_FUNCTION(6, "I2S3_DO"),
+		MTK_FUNCTION(7, "DBG_MON_A19")
+	),
+	MTK_PIN(
+		21, "GPIO21",
+		MTK_EINT_FUNCTION(0, 21),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO21"),
+		MTK_FUNCTION(1, "DBPI_D8"),
+		MTK_FUNCTION(2, "SPI3_MI"),
+		MTK_FUNCTION(3, "CONN_MCU_TMS"),
+		MTK_FUNCTION(4, "DAP_MD32_SWD"),
+		MTK_FUNCTION(5, "CONN_MCU_AICE_TMSC"),
+		MTK_FUNCTION(6, "I2S2_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B5")
+	),
+	MTK_PIN(
+		22, "GPIO22",
+		MTK_EINT_FUNCTION(0, 22),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO22"),
+		MTK_FUNCTION(1, "DBPI_D9"),
+		MTK_FUNCTION(2, "SPI3_CSB"),
+		MTK_FUNCTION(3, "CONN_MCU_TCK"),
+		MTK_FUNCTION(4, "DAP_MD32_SWCK"),
+		MTK_FUNCTION(5, "CONN_MCU_AICE_TCKC"),
+		MTK_FUNCTION(6, "I2S2_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_B6")
+	),
+	MTK_PIN(
+		23, "GPIO23",
+		MTK_EINT_FUNCTION(0, 23),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO23"),
+		MTK_FUNCTION(1, "DBPI_D10"),
+		MTK_FUNCTION(2, "SPI3_MO"),
+		MTK_FUNCTION(3, "CONN_MCU_TDI"),
+		MTK_FUNCTION(4, "UCTS1"),
+		MTK_FUNCTION(5, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(6, "I2S2_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_B7")
+	),
+	MTK_PIN(
+		24, "GPIO24",
+		MTK_EINT_FUNCTION(0, 24),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO24"),
+		MTK_FUNCTION(1, "DBPI_D11"),
+		MTK_FUNCTION(2, "SPI3_CLK"),
+		MTK_FUNCTION(3, "SRCLKENAI0"),
+		MTK_FUNCTION(4, "URTS1"),
+		MTK_FUNCTION(5, "IO_JTAG_TCK"),
+		MTK_FUNCTION(6, "I2S2_DI"),
+		MTK_FUNCTION(7, "DBG_MON_B31")
+	),
+	MTK_PIN(
+		25, "GPIO25",
+		MTK_EINT_FUNCTION(0, 25),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO25"),
+		MTK_FUNCTION(1, "DBPI_HSYNC"),
+		MTK_FUNCTION(2, "ANT_SEL0"),
+		MTK_FUNCTION(3, "SCL6"),
+		MTK_FUNCTION(4, "KPCOL2"),
+		MTK_FUNCTION(5, "IO_JTAG_TMS"),
+		MTK_FUNCTION(6, "I2S1_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B0")
+	),
+	MTK_PIN(
+		26, "GPIO26",
+		MTK_EINT_FUNCTION(0, 26),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO26"),
+		MTK_FUNCTION(1, "DBPI_VSYNC"),
+		MTK_FUNCTION(2, "ANT_SEL1"),
+		MTK_FUNCTION(3, "SDA6"),
+		MTK_FUNCTION(4, "KPROW2"),
+		MTK_FUNCTION(5, "IO_JTAG_TDI"),
+		MTK_FUNCTION(6, "I2S1_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_B1")
+	),
+	MTK_PIN(
+		27, "GPIO27",
+		MTK_EINT_FUNCTION(0, 27),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO27"),
+		MTK_FUNCTION(1, "DBPI_DE"),
+		MTK_FUNCTION(2, "ANT_SEL2"),
+		MTK_FUNCTION(3, "SCL7"),
+		MTK_FUNCTION(4, "DMIC_CLK"),
+		MTK_FUNCTION(5, "IO_JTAG_TDO"),
+		MTK_FUNCTION(6, "I2S1_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_B9")
+	),
+	MTK_PIN(
+		28, "GPIO28",
+		MTK_EINT_FUNCTION(0, 28),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO28"),
+		MTK_FUNCTION(1, "DBPI_CK"),
+		MTK_FUNCTION(2, "DVFSRC_EXT_REQ"),
+		MTK_FUNCTION(3, "SDA7"),
+		MTK_FUNCTION(4, "DMIC_DAT"),
+		MTK_FUNCTION(5, "IO_JTAG_TRSTN"),
+		MTK_FUNCTION(6, "I2S1_DO"),
+		MTK_FUNCTION(7, "DBG_MON_B32")
+	),
+	MTK_PIN(
+		29, "GPIO29",
+		MTK_EINT_FUNCTION(0, 29),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO29"),
+		MTK_FUNCTION(1, "MSDC1_CLK"),
+		MTK_FUNCTION(2, "IO_JTAG_TCK"),
+		MTK_FUNCTION(3, "UDI_TCK"),
+		MTK_FUNCTION(4, "CONN_DSP_JCK"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TCK"),
+		MTK_FUNCTION(6, "PCM1_CLK"),
+		MTK_FUNCTION(7, "DBG_MON_A6")
+	),
+	MTK_PIN(
+		30, "GPIO30",
+		MTK_EINT_FUNCTION(0, 30),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO30"),
+		MTK_FUNCTION(1, "MSDC1_DAT3"),
+		MTK_FUNCTION(2, "DAP_MD32_SWD"),
+		MTK_FUNCTION(3, "CONN_MCU_AICE_TMSC"),
+		MTK_FUNCTION(4, "CONN_DSP_JINTP"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TRSTN"),
+		MTK_FUNCTION(6, "PCM1_DI"),
+		MTK_FUNCTION(7, "DBG_MON_A7")
+	),
+	MTK_PIN(
+		31, "GPIO31",
+		MTK_EINT_FUNCTION(0, 31),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO31"),
+		MTK_FUNCTION(1, "MSDC1_CMD"),
+		MTK_FUNCTION(2, "IO_JTAG_TMS"),
+		MTK_FUNCTION(3, "UDI_TMS"),
+		MTK_FUNCTION(4, "CONN_DSP_JMS"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TMS"),
+		MTK_FUNCTION(6, "PCM1_SYNC"),
+		MTK_FUNCTION(7, "DBG_MON_A8")
+	),
+	MTK_PIN(
+		32, "GPIO32",
+		MTK_EINT_FUNCTION(0, 32),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO32"),
+		MTK_FUNCTION(1, "MSDC1_DAT0"),
+		MTK_FUNCTION(2, "IO_JTAG_TDI"),
+		MTK_FUNCTION(3, "UDI_TDI"),
+		MTK_FUNCTION(4, "CONN_DSP_JDI"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TDI"),
+		MTK_FUNCTION(6, "PCM1_DO0"),
+		MTK_FUNCTION(7, "DBG_MON_A9")
+	),
+	MTK_PIN(
+		33, "GPIO33",
+		MTK_EINT_FUNCTION(0, 33),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO33"),
+		MTK_FUNCTION(1, "MSDC1_DAT2"),
+		MTK_FUNCTION(2, "IO_JTAG_TRSTN"),
+		MTK_FUNCTION(3, "UDI_NTRST"),
+		MTK_FUNCTION(4, "DAP_MD32_SWCK"),
+		MTK_FUNCTION(5, "CONN_MCU_AICE_TCKC"),
+		MTK_FUNCTION(6, "PCM1_DO2"),
+		MTK_FUNCTION(7, "DBG_MON_A10")
+	),
+	MTK_PIN(
+		34, "GPIO34",
+		MTK_EINT_FUNCTION(0, 34),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO34"),
+		MTK_FUNCTION(1, "MSDC1_DAT1"),
+		MTK_FUNCTION(2, "IO_JTAG_TDO"),
+		MTK_FUNCTION(3, "UDI_TDO"),
+		MTK_FUNCTION(4, "CONN_DSP_JDO"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TDO"),
+		MTK_FUNCTION(6, "PCM1_DO1"),
+		MTK_FUNCTION(7, "DBG_MON_A11")
+	),
+	MTK_PIN(
+		35, "GPIO35",
+		MTK_EINT_FUNCTION(0, 35),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO35"),
+		MTK_FUNCTION(1, "MD1_SIM2_SIO"),
+		MTK_FUNCTION(2, "CCU_JTAG_TDO"),
+		MTK_FUNCTION(3, "MD1_SIM1_SIO"),
+		MTK_FUNCTION(5, "SCP_JTAG_TDO"),
+		MTK_FUNCTION(6, "CONN_DSP_JMS"),
+		MTK_FUNCTION(7, "DBG_MON_A28")
+	),
+	MTK_PIN(
+		36, "GPIO36",
+		MTK_EINT_FUNCTION(0, 36),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO36"),
+		MTK_FUNCTION(1, "MD1_SIM2_SRST"),
+		MTK_FUNCTION(2, "CCU_JTAG_TMS"),
+		MTK_FUNCTION(3, "MD1_SIM1_SRST"),
+		MTK_FUNCTION(4, "CONN_MCU_AICE_TMSC"),
+		MTK_FUNCTION(5, "SCP_JTAG_TMS"),
+		MTK_FUNCTION(6, "CONN_DSP_JINTP"),
+		MTK_FUNCTION(7, "DBG_MON_A29")
+	),
+	MTK_PIN(
+		37, "GPIO37",
+		MTK_EINT_FUNCTION(0, 37),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO37"),
+		MTK_FUNCTION(1, "MD1_SIM2_SCLK"),
+		MTK_FUNCTION(2, "CCU_JTAG_TDI"),
+		MTK_FUNCTION(3, "MD1_SIM1_SCLK"),
+		MTK_FUNCTION(5, "SCP_JTAG_TDI"),
+		MTK_FUNCTION(6, "CONN_DSP_JDO"),
+		MTK_FUNCTION(7, "DBG_MON_A30")
+	),
+	MTK_PIN(
+		38, "GPIO38",
+		MTK_EINT_FUNCTION(0, 38),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO38"),
+		MTK_FUNCTION(1, "MD1_SIM1_SCLK"),
+		MTK_FUNCTION(3, "MD1_SIM2_SCLK"),
+		MTK_FUNCTION(4, "CONN_MCU_AICE_TCKC"),
+		MTK_FUNCTION(7, "DBG_MON_A20")
+	),
+	MTK_PIN(
+		39, "GPIO39",
+		MTK_EINT_FUNCTION(0, 39),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO39"),
+		MTK_FUNCTION(1, "MD1_SIM1_SRST"),
+		MTK_FUNCTION(2, "CCU_JTAG_TCK"),
+		MTK_FUNCTION(3, "MD1_SIM2_SRST"),
+		MTK_FUNCTION(5, "SCP_JTAG_TCK"),
+		MTK_FUNCTION(6, "CONN_DSP_JCK"),
+		MTK_FUNCTION(7, "DBG_MON_A31")
+	),
+	MTK_PIN(
+		40, "GPIO40",
+		MTK_EINT_FUNCTION(0, 40),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO40"),
+		MTK_FUNCTION(1, "MD1_SIM1_SIO"),
+		MTK_FUNCTION(2, "CCU_JTAG_TRST"),
+		MTK_FUNCTION(3, "MD1_SIM2_SIO"),
+		MTK_FUNCTION(5, "SCP_JTAG_TRSTN"),
+		MTK_FUNCTION(6, "CONN_DSP_JDI"),
+		MTK_FUNCTION(7, "DBG_MON_A32")
+	),
+	MTK_PIN(
+		41, "GPIO41",
+		MTK_EINT_FUNCTION(0, 41),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO41"),
+		MTK_FUNCTION(1, "IDDIG"),
+		MTK_FUNCTION(2, "URXD1"),
+		MTK_FUNCTION(3, "UCTS0"),
+		MTK_FUNCTION(4, "SSPM_UTXD_AO"),
+		MTK_FUNCTION(5, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(6, "DMIC_CLK")
+	),
+	MTK_PIN(
+		42, "GPIO42",
+		MTK_EINT_FUNCTION(0, 42),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO42"),
+		MTK_FUNCTION(1, "USB_DRVVBUS"),
+		MTK_FUNCTION(2, "UTXD1"),
+		MTK_FUNCTION(3, "URTS0"),
+		MTK_FUNCTION(4, "SSPM_URXD_AO"),
+		MTK_FUNCTION(5, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(6, "DMIC_DAT")
+	),
+	MTK_PIN(
+		43, "GPIO43",
+		MTK_EINT_FUNCTION(0, 43),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO43"),
+		MTK_FUNCTION(1, "DISP_PWM")
+	),
+	MTK_PIN(
+		44, "GPIO44",
+		MTK_EINT_FUNCTION(0, 44),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO44"),
+		MTK_FUNCTION(1, "DSI_TE")
+	),
+	MTK_PIN(
+		45, "GPIO45",
+		MTK_EINT_FUNCTION(0, 45),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO45"),
+		MTK_FUNCTION(1, "LCM_RST")
+	),
+	MTK_PIN(
+		46, "GPIO46",
+		MTK_EINT_FUNCTION(0, 46),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO46"),
+		MTK_FUNCTION(1, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(2, "URXD1"),
+		MTK_FUNCTION(3, "UCTS1"),
+		MTK_FUNCTION(4, "CCU_UTXD_AO"),
+		MTK_FUNCTION(5, "TP_UCTS1_AO"),
+		MTK_FUNCTION(6, "IDDIG"),
+		MTK_FUNCTION(7, "I2S5_LRCK")
+	),
+	MTK_PIN(
+		47, "GPIO47",
+		MTK_EINT_FUNCTION(0, 47),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO47"),
+		MTK_FUNCTION(1, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(2, "UTXD1"),
+		MTK_FUNCTION(3, "URTS1"),
+		MTK_FUNCTION(4, "CCU_URXD_AO"),
+		MTK_FUNCTION(5, "TP_URTS1_AO"),
+		MTK_FUNCTION(6, "USB_DRVVBUS"),
+		MTK_FUNCTION(7, "I2S5_DO")
+	),
+	MTK_PIN(
+		48, "GPIO48",
+		MTK_EINT_FUNCTION(0, 48),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO48"),
+		MTK_FUNCTION(1, "SCL5")
+	),
+	MTK_PIN(
+		49, "GPIO49",
+		MTK_EINT_FUNCTION(0, 49),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO49"),
+		MTK_FUNCTION(1, "SDA5")
+	),
+	MTK_PIN(
+		50, "GPIO50",
+		MTK_EINT_FUNCTION(0, 50),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO50"),
+		MTK_FUNCTION(1, "SCL3")
+	),
+	MTK_PIN(
+		51, "GPIO51",
+		MTK_EINT_FUNCTION(0, 51),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO51"),
+		MTK_FUNCTION(1, "SDA3")
+	),
+	MTK_PIN(
+		52, "GPIO52",
+		MTK_EINT_FUNCTION(0, 52),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO52"),
+		MTK_FUNCTION(1, "BPI_ANT2")
+	),
+	MTK_PIN(
+		53, "GPIO53",
+		MTK_EINT_FUNCTION(0, 53),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO53"),
+		MTK_FUNCTION(1, "BPI_ANT0")
+	),
+	MTK_PIN(
+		54, "GPIO54",
+		MTK_EINT_FUNCTION(0, 54),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO54"),
+		MTK_FUNCTION(1, "BPI_OLAT1")
+	),
+	MTK_PIN(
+		55, "GPIO55",
+		MTK_EINT_FUNCTION(0, 55),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO55"),
+		MTK_FUNCTION(1, "BPI_BUS8")
+	),
+	MTK_PIN(
+		56, "GPIO56",
+		MTK_EINT_FUNCTION(0, 56),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO56"),
+		MTK_FUNCTION(1, "BPI_BUS9"),
+		MTK_FUNCTION(2, "SCL_6306")
+	),
+	MTK_PIN(
+		57, "GPIO57",
+		MTK_EINT_FUNCTION(0, 57),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO57"),
+		MTK_FUNCTION(1, "BPI_BUS10"),
+		MTK_FUNCTION(2, "SDA_6306")
+	),
+	MTK_PIN(
+		58, "GPIO58",
+		MTK_EINT_FUNCTION(0, 58),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO58"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D2"),
+		MTK_FUNCTION(2, "SPM_BSI_D2"),
+		MTK_FUNCTION(3, "PWM_B")
+	),
+	MTK_PIN(
+		59, "GPIO59",
+		MTK_EINT_FUNCTION(0, 59),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO59"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D1"),
+		MTK_FUNCTION(2, "SPM_BSI_D1")
+	),
+	MTK_PIN(
+		60, "GPIO60",
+		MTK_EINT_FUNCTION(0, 60),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO60"),
+		MTK_FUNCTION(1, "RFIC0_BSI_D0"),
+		MTK_FUNCTION(2, "SPM_BSI_D0")
+	),
+	MTK_PIN(
+		61, "GPIO61",
+		MTK_EINT_FUNCTION(0, 61),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO61"),
+		MTK_FUNCTION(1, "MIPI1_SDATA")
+	),
+	MTK_PIN(
+		62, "GPIO62",
+		MTK_EINT_FUNCTION(0, 62),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO62"),
+		MTK_FUNCTION(1, "MIPI1_SCLK")
+	),
+	MTK_PIN(
+		63, "GPIO63",
+		MTK_EINT_FUNCTION(0, 63),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO63"),
+		MTK_FUNCTION(1, "MIPI0_SDATA")
+	),
+	MTK_PIN(
+		64, "GPIO64",
+		MTK_EINT_FUNCTION(0, 64),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO64"),
+		MTK_FUNCTION(1, "MIPI0_SCLK")
+	),
+	MTK_PIN(
+		65, "GPIO65",
+		MTK_EINT_FUNCTION(0, 65),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO65"),
+		MTK_FUNCTION(1, "MIPI3_SDATA"),
+		MTK_FUNCTION(2, "BPI_OLAT2")
+	),
+	MTK_PIN(
+		66, "GPIO66",
+		MTK_EINT_FUNCTION(0, 66),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO66"),
+		MTK_FUNCTION(1, "MIPI3_SCLK"),
+		MTK_FUNCTION(2, "BPI_OLAT3")
+	),
+	MTK_PIN(
+		67, "GPIO67",
+		MTK_EINT_FUNCTION(0, 67),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO67"),
+		MTK_FUNCTION(1, "MIPI2_SDATA")
+	),
+	MTK_PIN(
+		68, "GPIO68",
+		MTK_EINT_FUNCTION(0, 68),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO68"),
+		MTK_FUNCTION(1, "MIPI2_SCLK")
+	),
+	MTK_PIN(
+		69, "GPIO69",
+		MTK_EINT_FUNCTION(0, 69),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO69"),
+		MTK_FUNCTION(1, "BPI_BUS7")
+	),
+	MTK_PIN(
+		70, "GPIO70",
+		MTK_EINT_FUNCTION(0, 70),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO70"),
+		MTK_FUNCTION(1, "BPI_BUS6")
+	),
+	MTK_PIN(
+		71, "GPIO71",
+		MTK_EINT_FUNCTION(0, 71),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO71"),
+		MTK_FUNCTION(1, "BPI_BUS5")
+	),
+	MTK_PIN(
+		72, "GPIO72",
+		MTK_EINT_FUNCTION(0, 72),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO72"),
+		MTK_FUNCTION(1, "BPI_BUS4")
+	),
+	MTK_PIN(
+		73, "GPIO73",
+		MTK_EINT_FUNCTION(0, 73),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO73"),
+		MTK_FUNCTION(1, "BPI_BUS3")
+	),
+	MTK_PIN(
+		74, "GPIO74",
+		MTK_EINT_FUNCTION(0, 74),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO74"),
+		MTK_FUNCTION(1, "BPI_BUS2")
+	),
+	MTK_PIN(
+		75, "GPIO75",
+		MTK_EINT_FUNCTION(0, 75),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO75"),
+		MTK_FUNCTION(1, "BPI_BUS1")
+	),
+	MTK_PIN(
+		76, "GPIO76",
+		MTK_EINT_FUNCTION(0, 76),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO76"),
+		MTK_FUNCTION(1, "BPI_BUS0")
+	),
+	MTK_PIN(
+		77, "GPIO77",
+		MTK_EINT_FUNCTION(0, 77),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO77"),
+		MTK_FUNCTION(1, "BPI_ANT1")
+	),
+	MTK_PIN(
+		78, "GPIO78",
+		MTK_EINT_FUNCTION(0, 78),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO78"),
+		MTK_FUNCTION(1, "BPI_OLAT0")
+	),
+	MTK_PIN(
+		79, "GPIO79",
+		MTK_EINT_FUNCTION(0, 79),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO79"),
+		MTK_FUNCTION(1, "BPI_PA_VM1"),
+		MTK_FUNCTION(2, "MIPI4_SDATA")
+	),
+	MTK_PIN(
+		80, "GPIO80",
+		MTK_EINT_FUNCTION(0, 80),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO80"),
+		MTK_FUNCTION(1, "BPI_PA_VM0"),
+		MTK_FUNCTION(2, "MIPI4_SCLK")
+	),
+	MTK_PIN(
+		81, "GPIO81",
+		MTK_EINT_FUNCTION(0, 81),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO81"),
+		MTK_FUNCTION(1, "SDA1")
+	),
+	MTK_PIN(
+		82, "GPIO82",
+		MTK_EINT_FUNCTION(0, 82),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO82"),
+		MTK_FUNCTION(1, "SDA0")
+	),
+	MTK_PIN(
+		83, "GPIO83",
+		MTK_EINT_FUNCTION(0, 83),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO83"),
+		MTK_FUNCTION(1, "SCL0")
+	),
+	MTK_PIN(
+		84, "GPIO84",
+		MTK_EINT_FUNCTION(0, 84),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO84"),
+		MTK_FUNCTION(1, "SCL1")
+	),
+	MTK_PIN(
+		85, "GPIO85",
+		MTK_EINT_FUNCTION(0, 85),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO85"),
+		MTK_FUNCTION(1, "SPI0_MI"),
+		MTK_FUNCTION(2, "SCP_SPI0_MI"),
+		MTK_FUNCTION(3, "CLKM3"),
+		MTK_FUNCTION(4, "I2S1_BCK"),
+		MTK_FUNCTION(5, "MFG_DFD_JTAG_TDO"),
+		MTK_FUNCTION(6, "DFD_TDO"),
+		MTK_FUNCTION(7, "JTDO_SEL1")
+	),
+	MTK_PIN(
+		86, "GPIO86",
+		MTK_EINT_FUNCTION(0, 86),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO86"),
+		MTK_FUNCTION(1, "SPI0_CSB"),
+		MTK_FUNCTION(2, "SCP_SPI0_CS"),
+		MTK_FUNCTION(3, "CLKM0"),
+		MTK_FUNCTION(4, "I2S1_LRCK"),
+		MTK_FUNCTION(5, "MFG_DFD_JTAG_TMS"),
+		MTK_FUNCTION(6, "DFD_TMS"),
+		MTK_FUNCTION(7, "JTMS_SEL1")
+	),
+	MTK_PIN(
+		87, "GPIO87",
+		MTK_EINT_FUNCTION(0, 87),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO87"),
+		MTK_FUNCTION(1, "SPI0_MO"),
+		MTK_FUNCTION(2, "SCP_SPI0_MO"),
+		MTK_FUNCTION(3, "SDA1"),
+		MTK_FUNCTION(4, "I2S1_DO"),
+		MTK_FUNCTION(5, "MFG_DFD_JTAG_TDI"),
+		MTK_FUNCTION(6, "DFD_TDI"),
+		MTK_FUNCTION(7, "JTDI_SEL1")
+	),
+	MTK_PIN(
+		88, "GPIO88",
+		MTK_EINT_FUNCTION(0, 88),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO88"),
+		MTK_FUNCTION(1, "SPI0_CLK"),
+		MTK_FUNCTION(2, "SCP_SPI0_CK"),
+		MTK_FUNCTION(3, "SCL1"),
+		MTK_FUNCTION(4, "I2S1_MCK"),
+		MTK_FUNCTION(5, "MFG_DFD_JTAG_TCK"),
+		MTK_FUNCTION(6, "DFD_TCK_XI"),
+		MTK_FUNCTION(7, "JTCK_SEL1")
+	),
+	MTK_PIN(
+		89, "GPIO89",
+		MTK_EINT_FUNCTION(0, 89),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO89"),
+		MTK_FUNCTION(1, "SRCLKENAI0"),
+		MTK_FUNCTION(2, "PWM_C"),
+		MTK_FUNCTION(3, "I2S5_BCK"),
+		MTK_FUNCTION(4, "ANT_SEL6"),
+		MTK_FUNCTION(5, "SDA8"),
+		MTK_FUNCTION(6, "CMVREF0"),
+		MTK_FUNCTION(7, "DBG_MON_A21")
+	),
+	MTK_PIN(
+		90, "GPIO90",
+		MTK_EINT_FUNCTION(0, 90),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO90"),
+		MTK_FUNCTION(1, "PWM_A"),
+		MTK_FUNCTION(2, "CMMCLK2"),
+		MTK_FUNCTION(3, "I2S5_LRCK"),
+		MTK_FUNCTION(4, "SCP_VREQ_VAO"),
+		MTK_FUNCTION(5, "SCL8"),
+		MTK_FUNCTION(6, "PTA_RXD"),
+		MTK_FUNCTION(7, "DBG_MON_A22")
+	),
+	MTK_PIN(
+		91, "GPIO91",
+		MTK_EINT_FUNCTION(0, 91),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO91"),
+		MTK_FUNCTION(1, "KPROW1"),
+		MTK_FUNCTION(2, "PWM_B"),
+		MTK_FUNCTION(3, "I2S5_DO"),
+		MTK_FUNCTION(4, "ANT_SEL7"),
+		MTK_FUNCTION(5, "CMMCLK3"),
+		MTK_FUNCTION(6, "PTA_TXD")
+	),
+	MTK_PIN(
+		92, "GPIO92",
+		MTK_EINT_FUNCTION(0, 92),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO92"),
+		MTK_FUNCTION(1, "KPROW0")
+	),
+	MTK_PIN(
+		93, "GPIO93",
+		MTK_EINT_FUNCTION(0, 93),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO93"),
+		MTK_FUNCTION(1, "KPCOL0"),
+		MTK_FUNCTION(7, "DBG_MON_B27")
+	),
+	MTK_PIN(
+		94, "GPIO94",
+		MTK_EINT_FUNCTION(0, 94),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO94"),
+		MTK_FUNCTION(1, "KPCOL1"),
+		MTK_FUNCTION(2, "I2S2_DI2"),
+		MTK_FUNCTION(3, "I2S5_MCK"),
+		MTK_FUNCTION(4, "CMMCLK2"),
+		MTK_FUNCTION(5, "SCP_SPI2_MI"),
+		MTK_FUNCTION(6, "SRCLKENAI1"),
+		MTK_FUNCTION(7, "SPI2_MI")
+	),
+	MTK_PIN(
+		95, "GPIO95",
+		MTK_EINT_FUNCTION(0, 95),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO95"),
+		MTK_FUNCTION(1, "URXD0"),
+		MTK_FUNCTION(2, "UTXD0"),
+		MTK_FUNCTION(3, "MD_URXD0"),
+		MTK_FUNCTION(4, "MD_URXD1"),
+		MTK_FUNCTION(5, "SSPM_URXD_AO"),
+		MTK_FUNCTION(6, "CCU_URXD_AO")
+	),
+	MTK_PIN(
+		96, "GPIO96",
+		MTK_EINT_FUNCTION(0, 96),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO96"),
+		MTK_FUNCTION(1, "UTXD0"),
+		MTK_FUNCTION(2, "URXD0"),
+		MTK_FUNCTION(3, "MD_UTXD0"),
+		MTK_FUNCTION(4, "MD_UTXD1"),
+		MTK_FUNCTION(5, "SSPM_UTXD_AO"),
+		MTK_FUNCTION(6, "CCU_UTXD_AO"),
+		MTK_FUNCTION(7, "DBG_MON_B2")
+	),
+	MTK_PIN(
+		97, "GPIO97",
+		MTK_EINT_FUNCTION(0, 97),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO97"),
+		MTK_FUNCTION(1, "UCTS0"),
+		MTK_FUNCTION(2, "I2S2_MCK"),
+		MTK_FUNCTION(3, "IDDIG"),
+		MTK_FUNCTION(4, "CONN_MCU_TDO"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TDO"),
+		MTK_FUNCTION(6, "IO_JTAG_TDO"),
+		MTK_FUNCTION(7, "DBG_MON_B3")
+	),
+	MTK_PIN(
+		98, "GPIO98",
+		MTK_EINT_FUNCTION(0, 98),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO98"),
+		MTK_FUNCTION(1, "URTS0"),
+		MTK_FUNCTION(2, "I2S2_BCK"),
+		MTK_FUNCTION(3, "USB_DRVVBUS"),
+		MTK_FUNCTION(4, "CONN_MCU_TMS"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TMS"),
+		MTK_FUNCTION(6, "IO_JTAG_TMS"),
+		MTK_FUNCTION(7, "DBG_MON_B4")
+	),
+	MTK_PIN(
+		99, "GPIO99",
+		MTK_EINT_FUNCTION(0, 99),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO99"),
+		MTK_FUNCTION(1, "CMMCLK0"),
+		MTK_FUNCTION(4, "CONN_MCU_AICE_TMSC"),
+		MTK_FUNCTION(7, "DBG_MON_B28")
+	),
+	MTK_PIN(
+		100, "GPIO100",
+		MTK_EINT_FUNCTION(0, 100),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO100"),
+		MTK_FUNCTION(1, "CMMCLK1"),
+		MTK_FUNCTION(2, "PWM_C"),
+		MTK_FUNCTION(3, "MD_INT1_C2K_UIM0_HOT_PLUG"),
+		MTK_FUNCTION(4, "CONN_MCU_AICE_TCKC"),
+		MTK_FUNCTION(7, "DBG_MON_B29")
+	),
+	MTK_PIN(
+		101, "GPIO101",
+		MTK_EINT_FUNCTION(0, 101),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO101"),
+		MTK_FUNCTION(1, "CLKM2"),
+		MTK_FUNCTION(2, "I2S2_LRCK"),
+		MTK_FUNCTION(3, "CMVREF1"),
+		MTK_FUNCTION(4, "CONN_MCU_TCK"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TCK"),
+		MTK_FUNCTION(6, "IO_JTAG_TCK")
+	),
+	MTK_PIN(
+		102, "GPIO102",
+		MTK_EINT_FUNCTION(0, 102),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO102"),
+		MTK_FUNCTION(1, "CLKM1"),
+		MTK_FUNCTION(2, "I2S2_DI"),
+		MTK_FUNCTION(3, "DVFSRC_EXT_REQ"),
+		MTK_FUNCTION(4, "CONN_MCU_TDI"),
+		MTK_FUNCTION(5, "SSPM_JTAG_TDI"),
+		MTK_FUNCTION(6, "IO_JTAG_TDI"),
+		MTK_FUNCTION(7, "DBG_MON_B8")
+	),
+	MTK_PIN(
+		103, "GPIO103",
+		MTK_EINT_FUNCTION(0, 103),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO103"),
+		MTK_FUNCTION(1, "SCL2")
+	),
+	MTK_PIN(
+		104, "GPIO104",
+		MTK_EINT_FUNCTION(0, 104),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO104"),
+		MTK_FUNCTION(1, "SDA2")
+	),
+	MTK_PIN(
+		105, "GPIO105",
+		MTK_EINT_FUNCTION(0, 105),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO105"),
+		MTK_FUNCTION(1, "SCL4")
+	),
+	MTK_PIN(
+		106, "GPIO106",
+		MTK_EINT_FUNCTION(0, 106),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO106"),
+		MTK_FUNCTION(1, "SDA4")
+	),
+	MTK_PIN(
+		107, "GPIO107",
+		MTK_EINT_FUNCTION(0, 107),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO107"),
+		MTK_FUNCTION(1, "DMIC_CLK"),
+		MTK_FUNCTION(2, "ANT_SEL0"),
+		MTK_FUNCTION(3, "CLKM0"),
+		MTK_FUNCTION(4, "SDA7"),
+		MTK_FUNCTION(5, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(6, "PWM_A"),
+		MTK_FUNCTION(7, "DBG_MON_B12")
+	),
+	MTK_PIN(
+		108, "GPIO108",
+		MTK_EINT_FUNCTION(0, 108),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO108"),
+		MTK_FUNCTION(1, "CMMCLK2"),
+		MTK_FUNCTION(2, "ANT_SEL1"),
+		MTK_FUNCTION(3, "CLKM1"),
+		MTK_FUNCTION(4, "SCL8"),
+		MTK_FUNCTION(5, "DAP_MD32_SWD"),
+		MTK_FUNCTION(6, "PWM_B"),
+		MTK_FUNCTION(7, "DBG_MON_B13")
+	),
+	MTK_PIN(
+		109, "GPIO109",
+		MTK_EINT_FUNCTION(0, 109),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO109"),
+		MTK_FUNCTION(1, "DMIC_DAT"),
+		MTK_FUNCTION(2, "ANT_SEL2"),
+		MTK_FUNCTION(3, "CLKM2"),
+		MTK_FUNCTION(4, "SDA8"),
+		MTK_FUNCTION(5, "DAP_MD32_SWCK"),
+		MTK_FUNCTION(6, "PWM_C"),
+		MTK_FUNCTION(7, "DBG_MON_B14")
+	),
+	MTK_PIN(
+		110, "GPIO110",
+		MTK_EINT_FUNCTION(0, 110),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO110"),
+		MTK_FUNCTION(1, "SCL7"),
+		MTK_FUNCTION(2, "ANT_SEL0"),
+		MTK_FUNCTION(3, "TP_URXD1_AO"),
+		MTK_FUNCTION(4, "USB_DRVVBUS"),
+		MTK_FUNCTION(5, "SRCLKENAI1"),
+		MTK_FUNCTION(6, "KPCOL2"),
+		MTK_FUNCTION(7, "URXD1")
+	),
+	MTK_PIN(
+		111, "GPIO111",
+		MTK_EINT_FUNCTION(0, 111),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO111"),
+		MTK_FUNCTION(1, "CMMCLK3"),
+		MTK_FUNCTION(2, "ANT_SEL1"),
+		MTK_FUNCTION(3, "SRCLKENAI0"),
+		MTK_FUNCTION(4, "SCP_VREQ_VAO"),
+		MTK_FUNCTION(5, "MD_INT2_C2K_UIM1_HOT_PLUG"),
+		MTK_FUNCTION(7, "DVFSRC_EXT_REQ")
+	),
+	MTK_PIN(
+		112, "GPIO112",
+		MTK_EINT_FUNCTION(0, 112),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO112"),
+		MTK_FUNCTION(1, "SDA7"),
+		MTK_FUNCTION(2, "ANT_SEL2"),
+		MTK_FUNCTION(3, "TP_UTXD1_AO"),
+		MTK_FUNCTION(4, "IDDIG"),
+		MTK_FUNCTION(5, "AGPS_SYNC"),
+		MTK_FUNCTION(6, "KPROW2"),
+		MTK_FUNCTION(7, "UTXD1")
+	),
+	MTK_PIN(
+		113, "GPIO113",
+		MTK_EINT_FUNCTION(0, 113),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO113"),
+		MTK_FUNCTION(1, "CONN_TOP_CLK"),
+		MTK_FUNCTION(3, "SCL6"),
+		MTK_FUNCTION(4, "AUXIF_CLK0"),
+		MTK_FUNCTION(6, "TP_UCTS1_AO")
+	),
+	MTK_PIN(
+		114, "GPIO114",
+		MTK_EINT_FUNCTION(0, 114),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO114"),
+		MTK_FUNCTION(1, "CONN_TOP_DATA"),
+		MTK_FUNCTION(3, "SDA6"),
+		MTK_FUNCTION(4, "AUXIF_ST0"),
+		MTK_FUNCTION(6, "TP_URTS1_AO")
+	),
+	MTK_PIN(
+		115, "GPIO115",
+		MTK_EINT_FUNCTION(0, 115),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO115"),
+		MTK_FUNCTION(1, "CONN_BT_CLK"),
+		MTK_FUNCTION(2, "UTXD1"),
+		MTK_FUNCTION(3, "PTA_TXD"),
+		MTK_FUNCTION(4, "AUXIF_CLK1"),
+		MTK_FUNCTION(5, "DAP_MD32_SWD"),
+		MTK_FUNCTION(6, "TP_UTXD1_AO")
+	),
+	MTK_PIN(
+		116, "GPIO116",
+		MTK_EINT_FUNCTION(0, 116),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO116"),
+		MTK_FUNCTION(1, "CONN_BT_DATA"),
+		MTK_FUNCTION(2, "IPU_JTAG_TRST"),
+		MTK_FUNCTION(4, "AUXIF_ST1"),
+		MTK_FUNCTION(5, "DAP_MD32_SWCK"),
+		MTK_FUNCTION(6, "TP_URXD2_AO"),
+		MTK_FUNCTION(7, "DBG_MON_A0")
+	),
+	MTK_PIN(
+		117, "GPIO117",
+		MTK_EINT_FUNCTION(0, 117),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO117"),
+		MTK_FUNCTION(1, "CONN_WF_HB0"),
+		MTK_FUNCTION(2, "IPU_JTAG_TDO"),
+		MTK_FUNCTION(6, "TP_UTXD2_AO"),
+		MTK_FUNCTION(7, "DBG_MON_A4")
+	),
+	MTK_PIN(
+		118, "GPIO118",
+		MTK_EINT_FUNCTION(0, 118),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO118"),
+		MTK_FUNCTION(1, "CONN_WF_HB1"),
+		MTK_FUNCTION(2, "IPU_JTAG_TDI"),
+		MTK_FUNCTION(5, "SSPM_URXD_AO"),
+		MTK_FUNCTION(6, "TP_UCTS2_AO"),
+		MTK_FUNCTION(7, "DBG_MON_A5")
+	),
+	MTK_PIN(
+		119, "GPIO119",
+		MTK_EINT_FUNCTION(0, 119),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO119"),
+		MTK_FUNCTION(1, "CONN_WF_HB2"),
+		MTK_FUNCTION(2, "IPU_JTAG_TCK"),
+		MTK_FUNCTION(5, "SSPM_UTXD_AO"),
+		MTK_FUNCTION(6, "TP_URTS2_AO")
+	),
+	MTK_PIN(
+		120, "GPIO120",
+		MTK_EINT_FUNCTION(0, 120),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO120"),
+		MTK_FUNCTION(1, "CONN_WB_PTA"),
+		MTK_FUNCTION(2, "IPU_JTAG_TMS"),
+		MTK_FUNCTION(5, "CCU_URXD_AO")
+	),
+	MTK_PIN(
+		121, "GPIO121",
+		MTK_EINT_FUNCTION(0, 121),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO121"),
+		MTK_FUNCTION(1, "CONN_HRST_B"),
+		MTK_FUNCTION(2, "URXD1"),
+		MTK_FUNCTION(3, "PTA_RXD"),
+		MTK_FUNCTION(5, "CCU_UTXD_AO"),
+		MTK_FUNCTION(6, "TP_URXD1_AO")
+	),
+	MTK_PIN(
+		122, "GPIO122",
+		MTK_EINT_FUNCTION(0, 122),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO122"),
+		MTK_FUNCTION(1, "MSDC0_CMD"),
+		MTK_FUNCTION(2, "SSPM_URXD2_AO"),
+		MTK_FUNCTION(3, "ANT_SEL1"),
+		MTK_FUNCTION(7, "DBG_MON_A12")
+	),
+	MTK_PIN(
+		123, "GPIO123",
+		MTK_EINT_FUNCTION(0, 123),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO123"),
+		MTK_FUNCTION(1, "MSDC0_DAT0"),
+		MTK_FUNCTION(3, "ANT_SEL0"),
+		MTK_FUNCTION(7, "DBG_MON_A13")
+	),
+	MTK_PIN(
+		124, "GPIO124",
+		MTK_EINT_FUNCTION(0, 124),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO124"),
+		MTK_FUNCTION(1, "MSDC0_CLK"),
+		MTK_FUNCTION(7, "DBG_MON_A14")
+	),
+	MTK_PIN(
+		125, "GPIO125",
+		MTK_EINT_FUNCTION(0, 125),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO125"),
+		MTK_FUNCTION(1, "MSDC0_DAT2"),
+		MTK_FUNCTION(3, "MRG_CLK"),
+		MTK_FUNCTION(7, "DBG_MON_A15")
+	),
+	MTK_PIN(
+		126, "GPIO126",
+		MTK_EINT_FUNCTION(0, 126),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO126"),
+		MTK_FUNCTION(1, "MSDC0_DAT4"),
+		MTK_FUNCTION(3, "ANT_SEL5"),
+		MTK_FUNCTION(6, "UFS_MPHY_SCL"),
+		MTK_FUNCTION(7, "DBG_MON_A16")
+	),
+	MTK_PIN(
+		127, "GPIO127",
+		MTK_EINT_FUNCTION(0, 127),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO127"),
+		MTK_FUNCTION(1, "MSDC0_DAT6"),
+		MTK_FUNCTION(3, "ANT_SEL4"),
+		MTK_FUNCTION(6, "UFS_MPHY_SDA"),
+		MTK_FUNCTION(7, "DBG_MON_A17")
+	),
+	MTK_PIN(
+		128, "GPIO128",
+		MTK_EINT_FUNCTION(0, 128),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO128"),
+		MTK_FUNCTION(1, "MSDC0_DAT1"),
+		MTK_FUNCTION(3, "ANT_SEL2"),
+		MTK_FUNCTION(6, "UFS_UNIPRO_SDA"),
+		MTK_FUNCTION(7, "DBG_MON_A18")
+	),
+	MTK_PIN(
+		129, "GPIO129",
+		MTK_EINT_FUNCTION(0, 129),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO129"),
+		MTK_FUNCTION(1, "MSDC0_DAT5"),
+		MTK_FUNCTION(3, "ANT_SEL3"),
+		MTK_FUNCTION(6, "UFS_UNIPRO_SCL"),
+		MTK_FUNCTION(7, "DBG_MON_A23")
+	),
+	MTK_PIN(
+		130, "GPIO130",
+		MTK_EINT_FUNCTION(0, 130),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO130"),
+		MTK_FUNCTION(1, "MSDC0_DAT7"),
+		MTK_FUNCTION(3, "MRG_DO"),
+		MTK_FUNCTION(7, "DBG_MON_A24")
+	),
+	MTK_PIN(
+		131, "GPIO131",
+		MTK_EINT_FUNCTION(0, 131),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO131"),
+		MTK_FUNCTION(1, "MSDC0_DSL"),
+		MTK_FUNCTION(3, "MRG_SYNC"),
+		MTK_FUNCTION(7, "DBG_MON_A25")
+	),
+	MTK_PIN(
+		132, "GPIO132",
+		MTK_EINT_FUNCTION(0, 132),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO132"),
+		MTK_FUNCTION(1, "MSDC0_DAT3"),
+		MTK_FUNCTION(3, "MRG_DI"),
+		MTK_FUNCTION(7, "DBG_MON_A26")
+	),
+	MTK_PIN(
+		133, "GPIO133",
+		MTK_EINT_FUNCTION(0, 133),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO133"),
+		MTK_FUNCTION(1, "MSDC0_RSTB"),
+		MTK_FUNCTION(3, "AGPS_SYNC"),
+		MTK_FUNCTION(7, "DBG_MON_A27")
+	),
+	MTK_PIN(
+		134, "GPIO134",
+		MTK_EINT_FUNCTION(0, 134),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO134"),
+		MTK_FUNCTION(1, "RTC32K_CK")
+	),
+	MTK_PIN(
+		135, "GPIO135",
+		MTK_EINT_FUNCTION(0, 135),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO135"),
+		MTK_FUNCTION(1, "WATCHDOG")
+	),
+	MTK_PIN(
+		136, "GPIO136",
+		MTK_EINT_FUNCTION(0, 136),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO136"),
+		MTK_FUNCTION(1, "AUD_CLK_MOSI"),
+		MTK_FUNCTION(2, "AUD_CLK_MISO"),
+		MTK_FUNCTION(3, "I2S1_MCK"),
+		MTK_FUNCTION(6, "UFS_UNIPRO_SCL")
+	),
+	MTK_PIN(
+		137, "GPIO137",
+		MTK_EINT_FUNCTION(0, 137),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO137"),
+		MTK_FUNCTION(1, "AUD_SYNC_MOSI"),
+		MTK_FUNCTION(2, "AUD_SYNC_MISO"),
+		MTK_FUNCTION(3, "I2S1_BCK")
+	),
+	MTK_PIN(
+		138, "GPIO138",
+		MTK_EINT_FUNCTION(0, 138),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO138"),
+		MTK_FUNCTION(1, "AUD_DAT_MOSI0"),
+		MTK_FUNCTION(2, "AUD_DAT_MISO0"),
+		MTK_FUNCTION(3, "I2S1_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_B24")
+	),
+	MTK_PIN(
+		139, "GPIO139",
+		MTK_EINT_FUNCTION(0, 139),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO139"),
+		MTK_FUNCTION(1, "AUD_DAT_MOSI1"),
+		MTK_FUNCTION(2, "AUD_DAT_MISO1"),
+		MTK_FUNCTION(3, "I2S1_DO"),
+		MTK_FUNCTION(6, "UFS_MPHY_SDA")
+	),
+	MTK_PIN(
+		140, "GPIO140",
+		MTK_EINT_FUNCTION(0, 140),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO140"),
+		MTK_FUNCTION(1, "AUD_CLK_MISO"),
+		MTK_FUNCTION(2, "AUD_CLK_MOSI"),
+		MTK_FUNCTION(3, "I2S0_MCK"),
+		MTK_FUNCTION(6, "UFS_UNIPRO_SDA")
+	),
+	MTK_PIN(
+		141, "GPIO141",
+		MTK_EINT_FUNCTION(0, 141),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO141"),
+		MTK_FUNCTION(1, "AUD_SYNC_MISO"),
+		MTK_FUNCTION(2, "AUD_SYNC_MOSI"),
+		MTK_FUNCTION(3, "I2S0_BCK")
+	),
+	MTK_PIN(
+		142, "GPIO142",
+		MTK_EINT_FUNCTION(0, 142),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO142"),
+		MTK_FUNCTION(1, "AUD_DAT_MISO0"),
+		MTK_FUNCTION(2, "AUD_DAT_MOSI0"),
+		MTK_FUNCTION(3, "I2S0_LRCK"),
+		MTK_FUNCTION(4, "VOW_DAT_MISO"),
+		MTK_FUNCTION(7, "DBG_MON_B25")
+	),
+	MTK_PIN(
+		143, "GPIO143",
+		MTK_EINT_FUNCTION(0, 143),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO143"),
+		MTK_FUNCTION(1, "AUD_DAT_MISO1"),
+		MTK_FUNCTION(2, "AUD_DAT_MOSI1"),
+		MTK_FUNCTION(3, "I2S0_DI"),
+		MTK_FUNCTION(4, "VOW_CLK_MISO"),
+		MTK_FUNCTION(6, "UFS_MPHY_SCL"),
+		MTK_FUNCTION(7, "DBG_MON_B26")
+	),
+	MTK_PIN(
+		144, "GPIO144",
+		MTK_EINT_FUNCTION(0, 144),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO144"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_MI"),
+		MTK_FUNCTION(2, "PWRAP_SPI0_MO")
+	),
+	MTK_PIN(
+		145, "GPIO145",
+		MTK_EINT_FUNCTION(0, 145),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO145"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_CSN")
+	),
+	MTK_PIN(
+		146, "GPIO146",
+		MTK_EINT_FUNCTION(0, 146),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO146"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_MO"),
+		MTK_FUNCTION(2, "PWRAP_SPI0_MI")
+	),
+	MTK_PIN(
+		147, "GPIO147",
+		MTK_EINT_FUNCTION(0, 147),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO147"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_CK")
+	),
+	MTK_PIN(
+		148, "GPIO148",
+		MTK_EINT_FUNCTION(0, 148),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO148"),
+		MTK_FUNCTION(1, "SRCLKENA0")
+	),
+	MTK_PIN(
+		149, "GPIO149",
+		MTK_EINT_FUNCTION(0, 149),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO149"),
+		MTK_FUNCTION(1, "SRCLKENA1")
+	),
+	MTK_PIN(
+		150, "GPIO150",
+		MTK_EINT_FUNCTION(0, 150),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO150"),
+		MTK_FUNCTION(1, "PWM_A"),
+		MTK_FUNCTION(2, "CMFLASH"),
+		MTK_FUNCTION(3, "CLKM0"),
+		MTK_FUNCTION(7, "DBG_MON_B30")
+	),
+	MTK_PIN(
+		151, "GPIO151",
+		MTK_EINT_FUNCTION(0, 151),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO151"),
+		MTK_FUNCTION(1, "PWM_B"),
+		MTK_FUNCTION(2, "CMVREF0"),
+		MTK_FUNCTION(3, "CLKM1"),
+		MTK_FUNCTION(7, "DBG_MON_B20")
+	),
+	MTK_PIN(
+		152, "GPIO152",
+		MTK_EINT_FUNCTION(0, 152),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO152"),
+		MTK_FUNCTION(1, "PWM_C"),
+		MTK_FUNCTION(2, "CMFLASH"),
+		MTK_FUNCTION(3, "CLKM2"),
+		MTK_FUNCTION(7, "DBG_MON_B21")
+	),
+	MTK_PIN(
+		153, "GPIO153",
+		MTK_EINT_FUNCTION(0, 153),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO153"),
+		MTK_FUNCTION(1, "PWM_A"),
+		MTK_FUNCTION(2, "CMVREF0"),
+		MTK_FUNCTION(3, "CLKM3"),
+		MTK_FUNCTION(7, "DBG_MON_B22")
+	),
+	MTK_PIN(
+		154, "GPIO154",
+		MTK_EINT_FUNCTION(0, 154),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO154"),
+		MTK_FUNCTION(1, "SCP_VREQ_VAO"),
+		MTK_FUNCTION(2, "DVFSRC_EXT_REQ"),
+		MTK_FUNCTION(7, "DBG_MON_B18")
+	),
+	MTK_PIN(
+		155, "GPIO155",
+		MTK_EINT_FUNCTION(0, 155),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO155"),
+		MTK_FUNCTION(1, "ANT_SEL0"),
+		MTK_FUNCTION(2, "DVFSRC_EXT_REQ"),
+		MTK_FUNCTION(3, "CMVREF1"),
+		MTK_FUNCTION(7, "SCP_JTAG_TDI")
+	),
+	MTK_PIN(
+		156, "GPIO156",
+		MTK_EINT_FUNCTION(0, 156),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO156"),
+		MTK_FUNCTION(1, "ANT_SEL1"),
+		MTK_FUNCTION(2, "SRCLKENAI0"),
+		MTK_FUNCTION(3, "SCL6"),
+		MTK_FUNCTION(4, "KPCOL2"),
+		MTK_FUNCTION(5, "IDDIG"),
+		MTK_FUNCTION(7, "SCP_JTAG_TCK")
+	),
+	MTK_PIN(
+		157, "GPIO157",
+		MTK_EINT_FUNCTION(0, 157),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO157"),
+		MTK_FUNCTION(1, "ANT_SEL2"),
+		MTK_FUNCTION(2, "SRCLKENAI1"),
+		MTK_FUNCTION(3, "SDA6"),
+		MTK_FUNCTION(4, "KPROW2"),
+		MTK_FUNCTION(5, "USB_DRVVBUS"),
+		MTK_FUNCTION(7, "SCP_JTAG_TRSTN")
+	),
+	MTK_PIN(
+		158, "GPIO158",
+		MTK_EINT_FUNCTION(0, 158),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO158"),
+		MTK_FUNCTION(1, "ANT_SEL3")
+	),
+	MTK_PIN(
+		159, "GPIO159",
+		MTK_EINT_FUNCTION(0, 159),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO159"),
+		MTK_FUNCTION(1, "ANT_SEL4")
+	),
+	MTK_PIN(
+		160, "GPIO160",
+		MTK_EINT_FUNCTION(0, 160),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO160"),
+		MTK_FUNCTION(1, "ANT_SEL5")
+	),
+	MTK_PIN(
+		161, "GPIO161",
+		MTK_EINT_FUNCTION(0, 161),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO161"),
+		MTK_FUNCTION(1, "SPI1_A_MI"),
+		MTK_FUNCTION(2, "SCP_SPI1_MI"),
+		MTK_FUNCTION(3, "IDDIG"),
+		MTK_FUNCTION(4, "ANT_SEL6"),
+		MTK_FUNCTION(5, "KPCOL2"),
+		MTK_FUNCTION(6, "PTA_RXD"),
+		MTK_FUNCTION(7, "DBG_MON_B19")
+	),
+	MTK_PIN(
+		162, "GPIO162",
+		MTK_EINT_FUNCTION(0, 162),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO162"),
+		MTK_FUNCTION(1, "SPI1_A_CSB"),
+		MTK_FUNCTION(2, "SCP_SPI1_CS"),
+		MTK_FUNCTION(3, "USB_DRVVBUS"),
+		MTK_FUNCTION(4, "ANT_SEL5"),
+		MTK_FUNCTION(5, "KPROW2"),
+		MTK_FUNCTION(6, "PTA_TXD")
+	),
+	MTK_PIN(
+		163, "GPIO163",
+		MTK_EINT_FUNCTION(0, 163),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO163"),
+		MTK_FUNCTION(1, "SPI1_A_MO"),
+		MTK_FUNCTION(2, "SCP_SPI1_MO"),
+		MTK_FUNCTION(3, "SDA1"),
+		MTK_FUNCTION(4, "ANT_SEL4"),
+		MTK_FUNCTION(5, "CMMCLK2"),
+		MTK_FUNCTION(6, "DMIC_CLK")
+	),
+	MTK_PIN(
+		164, "GPIO164",
+		MTK_EINT_FUNCTION(0, 164),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO164"),
+		MTK_FUNCTION(1, "SPI1_A_CLK"),
+		MTK_FUNCTION(2, "SCP_SPI1_CK"),
+		MTK_FUNCTION(3, "SCL1"),
+		MTK_FUNCTION(4, "ANT_SEL3"),
+		MTK_FUNCTION(5, "CMMCLK3"),
+		MTK_FUNCTION(6, "DMIC_DAT")
+	),
+	MTK_PIN(
+		165, "GPIO165",
+		MTK_EINT_FUNCTION(0, 165),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO165"),
+		MTK_FUNCTION(1, "PWM_B"),
+		MTK_FUNCTION(2, "CMMCLK2"),
+		MTK_FUNCTION(3, "SCP_VREQ_VAO"),
+		MTK_FUNCTION(6, "TDM_MCK_2ND"),
+		MTK_FUNCTION(7, "SCP_JTAG_TDO")
+	),
+	MTK_PIN(
+		166, "GPIO166",
+		MTK_EINT_FUNCTION(0, 166),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO166"),
+		MTK_FUNCTION(1, "ANT_SEL6")
+	),
+	MTK_PIN(
+		167, "GPIO167",
+		MTK_EINT_FUNCTION(0, 167),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO167"),
+		MTK_FUNCTION(1, "RFIC0_BSI_EN"),
+		MTK_FUNCTION(2, "SPM_BSI_EN")
+	),
+	MTK_PIN(
+		168, "GPIO168",
+		MTK_EINT_FUNCTION(0, 168),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO168"),
+		MTK_FUNCTION(1, "RFIC0_BSI_CK"),
+		MTK_FUNCTION(2, "SPM_BSI_CK")
+	),
+	MTK_PIN(
+		169, "GPIO169",
+		MTK_EINT_FUNCTION(0, 169),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO169"),
+		MTK_FUNCTION(1, "PWM_C"),
+		MTK_FUNCTION(2, "CMMCLK3"),
+		MTK_FUNCTION(3, "CMVREF1"),
+		MTK_FUNCTION(4, "ANT_SEL7"),
+		MTK_FUNCTION(5, "AGPS_SYNC"),
+		MTK_FUNCTION(6, "TDM_BCK_2ND"),
+		MTK_FUNCTION(7, "SCP_JTAG_TMS")
+	),
+	MTK_PIN(
+		170, "GPIO170",
+		MTK_EINT_FUNCTION(0, 170),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO170"),
+		MTK_FUNCTION(1, "I2S1_BCK"),
+		MTK_FUNCTION(2, "I2S3_BCK"),
+		MTK_FUNCTION(3, "SCL7"),
+		MTK_FUNCTION(4, "I2S5_BCK"),
+		MTK_FUNCTION(5, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(6, "TDM_LRCK_2ND"),
+		MTK_FUNCTION(7, "ANT_SEL3")
+	),
+	MTK_PIN(
+		171, "GPIO171",
+		MTK_EINT_FUNCTION(0, 184),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO171"),
+		MTK_FUNCTION(1, "I2S1_LRCK"),
+		MTK_FUNCTION(2, "I2S3_LRCK"),
+		MTK_FUNCTION(3, "SDA7"),
+		MTK_FUNCTION(4, "I2S5_LRCK"),
+		MTK_FUNCTION(5, "URXD1"),
+		MTK_FUNCTION(6, "TDM_DATA0_2ND"),
+		MTK_FUNCTION(7, "ANT_SEL4")
+	),
+	MTK_PIN(
+		172, "GPIO172",
+		MTK_EINT_FUNCTION(0, 185),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO172"),
+		MTK_FUNCTION(1, "I2S1_DO"),
+		MTK_FUNCTION(2, "I2S3_DO"),
+		MTK_FUNCTION(3, "SCL8"),
+		MTK_FUNCTION(4, "I2S5_DO"),
+		MTK_FUNCTION(5, "UTXD1"),
+		MTK_FUNCTION(6, "TDM_DATA1_2ND"),
+		MTK_FUNCTION(7, "ANT_SEL5")
+	),
+	MTK_PIN(
+		173, "GPIO173",
+		MTK_EINT_FUNCTION(0, 186),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO173"),
+		MTK_FUNCTION(1, "I2S1_MCK"),
+		MTK_FUNCTION(2, "I2S3_MCK"),
+		MTK_FUNCTION(3, "SDA8"),
+		MTK_FUNCTION(4, "I2S5_MCK"),
+		MTK_FUNCTION(5, "UCTS0"),
+		MTK_FUNCTION(6, "TDM_DATA2_2ND"),
+		MTK_FUNCTION(7, "ANT_SEL6")
+	),
+	MTK_PIN(
+		174, "GPIO174",
+		MTK_EINT_FUNCTION(0, 187),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO174"),
+		MTK_FUNCTION(1, "I2S2_DI"),
+		MTK_FUNCTION(2, "I2S0_DI"),
+		MTK_FUNCTION(3, "DVFSRC_EXT_REQ"),
+		MTK_FUNCTION(4, "I2S2_DI2"),
+		MTK_FUNCTION(5, "URTS0"),
+		MTK_FUNCTION(6, "TDM_DATA3_2ND"),
+		MTK_FUNCTION(7, "ANT_SEL7")
+	),
+	MTK_PIN(
+		175, "GPIO175",
+		MTK_EINT_FUNCTION(0, 188),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO175"),
+		MTK_FUNCTION(1, "ANT_SEL7")
+	),
+	MTK_PIN(
+		176, "GPIO176",
+		MTK_EINT_FUNCTION(0, 189),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO176")
+	),
+	MTK_PIN(
+		177, "GPIO177",
+		MTK_EINT_FUNCTION(0, 190),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO177")
+	),
+	MTK_PIN(
+		178, "GPIO178",
+		MTK_EINT_FUNCTION(0, 191),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO178")
+	),
+	MTK_PIN(
+		179, "GPIO179",
+		MTK_EINT_FUNCTION(0, 192),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO179")
+	),
+	MTK_PIN(
+		180, "GPIO180",
+		MTK_EINT_FUNCTION(0, 171),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO180")
+	),
+	MTK_PIN(
+		181, "GPIO181",
+		MTK_EINT_FUNCTION(0, 172),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO181")
+	),
+	MTK_PIN(
+		182, "GPIO182",
+		MTK_EINT_FUNCTION(0, 173),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO182")
+	),
+	MTK_PIN(
+		183, "GPIO183",
+		MTK_EINT_FUNCTION(0, 174),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO183")
+	),
+	MTK_PIN(
+		184, "GPIO184",
+		MTK_EINT_FUNCTION(0, 175),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO184")
+	),
+	MTK_PIN(
+		185, "GPIO185",
+		MTK_EINT_FUNCTION(0, 177),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO185")
+	),
+	MTK_PIN(
+		186, "GPIO186",
+		MTK_EINT_FUNCTION(0, 178),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO186")
+	),
+	MTK_PIN(
+		187, "GPIO187",
+		MTK_EINT_FUNCTION(0, 179),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO187")
+	),
+	MTK_PIN(
+		188, "GPIO188",
+		MTK_EINT_FUNCTION(0, 180),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO188")
+	),
+	MTK_PIN(
+		189, "GPIO189",
+		MTK_EINT_FUNCTION(0, 181),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO189")
+	),
+	MTK_PIN(
+		190, "GPIO190",
+		MTK_EINT_FUNCTION(0, 182),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO190")
+	),
+	MTK_PIN(
+		191, "GPIO191",
+		MTK_EINT_FUNCTION(0, 183),
+		DRV_GRP4,
+		MTK_FUNCTION(0, "GPIO191")
+	),
+};
+
+#endif /* __PINCTRL_MTK_MT8183_H */
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mtk-mt8516.h
@@ -0,0 +1,1182 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2019 MediaTek Inc.
+ */
+#ifndef __PINCTRL_MTK_MT8516_H
+#define __PINCTRL_MTK_MT8516_H
+
+#include <linux/pinctrl/pinctrl.h>
+#include "pinctrl-mtk-common.h"
+
+static const struct mtk_desc_pin mtk_pins_mt8516[] = {
+	MTK_PIN(
+		PINCTRL_PIN(0, "EINT0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 0),
+		MTK_FUNCTION(0, "GPIO0"),
+		MTK_FUNCTION(1, "PWM_B"),
+		MTK_FUNCTION(3, "I2S2_BCK"),
+		MTK_FUNCTION(4, "EXT_TXD0"),
+		MTK_FUNCTION(6, "SQICS"),
+		MTK_FUNCTION(7, "DBG_MON_A[6]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(1, "EINT1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 1),
+		MTK_FUNCTION(0, "GPIO1"),
+		MTK_FUNCTION(1, "PWM_C"),
+		MTK_FUNCTION(3, "I2S2_DI"),
+		MTK_FUNCTION(4, "EXT_TXD1"),
+		MTK_FUNCTION(5, "CONN_MCU_TDO"),
+		MTK_FUNCTION(6, "SQISO"),
+		MTK_FUNCTION(7, "DBG_MON_A[7]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(2, "EINT2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 2),
+		MTK_FUNCTION(0, "GPIO2"),
+		MTK_FUNCTION(1, "CLKM0"),
+		MTK_FUNCTION(3, "I2S2_LRCK"),
+		MTK_FUNCTION(4, "EXT_TXD2"),
+		MTK_FUNCTION(5, "CONN_MCU_DBGACK_N"),
+		MTK_FUNCTION(6, "SQISI"),
+		MTK_FUNCTION(7, "DBG_MON_A[8]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(3, "EINT3"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 3),
+		MTK_FUNCTION(0, "GPIO3"),
+		MTK_FUNCTION(1, "CLKM1"),
+		MTK_FUNCTION(3, "SPI_MI"),
+		MTK_FUNCTION(4, "EXT_TXD3"),
+		MTK_FUNCTION(5, "CONN_MCU_DBGI_N"),
+		MTK_FUNCTION(6, "SQIWP"),
+		MTK_FUNCTION(7, "DBG_MON_A[9]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(4, "EINT4"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 4),
+		MTK_FUNCTION(0, "GPIO4"),
+		MTK_FUNCTION(1, "CLKM2"),
+		MTK_FUNCTION(3, "SPI_MO"),
+		MTK_FUNCTION(4, "EXT_TXC"),
+		MTK_FUNCTION(5, "CONN_MCU_TCK"),
+		MTK_FUNCTION(6, "CONN_MCU_AICE_JCKC"),
+		MTK_FUNCTION(7, "DBG_MON_A[10]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(5, "EINT5"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 5),
+		MTK_FUNCTION(0, "GPIO5"),
+		MTK_FUNCTION(1, "UCTS2"),
+		MTK_FUNCTION(3, "SPI_CSB"),
+		MTK_FUNCTION(4, "EXT_RXER"),
+		MTK_FUNCTION(5, "CONN_MCU_TDI"),
+		MTK_FUNCTION(6, "CONN_TEST_CK"),
+		MTK_FUNCTION(7, "DBG_MON_A[11]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(6, "EINT6"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 6),
+		MTK_FUNCTION(0, "GPIO6"),
+		MTK_FUNCTION(1, "URTS2"),
+		MTK_FUNCTION(3, "SPI_CLK"),
+		MTK_FUNCTION(4, "EXT_RXC"),
+		MTK_FUNCTION(5, "CONN_MCU_TRST_B"),
+		MTK_FUNCTION(7, "DBG_MON_A[12]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(7, "EINT7"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 7),
+		MTK_FUNCTION(0, "GPIO7"),
+		MTK_FUNCTION(1, "SQIRST"),
+		MTK_FUNCTION(3, "SDA1_0"),
+		MTK_FUNCTION(4, "EXT_RXDV"),
+		MTK_FUNCTION(5, "CONN_MCU_TMS"),
+		MTK_FUNCTION(6, "CONN_MCU_AICE_JMSC"),
+		MTK_FUNCTION(7, "DBG_MON_A[13]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(8, "EINT8"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 8),
+		MTK_FUNCTION(0, "GPIO8"),
+		MTK_FUNCTION(1, "SQICK"),
+		MTK_FUNCTION(2, "CLKM3"),
+		MTK_FUNCTION(3, "SCL1_0"),
+		MTK_FUNCTION(4, "EXT_RXD0"),
+		MTK_FUNCTION(5, "ANT_SEL0"),
+		MTK_FUNCTION(7, "DBG_MON_A[14]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(9, "EINT9"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 9),
+		MTK_FUNCTION(0, "GPIO9"),
+		MTK_FUNCTION(1, "CLKM4"),
+		MTK_FUNCTION(2, "SDA2_0"),
+		MTK_FUNCTION(3, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(4, "EXT_RXD1"),
+		MTK_FUNCTION(5, "ANT_SEL1"),
+		MTK_FUNCTION(7, "DBG_MON_A[15]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(10, "EINT10"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 10),
+		MTK_FUNCTION(0, "GPIO10"),
+		MTK_FUNCTION(1, "CLKM5"),
+		MTK_FUNCTION(2, "SCL2_0"),
+		MTK_FUNCTION(3, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(4, "EXT_RXD2"),
+		MTK_FUNCTION(5, "ANT_SEL2"),
+		MTK_FUNCTION(7, "DBG_MON_A[16]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(11, "EINT11"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 11),
+		MTK_FUNCTION(0, "GPIO11"),
+		MTK_FUNCTION(1, "CLKM4"),
+		MTK_FUNCTION(2, "PWM_C"),
+		MTK_FUNCTION(3, "CONN_TEST_CK"),
+		MTK_FUNCTION(4, "ANT_SEL3"),
+		MTK_FUNCTION(6, "EXT_RXD3"),
+		MTK_FUNCTION(7, "DBG_MON_A[17]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(12, "EINT12"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 12),
+		MTK_FUNCTION(0, "GPIO12"),
+		MTK_FUNCTION(1, "CLKM5"),
+		MTK_FUNCTION(2, "PWM_A"),
+		MTK_FUNCTION(3, "SPDIF_OUT"),
+		MTK_FUNCTION(4, "ANT_SEL4"),
+		MTK_FUNCTION(6, "EXT_TXEN"),
+		MTK_FUNCTION(7, "DBG_MON_A[18]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(13, "EINT13"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 13),
+		MTK_FUNCTION(0, "GPIO13"),
+		MTK_FUNCTION(3, "TSF_IN"),
+		MTK_FUNCTION(4, "ANT_SEL5"),
+		MTK_FUNCTION(6, "SPDIF_IN"),
+		MTK_FUNCTION(7, "DBG_MON_A[19]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(14, "EINT14"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 14),
+		MTK_FUNCTION(0, "GPIO14"),
+		MTK_FUNCTION(2, "I2S_8CH_DO1"),
+		MTK_FUNCTION(3, "TDM_RX_MCK"),
+		MTK_FUNCTION(4, "ANT_SEL1"),
+		MTK_FUNCTION(5, "CONN_MCU_DBGACK_N"),
+		MTK_FUNCTION(6, "NCLE"),
+		MTK_FUNCTION(7, "DBG_MON_B[8]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(15, "EINT15"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 15),
+		MTK_FUNCTION(0, "GPIO15"),
+		MTK_FUNCTION(2, "I2S_8CH_LRCK"),
+		MTK_FUNCTION(3, "TDM_RX_BCK"),
+		MTK_FUNCTION(4, "ANT_SEL2"),
+		MTK_FUNCTION(5, "CONN_MCU_DBGI_N"),
+		MTK_FUNCTION(6, "NCEB1"),
+		MTK_FUNCTION(7, "DBG_MON_B[9]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(16, "EINT16"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 16),
+		MTK_FUNCTION(0, "GPIO16"),
+		MTK_FUNCTION(2, "I2S_8CH_BCK"),
+		MTK_FUNCTION(3, "TDM_RX_LRCK"),
+		MTK_FUNCTION(4, "ANT_SEL3"),
+		MTK_FUNCTION(5, "CONN_MCU_TRST_B"),
+		MTK_FUNCTION(6, "NCEB0"),
+		MTK_FUNCTION(7, "DBG_MON_B[10]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(17, "EINT17"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 17),
+		MTK_FUNCTION(0, "GPIO17"),
+		MTK_FUNCTION(2, "I2S_8CH_MCK"),
+		MTK_FUNCTION(3, "TDM_RX_DI"),
+		MTK_FUNCTION(4, "IDDIG"),
+		MTK_FUNCTION(5, "ANT_SEL4"),
+		MTK_FUNCTION(6, "NREB"),
+		MTK_FUNCTION(7, "DBG_MON_B[11]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(18, "EINT18"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 18),
+		MTK_FUNCTION(0, "GPIO18"),
+		MTK_FUNCTION(2, "USB_DRVVBUS"),
+		MTK_FUNCTION(3, "I2S3_LRCK"),
+		MTK_FUNCTION(4, "CLKM1"),
+		MTK_FUNCTION(5, "ANT_SEL3"),
+		MTK_FUNCTION(6, "I2S2_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[20]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(19, "EINT19"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 19),
+		MTK_FUNCTION(0, "GPIO19"),
+		MTK_FUNCTION(1, "UCTS1"),
+		MTK_FUNCTION(2, "IDDIG"),
+		MTK_FUNCTION(3, "I2S3_BCK"),
+		MTK_FUNCTION(4, "CLKM2"),
+		MTK_FUNCTION(5, "ANT_SEL4"),
+		MTK_FUNCTION(6, "I2S2_DI"),
+		MTK_FUNCTION(7, "DBG_MON_A[21]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(20, "EINT20"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 20),
+		MTK_FUNCTION(0, "GPIO20"),
+		MTK_FUNCTION(1, "URTS1"),
+		MTK_FUNCTION(3, "I2S3_DO"),
+		MTK_FUNCTION(4, "CLKM3"),
+		MTK_FUNCTION(5, "ANT_SEL5"),
+		MTK_FUNCTION(6, "I2S2_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[22]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(21, "EINT21"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 21),
+		MTK_FUNCTION(0, "GPIO21"),
+		MTK_FUNCTION(1, "NRNB"),
+		MTK_FUNCTION(2, "ANT_SEL0"),
+		MTK_FUNCTION(3, "I2S_8CH_DO4"),
+		MTK_FUNCTION(7, "DBG_MON_B[31]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(22, "EINT22"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 22),
+		MTK_FUNCTION(0, "GPIO22"),
+		MTK_FUNCTION(2, "I2S_8CH_DO2"),
+		MTK_FUNCTION(3, "TSF_IN"),
+		MTK_FUNCTION(4, "USB_DRVVBUS"),
+		MTK_FUNCTION(5, "SPDIF_OUT"),
+		MTK_FUNCTION(6, "NRE_C"),
+		MTK_FUNCTION(7, "DBG_MON_B[12]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(23, "EINT23"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 23),
+		MTK_FUNCTION(0, "GPIO23"),
+		MTK_FUNCTION(2, "I2S_8CH_DO3"),
+		MTK_FUNCTION(3, "CLKM0"),
+		MTK_FUNCTION(4, "IR"),
+		MTK_FUNCTION(5, "SPDIF_IN"),
+		MTK_FUNCTION(6, "NDQS_C"),
+		MTK_FUNCTION(7, "DBG_MON_B[13]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(24, "EINT24"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 24),
+		MTK_FUNCTION(0, "GPIO24"),
+		MTK_FUNCTION(3, "ANT_SEL1"),
+		MTK_FUNCTION(4, "UCTS2"),
+		MTK_FUNCTION(5, "PWM_A"),
+		MTK_FUNCTION(6, "I2S0_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[0]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(25, "EINT25"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 25),
+		MTK_FUNCTION(0, "GPIO25"),
+		MTK_FUNCTION(3, "ANT_SEL0"),
+		MTK_FUNCTION(4, "URTS2"),
+		MTK_FUNCTION(5, "PWM_B"),
+		MTK_FUNCTION(6, "I2S_8CH_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[1]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(26, "PWRAP_SPI0_MI"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 26),
+		MTK_FUNCTION(0, "GPIO26"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_MO"),
+		MTK_FUNCTION(2, "PWRAP_SPI0_MI")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(27, "PWRAP_SPI0_MO"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 27),
+		MTK_FUNCTION(0, "GPIO27"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_MI"),
+		MTK_FUNCTION(2, "PWRAP_SPI0_MO")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(28, "PWRAP_INT"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 28),
+		MTK_FUNCTION(0, "GPIO28"),
+		MTK_FUNCTION(1, "I2S0_MCK"),
+		MTK_FUNCTION(4, "I2S_8CH_MCK"),
+		MTK_FUNCTION(5, "I2S2_MCK"),
+		MTK_FUNCTION(6, "I2S3_MCK")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(29, "PWRAP_SPI0_CK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 29),
+		MTK_FUNCTION(0, "GPIO29"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_CK")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(30, "PWRAP_SPI0_CSN"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 30),
+		MTK_FUNCTION(0, "GPIO30"),
+		MTK_FUNCTION(1, "PWRAP_SPI0_CSN")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(31, "RTC32K_CK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 31),
+		MTK_FUNCTION(0, "GPIO31"),
+		MTK_FUNCTION(1, "RTC32K_CK")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(32, "WATCHDOG"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 32),
+		MTK_FUNCTION(0, "GPIO32"),
+		MTK_FUNCTION(1, "WATCHDOG")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(33, "SRCLKENA"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 33),
+		MTK_FUNCTION(0, "GPIO33"),
+		MTK_FUNCTION(1, "SRCLKENA0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(34, "URXD2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 34),
+		MTK_FUNCTION(0, "GPIO34"),
+		MTK_FUNCTION(1, "URXD2"),
+		MTK_FUNCTION(3, "UTXD2"),
+		MTK_FUNCTION(4, "DBG_SCL"),
+		MTK_FUNCTION(6, "I2S2_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[0]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(35, "UTXD2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 35),
+		MTK_FUNCTION(0, "GPIO35"),
+		MTK_FUNCTION(1, "UTXD2"),
+		MTK_FUNCTION(3, "URXD2"),
+		MTK_FUNCTION(4, "DBG_SDA"),
+		MTK_FUNCTION(6, "I2S3_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[1]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(36, "MRG_CLK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 36),
+		MTK_FUNCTION(0, "GPIO36"),
+		MTK_FUNCTION(1, "MRG_CLK"),
+		MTK_FUNCTION(3, "I2S0_BCK"),
+		MTK_FUNCTION(4, "I2S3_BCK"),
+		MTK_FUNCTION(5, "PCM0_CLK"),
+		MTK_FUNCTION(6, "IR"),
+		MTK_FUNCTION(7, "DBG_MON_A[2]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(37, "MRG_SYNC"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 37),
+		MTK_FUNCTION(0, "GPIO37"),
+		MTK_FUNCTION(1, "MRG_SYNC"),
+		MTK_FUNCTION(3, "I2S0_LRCK"),
+		MTK_FUNCTION(4, "I2S3_LRCK"),
+		MTK_FUNCTION(5, "PCM0_SYNC"),
+		MTK_FUNCTION(6, "EXT_COL"),
+		MTK_FUNCTION(7, "DBG_MON_A[3]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(38, "MRG_DI"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 38),
+		MTK_FUNCTION(0, "GPIO38"),
+		MTK_FUNCTION(1, "MRG_DI"),
+		MTK_FUNCTION(3, "I2S0_DI"),
+		MTK_FUNCTION(4, "I2S3_DO"),
+		MTK_FUNCTION(5, "PCM0_DI"),
+		MTK_FUNCTION(6, "EXT_MDIO"),
+		MTK_FUNCTION(7, "DBG_MON_A[4]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(39, "MRG_DO"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 39),
+		MTK_FUNCTION(0, "GPIO39"),
+		MTK_FUNCTION(1, "MRG_DO"),
+		MTK_FUNCTION(3, "I2S0_MCK"),
+		MTK_FUNCTION(4, "I2S3_MCK"),
+		MTK_FUNCTION(5, "PCM0_DO"),
+		MTK_FUNCTION(6, "EXT_MDC"),
+		MTK_FUNCTION(7, "DBG_MON_A[5]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(40, "KPROW0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 40),
+		MTK_FUNCTION(0, "GPIO40"),
+		MTK_FUNCTION(1, "KPROW0"),
+		MTK_FUNCTION(7, "DBG_MON_B[4]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(41, "KPROW1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 41),
+		MTK_FUNCTION(0, "GPIO41"),
+		MTK_FUNCTION(1, "KPROW1"),
+		MTK_FUNCTION(2, "IDDIG"),
+		MTK_FUNCTION(3, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(7, "DBG_MON_B[5]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(42, "KPCOL0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 42),
+		MTK_FUNCTION(0, "GPIO42"),
+		MTK_FUNCTION(1, "KPCOL0"),
+		MTK_FUNCTION(7, "DBG_MON_B[6]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(43, "KPCOL1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 43),
+		MTK_FUNCTION(0, "GPIO43"),
+		MTK_FUNCTION(1, "KPCOL1"),
+		MTK_FUNCTION(2, "USB_DRVVBUS"),
+		MTK_FUNCTION(3, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(4, "TSF_IN"),
+		MTK_FUNCTION(7, "DBG_MON_B[7]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(44, "JTMS"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 44),
+		MTK_FUNCTION(0, "GPIO44"),
+		MTK_FUNCTION(1, "JTMS"),
+		MTK_FUNCTION(2, "CONN_MCU_TMS"),
+		MTK_FUNCTION(3, "CONN_MCU_AICE_JMSC")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(45, "JTCK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 45),
+		MTK_FUNCTION(0, "GPIO45"),
+		MTK_FUNCTION(1, "JTCK"),
+		MTK_FUNCTION(2, "CONN_MCU_TCK"),
+		MTK_FUNCTION(3, "CONN_MCU_AICE_JCKC")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(46, "JTDI"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 46),
+		MTK_FUNCTION(0, "GPIO46"),
+		MTK_FUNCTION(1, "JTDI"),
+		MTK_FUNCTION(2, "CONN_MCU_TDI")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(47, "JTDO"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 47),
+		MTK_FUNCTION(0, "GPIO47"),
+		MTK_FUNCTION(1, "JTDO"),
+		MTK_FUNCTION(2, "CONN_MCU_TDO")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(48, "SPI_CS"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 48),
+		MTK_FUNCTION(0, "GPIO48"),
+		MTK_FUNCTION(1, "SPI_CSB"),
+		MTK_FUNCTION(3, "I2S0_DI"),
+		MTK_FUNCTION(4, "I2S2_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[23]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(49, "SPI_CK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 49),
+		MTK_FUNCTION(0, "GPIO49"),
+		MTK_FUNCTION(1, "SPI_CLK"),
+		MTK_FUNCTION(3, "I2S0_LRCK"),
+		MTK_FUNCTION(4, "I2S2_DI"),
+		MTK_FUNCTION(7, "DBG_MON_A[24]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(50, "SPI_MI"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 50),
+		MTK_FUNCTION(0, "GPIO50"),
+		MTK_FUNCTION(1, "SPI_MI"),
+		MTK_FUNCTION(2, "SPI_MO"),
+		MTK_FUNCTION(3, "I2S0_BCK"),
+		MTK_FUNCTION(4, "I2S2_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[25]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(51, "SPI_MO"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 51),
+		MTK_FUNCTION(0, "GPIO51"),
+		MTK_FUNCTION(1, "SPI_MO"),
+		MTK_FUNCTION(2, "SPI_MI"),
+		MTK_FUNCTION(3, "I2S0_MCK"),
+		MTK_FUNCTION(4, "I2S2_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[26]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(52, "SDA1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 52),
+		MTK_FUNCTION(0, "GPIO52"),
+		MTK_FUNCTION(1, "SDA1_0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(53, "SCL1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 53),
+		MTK_FUNCTION(0, "GPIO53"),
+		MTK_FUNCTION(1, "SCL1_0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(54, "GPIO54"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 54),
+		MTK_FUNCTION(0, "GPIO54"),
+		MTK_FUNCTION(2, "PWM_B"),
+		MTK_FUNCTION(7, "DBG_MON_B[2]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(55, "I2S_DATA_IN"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 55),
+		MTK_FUNCTION(0, "GPIO55"),
+		MTK_FUNCTION(1, "I2S0_DI"),
+		MTK_FUNCTION(2, "UCTS0"),
+		MTK_FUNCTION(3, "I2S3_DO"),
+		MTK_FUNCTION(4, "I2S_8CH_DO1"),
+		MTK_FUNCTION(5, "PWM_A"),
+		MTK_FUNCTION(6, "I2S2_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[28]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(56, "I2S_LRCK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 56),
+		MTK_FUNCTION(0, "GPIO56"),
+		MTK_FUNCTION(1, "I2S0_LRCK"),
+		MTK_FUNCTION(3, "I2S3_LRCK"),
+		MTK_FUNCTION(4, "I2S_8CH_LRCK"),
+		MTK_FUNCTION(5, "PWM_B"),
+		MTK_FUNCTION(6, "I2S2_DI"),
+		MTK_FUNCTION(7, "DBG_MON_A[29]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(57, "I2S_BCK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 57),
+		MTK_FUNCTION(0, "GPIO57"),
+		MTK_FUNCTION(1, "I2S0_BCK"),
+		MTK_FUNCTION(2, "URTS0"),
+		MTK_FUNCTION(3, "I2S3_BCK"),
+		MTK_FUNCTION(4, "I2S_8CH_BCK"),
+		MTK_FUNCTION(5, "PWM_C"),
+		MTK_FUNCTION(6, "I2S2_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_A[30]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(58, "SDA0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 58),
+		MTK_FUNCTION(0, "GPIO58"),
+		MTK_FUNCTION(1, "SDA0_0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(59, "SCL0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 59),
+		MTK_FUNCTION(0, "GPIO59"),
+		MTK_FUNCTION(1, "SCL0_0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(60, "SDA2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 60),
+		MTK_FUNCTION(0, "GPIO60"),
+		MTK_FUNCTION(1, "SDA2_0"),
+		MTK_FUNCTION(2, "PWM_B")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(61, "SCL2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 61),
+		MTK_FUNCTION(0, "GPIO61"),
+		MTK_FUNCTION(1, "SCL2_0"),
+		MTK_FUNCTION(2, "PWM_C")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(62, "URXD0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 62),
+		MTK_FUNCTION(0, "GPIO62"),
+		MTK_FUNCTION(1, "URXD0"),
+		MTK_FUNCTION(2, "UTXD0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(63, "UTXD0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 63),
+		MTK_FUNCTION(0, "GPIO63"),
+		MTK_FUNCTION(1, "UTXD0"),
+		MTK_FUNCTION(2, "URXD0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(64, "URXD1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 64),
+		MTK_FUNCTION(0, "GPIO64"),
+		MTK_FUNCTION(1, "URXD1"),
+		MTK_FUNCTION(2, "UTXD1"),
+		MTK_FUNCTION(7, "DBG_MON_A[27]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(65, "UTXD1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 65),
+		MTK_FUNCTION(0, "GPIO65"),
+		MTK_FUNCTION(1, "UTXD1"),
+		MTK_FUNCTION(2, "URXD1"),
+		MTK_FUNCTION(7, "DBG_MON_A[31]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(66, "LCM_RST"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 66),
+		MTK_FUNCTION(0, "GPIO66"),
+		MTK_FUNCTION(1, "LCM_RST"),
+		MTK_FUNCTION(3, "I2S0_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[3]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(67, "GPIO67"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 67),
+		MTK_FUNCTION(0, "GPIO67"),
+		MTK_FUNCTION(3, "I2S_8CH_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[14]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(68, "MSDC2_CMD"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 68),
+		MTK_FUNCTION(0, "GPIO68"),
+		MTK_FUNCTION(1, "MSDC2_CMD"),
+		MTK_FUNCTION(2, "I2S_8CH_DO4"),
+		MTK_FUNCTION(3, "SDA1_0"),
+		MTK_FUNCTION(5, "USB_SDA"),
+		MTK_FUNCTION(6, "I2S3_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[15]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(69, "MSDC2_CLK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 69),
+		MTK_FUNCTION(0, "GPIO69"),
+		MTK_FUNCTION(1, "MSDC2_CLK"),
+		MTK_FUNCTION(2, "I2S_8CH_DO3"),
+		MTK_FUNCTION(3, "SCL1_0"),
+		MTK_FUNCTION(5, "USB_SCL"),
+		MTK_FUNCTION(6, "I2S3_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[16]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(70, "MSDC2_DAT0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 70),
+		MTK_FUNCTION(0, "GPIO70"),
+		MTK_FUNCTION(1, "MSDC2_DAT0"),
+		MTK_FUNCTION(2, "I2S_8CH_DO2"),
+		MTK_FUNCTION(5, "UTXD0"),
+		MTK_FUNCTION(6, "I2S3_DO"),
+		MTK_FUNCTION(7, "DBG_MON_B[17]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(71, "MSDC2_DAT1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 71),
+		MTK_FUNCTION(0, "GPIO71"),
+		MTK_FUNCTION(1, "MSDC2_DAT1"),
+		MTK_FUNCTION(2, "I2S_8CH_DO1"),
+		MTK_FUNCTION(3, "PWM_A"),
+		MTK_FUNCTION(4, "I2S3_MCK"),
+		MTK_FUNCTION(5, "URXD0"),
+		MTK_FUNCTION(6, "PWM_B"),
+		MTK_FUNCTION(7, "DBG_MON_B[18]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(72, "MSDC2_DAT2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 72),
+		MTK_FUNCTION(0, "GPIO72"),
+		MTK_FUNCTION(1, "MSDC2_DAT2"),
+		MTK_FUNCTION(2, "I2S_8CH_LRCK"),
+		MTK_FUNCTION(3, "SDA2_0"),
+		MTK_FUNCTION(5, "UTXD1"),
+		MTK_FUNCTION(6, "PWM_C"),
+		MTK_FUNCTION(7, "DBG_MON_B[19]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(73, "MSDC2_DAT3"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 73),
+		MTK_FUNCTION(0, "GPIO73"),
+		MTK_FUNCTION(1, "MSDC2_DAT3"),
+		MTK_FUNCTION(2, "I2S_8CH_BCK"),
+		MTK_FUNCTION(3, "SCL2_0"),
+		MTK_FUNCTION(4, "EXT_FRAME_SYNC"),
+		MTK_FUNCTION(5, "URXD1"),
+		MTK_FUNCTION(6, "PWM_A"),
+		MTK_FUNCTION(7, "DBG_MON_B[20]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(74, "TDN3"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 74),
+		MTK_FUNCTION(0, "GPIO74"),
+		MTK_FUNCTION(1, "TDN3")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(75, "TDP3"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 75),
+		MTK_FUNCTION(0, "GPIO75"),
+		MTK_FUNCTION(1, "TDP3")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(76, "TDN2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 76),
+		MTK_FUNCTION(0, "GPIO76"),
+		MTK_FUNCTION(1, "TDN2")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(77, "TDP2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 77),
+		MTK_FUNCTION(0, "GPIO77"),
+		MTK_FUNCTION(1, "TDP2")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(78, "TCN"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 78),
+		MTK_FUNCTION(0, "GPIO78"),
+		MTK_FUNCTION(1, "TCN")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(79, "TCP"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 79),
+		MTK_FUNCTION(0, "GPIO79"),
+		MTK_FUNCTION(1, "TCP")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(80, "TDN1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 80),
+		MTK_FUNCTION(0, "GPIO80"),
+		MTK_FUNCTION(1, "TDN1")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(81, "TDP1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 81),
+		MTK_FUNCTION(0, "GPIO81"),
+		MTK_FUNCTION(1, "TDP1")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(82, "TDN0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 82),
+		MTK_FUNCTION(0, "GPIO82"),
+		MTK_FUNCTION(1, "TDN0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(83, "TDP0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 83),
+		MTK_FUNCTION(0, "GPIO83"),
+		MTK_FUNCTION(1, "TDP0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(84, "RDN0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 84),
+		MTK_FUNCTION(0, "GPIO84"),
+		MTK_FUNCTION(1, "RDN0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(85, "RDP0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 85),
+		MTK_FUNCTION(0, "GPIO85"),
+		MTK_FUNCTION(1, "RDP0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(86, "RDN1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 86),
+		MTK_FUNCTION(0, "GPIO86"),
+		MTK_FUNCTION(1, "RDN1")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(87, "RDP1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 87),
+		MTK_FUNCTION(0, "GPIO87"),
+		MTK_FUNCTION(1, "RDP1")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(88, "RCN"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 88),
+		MTK_FUNCTION(0, "GPIO88"),
+		MTK_FUNCTION(1, "RCN")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(89, "RCP"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 89),
+		MTK_FUNCTION(0, "GPIO89"),
+		MTK_FUNCTION(1, "RCP")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(90, "RDN2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 90),
+		MTK_FUNCTION(0, "GPIO90"),
+		MTK_FUNCTION(1, "RDN2"),
+		MTK_FUNCTION(2, "CMDAT8")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(91, "RDP2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 91),
+		MTK_FUNCTION(0, "GPIO91"),
+		MTK_FUNCTION(1, "RDP2"),
+		MTK_FUNCTION(2, "CMDAT9")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(92, "RDN3"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 92),
+		MTK_FUNCTION(0, "GPIO92"),
+		MTK_FUNCTION(1, "RDN3"),
+		MTK_FUNCTION(2, "CMDAT4")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(93, "RDP3"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 93),
+		MTK_FUNCTION(0, "GPIO93"),
+		MTK_FUNCTION(1, "RDP3"),
+		MTK_FUNCTION(2, "CMDAT5")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(94, "RCN_A"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 94),
+		MTK_FUNCTION(0, "GPIO94"),
+		MTK_FUNCTION(1, "RCN_A"),
+		MTK_FUNCTION(2, "CMDAT6")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(95, "RCP_A"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 95),
+		MTK_FUNCTION(0, "GPIO95"),
+		MTK_FUNCTION(1, "RCP_A"),
+		MTK_FUNCTION(2, "CMDAT7")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(96, "RDN1_A"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 96),
+		MTK_FUNCTION(0, "GPIO96"),
+		MTK_FUNCTION(1, "RDN1_A"),
+		MTK_FUNCTION(2, "CMDAT2"),
+		MTK_FUNCTION(3, "CMCSD2")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(97, "RDP1_A"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 97),
+		MTK_FUNCTION(0, "GPIO97"),
+		MTK_FUNCTION(1, "RDP1_A"),
+		MTK_FUNCTION(2, "CMDAT3"),
+		MTK_FUNCTION(3, "CMCSD3")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(98, "RDN0_A"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 98),
+		MTK_FUNCTION(0, "GPIO98"),
+		MTK_FUNCTION(1, "RDN0_A"),
+		MTK_FUNCTION(2, "CMHSYNC")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(99, "RDP0_A"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 99),
+		MTK_FUNCTION(0, "GPIO99"),
+		MTK_FUNCTION(1, "RDP0_A"),
+		MTK_FUNCTION(2, "CMVSYNC")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(100, "CMDAT0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 100),
+		MTK_FUNCTION(0, "GPIO100"),
+		MTK_FUNCTION(1, "CMDAT0"),
+		MTK_FUNCTION(2, "CMCSD0"),
+		MTK_FUNCTION(3, "ANT_SEL2"),
+		MTK_FUNCTION(5, "TDM_RX_MCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[21]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(101, "CMDAT1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 101),
+		MTK_FUNCTION(0, "GPIO101"),
+		MTK_FUNCTION(1, "CMDAT1"),
+		MTK_FUNCTION(2, "CMCSD1"),
+		MTK_FUNCTION(3, "ANT_SEL3"),
+		MTK_FUNCTION(4, "CMFLASH"),
+		MTK_FUNCTION(5, "TDM_RX_BCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[22]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(102, "CMMCLK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 102),
+		MTK_FUNCTION(0, "GPIO102"),
+		MTK_FUNCTION(1, "CMMCLK"),
+		MTK_FUNCTION(3, "ANT_SEL4"),
+		MTK_FUNCTION(5, "TDM_RX_LRCK"),
+		MTK_FUNCTION(7, "DBG_MON_B[23]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(103, "CMPCLK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 103),
+		MTK_FUNCTION(0, "GPIO103"),
+		MTK_FUNCTION(1, "CMPCLK"),
+		MTK_FUNCTION(2, "CMCSK"),
+		MTK_FUNCTION(3, "ANT_SEL5"),
+		MTK_FUNCTION(5, " TDM_RX_DI"),
+		MTK_FUNCTION(7, "DBG_MON_B[24]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(104, "MSDC1_CMD"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 104),
+		MTK_FUNCTION(0, "GPIO104"),
+		MTK_FUNCTION(1, "MSDC1_CMD"),
+		MTK_FUNCTION(4, "SQICS"),
+		MTK_FUNCTION(7, "DBG_MON_B[25]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(105, "MSDC1_CLK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 105),
+		MTK_FUNCTION(0, "GPIO105"),
+		MTK_FUNCTION(1, "MSDC1_CLK"),
+		MTK_FUNCTION(4, "SQISO"),
+		MTK_FUNCTION(7, "DBG_MON_B[26]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(106, "MSDC1_DAT0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 106),
+		MTK_FUNCTION(0, "GPIO106"),
+		MTK_FUNCTION(1, "MSDC1_DAT0"),
+		MTK_FUNCTION(4, "SQISI"),
+		MTK_FUNCTION(7, "DBG_MON_B[27]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(107, "MSDC1_DAT1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 107),
+		MTK_FUNCTION(0, "GPIO107"),
+		MTK_FUNCTION(1, "MSDC1_DAT1"),
+		MTK_FUNCTION(4, "SQIWP"),
+		MTK_FUNCTION(7, "DBG_MON_B[28]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(108, "MSDC1_DAT2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 108),
+		MTK_FUNCTION(0, "GPIO108"),
+		MTK_FUNCTION(1, "MSDC1_DAT2"),
+		MTK_FUNCTION(4, "SQIRST"),
+		MTK_FUNCTION(7, "DBG_MON_B[29]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(109, "MSDC1_DAT3"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 109),
+		MTK_FUNCTION(0, "GPIO109"),
+		MTK_FUNCTION(1, "MSDC1_DAT3"),
+		MTK_FUNCTION(4, "SQICK"), /* WIP */
+		MTK_FUNCTION(7, "DBG_MON_B[30]")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(110, "MSDC0_DAT7"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 110),
+		MTK_FUNCTION(0, "GPIO110"),
+		MTK_FUNCTION(1, "MSDC0_DAT7"),
+		MTK_FUNCTION(4, "NLD7")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(111, "MSDC0_DAT6"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 111),
+		MTK_FUNCTION(0, "GPIO111"),
+		MTK_FUNCTION(1, "MSDC0_DAT6"),
+		MTK_FUNCTION(4, "NLD6")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(112, "MSDC0_DAT5"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 112),
+		MTK_FUNCTION(0, "GPIO112"),
+		MTK_FUNCTION(1, "MSDC0_DAT5"),
+		MTK_FUNCTION(4, "NLD4")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(113, "MSDC0_DAT4"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 113),
+		MTK_FUNCTION(0, "GPIO113"),
+		MTK_FUNCTION(1, "MSDC0_DAT4"),
+		MTK_FUNCTION(4, "NLD3")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(114, "MSDC0_RSTB"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 114),
+		MTK_FUNCTION(0, "GPIO114"),
+		MTK_FUNCTION(1, "MSDC0_RSTB"),
+		MTK_FUNCTION(4, "NLD0")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(115, "MSDC0_CMD"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 115),
+		MTK_FUNCTION(0, "GPIO115"),
+		MTK_FUNCTION(1, "MSDC0_CMD"),
+		MTK_FUNCTION(4, "NALE")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(116, "MSDC0_CLK"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 116),
+		MTK_FUNCTION(0, "GPIO116"),
+		MTK_FUNCTION(1, "MSDC0_CLK"),
+		MTK_FUNCTION(4, "NWEB")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(117, "MSDC0_DAT3"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 117),
+		MTK_FUNCTION(0, "GPIO117"),
+		MTK_FUNCTION(1, "MSDC0_DAT3"),
+		MTK_FUNCTION(4, "NLD1")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(118, "MSDC0_DAT2"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 118),
+		MTK_FUNCTION(0, "GPIO118"),
+		MTK_FUNCTION(1, "MSDC0_DAT2"),
+		MTK_FUNCTION(4, "NLD5")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(119, "MSDC0_DAT1"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 119),
+		MTK_FUNCTION(0, "GPIO119"),
+		MTK_FUNCTION(1, "MSDC0_DAT1"),
+		MTK_FUNCTION(4, "NLD8")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(120, "MSDC0_DAT0"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 120),
+		MTK_FUNCTION(0, "GPIO120"),
+		MTK_FUNCTION(1, "MSDC0_DAT0"),
+		MTK_FUNCTION(4, "WATCHDOG"),
+		MTK_FUNCTION(5, "NLD2")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(121, "GPIO121"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 121),
+		MTK_FUNCTION(0, "GPIO121")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(122, "GPIO122"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 122),
+		MTK_FUNCTION(0, "GPIO122")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(123, "GPIO123"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 123),
+		MTK_FUNCTION(0, "GPIO123")
+	),
+	MTK_PIN(
+		PINCTRL_PIN(124, "GPIO124"),
+		NULL, "mt8516",
+		MTK_EINT_FUNCTION(0, 124),
+		MTK_FUNCTION(0, "GPIO124")
+	),
+};
+
+#endif /* __PINCTRL_MTK_MT8516_H */
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-paris.c
@@ -0,0 +1,947 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * MediaTek Pinctrl Paris Driver, which implement the vendor per-pin
+ * bindings for MediaTek SoC.
+ *
+ * Copyright (C) 2018 MediaTek Inc.
+ * Author: Sean Wang <sean.wang@mediatek.com>
+ *	   Zhiyong Tao <zhiyong.tao@mediatek.com>
+ *	   Hongzhou.Yang <hongzhou.yang@mediatek.com>
+ */
+
+#include <linux/gpio/driver.h>
+#include <dt-bindings/pinctrl/mt65xx.h>
+#include "pinctrl-paris.h"
+
+#define PINCTRL_PINCTRL_DEV	KBUILD_MODNAME
+
+/* Custom pinconf parameters */
+#define MTK_PIN_CONFIG_TDSEL	(PIN_CONFIG_END + 1)
+#define MTK_PIN_CONFIG_RDSEL	(PIN_CONFIG_END + 2)
+#define MTK_PIN_CONFIG_PU_ADV	(PIN_CONFIG_END + 3)
+#define MTK_PIN_CONFIG_PD_ADV	(PIN_CONFIG_END + 4)
+#define MTK_PIN_CONFIG_DRV_ADV	(PIN_CONFIG_END + 5)
+
+static const struct pinconf_generic_params mtk_custom_bindings[] = {
+	{"mediatek,tdsel",	MTK_PIN_CONFIG_TDSEL,		0},
+	{"mediatek,rdsel",	MTK_PIN_CONFIG_RDSEL,		0},
+	{"mediatek,pull-up-adv", MTK_PIN_CONFIG_PU_ADV,		1},
+	{"mediatek,pull-down-adv", MTK_PIN_CONFIG_PD_ADV,	1},
+	{"mediatek,drive-strength-adv", MTK_PIN_CONFIG_DRV_ADV,	2},
+};
+
+#ifdef CONFIG_DEBUG_FS
+static const struct pin_config_item mtk_conf_items[] = {
+	PCONFDUMP(MTK_PIN_CONFIG_TDSEL, "tdsel", NULL, true),
+	PCONFDUMP(MTK_PIN_CONFIG_RDSEL, "rdsel", NULL, true),
+	PCONFDUMP(MTK_PIN_CONFIG_PU_ADV, "pu-adv", NULL, true),
+	PCONFDUMP(MTK_PIN_CONFIG_PD_ADV, "pd-adv", NULL, true),
+	PCONFDUMP(MTK_PIN_CONFIG_DRV_ADV, "drive-strength-adv", NULL, true),
+};
+#endif
+
+static const char * const mtk_gpio_functions[] = {
+	"func0", "func1", "func2", "func3",
+	"func4", "func5", "func6", "func7",
+	"func8", "func9", "func10", "func11",
+	"func12", "func13", "func14", "func15",
+};
+
+static int mtk_pinmux_gpio_request_enable(struct pinctrl_dev *pctldev,
+					  struct pinctrl_gpio_range *range,
+					  unsigned int pin)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+	return mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_MODE,
+				hw->soc->gpio_m);
+}
+
+static int mtk_pinmux_gpio_set_direction(struct pinctrl_dev *pctldev,
+					 struct pinctrl_gpio_range *range,
+					 unsigned int pin, bool input)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+	/* hardware would take 0 as input direction */
+	return mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR, !input);
+}
+
+static int mtk_pinconf_get(struct pinctrl_dev *pctldev,
+			   unsigned int pin, unsigned long *config)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	u32 param = pinconf_to_config_param(*config);
+	int val, val2, err, reg, ret = 1;
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+	switch (param) {
+	case PIN_CONFIG_BIAS_DISABLE:
+		if (hw->soc->bias_disable_get) {
+			err = hw->soc->bias_disable_get(hw, desc, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_BIAS_PULL_UP:
+		if (hw->soc->bias_get) {
+			err = hw->soc->bias_get(hw, desc, 1, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_BIAS_PULL_DOWN:
+		if (hw->soc->bias_get) {
+			err = hw->soc->bias_get(hw, desc, 0, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_SLEW_RATE:
+		err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_SR, &val);
+		if (err)
+			return err;
+
+		if (!val)
+			return -EINVAL;
+
+		break;
+	case PIN_CONFIG_INPUT_ENABLE:
+	case PIN_CONFIG_OUTPUT_ENABLE:
+		err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DIR, &val);
+		if (err)
+			return err;
+
+		/* HW takes input mode as zero; output mode as non-zero */
+		if ((val && param == PIN_CONFIG_INPUT_ENABLE) ||
+		    (!val && param == PIN_CONFIG_OUTPUT_ENABLE))
+			return -EINVAL;
+
+		break;
+	case PIN_CONFIG_INPUT_SCHMITT_ENABLE:
+		err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DIR, &val);
+		if (err)
+			return err;
+
+		err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_SMT, &val2);
+		if (err)
+			return err;
+
+		if (val || !val2)
+			return -EINVAL;
+
+		break;
+	case PIN_CONFIG_DRIVE_STRENGTH:
+		if (hw->soc->drive_get) {
+			err = hw->soc->drive_get(hw, desc, &ret);
+			if (err)
+				return err;
+		} else {
+			err = -ENOTSUPP;
+		}
+		break;
+	case MTK_PIN_CONFIG_TDSEL:
+	case MTK_PIN_CONFIG_RDSEL:
+		reg = (param == MTK_PIN_CONFIG_TDSEL) ?
+		       PINCTRL_PIN_REG_TDSEL : PINCTRL_PIN_REG_RDSEL;
+
+		err = mtk_hw_get_value(hw, desc, reg, &val);
+		if (err)
+			return err;
+
+		ret = val;
+
+		break;
+	case MTK_PIN_CONFIG_PU_ADV:
+	case MTK_PIN_CONFIG_PD_ADV:
+		if (hw->soc->adv_pull_get) {
+			bool pullup;
+
+			pullup = param == MTK_PIN_CONFIG_PU_ADV;
+			err = hw->soc->adv_pull_get(hw, desc, pullup, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case MTK_PIN_CONFIG_DRV_ADV:
+		if (hw->soc->adv_drive_get) {
+			err = hw->soc->adv_drive_get(hw, desc, &ret);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	default:
+		return -ENOTSUPP;
+	}
+
+	*config = pinconf_to_config_packed(param, ret);
+
+	return 0;
+}
+
+static int mtk_pinconf_set(struct pinctrl_dev *pctldev, unsigned int pin,
+			   enum pin_config_param param,
+			   enum pin_config_param arg)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	const struct mtk_pin_desc *desc;
+	int err = 0;
+	u32 reg;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[pin];
+
+	switch ((u32)param) {
+	case PIN_CONFIG_BIAS_DISABLE:
+		if (hw->soc->bias_disable_set) {
+			err = hw->soc->bias_disable_set(hw, desc);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_BIAS_PULL_UP:
+		if (hw->soc->bias_set) {
+			err = hw->soc->bias_set(hw, desc, 1);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_BIAS_PULL_DOWN:
+		if (hw->soc->bias_set) {
+			err = hw->soc->bias_set(hw, desc, 0);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case PIN_CONFIG_OUTPUT_ENABLE:
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_SMT,
+				       MTK_DISABLE);
+		if (err)
+			goto err;
+
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR,
+				       MTK_OUTPUT);
+		if (err)
+			goto err;
+		break;
+	case PIN_CONFIG_INPUT_ENABLE:
+		if (hw->soc->ies_present) {
+			mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_IES,
+					 MTK_ENABLE);
+		}
+
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR,
+				       MTK_INPUT);
+		if (err)
+			goto err;
+		break;
+	case PIN_CONFIG_SLEW_RATE:
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_SR,
+				       arg);
+		if (err)
+			goto err;
+
+		break;
+	case PIN_CONFIG_OUTPUT:
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR,
+				       MTK_OUTPUT);
+		if (err)
+			goto err;
+
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DO,
+				       arg);
+		if (err)
+			goto err;
+		break;
+	case PIN_CONFIG_INPUT_SCHMITT_ENABLE:
+		/* arg = 1: Input mode & SMT enable ;
+		 * arg = 0: Output mode & SMT disable
+		 */
+		arg = arg ? 2 : 1;
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DIR,
+				       arg & 1);
+		if (err)
+			goto err;
+
+		err = mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_SMT,
+				       !!(arg & 2));
+		if (err)
+			goto err;
+		break;
+	case PIN_CONFIG_DRIVE_STRENGTH:
+		if (hw->soc->drive_set) {
+			err = hw->soc->drive_set(hw, desc, arg);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case MTK_PIN_CONFIG_TDSEL:
+	case MTK_PIN_CONFIG_RDSEL:
+		reg = (param == MTK_PIN_CONFIG_TDSEL) ?
+		       PINCTRL_PIN_REG_TDSEL : PINCTRL_PIN_REG_RDSEL;
+
+		err = mtk_hw_set_value(hw, desc, reg, arg);
+		if (err)
+			goto err;
+		break;
+	case MTK_PIN_CONFIG_PU_ADV:
+	case MTK_PIN_CONFIG_PD_ADV:
+		if (hw->soc->adv_pull_set) {
+			bool pullup;
+
+			pullup = param == MTK_PIN_CONFIG_PU_ADV;
+			err = hw->soc->adv_pull_set(hw, desc, pullup,
+						    arg);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	case MTK_PIN_CONFIG_DRV_ADV:
+		if (hw->soc->adv_drive_set) {
+			err = hw->soc->adv_drive_set(hw, desc, arg);
+			if (err)
+				return err;
+		} else {
+			return -ENOTSUPP;
+		}
+		break;
+	default:
+		err = -ENOTSUPP;
+	}
+
+err:
+	return err;
+}
+
+static struct mtk_pinctrl_group *
+mtk_pctrl_find_group_by_pin(struct mtk_pinctrl *hw, u32 pin)
+{
+	int i;
+
+	for (i = 0; i < hw->soc->ngrps; i++) {
+		struct mtk_pinctrl_group *grp = hw->groups + i;
+
+		if (grp->pin == pin)
+			return grp;
+	}
+
+	return NULL;
+}
+
+static const struct mtk_func_desc *
+mtk_pctrl_find_function_by_pin(struct mtk_pinctrl *hw, u32 pin_num, u32 fnum)
+{
+	const struct mtk_pin_desc *pin = hw->soc->pins + pin_num;
+	const struct mtk_func_desc *func = pin->funcs;
+
+	while (func && func->name) {
+		if (func->muxval == fnum)
+			return func;
+		func++;
+	}
+
+	return NULL;
+}
+
+static bool mtk_pctrl_is_function_valid(struct mtk_pinctrl *hw, u32 pin_num,
+					u32 fnum)
+{
+	int i;
+
+	for (i = 0; i < hw->soc->npins; i++) {
+		const struct mtk_pin_desc *pin = hw->soc->pins + i;
+
+		if (pin->number == pin_num) {
+			const struct mtk_func_desc *func = pin->funcs;
+
+			while (func && func->name) {
+				if (func->muxval == fnum)
+					return true;
+				func++;
+			}
+
+			break;
+		}
+	}
+
+	return false;
+}
+
+static int mtk_pctrl_dt_node_to_map_func(struct mtk_pinctrl *pctl,
+					 u32 pin, u32 fnum,
+					 struct mtk_pinctrl_group *grp,
+					 struct pinctrl_map **map,
+					 unsigned *reserved_maps,
+					 unsigned *num_maps)
+{
+	bool ret;
+
+	if (*num_maps == *reserved_maps)
+		return -ENOSPC;
+
+	(*map)[*num_maps].type = PIN_MAP_TYPE_MUX_GROUP;
+	(*map)[*num_maps].data.mux.group = grp->name;
+
+	ret = mtk_pctrl_is_function_valid(pctl, pin, fnum);
+	if (!ret) {
+		dev_err(pctl->dev, "invalid function %d on pin %d .\n",
+			fnum, pin);
+		return -EINVAL;
+	}
+
+	(*map)[*num_maps].data.mux.function = mtk_gpio_functions[fnum];
+	(*num_maps)++;
+
+	return 0;
+}
+
+static int mtk_pctrl_dt_subnode_to_map(struct pinctrl_dev *pctldev,
+				       struct device_node *node,
+				       struct pinctrl_map **map,
+				       unsigned *reserved_maps,
+				       unsigned *num_maps)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	int num_pins, num_funcs, maps_per_pin, i, err;
+	struct mtk_pinctrl_group *grp;
+	unsigned int num_configs;
+	bool has_config = false;
+	unsigned long *configs;
+	u32 pinfunc, pin, func;
+	struct property *pins;
+	unsigned reserve = 0;
+
+	pins = of_find_property(node, "pinmux", NULL);
+	if (!pins) {
+		dev_err(hw->dev, "missing pins property in node %pOFn .\n",
+			node);
+		return -EINVAL;
+	}
+
+	err = pinconf_generic_parse_dt_config(node, pctldev, &configs,
+					      &num_configs);
+	if (err)
+		return err;
+
+	if (num_configs)
+		has_config = true;
+
+	num_pins = pins->length / sizeof(u32);
+	num_funcs = num_pins;
+	maps_per_pin = 0;
+	if (num_funcs)
+		maps_per_pin++;
+	if (has_config && num_pins >= 1)
+		maps_per_pin++;
+
+	if (!num_pins || !maps_per_pin) {
+		err = -EINVAL;
+		goto exit;
+	}
+
+	reserve = num_pins * maps_per_pin;
+
+	err = pinctrl_utils_reserve_map(pctldev, map, reserved_maps, num_maps,
+					reserve);
+	if (err < 0)
+		goto exit;
+
+	for (i = 0; i < num_pins; i++) {
+		err = of_property_read_u32_index(node, "pinmux", i, &pinfunc);
+		if (err)
+			goto exit;
+
+		pin = MTK_GET_PIN_NO(pinfunc);
+		func = MTK_GET_PIN_FUNC(pinfunc);
+
+		if (pin >= hw->soc->npins ||
+		    func >= ARRAY_SIZE(mtk_gpio_functions)) {
+			dev_err(hw->dev, "invalid pins value.\n");
+			err = -EINVAL;
+			goto exit;
+		}
+
+		grp = mtk_pctrl_find_group_by_pin(hw, pin);
+		if (!grp) {
+			dev_err(hw->dev, "unable to match pin %d to group\n",
+				pin);
+			err = -EINVAL;
+			goto exit;
+		}
+
+		err = mtk_pctrl_dt_node_to_map_func(hw, pin, func, grp, map,
+						    reserved_maps, num_maps);
+		if (err < 0)
+			goto exit;
+
+		if (has_config) {
+			err = pinctrl_utils_add_map_configs(pctldev, map,
+							    reserved_maps,
+							    num_maps,
+							    grp->name,
+							    configs,
+							    num_configs,
+							    PIN_MAP_TYPE_CONFIGS_GROUP);
+			if (err < 0)
+				goto exit;
+		}
+	}
+
+	err = 0;
+
+exit:
+	kfree(configs);
+	return err;
+}
+
+static int mtk_pctrl_dt_node_to_map(struct pinctrl_dev *pctldev,
+				    struct device_node *np_config,
+				    struct pinctrl_map **map,
+				    unsigned *num_maps)
+{
+	struct device_node *np;
+	unsigned reserved_maps;
+	int ret;
+
+	*map = NULL;
+	*num_maps = 0;
+	reserved_maps = 0;
+
+	for_each_child_of_node(np_config, np) {
+		ret = mtk_pctrl_dt_subnode_to_map(pctldev, np, map,
+						  &reserved_maps,
+						  num_maps);
+		if (ret < 0) {
+			pinctrl_utils_free_map(pctldev, *map, *num_maps);
+			of_node_put(np);
+			return ret;
+		}
+	}
+
+	return 0;
+}
+
+static int mtk_pctrl_get_groups_count(struct pinctrl_dev *pctldev)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+
+	return hw->soc->ngrps;
+}
+
+static const char *mtk_pctrl_get_group_name(struct pinctrl_dev *pctldev,
+					    unsigned group)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+
+	return hw->groups[group].name;
+}
+
+static int mtk_pctrl_get_group_pins(struct pinctrl_dev *pctldev,
+				    unsigned group, const unsigned **pins,
+				    unsigned *num_pins)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+
+	*pins = (unsigned *)&hw->groups[group].pin;
+	*num_pins = 1;
+
+	return 0;
+}
+
+static const struct pinctrl_ops mtk_pctlops = {
+	.dt_node_to_map		= mtk_pctrl_dt_node_to_map,
+	.dt_free_map		= pinctrl_utils_free_map,
+	.get_groups_count	= mtk_pctrl_get_groups_count,
+	.get_group_name		= mtk_pctrl_get_group_name,
+	.get_group_pins		= mtk_pctrl_get_group_pins,
+};
+
+static int mtk_pmx_get_funcs_cnt(struct pinctrl_dev *pctldev)
+{
+	return ARRAY_SIZE(mtk_gpio_functions);
+}
+
+static const char *mtk_pmx_get_func_name(struct pinctrl_dev *pctldev,
+					 unsigned selector)
+{
+	return mtk_gpio_functions[selector];
+}
+
+static int mtk_pmx_get_func_groups(struct pinctrl_dev *pctldev,
+				   unsigned function,
+				   const char * const **groups,
+				   unsigned * const num_groups)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+
+	*groups = hw->grp_names;
+	*num_groups = hw->soc->ngrps;
+
+	return 0;
+}
+
+static int mtk_pmx_set_mux(struct pinctrl_dev *pctldev,
+			   unsigned function,
+			   unsigned group)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	struct mtk_pinctrl_group *grp = hw->groups + group;
+	const struct mtk_func_desc *desc_func;
+	const struct mtk_pin_desc *desc;
+	bool ret;
+
+	ret = mtk_pctrl_is_function_valid(hw, grp->pin, function);
+	if (!ret) {
+		dev_err(hw->dev, "invalid function %d on group %d .\n",
+			function, group);
+		return -EINVAL;
+	}
+
+	desc_func = mtk_pctrl_find_function_by_pin(hw, grp->pin, function);
+	if (!desc_func)
+		return -EINVAL;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[grp->pin];
+	mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_MODE, desc_func->muxval);
+
+	return 0;
+}
+
+static const struct pinmux_ops mtk_pmxops = {
+	.get_functions_count	= mtk_pmx_get_funcs_cnt,
+	.get_function_name	= mtk_pmx_get_func_name,
+	.get_function_groups	= mtk_pmx_get_func_groups,
+	.set_mux		= mtk_pmx_set_mux,
+	.gpio_set_direction	= mtk_pinmux_gpio_set_direction,
+	.gpio_request_enable	= mtk_pinmux_gpio_request_enable,
+};
+
+static int mtk_pconf_group_get(struct pinctrl_dev *pctldev, unsigned group,
+			       unsigned long *config)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+
+	*config = hw->groups[group].config;
+
+	return 0;
+}
+
+static int mtk_pconf_group_set(struct pinctrl_dev *pctldev, unsigned group,
+			       unsigned long *configs, unsigned num_configs)
+{
+	struct mtk_pinctrl *hw = pinctrl_dev_get_drvdata(pctldev);
+	struct mtk_pinctrl_group *grp = &hw->groups[group];
+	int i, ret;
+
+	for (i = 0; i < num_configs; i++) {
+		ret = mtk_pinconf_set(pctldev, grp->pin,
+				      pinconf_to_config_param(configs[i]),
+				      pinconf_to_config_argument(configs[i]));
+		if (ret < 0)
+			return ret;
+
+		grp->config = configs[i];
+	}
+
+	return 0;
+}
+
+static const struct pinconf_ops mtk_confops = {
+	.pin_config_get = mtk_pinconf_get,
+	.pin_config_group_get	= mtk_pconf_group_get,
+	.pin_config_group_set	= mtk_pconf_group_set,
+};
+
+static struct pinctrl_desc mtk_desc = {
+	.name = PINCTRL_PINCTRL_DEV,
+	.pctlops = &mtk_pctlops,
+	.pmxops = &mtk_pmxops,
+	.confops = &mtk_confops,
+	.owner = THIS_MODULE,
+};
+
+static int mtk_gpio_get_direction(struct gpio_chip *chip, unsigned int gpio)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+	int value, err;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[gpio];
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DIR, &value);
+	if (err)
+		return err;
+
+	return !value;
+}
+
+static int mtk_gpio_get(struct gpio_chip *chip, unsigned int gpio)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+	int value, err;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[gpio];
+
+	err = mtk_hw_get_value(hw, desc, PINCTRL_PIN_REG_DI, &value);
+	if (err)
+		return err;
+
+	return !!value;
+}
+
+static void mtk_gpio_set(struct gpio_chip *chip, unsigned int gpio, int value)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[gpio];
+
+	mtk_hw_set_value(hw, desc, PINCTRL_PIN_REG_DO, !!value);
+}
+
+static int mtk_gpio_direction_input(struct gpio_chip *chip, unsigned int gpio)
+{
+	return pinctrl_gpio_direction_input(chip->base + gpio);
+}
+
+static int mtk_gpio_direction_output(struct gpio_chip *chip, unsigned int gpio,
+				     int value)
+{
+	mtk_gpio_set(chip, gpio, value);
+
+	return pinctrl_gpio_direction_output(chip->base + gpio);
+}
+
+static int mtk_gpio_to_irq(struct gpio_chip *chip, unsigned int offset)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+
+	if (!hw->eint)
+		return -ENOTSUPP;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[offset];
+
+	if (desc->eint.eint_n == EINT_NA)
+		return -ENOTSUPP;
+
+	return mtk_eint_find_irq(hw->eint, desc->eint.eint_n);
+}
+
+static int mtk_gpio_set_config(struct gpio_chip *chip, unsigned int offset,
+			       unsigned long config)
+{
+	struct mtk_pinctrl *hw = gpiochip_get_data(chip);
+	const struct mtk_pin_desc *desc;
+	u32 debounce;
+
+	desc = (const struct mtk_pin_desc *)&hw->soc->pins[offset];
+
+	if (!hw->eint ||
+	    pinconf_to_config_param(config) != PIN_CONFIG_INPUT_DEBOUNCE ||
+	    desc->eint.eint_n == EINT_NA)
+		return -ENOTSUPP;
+
+	debounce = pinconf_to_config_argument(config);
+
+	return mtk_eint_set_debounce(hw->eint, desc->eint.eint_n, debounce);
+}
+
+static int mtk_build_gpiochip(struct mtk_pinctrl *hw, struct device_node *np)
+{
+	struct gpio_chip *chip = &hw->chip;
+	int ret;
+
+	chip->label		= PINCTRL_PINCTRL_DEV;
+	chip->parent		= hw->dev;
+	chip->request		= gpiochip_generic_request;
+	chip->free		= gpiochip_generic_free;
+	chip->get_direction	= mtk_gpio_get_direction;
+	chip->direction_input	= mtk_gpio_direction_input;
+	chip->direction_output	= mtk_gpio_direction_output;
+	chip->get		= mtk_gpio_get;
+	chip->set		= mtk_gpio_set;
+	chip->to_irq		= mtk_gpio_to_irq,
+	chip->set_config	= mtk_gpio_set_config,
+	chip->base		= -1;
+	chip->ngpio		= hw->soc->npins;
+	chip->of_node		= np;
+	chip->of_gpio_n_cells	= 2;
+
+	ret = gpiochip_add_data(chip, hw);
+	if (ret < 0)
+		return ret;
+
+	return 0;
+}
+
+static int mtk_pctrl_build_state(struct platform_device *pdev)
+{
+	struct mtk_pinctrl *hw = platform_get_drvdata(pdev);
+	int i;
+
+	/* Allocate groups */
+	hw->groups = devm_kmalloc_array(&pdev->dev, hw->soc->ngrps,
+					sizeof(*hw->groups), GFP_KERNEL);
+	if (!hw->groups)
+		return -ENOMEM;
+
+	/* We assume that one pin is one group, use pin name as group name. */
+	hw->grp_names = devm_kmalloc_array(&pdev->dev, hw->soc->ngrps,
+					   sizeof(*hw->grp_names), GFP_KERNEL);
+	if (!hw->grp_names)
+		return -ENOMEM;
+
+	for (i = 0; i < hw->soc->npins; i++) {
+		const struct mtk_pin_desc *pin = hw->soc->pins + i;
+		struct mtk_pinctrl_group *group = hw->groups + i;
+
+		group->name = pin->name;
+		group->pin = pin->number;
+
+		hw->grp_names[i] = pin->name;
+	}
+
+	return 0;
+}
+
+int mtk_paris_pinctrl_probe(struct platform_device *pdev,
+			    const struct mtk_pin_soc *soc)
+{
+	struct pinctrl_pin_desc *pins;
+	struct mtk_pinctrl *hw;
+	struct resource *res;
+	int err, i;
+
+	hw = devm_kzalloc(&pdev->dev, sizeof(*hw), GFP_KERNEL);
+	if (!hw)
+		return -ENOMEM;
+
+	platform_set_drvdata(pdev, hw);
+	hw->soc = soc;
+	hw->dev = &pdev->dev;
+
+	if (!hw->soc->nbase_names) {
+		dev_err(&pdev->dev,
+			"SoC should be assigned at least one register base\n");
+		return -EINVAL;
+	}
+
+	hw->base = devm_kmalloc_array(&pdev->dev, hw->soc->nbase_names,
+				      sizeof(*hw->base), GFP_KERNEL);
+	if (!hw->base)
+		return -ENOMEM;
+
+	for (i = 0; i < hw->soc->nbase_names; i++) {
+		res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
+						   hw->soc->base_names[i]);
+		if (!res) {
+			dev_err(&pdev->dev, "missing IO resource\n");
+			return -ENXIO;
+		}
+
+		hw->base[i] = devm_ioremap_resource(&pdev->dev, res);
+		if (IS_ERR(hw->base[i]))
+			return PTR_ERR(hw->base[i]);
+	}
+
+	hw->nbase = hw->soc->nbase_names;
+
+	err = mtk_pctrl_build_state(pdev);
+	if (err) {
+		dev_err(&pdev->dev, "build state failed: %d\n", err);
+		return -EINVAL;
+	}
+
+	/* Copy from internal struct mtk_pin_desc to register to the core */
+	pins = devm_kmalloc_array(&pdev->dev, hw->soc->npins, sizeof(*pins),
+				  GFP_KERNEL);
+	if (!pins)
+		return -ENOMEM;
+
+	for (i = 0; i < hw->soc->npins; i++) {
+		pins[i].number = hw->soc->pins[i].number;
+		pins[i].name = hw->soc->pins[i].name;
+	}
+
+	/* Setup pins descriptions per SoC types */
+	mtk_desc.pins = (const struct pinctrl_pin_desc *)pins;
+	mtk_desc.npins = hw->soc->npins;
+	mtk_desc.num_custom_params = ARRAY_SIZE(mtk_custom_bindings);
+	mtk_desc.custom_params = mtk_custom_bindings;
+#ifdef CONFIG_DEBUG_FS
+	mtk_desc.custom_conf_items = mtk_conf_items;
+#endif
+
+	err = devm_pinctrl_register_and_init(&pdev->dev, &mtk_desc, hw,
+					     &hw->pctrl);
+	if (err)
+		return err;
+
+	err = pinctrl_enable(hw->pctrl);
+	if (err)
+		return err;
+
+	err = mtk_build_eint(hw, pdev);
+	if (err)
+		dev_warn(&pdev->dev,
+			 "Failed to add EINT, but pinctrl still can work\n");
+
+	/* Build gpiochip should be after pinctrl_enable is done */
+	err = mtk_build_gpiochip(hw, pdev->dev.of_node);
+	if (err) {
+		dev_err(&pdev->dev, "Failed to add gpio_chip\n");
+		return err;
+	}
+
+	platform_set_drvdata(pdev, hw);
+
+	return 0;
+}
+
+static int mtk_paris_pinctrl_suspend(struct device *device)
+{
+	struct mtk_pinctrl *pctl = dev_get_drvdata(device);
+
+	return mtk_eint_do_suspend(pctl->eint);
+}
+
+static int mtk_paris_pinctrl_resume(struct device *device)
+{
+	struct mtk_pinctrl *pctl = dev_get_drvdata(device);
+
+	return mtk_eint_do_resume(pctl->eint);
+}
+
+const struct dev_pm_ops mtk_paris_pinctrl_pm_ops = {
+	.suspend_noirq = mtk_paris_pinctrl_suspend,
+	.resume_noirq = mtk_paris_pinctrl_resume,
+};
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-paris.h
@@ -0,0 +1,65 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2018 MediaTek Inc.
+ *
+ * Author: Sean Wang <sean.wang@mediatek.com>
+ *	   Zhiyong Tao <zhiyong.tao@mediatek.com>
+ *	   Hongzhou.Yang <hongzhou.yang@mediatek.com>
+ */
+#ifndef __PINCTRL_PARIS_H
+#define __PINCTRL_PARIS_H
+
+#include <linux/io.h>
+#include <linux/init.h>
+#include <linux/of.h>
+#include <linux/of_platform.h>
+#include <linux/platform_device.h>
+#include <linux/pinctrl/pinctrl.h>
+#include <linux/pinctrl/pinmux.h>
+#include <linux/pinctrl/pinconf.h>
+#include <linux/pinctrl/pinconf-generic.h>
+
+#include "../core.h"
+#include "../pinconf.h"
+#include "../pinctrl-utils.h"
+#include "../pinmux.h"
+#include "mtk-eint.h"
+#include "pinctrl-mtk-common-v2.h"
+
+#define MTK_RANGE(_a)		{ .range = (_a), .nranges = ARRAY_SIZE(_a), }
+
+#define MTK_EINT_FUNCTION(_eintmux, _eintnum)				\
+	{							\
+		.eint_m = _eintmux,					\
+		.eint_n = _eintnum,					\
+	}
+
+#define MTK_FUNCTION(_val, _name)				\
+	{							\
+		.muxval = _val,					\
+		.name = _name,					\
+	}
+
+#define MTK_PIN(_number, _name, _eint, _drv_n, ...) {	\
+		.number = _number,			\
+		.name = _name,				\
+		.eint = _eint,				\
+		.drv_n = _drv_n,			\
+		.funcs = (struct mtk_func_desc[]){	\
+			__VA_ARGS__, { } },				\
+	}
+
+#define PINCTRL_PIN_GROUP(name, id)			\
+	{						\
+		name,					\
+		id##_pins,				\
+		ARRAY_SIZE(id##_pins),			\
+		id##_funcs,				\
+	}
+
+int mtk_paris_pinctrl_probe(struct platform_device *pdev,
+			    const struct mtk_pin_soc *soc);
+
+extern const struct dev_pm_ops mtk_paris_pinctrl_pm_ops;
+
+#endif /* __PINCTRL_PARIS_H */
