From f2c46d48d1aa0f7b87b179434162eac6624122f7 Mon Sep 17 00:00:00 2001
From: Jonathan Bell <jonathan@raspberrypi.org>
Date: Tue, 11 Jun 2019 11:42:03 +0100
Subject: [PATCH] usbhid: call usb_fixup_endpoint after mangling
 intervals

Lets the mousepoll override mechanism work with xhci.

Signed-off-by: Jonathan Bell <jonathan@raspberrypi.org>
---
 drivers/hid/usbhid/hid-core.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/hid/usbhid/hid-core.c
+++ b/drivers/hid/usbhid/hid-core.c
@@ -1118,6 +1118,7 @@ static int usbhid_start(struct hid_devic
 				interval = hid_kbpoll_interval;
 			break;
 		}
+		usb_fixup_endpoint(dev, endpoint->bEndpointAddress, interval);
 
 		ret = -ENOMEM;
 		if (usb_endpoint_dir_in(endpoint)) {
