From 09f145f417a5d64d6b8d4476699dfb0eccc6c784 Mon Sep 17 00:00:00 2001
From: Abhishek Sahu <absahu@codeaurora.org>
Date: Tue, 7 May 2019 10:14:05 +0300
Subject: [PATCH] ipq40xx: fix high resolution timer

Cherry-picked from CAF QSDK repo.
Original commit message:
The kernel is failing in switching the timer for high resolution
mode and clock source operates in 10ms resolution. The always-on
property needs to be given for timer device tree node to make
clock source working in 1ns resolution.

Change-Id: I7c00b3c74d97c2a30ac9f05e18b511a0550fd459
Signed-off-by: Abhishek Sahu <absahu@codeaurora.org>
Signed-off-by: Pavel Kubelun <be.dissent@gmail.com>
---
 arch/arm/boot/dts/qcom-ipq4019.dtsi | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -167,6 +167,7 @@
 			     <1 4 0xf08>,
 			     <1 1 0xf08>;
 		clock-frequency = <48000000>;
+		always-on;
 	};
 
 	soc {
