From 8e3577ac67382beda74437cb6f6bff5dbdb83fc9 Mon Sep 17 00:00:00 2001
From: hdoverobinson <hdoverobinson@gmail.com>
Date: Tue, 13 Mar 2018 06:58:39 -0400
Subject: [PATCH] added capture_clear option to pps-gpio via dtoverlay
 (#2433)

---
 drivers/pps/clients/pps-gpio.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/pps/clients/pps-gpio.c
+++ b/drivers/pps/clients/pps-gpio.c
@@ -119,6 +119,9 @@ static int pps_gpio_probe(struct platfor
 
 		if (of_get_property(np, "assert-falling-edge", NULL))
 			data->assert_falling_edge = true;
+
+                if (of_get_property(np, "capture-clear", NULL))
+                        data->capture_clear = true;
 	}
 
 	/* GPIO setup */
