From a43379dddf1ba14b6a9d50d95175117bbdf52ed2 Mon Sep 17 00:00:00 2001
From: Ryder Lee <ryder.lee@mediatek.com>
Date: Tue, 29 Jan 2019 12:31:18 +0800
Subject: [PATCH] arm: mediatek: add MT7629 smp bring up code

Add support for booting secondary CPUs on MT7629.

Signed-off-by: Ryder Lee <ryder.lee@mediatek.com>
Signed-off-by: Matthias Brugger <matthias.bgg@gmail.com>
---
 arch/arm/mach-mediatek/Kconfig    | 4 ++++
 arch/arm/mach-mediatek/mediatek.c | 1 +
 arch/arm/mach-mediatek/platsmp.c  | 1 +
 3 files changed, 6 insertions(+)

--- a/arch/arm/mach-mediatek/Kconfig
+++ b/arch/arm/mach-mediatek/Kconfig
@@ -26,6 +26,10 @@ config MACH_MT7623
 	bool "MediaTek MT7623 SoCs support"
 	default ARCH_MEDIATEK
 
+config MACH_MT7629
+	bool "MediaTek MT7629 SoCs support"
+	default ARCH_MEDIATEK
+
 config MACH_MT8127
 	bool "MediaTek MT8127 SoCs support"
 	default ARCH_MEDIATEK
--- a/arch/arm/mach-mediatek/mediatek.c
+++ b/arch/arm/mach-mediatek/mediatek.c
@@ -49,6 +49,7 @@ static const char * const mediatek_board
 	"mediatek,mt6589",
 	"mediatek,mt6592",
 	"mediatek,mt7623",
+	"mediatek,mt7629",
 	"mediatek,mt8127",
 	"mediatek,mt8135",
 	NULL,
--- a/arch/arm/mach-mediatek/platsmp.c
+++ b/arch/arm/mach-mediatek/platsmp.c
@@ -60,6 +60,7 @@ static const struct of_device_id mtk_tz_
 static const struct of_device_id mtk_smp_boot_infos[] __initconst = {
 	{ .compatible   = "mediatek,mt6589", .data = &mtk_mt6589_boot },
 	{ .compatible   = "mediatek,mt7623", .data = &mtk_mt7623_boot },
+	{ .compatible   = "mediatek,mt7629", .data = &mtk_mt7623_boot },
 	{},
 };
 
