From 50d3f15ea5d6ca2705a009722dd7d4108c9f75d9 Mon Sep 17 00:00:00 2001
From: Peter Robinson <pbrobinson@gmail.com>
Date: Sun, 5 May 2019 21:07:12 +0100
Subject: [PATCH] arm: dts: overlays: rpi-sense: add upstream humidity
 compatible

The upstream humidiity driver uses "st,hts221" for the compatible
string so add that in as well so it will work with an unmodified
upstream kernel driver. We leave the downstream as the priority.

Signed-off-by: Peter Robinson <pbrobinson@gmail.com>
---
 arch/arm/boot/dts/overlays/rpi-sense-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/rpi-sense-overlay.dts
+++ b/arch/arm/boot/dts/overlays/rpi-sense-overlay.dts
@@ -38,7 +38,7 @@
 			};
 
 			hts221-humid@5f {
-				compatible = "st,hts221-humid";
+				compatible = "st,hts221-humid", "st,hts221";
 				reg = <0x5f>;
 				status = "okay";
 			};
