From 4d4d714061ee6f54dc5feeaeda4389e2346386aa Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 17 Jun 2019 10:06:55 +0100
Subject: [PATCH] arm: dts: Fix Pi4 PWR LED configuration

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2711-rpi-4-b.dts | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm/boot/dts/bcm2711-rpi-4-b.dts
+++ b/arch/arm/boot/dts/bcm2711-rpi-4-b.dts
@@ -126,13 +126,13 @@
 	act_led: act {
 		label = "led0";
 		linux,default-trigger = "mmc0";
-		gpios = <&gpio 42 0>;
+		gpios = <&gpio 42 GPIO_ACTIVE_HIGH>;
 	};
 
 	pwr_led: pwr {
 		label = "led1";
-		linux,default-trigger = "input";
-		gpios = <&expgpio 2 0>;
+		linux,default-trigger = "default-on";
+		gpios = <&expgpio 2 GPIO_ACTIVE_LOW>;
 	};
 };
 
