From 4a09c51bc328b2b83ffa20a6db02ac18139a963d Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Thu, 12 Oct 2017 18:11:32 +0100
Subject: [PATCH] dts: Use fb rather than leds for dpi overlay

---
 arch/arm/boot/dts/overlays/dpi18-overlay.dts | 2 +-
 arch/arm/boot/dts/overlays/dpi24-overlay.dts | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/overlays/dpi18-overlay.dts
+++ b/arch/arm/boot/dts/overlays/dpi18-overlay.dts
@@ -9,7 +9,7 @@
 	// reference on - leds will do
 
 	fragment@0 {
-		target = <&leds>;
+		target = <&fb>;
 		__overlay__ {
 			pinctrl-names = "default";
 			pinctrl-0 = <&dpi18_pins>;
--- a/arch/arm/boot/dts/overlays/dpi24-overlay.dts
+++ b/arch/arm/boot/dts/overlays/dpi24-overlay.dts
@@ -9,7 +9,7 @@
 	// reference on - leds will do
 
 	fragment@0 {
-		target = <&leds>;
+		target = <&fb>;
 		__overlay__ {
 			pinctrl-names = "default";
 			pinctrl-0 = <&dpi24_pins>;
