From 2d35ddcd988499ac7bfd08997086cecfc6b5acb3 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Tue, 7 May 2019 15:00:02 +0100
Subject: [PATCH] drm: vc4: Fixup typo when setting HDMI aspect ratio

Assignment was to the wrong structure.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 drivers/gpu/drm/vc4/vc4_firmware_kms.c | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_firmware_kms.c
+++ b/drivers/gpu/drm/vc4/vc4_firmware_kms.c
@@ -717,19 +717,19 @@ static void vc4_crtc_mode_set_nofb(struc
 	switch (frame.avi.picture_aspect) {
 	default:
 	case HDMI_PICTURE_ASPECT_NONE:
-		mode->flags |= TIMINGS_FLAGS_ASPECT_NONE;
+		mb.timings.flags |= TIMINGS_FLAGS_ASPECT_NONE;
 		break;
 	case HDMI_PICTURE_ASPECT_4_3:
-		mode->flags |= TIMINGS_FLAGS_ASPECT_4_3;
+		mb.timings.flags |= TIMINGS_FLAGS_ASPECT_4_3;
 		break;
 	case HDMI_PICTURE_ASPECT_16_9:
-		mode->flags |= TIMINGS_FLAGS_ASPECT_16_9;
+		mb.timings.flags |= TIMINGS_FLAGS_ASPECT_16_9;
 		break;
 	case HDMI_PICTURE_ASPECT_64_27:
-		mode->flags |= TIMINGS_FLAGS_ASPECT_64_27;
+		mb.timings.flags |= TIMINGS_FLAGS_ASPECT_64_27;
 		break;
 	case HDMI_PICTURE_ASPECT_256_135:
-		mode->flags |= TIMINGS_FLAGS_ASPECT_256_135;
+		mb.timings.flags |= TIMINGS_FLAGS_ASPECT_256_135;
 		break;
 	}
 
