From 8b9843afd665a52df07cc804d6fcb624b22cd85e Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Sun, 17 Jun 2018 13:22:07 +0100
Subject: [PATCH] vc4_firmware_kms: fix build

---
 drivers/gpu/drm/vc4/vc4_firmware_kms.c | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_firmware_kms.c
+++ b/drivers/gpu/drm/vc4/vc4_firmware_kms.c
@@ -33,6 +33,8 @@
 #define SMICS 0x0
 #define SMICS_INTERRUPTS (BIT(9) | BIT(10) | BIT(11))
 
+#define vc4_crtc vc4_kms_crtc
+#define to_vc4_crtc to_vc4_kms_crtc
 struct vc4_crtc {
 	struct drm_crtc base;
 	struct drm_encoder *encoder;
@@ -273,7 +275,7 @@ static int vc4_plane_atomic_check(struct
 
 static void vc4_plane_destroy(struct drm_plane *plane)
 {
-	drm_plane_helper_disable(plane);
+	drm_plane_helper_disable(plane, NULL);
 	drm_plane_cleanup(plane);
 }
 
@@ -591,7 +593,7 @@ static struct drm_connector *vc4_fkms_co
 	connector->interlace_allowed = 0;
 	connector->doublescan_allowed = 0;
 
-	drm_mode_connector_attach_encoder(connector, encoder);
+	drm_connector_attach_encoder(connector, encoder);
 
 	return connector;
 
