From a1905aed89ee45f6662f03b77dc604ff1a169671 Mon Sep 17 00:00:00 2001
From: Stefan Wahren <wahrenst@gmx.net>
Date: Tue, 17 Sep 2019 19:16:17 +0200
Subject: [PATCH] ARM: dts: bcm283x: Define MMC interfaces at board
 level

commit e7774049ff255c8ba72bcee9c7ab307a95e8d7bc upstream.

Starting with RPi 4 this is the first board, which doesn't use sdhost
as default SD interface. So the MMC interfaces should be defined finally at
board level. Since all boards using sdhci already does this, we can drop the
pinctrl part from bcm2835-rpi.dtsi.

Signed-off-by: Stefan Wahren <wahrenst@gmx.net>
Acked-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/bcm2835-rpi-a-plus.dts  |  7 +++++++
 arch/arm/boot/dts/bcm2835-rpi-a.dts       |  7 +++++++
 arch/arm/boot/dts/bcm2835-rpi-b-plus.dts  |  7 +++++++
 arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts  |  7 +++++++
 arch/arm/boot/dts/bcm2835-rpi-b.dts       |  7 +++++++
 arch/arm/boot/dts/bcm2835-rpi-cm1-io1.dts |  7 +++++++
 arch/arm/boot/dts/bcm2835-rpi-zero-w.dts  |  7 +++++++
 arch/arm/boot/dts/bcm2835-rpi-zero.dts    |  7 +++++++
 arch/arm/boot/dts/bcm2835-rpi.dtsi        | 13 -------------
 arch/arm/boot/dts/bcm2836-rpi-2-b.dts     |  7 +++++++
 10 files changed, 63 insertions(+), 13 deletions(-)

--- a/arch/arm/boot/dts/bcm2835-rpi-a-plus.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-a-plus.dts
@@ -108,6 +108,13 @@
 	status = "okay";
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio14>;
--- a/arch/arm/boot/dts/bcm2835-rpi-a.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-a.dts
@@ -103,6 +103,13 @@
 	status = "okay";
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio14>;
--- a/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
@@ -110,6 +110,13 @@
 	status = "okay";
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio14>;
--- a/arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts
@@ -103,6 +103,13 @@
 	status = "okay";
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio14>;
--- a/arch/arm/boot/dts/bcm2835-rpi-b.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b.dts
@@ -98,6 +98,13 @@
 	status = "okay";
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio14>;
--- a/arch/arm/boot/dts/bcm2835-rpi-cm1-io1.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-cm1-io1.dts
@@ -81,6 +81,13 @@
 	hpd-gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio14>;
--- a/arch/arm/boot/dts/bcm2835-rpi-zero-w.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-zero-w.dts
@@ -129,6 +129,13 @@
 	};
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio32 &uart0_ctsrts_gpio30>;
--- a/arch/arm/boot/dts/bcm2835-rpi-zero.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-zero.dts
@@ -105,6 +105,13 @@
 	hpd-gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio14>;
--- a/arch/arm/boot/dts/bcm2835-rpi.dtsi
+++ b/arch/arm/boot/dts/bcm2835-rpi.dtsi
@@ -84,19 +84,6 @@
 	status = "okay";
 };
 
-&sdhci {
-	pinctrl-names = "default";
-	pinctrl-0 = <&emmc_gpio48>;
-	bus-width = <4>;
-};
-
-&sdhost {
-	pinctrl-names = "default";
-	pinctrl-0 = <&sdhost_gpio48>;
-	status = "okay";
-	bus-width = <4>;
-};
-
 &usb {
 	power-domains = <&power RPI_POWER_DOMAIN_USB>;
 };
--- a/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
+++ b/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
@@ -48,6 +48,13 @@
 	status = "okay";
 };
 
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_gpio14>;
