From 7f67e8ed8ae17ddca0748975de0c0efad6a5e6bb Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Tue, 15 Jan 2019 16:32:33 +0000
Subject: [PATCH] staging: bcm2835-camera: Set the field value within
 each buffer

Fixes a v4l2-compliance failure
v4l2-test-buffers.cpp(415): g_field() == V4L2_FIELD_ANY

The driver only ever produces progresive frames, so field should
always be set to V4L2_FIELD_NONE.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 drivers/staging/vc04_services/bcm2835-camera/bcm2835-camera.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/staging/vc04_services/bcm2835-camera/bcm2835-camera.c
+++ b/drivers/staging/vc04_services/bcm2835-camera/bcm2835-camera.c
@@ -443,6 +443,7 @@ static void buffer_cb(struct vchiq_mmal_
 	}
 	dev->capture.last_timestamp = buf->vb.vb2_buf.timestamp;
 	buf->vb.sequence = dev->capture.sequence++;
+	buf->vb.field = V4L2_FIELD_NONE;
 
 	vb2_set_plane_payload(&buf->vb.vb2_buf, 0, mmal_buf->length);
 	if (mmal_buf->mmal_flags & MMAL_BUFFER_HEADER_FLAG_KEYFRAME)
