From 17eaf7c6e8dfcd76b4ed28587b07892e2a5a4ff5 Mon Sep 17 00:00:00 2001
From: Stefan Wahren <stefan.wahren@i2se.com>
Date: Sun, 21 Oct 2018 19:08:29 +0200
Subject: [PATCH] staging: bcm2835-camera: Add hint about possible
 faulty GPU mem config

As per default the GPU memory config of the Raspberry Pi isn't sufficient
for the camera usage. Even worse the bcm2835 camera doesn't provide a
helpful error message in this case. So let's add a hint to point the user
to the likely cause.

Signed-off-by: Stefan Wahren <stefan.wahren@i2se.com>
---
 drivers/staging/vc04_services/bcm2835-camera/mmal-vchiq.c | 5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

--- a/drivers/staging/vc04_services/bcm2835-camera/mmal-vchiq.c
+++ b/drivers/staging/vc04_services/bcm2835-camera/mmal-vchiq.c
@@ -1620,8 +1620,11 @@ int vchiq_mmal_component_init(struct vch
 	component = &instance->component[instance->component_idx];
 
 	ret = create_component(instance, component, name);
-	if (ret < 0)
+	if (ret < 0) {
+		pr_err("%s: failed to create component %d (Not enough GPU mem?)\n",
+		       __func__, ret);
 		goto unlock;
+	}
 
 	/* ports info needs gathering */
 	component->control.type = MMAL_PORT_TYPE_CONTROL;
