From d4aef159394d5940bd7158ab789969dab82f7c76 Mon Sep 17 00:00:00 2001
From: Soeren Moch <smoch@web.de>
Date: Thu, 12 Dec 2019 00:52:49 +0100
Subject: [PATCH 5/7] brcmfmac: add support for BCM4359 SDIO chipset

BCM4359 is a 2x2 802.11 abgn+ac Dual-Band HT80 combo chip and it
supports Real Simultaneous Dual Band feature.

Based on a similar patch by: Wright Feng <wright.feng@cypress.com>

Signed-off-by: Soeren Moch <smoch@web.de>
Acked-by: Chi-Hsien Lin <chi-hsien.lin@cypress.com>
Acked-by: Ulf Hansson <ulf.hansson@linaro.org>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c | 2 ++
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.c   | 1 +
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c   | 2 ++
 include/linux/mmc/sdio_ids.h                              | 2 ++
 4 files changed, 7 insertions(+)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c
@@ -973,8 +973,10 @@ static const struct sdio_device_id brcmf
 	BRCMF_SDIO_DEVICE(SDIO_DEVICE_ID_BROADCOM_43455),
 	BRCMF_SDIO_DEVICE(SDIO_DEVICE_ID_BROADCOM_4354),
 	BRCMF_SDIO_DEVICE(SDIO_DEVICE_ID_BROADCOM_4356),
+	BRCMF_SDIO_DEVICE(SDIO_DEVICE_ID_BROADCOM_4359),
 	BRCMF_SDIO_DEVICE(SDIO_DEVICE_ID_CYPRESS_4373),
 	BRCMF_SDIO_DEVICE(SDIO_DEVICE_ID_CYPRESS_43012),
+	BRCMF_SDIO_DEVICE(SDIO_DEVICE_ID_CYPRESS_89359),
 	{ /* end: all zeroes */ }
 };
 MODULE_DEVICE_TABLE(sdio, brcmf_sdmmc_ids);
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.c
@@ -1408,6 +1408,7 @@ bool brcmf_chip_sr_capable(struct brcmf_
 		addr = CORE_CC_REG(base, sr_control0);
 		reg = chip->ops->read32(chip->ctx, addr);
 		return (reg & CC_SR_CTL0_ENABLE_MASK) != 0;
+	case BRCM_CC_4359_CHIP_ID:
 	case CY_CC_43012_CHIP_ID:
 		addr = CORE_CC_REG(pmu->base, retention_ctl);
 		reg = chip->ops->read32(chip->ctx, addr);
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
@@ -616,6 +616,7 @@ BRCMF_FW_DEF(43455, "brcmfmac43455-sdio"
 BRCMF_FW_DEF(43456, "brcmfmac43456-sdio");
 BRCMF_FW_DEF(4354, "brcmfmac4354-sdio");
 BRCMF_FW_DEF(4356, "brcmfmac4356-sdio");
+BRCMF_FW_DEF(4359, "brcmfmac4359-sdio");
 BRCMF_FW_DEF(4373, "brcmfmac4373-sdio");
 BRCMF_FW_DEF(43012, "brcmfmac43012-sdio");
 
@@ -638,6 +639,7 @@ static const struct brcmf_firmware_mappi
 	BRCMF_FW_ENTRY(BRCM_CC_4345_CHIP_ID, 0xFFFFFDC0, 43455),
 	BRCMF_FW_ENTRY(BRCM_CC_4354_CHIP_ID, 0xFFFFFFFF, 4354),
 	BRCMF_FW_ENTRY(BRCM_CC_4356_CHIP_ID, 0xFFFFFFFF, 4356),
+	BRCMF_FW_ENTRY(BRCM_CC_4359_CHIP_ID, 0xFFFFFFFF, 4359),
 	BRCMF_FW_ENTRY(CY_CC_4373_CHIP_ID, 0xFFFFFFFF, 4373),
 	BRCMF_FW_ENTRY(CY_CC_43012_CHIP_ID, 0xFFFFFFFF, 43012)
 };
--- a/include/linux/mmc/sdio_ids.h
+++ b/include/linux/mmc/sdio_ids.h
@@ -41,8 +41,10 @@
 #define SDIO_DEVICE_ID_BROADCOM_43455		0xa9bf
 #define SDIO_DEVICE_ID_BROADCOM_4354		0x4354
 #define SDIO_DEVICE_ID_BROADCOM_4356		0x4356
+#define SDIO_DEVICE_ID_BROADCOM_4359		0x4359
 #define SDIO_DEVICE_ID_CYPRESS_4373		0x4373
 #define SDIO_DEVICE_ID_CYPRESS_43012		43012
+#define SDIO_DEVICE_ID_CYPRESS_89359		0x4355
 
 #define SDIO_VENDOR_ID_INTEL			0x0089
 #define SDIO_DEVICE_ID_INTEL_IWMC3200WIMAX	0x1402
