From 66808f706b3dcd83a9f5157997ff478a880a2906 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Mon, 30 Apr 2012 09:10:51 +0200
Subject: [PATCH 70/79] MIPS: BCM63XX: Add board definition for D-Link
 DSL-274xB rev F1

---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |  104 +++++++++++++++++++++++++++++
 1 files changed, 104 insertions(+), 0 deletions(-)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -126,6 +126,51 @@ static struct board_info __initdata boar
 		},
 	},
 };
+
+static struct board_info __initdata board_dsl_274xb_f1 = {
+	.name				= "AW4339U",
+	.expected_cpu_id		= 0x6328,
+
+	.has_pci			= 1,
+
+	.has_caldata			= 1,
+	.caldata = {
+		{
+			.vendor		= PCI_VENDOR_ID_ATHEROS,
+			.caldata_offset	= 0x7d1000,
+			.slot		= 0,
+			.led_pin	= -1,
+			.led_active_high	= 1,
+		},
+	},
+
+	.has_enetsw			= 1,
+
+	.enetsw = {
+		.used_ports = {
+			[0] = {
+				.used	= 1,
+				.phy_id = 1,
+				.name	= "Port 4",
+			},
+			[1] = {
+				.used	= 1,
+				.phy_id	= 2,
+				.name	= "Port 3",
+			},
+			[2] = {
+				.used	= 1,
+				.phy_id	= 3,
+				.name	= "Port 2",
+			},
+			[3] = {
+				.used	= 1,
+				.phy_id	= 4,
+				.name	= "Port 1",
+			},
+		},
+	},
+};
 #endif /* CONFIG_BCM63XX_CPU_6328 */
 
 /*
@@ -953,6 +998,7 @@ static const struct board_info __initcon
 #ifdef CONFIG_BCM63XX_CPU_6328
 	&board_96328avng,
 	&board_963281TAN,
+	&board_dsl_274xb_f1,
 #endif
 #ifdef CONFIG_BCM63XX_CPU_6338
 	&board_96338gw,
@@ -1011,6 +1057,7 @@ static struct of_device_id const bcm963x
 #ifdef CONFIG_BCM63XX_CPU_6328
 	{ .compatible = "brcm,bcm963281TAN", .data = &board_963281TAN, },
 	{ .compatible = "brcm,bcm96328avng", .data = &board_96328avng, },
+	{ .compatible = "d-link,dsl-274xb-f", .data = &board_dsl_274xb_f1, },
 #endif
 #ifdef CONFIG_BCM63XX_CPU_6338
 	{ .compatible = "brcm,bcm96338gw", .data = &board_96338gw, },
