From: Robert Marko <robimarko@gmail.com>
To: linux-mtd@lists.infradead.org
Subject: mtd: spi-nor: Add Winbond w25q128jv support
Date: Mon, 25 Jun 2018 13:17:48 +0200

Datasheet:
http://www.winbond.com/resource-files/w25q128jv%20revf%2003272018%20plus.pdf

Testing done on Mikrotik Routerboard  wAP R board.
It does not support Dual or Quad modes.

Signed-off-by: Robert Marko <robimarko@gmail.com>
---

Changes in v2:
	- Correct the title
---
 drivers/mtd/spi-nor/spi-nor.c | 5 +++++
 1 file changed, 5 insertions(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -1152,6 +1152,11 @@ static const struct flash_info spi_nor_i
 			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
 			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
 	},
+	{
+		"w25q128jv", INFO(0xef7018, 0, 64 * 1024, 256,
+			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
+			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
+	},
 	{ "w25q80", INFO(0xef5014, 0, 64 * 1024,  16, SECT_4K) },
 	{ "w25q80bl", INFO(0xef4014, 0, 64 * 1024,  16, SECT_4K) },
 	{ "w25q128", INFO(0xef4018, 0, 64 * 1024, 256, SECT_4K) },
