From ff78cbcd8d7d656a5f43abd2c744e610b8c6c740 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 29 May 2019 13:54:21 +0100
Subject: [PATCH] ARM: dts: Add bcm2711-rpi-4-b.dts and components

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/Makefile            |   1 +
 arch/arm/boot/dts/bcm2711-rpi-4-b.dts | 320 ++++++++++++
 arch/arm/boot/dts/bcm2711.dtsi        |  50 ++
 arch/arm/boot/dts/bcm2838.dtsi        | 724 ++++++++++++++++++++++++++
 4 files changed, 1095 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm2711-rpi-4-b.dts
 create mode 100644 arch/arm/boot/dts/bcm2711.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2838.dtsi

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -8,6 +8,7 @@ dtb-$(CONFIG_ARCH_BCM2835) += \
 	bcm2708-rpi-zero-w.dtb \
 	bcm2709-rpi-2-b.dtb \
 	bcm2710-rpi-3-b.dtb \
+	bcm2711-rpi-4-b.dtb \
 	bcm2710-rpi-3-b-plus.dtb \
 	bcm2710-rpi-cm3.dtb
 
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2711-rpi-4-b.dts
@@ -0,0 +1,320 @@
+/dts-v1/;
+
+#include "bcm2711.dtsi"
+
+/ {
+	compatible = "raspberrypi,4-model-b", "brcm,bcm2838", "brcm,bcm2837";
+	model = "Raspberry Pi 4 Model B";
+	#address-cells = <2>;
+	#size-cells = <1>;
+
+	memory {
+		device_type = "memory";
+		reg = <0x0 0x0 0x0>;
+	};
+
+	chosen {
+		bootargs = "8250.nr_uarts=1 cma=64M";
+	};
+
+	aliases {
+		serial0 = &uart1;
+		serial1 = &uart0;
+		mmc0 = &emmc2;
+		mmc1 = &mmcnr;
+		mmc2 = &sdhost;
+		/delete-property/ ethernet;
+		/delete-property/ intc;
+		ethernet0 = &genet;
+	};
+};
+
+&soc {
+	virtgpio: virtgpio {
+		compatible = "brcm,bcm2835-virtgpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		firmware = <&firmware>;
+		status = "okay";
+	};
+};
+
+&mmcnr {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&firmware {
+	expgpio: expgpio {
+		compatible = "raspberrypi,firmware-gpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		status = "okay";
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins &bt_pins>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>;
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+// =============================================
+// Board specific stuff here
+
+/ {
+
+	sd_io_1v8_reg: sd_io_1v8_reg {
+		status = "okay";
+		compatible = "regulator-gpio";
+		vin-supply = <&vdd_5v0_reg>;
+		regulator-name = "vdd-sd-io";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		regulator-always-on;
+		regulator-settling-time-us = <5000>;
+
+		gpios = <&expgpio 4 GPIO_ACTIVE_HIGH>;
+		states = <1800000 0x1
+			  3300000 0x0>;
+	};
+};
+
+&sdhost {
+	status = "disabled";
+};
+
+&emmc2 {
+	status = "okay";
+	broken-cd;
+	vqmmc-supply = <&sd_io_1v8_reg>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 42 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "input";
+		gpios = <&expgpio 2 0>;
+	};
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+&sdhost_gpio48 {
+	brcm,pins = <22 23 24 25 26 27>;
+	brcm,function = <BCM2835_FSEL_ALT0>;
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi3_pins: spi3_pins {
+		brcm,pins = <1 2 3>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi3_cs_pins: spi3_cs_pins {
+		brcm,pins = <0 24>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi4_pins: spi4_pins {
+		brcm,pins = <5 6 7>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi4_cs_pins: spi4_cs_pins {
+		brcm,pins = <4 25>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi5_pins: spi5_pins {
+		brcm,pins = <13 14 15>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi5_cs_pins: spi5_cs_pins {
+		brcm,pins = <12 26>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi6_pins: spi6_pins {
+		brcm,pins = <19 20 21>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi6_cs_pins: spi6_cs_pins {
+		brcm,pins = <18 27>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+
+	i2c3_pins: i2c3 {
+		brcm,pins = <4 5>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+
+	i2c4_pins: i2c4 {
+		brcm,pins = <8 9>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+
+	i2c5_pins: i2c5 {
+		brcm,pins = <12 13>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+
+	i2c6_pins: i2c6 {
+		brcm,pins = <22 23>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+
+	sdio_pins: sdio_pins {
+		brcm,pins =     <34 35 36 37 38 39>;
+		brcm,function = <BCM2835_FSEL_ALT3>; // alt3 = SD1
+		brcm,pull =     <0 2 2 2 2 2>;
+	};
+
+	bt_pins: bt_pins {
+		brcm,pins = "-"; // non-empty to keep btuart happy, //4 = 0
+				 // to fool pinctrl
+		brcm,function = <0>;
+		brcm,pull = <2>;
+	};
+
+	uart0_pins: uart0_pins {
+		brcm,pins = <32 33>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+		brcm,pull = <0 2>;
+	};
+
+	uart1_pins: uart1_pins {
+		brcm,pins;
+		brcm,function;
+		brcm,pull;
+	};
+
+	uart2_pins: uart2_pins {
+		brcm,pins = <0 1>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart3_pins: uart3_pins {
+		brcm,pins = <4 5>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart4_pins: uart4_pins {
+		brcm,pins = <8 9>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart5_pins: uart5_pins {
+		brcm,pins = <12 13>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <40 41>;
+		brcm,function = <4>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2711.dtsi
@@ -0,0 +1,50 @@
+#include "bcm2838.dtsi"
+#include "bcm270x.dtsi"
+#include "bcm2708-rpi.dtsi"
+
+/ {
+	soc {
+		/delete-node/ mailbox@7e00b840;
+		/delete-node/ v3d@7ec00000;
+	};
+
+	__overrides__ {
+		arm_freq;
+	};
+};
+
+&dma {
+	brcm,dma-channel-mask = <0x7ef5>;
+};
+
+&txp {
+	interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&firmwarekms {
+	interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&smi {
+	interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&mmc {
+	interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&mmcnr {
+	interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&usb {
+	reg = <0x7e980000 0x10000>,
+	      <0x7e00b200 0x200>;
+	interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
+		     <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&gpio {
+	interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>,
+		     <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>;
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2838.dtsi
@@ -0,0 +1,724 @@
+// SPDX-License-Identifier: GPL-2.0
+#include "bcm283x.dtsi"
+
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+#include <dt-bindings/soc/bcm2835-pm.h>
+
+/ {
+	compatible = "brcm,bcm2838", "brcm,bcm2837";
+
+	interrupt-parent = <&gicv2>;
+
+	soc {
+		ranges = <0x7e000000  0x0 0xfe000000  0x01800000>,
+			 <0x7c000000  0x0 0xfc000000  0x02000000>,
+			 <0x40000000  0x0 0xff800000  0x00800000>;
+		/* Emulate a contiguous 30-bit address range for DMA */
+		dma-ranges = <0xc0000000  0x0 0x00000000  0x3c000000>;
+
+		/delete-node/ mailbox@7e00b840;
+		/delete-node/ interrupt-controller@7e00f300;
+
+		local_intc: local_intc@40000000 {
+			compatible = "brcm,bcm2836-l1-intc";
+			reg = <0x40000000 0x100>;
+		};
+
+		gicv2: gic400@40041000 {
+			interrupt-controller;
+			#interrupt-cells = <3>;
+			compatible = "arm,gic-400";
+			reg =	<0x40041000 0x1000>,
+				<0x40042000 0x2000>,
+				<0x40046000 0x2000>,
+				<0x40048000 0x2000>;
+		};
+
+		thermal: thermal@7d5d2200 {
+			compatible = "brcm,avs-tmon-bcm2838";
+			reg = <0x7d5d2200 0x2c>;
+			interrupts = <GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "tmon";
+			clocks = <&clocks BCM2835_CLOCK_TSENS>;
+			#thermal-sensor-cells = <0>;
+			status = "okay";
+		};
+
+		pm: watchdog@7e100000 {
+			reg = <0x7e100000 0x114>,
+			      <0x7e00a000 0x24>,
+			      <0x7ec11000 0x20>;
+		};
+
+		rng@7e104000 {
+			interrupts = <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		uart2: serial@7e201400 {
+			compatible = "brcm,bcm2835-pl011", "arm,pl011", "arm,primecell";
+			reg = <0x7e201400 0x200>;
+			interrupts = <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_UART>,
+				 <&clocks BCM2835_CLOCK_VPU>;
+			clock-names = "uartclk", "apb_pclk";
+			arm,primecell-periphid = <0x00241011>;
+			status = "disabled";
+		};
+
+		uart3: serial@7e201600 {
+			compatible = "brcm,bcm2835-pl011", "arm,pl011", "arm,primecell";
+			reg = <0x7e201600 0x200>;
+			interrupts = <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_UART>,
+				 <&clocks BCM2835_CLOCK_VPU>;
+			clock-names = "uartclk", "apb_pclk";
+			arm,primecell-periphid = <0x00241011>;
+			status = "disabled";
+		};
+
+		uart4: serial@7e201800 {
+			compatible = "brcm,bcm2835-pl011", "arm,pl011", "arm,primecell";
+			reg = <0x7e201800 0x200>;
+			interrupts = <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_UART>,
+				 <&clocks BCM2835_CLOCK_VPU>;
+			clock-names = "uartclk", "apb_pclk";
+			arm,primecell-periphid = <0x00241011>;
+			status = "disabled";
+		};
+
+		uart5: serial@7e201a00 {
+			compatible = "brcm,bcm2835-pl011", "arm,pl011", "arm,primecell";
+			reg = <0x7e201a00 0x200>;
+			interrupts = <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_UART>,
+				 <&clocks BCM2835_CLOCK_VPU>;
+			clock-names = "uartclk", "apb_pclk";
+			arm,primecell-periphid = <0x00241011>;
+			status = "disabled";
+		};
+
+		spi@7e204000 {
+			reg = <0x7e204000 0x0200>;
+			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		spi3: spi@7e204600 {
+			compatible = "brcm,bcm2835-spi";
+			reg = <0x7e204600 0x0200>;
+			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		spi4: spi@7e204800 {
+			compatible = "brcm,bcm2835-spi";
+			reg = <0x7e204800 0x0200>;
+			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		spi5: spi@7e204a00 {
+			compatible = "brcm,bcm2835-spi";
+			reg = <0x7e204a00 0x0200>;
+			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		spi6: spi@7e204c00 {
+			compatible = "brcm,bcm2835-spi";
+			reg = <0x7e204c00 0x0200>;
+			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c3: i2c@7e205600 {
+			compatible = "brcm,bcm2835-i2c";
+			reg = <0x7e205600 0x200>;
+			interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c4: i2c@7e205800 {
+			compatible = "brcm,bcm2835-i2c";
+			reg = <0x7e205800 0x200>;
+			interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c5: i2c@7e205a00 {
+			compatible = "brcm,bcm2835-i2c";
+			reg = <0x7e205a00 0x200>;
+			interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c6: i2c@7e205c00 {
+			compatible = "brcm,bcm2835-i2c";
+			reg = <0x7e205c00 0x200>;
+			interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		pixelvalve@7e206000 {
+			interrupts = <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		pixelvalve@7e207000 {
+			interrupts = <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		emmc2: emmc2@7e340000 {
+			compatible = "brcm,bcm2711-emmc2";
+			status = "okay";
+			interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&clocks BCM2838_CLOCK_EMMC2>;
+			reg = <0x7e340000 0x100>;
+		};
+
+		hvs@7e400000 {
+			interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		pixelvalve@7e807000 {
+			interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
+		};
+	};
+
+	arm-pmu {
+		/*
+		 * N.B. the A72 PMU support only exists in arch/arm64, hence
+		 * the fallback to the A53 version.
+		 */
+		compatible = "arm,cortex-a72-pmu", "arm,cortex-a53-pmu";
+		interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>,
+			<GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>,
+			<GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>,
+			<GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	timer {
+		compatible = "arm,armv7-timer";
+		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) |
+					  IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) |
+					  IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) |
+					  IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) |
+					  IRQ_TYPE_LEVEL_LOW)>;
+		arm,cpu-registers-not-fw-configured;
+		always-on;
+	};
+
+	cpus: cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		enable-method = "brcm,bcm2836-smp"; // for ARM 32-bit
+
+		cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a72";
+			reg = <0>;
+			enable-method = "spin-table";
+			cpu-release-addr = <0x0 0x000000d8>;
+		};
+
+		cpu1: cpu@1 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a72";
+			reg = <1>;
+			enable-method = "spin-table";
+			cpu-release-addr = <0x0 0x000000e0>;
+		};
+
+		cpu2: cpu@2 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a72";
+			reg = <2>;
+			enable-method = "spin-table";
+			cpu-release-addr = <0x0 0x000000e8>;
+		};
+
+		cpu3: cpu@3 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a72";
+			reg = <3>;
+			enable-method = "spin-table";
+			cpu-release-addr = <0x0 0x000000f0>;
+		};
+	};
+
+	v3dbus {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges = <0x7c500000  0x0 0xfc500000  0x03300000>,
+			 <0x40000000  0x0 0xff800000  0x00800000>;
+		dma-ranges = <0x00000000  0x0 0x00000000  0x3c000000>;
+
+		v3d: v3d@7ec04000 {
+			compatible = "brcm,2711-v3d";
+			reg =
+			    <0x7ec00000 0x4000>,
+			    <0x7ec04000 0x4000>;
+			reg-names = "hub", "core0";
+
+			power-domains = <&pm BCM2835_POWER_DOMAIN_GRAFX_V3D>;
+			resets = <&pm BCM2835_RESET_V3D>;
+			clocks = <&clocks BCM2835_CLOCK_V3D>;
+			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
+			status = "okay";
+		};
+	};
+
+	scb: scb {
+		compatible = "simple-bus";
+		#address-cells = <2>;
+		#size-cells = <1>;
+
+		ranges = <0x0 0x7c000000  0x0 0xfc000000  0x03800000>,
+			 <0x0 0x40000000  0x0 0xff800000  0x00800000>,
+			 <0x6 0x00000000  0x6 0x00000000  0x40000000>,
+			 <0x0 0x00000000  0x0 0x00000000  0xfc000000>;
+		dma-ranges = <0x0 0x00000000  0x0 0x00000000  0xfc000000>;
+
+		pcie_0: pcie@7d500000 {
+			reg = <0x0 0x7d500000 0x9310>,
+			      <0x0 0x7e00f300 0x20>;
+			msi-controller;
+			msi-parent = <&pcie_0>;
+			#address-cells = <3>;
+			#interrupt-cells = <1>;
+			#size-cells = <2>;
+			bus-range = <0x0 0x01>;
+			compatible = "brcm,bcm7211-pcie", "brcm,bcm7445-pcie",
+				     "brcm,pci-plat-dev";
+			max-link-speed = <2>;
+			tot-num-pcie = <1>;
+			linux,pci-domain = <0>;
+			interrupts = <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "pcie", "msi";
+			interrupt-map-mask = <0x0 0x0 0x0 0x7>;
+			interrupt-map = <0 0 0 1 &gicv2 GIC_SPI 143
+						IRQ_TYPE_LEVEL_HIGH
+					 0 0 0 2 &gicv2 GIC_SPI 144
+						IRQ_TYPE_LEVEL_HIGH
+					 0 0 0 3 &gicv2 GIC_SPI 145
+						IRQ_TYPE_LEVEL_HIGH
+					 0 0 0 4 &gicv2 GIC_SPI 146
+						IRQ_TYPE_LEVEL_HIGH>;
+
+			/* Map outbound accesses from scb:0x6_00000000-03ffffff
+			 * to pci:0x0_f8000000-fbffffff
+			 */
+			ranges = <0x02000000 0x0 0xf8000000  0x6 0x00000000
+				  0x0 0x04000000>;
+			/* Map inbound accesses from pci:0x0_00000000..ffffffff
+			 * to scb:0x0_00000000-ffffffff
+			 */
+			dma-ranges = <0x02000000 0x0 0x00000000  0x0 0x00000000
+				      0x1 0x00000000>;
+			status = "okay";
+		};
+
+		genet: genet@7d580000 {
+			compatible = "brcm,genet-v5";
+			reg = <0x0 0x7d580000 0x10000>;
+			status = "okay";
+			#address-cells = <0x1>;
+			#size-cells = <0x1>;
+			interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>;
+			phy-handle = <&phy1>;
+			phy-mode = "rgmii";
+			mdio@e14 {
+				#address-cells = <0x0>;
+				#size-cells = <0x1>;
+				compatible = "brcm,genet-mdio-v5";
+				reg = <0xe14 0x8>;
+				reg-names = "mdio";
+				phy1: genet-phy@0 {
+					compatible =
+						"ethernet-phy-ieee802.3-c22";
+					/* No interrupts - use PHY_POLL */
+					max-speed = <1000>;
+					reg = <0x1>;
+				};
+			};
+		};
+
+		xhci: xhci@7e9c0000 {
+			compatible = "generic-xhci";
+			status = "disabled";
+			reg = <0x0 0x7e9c0000 0x100000>;
+			interrupts = <GIC_SPI 176 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		vchiq: mailbox@7e00b840 {
+			compatible = "brcm,bcm2838-vchiq";
+			reg = <0 0x7e00b840 0x3c>;
+			interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		hevc-decoder@7eb00000 {
+			compatible = "raspberrypi,argon-hevc-decoder";
+			reg = <0x0 0x7eb00000 0x10000>;
+			status = "okay";
+		};
+
+		argon-local-intc@7eb10000 {
+			compatible = "raspberrypi,argon-local-intc";
+			reg = <0x0 0x7eb10000 0x1000>;
+			status = "okay";
+			interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		h264-decoder@7eb20000 {
+			compatible = "raspberrypi,argon-h264-decoder";
+			reg = <0x0 0x7eb20000 0x10000>;
+			status = "okay";
+		};
+
+		vp9-decoder@7eb30000 {
+			compatible = "raspberrypi,argon-vp9-decoder";
+			reg = <0x0 0x7eb30000 0x10000>;
+			status = "okay";
+		};
+	};
+};
+
+&clk_osc {
+	clock-frequency = <54000000>;
+};
+
+&clocks {
+	compatible = "brcm,bcm2838-cprman";
+};
+
+&cpu_thermal {
+	coefficients = <(-487)  410040>;
+};
+
+&dsi0 {
+	interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&dsi1 {
+	interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&gpio {
+	gpclk0_gpio49: gpclk0_gpio49 {
+		brcm,pins = <49>;
+		brcm,function = <BCM2835_FSEL_ALT1>;
+		brcm,pull = <BCM2835_PUD_OFF>;
+	};
+	gpclk1_gpio50: gpclk1_gpio50 {
+		brcm,pins = <50>;
+		brcm,function = <BCM2835_FSEL_ALT1>;
+		brcm,pull = <BCM2835_PUD_OFF>;
+	};
+	gpclk2_gpio51: gpclk2_gpio51 {
+		brcm,pins = <51>;
+		brcm,function = <BCM2835_FSEL_ALT1>;
+		brcm,pull = <BCM2835_PUD_OFF>;
+	};
+
+	i2c0_gpio46: i2c0_gpio46 {
+		brcm,pins = <46 47>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+	i2c1_gpio46: i2c1_gpio46 {
+		brcm,pins = <46 47>;
+		brcm,function = <BCM2835_FSEL_ALT1>;
+	};
+	i2c3_gpio2: i2c3_gpio2 {
+		brcm,pins = <2 3>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	i2c3_gpio4: i2c3_gpio4 {
+		brcm,pins = <4 5>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	i2c4_gpio6: i2c4_gpio6 {
+		brcm,pins = <6 7>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	i2c4_gpio8: i2c4_gpio8 {
+		brcm,pins = <8 9>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	i2c5_gpio10: i2c5_gpio10 {
+		brcm,pins = <10 11>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	i2c5_gpio12: i2c5_gpio12 {
+		brcm,pins = <12 13>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	i2c6_gpio0: i2c6_gpio0 {
+		brcm,pins = <0 1>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	i2c6_gpio22: i2c6_gpio22 {
+		brcm,pins = <22 23>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	i2c_slave_gpio8: i2c_slave_gpio8 {
+		brcm,pins = <8 9 10 11>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	jtag_gpio48: jtag_gpio48 {
+		brcm,pins = <48 49 50 51 52 53>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+	};
+
+	mii_gpio28: mii_gpio28 {
+		brcm,pins = <28 29 30 31>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+	};
+	mii_gpio36: mii_gpio36 {
+		brcm,pins = <36 37 38 39>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+
+	pcm_gpio50: pcm_gpio50 {
+		brcm,pins = <50 51 52 53>;
+		brcm,function = <BCM2835_FSEL_ALT2>;
+	};
+
+	pwm0_gpio52: pwm0_gpio52 {
+		brcm,pins = <52>;
+		brcm,function = <BCM2835_FSEL_ALT1>;
+		brcm,pull = <BCM2835_PUD_OFF>;
+	};
+	pwm1_gpio53: pwm1_gpio53 {
+		brcm,pins = <53>;
+		brcm,function = <BCM2835_FSEL_ALT1>;
+		brcm,pull = <BCM2835_PUD_OFF>;
+	};
+
+	/* The following group consists of:
+         *  RGMII_START_STOP
+         *  RGMII_RX_OK
+         */
+	rgmii_gpio35: rgmii_gpio35 {
+		brcm,pins = <35 36>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+	};
+	rgmii_irq_gpio34: rgmii_irq_gpio34 {
+		brcm,pins = <34>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	rgmii_irq_gpio39: rgmii_irq_gpio39 {
+		brcm,pins = <39>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+	};
+	rgmii_mdio_gpio28: rgmii_mdio_gpio28 {
+		brcm,pins = <28 29>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	rgmii_mdio_gpio37: rgmii_mdio_gpio37 {
+		brcm,pins = <37 38>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+	};
+
+	spi0_gpio46: spi0_gpio46 {
+		brcm,pins = <46 47 48 49>;
+		brcm,function = <BCM2835_FSEL_ALT2>;
+	};
+	spi2_gpio46: spi2_gpio46 {
+		brcm,pins = <46 47 48 49 50>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+	};
+	spi3_gpio0: spi3_gpio0 {
+		brcm,pins = <0 1 2 3>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+	spi4_gpio4: spi4_gpio4 {
+		brcm,pins = <4 5 6 7>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+	spi5_gpio12: spi5_gpio12 {
+		brcm,pins = <12 13 14 15>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+	spi6_gpio18: spi6_gpio18 {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	uart2_gpio0: uart2_gpio0 {
+		brcm,pins = <0 1>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <BCM2835_PUD_OFF BCM2835_PUD_UP>;
+	};
+	uart2_ctsrts_gpio2: uart2_ctsrts_gpio2 {
+		brcm,pins = <2 3>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <BCM2835_PUD_UP BCM2835_PUD_OFF>;
+	};
+	uart3_gpio4: uart3_gpio4 {
+		brcm,pins = <4 5>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <BCM2835_PUD_OFF BCM2835_PUD_UP>;
+	};
+	uart3_ctsrts_gpio6: uart3_ctsrts_gpio6 {
+		brcm,pins = <6 7>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <BCM2835_PUD_UP BCM2835_PUD_OFF>;
+	};
+	uart4_gpio8: uart4_gpio8 {
+		brcm,pins = <8 9>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <BCM2835_PUD_OFF BCM2835_PUD_UP>;
+	};
+	uart4_ctsrts_gpio10: uart4_ctsrts_gpio10 {
+		brcm,pins = <10 11>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <BCM2835_PUD_UP BCM2835_PUD_OFF>;
+	};
+	uart5_gpio12: uart5_gpio12 {
+		brcm,pins = <12 13>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <BCM2835_PUD_OFF BCM2835_PUD_UP>;
+	};
+	uart5_ctsrts_gpio14: uart5_ctsrts_gpio14 {
+		brcm,pins = <14 15>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <BCM2835_PUD_UP BCM2835_PUD_OFF>;
+	};
+};
+
+&vec {
+	interrupts = <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&usb {
+	interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&hdmi {
+	interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>,
+		     <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&uart1 {
+	interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&spi1 {
+	interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&spi2 {
+	interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&csi0 {
+	interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&csi1 {
+	interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&sdhci {
+	interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&i2c0 {
+	interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&i2c1 {
+	interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&i2c2 {
+	interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&gpio {
+	interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>,
+		     <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>,
+		     <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>,
+		     <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&mailbox {
+	interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&rng {
+	compatible = "brcm,bcm2838-rng200";
+};
+
+&sdhost {
+	interrupts = <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&uart0 {
+	interrupts = <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&dma {
+	interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>,
+		<GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>,
+		<GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>,
+		<GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>,
+		<GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>,
+		<GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>,
+		<GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>,
+		<GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>, /* dmalite  7 */
+		<GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>, /* dmalite  8 */
+		<GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>, /* dmalite  9 */
+		<GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>, /* dmalite 10 */
+		/* DMA4 - 40 bit DMA engines */
+		<GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>, /* dma4    11 */
+		<GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>, /* dma4    12 */
+		<GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>, /* dma4    13 */
+		<GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>; /* dma4    14 */
+	interrupt-names = "dma0",
+			  "dma1",
+			  "dma2",
+			  "dma3",
+			  "dma4",
+			  "dma5",
+			  "dma6",
+			  "dma7",
+			  "dma8",
+			  "dma9",
+			  "dma10",
+			  "dma11",
+			  "dma12",
+			  "dma13",
+			  "dma14";
+	brcm,dma-channel-mask = <0x7ef5>;
+};
