From 592f7ebf2755acc81cd794b73916f3b2bcccaa68 Mon Sep 17 00:00:00 2001
From: Floris Bos <bos@je-eigen-domein.nl>
Date: Fri, 4 Oct 2019 16:41:30 +0200
Subject: [PATCH] pcie-brcmstb-bounce64.c: dev_err() -> dev_info() for
 info messages

"dmabounce: initialised" is not an error, so do not log it as such.
Prevents screen polution on OS with "quiet" as kernel parameter.

Closes #3266
---
 drivers/pci/controller/pcie-brcmstb-bounce64.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/pci/controller/pcie-brcmstb-bounce64.c
+++ b/drivers/pci/controller/pcie-brcmstb-bounce64.c
@@ -524,7 +524,7 @@ int brcm_pcie_bounce_init(struct device
 
 	g_dmabounce_device_info = device_info;
 
-	dev_err(dev, "dmabounce: initialised - %ld kB, threshold %pad\n",
+	dev_info(dev, "dmabounce: initialised - %ld kB, threshold %pad\n",
 		 buffer_size / 1024, &threshold);
 
 	return 0;
