From f1ab5c7dc1328f0baad2a437a80c792f725c455f Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Thu, 22 Nov 2018 17:28:02 +0000
Subject: [PATCH] media: bcm2835-unicam: Pass through the colorspace on
 try_fmt

The current colorspace was always returned from try_fmt for no
good reason.
Return what the source subdevice returns instead.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 drivers/media/platform/bcm2835/bcm2835-unicam.c | 6 +-----
 1 file changed, 1 insertion(+), 5 deletions(-)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -761,11 +761,7 @@ static int unicam_try_fmt_vid_cap(struct
 		unicam_info(dev, "Sensor trying to send interlaced video - results may be unpredictable\n");
 
 	v4l2_fill_pix_format(&f->fmt.pix, &sd_fmt.format);
-	/*
-	 * Use current colorspace for now, it will get
-	 * updated properly during s_fmt
-	 */
-	f->fmt.pix.colorspace = dev->v_fmt.fmt.pix.colorspace;
+
 	return unicam_calc_format_size_bpl(dev, fmt, f);
 }
 
