From acb69c6600c3df52f0b3610801f3fd44c4392333 Mon Sep 17 00:00:00 2001
Message-Id: <acb69c6600c3df52f0b3610801f3fd44c4392333.1559210220.git.ryder.lee@mediatek.com>
From: Ryder Lee <ryder.lee@mediatek.com>
Date: Wed, 13 Mar 2019 16:42:15 +0800
Subject: [PATCH] arm: dts: mediatek: add basic support for MT7629 SoC

This adds basic support for MT7629 reference board.

Signed-off-by: Ryder Lee <ryder.lee@mediatek.com>
---
 include/dt-bindings/reset/mt7629-resets.h |  71 ++++
 4 files changed, 704 insertions(+)
 create mode 100644 include/dt-bindings/reset/mt7629-resets.h

--- /dev/null
+++ b/include/dt-bindings/reset/mt7629-resets.h
@@ -0,0 +1,71 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2019 MediaTek Inc.
+ */
+
+#ifndef _DT_BINDINGS_RESET_CONTROLLER_MT7629
+#define _DT_BINDINGS_RESET_CONTROLLER_MT7629
+
+/* INFRACFG resets */
+#define MT7629_INFRA_EMI_MPU_RST		0
+#define MT7629_INFRA_UART5_RST			2
+#define MT7629_INFRA_CIRQ_EINT_RST		3
+#define MT7629_INFRA_APXGPT_RST			4
+#define MT7629_INFRA_SCPSYS_RST			5
+#define MT7629_INFRA_KP_RST			6
+#define MT7629_INFRA_SPI1_RST			7
+#define MT7629_INFRA_SPI4_RST			8
+#define MT7629_INFRA_SYSTIMER_RST		9
+#define MT7629_INFRA_IRRX_RST			10
+#define MT7629_INFRA_AO_BUS_RST			16
+#define MT7629_INFRA_EMI_RST			32
+#define MT7629_INFRA_APMIXED_RST		35
+#define MT7629_INFRA_MIPI_RST			36
+#define MT7629_INFRA_TRNG_RST			37
+#define MT7629_INFRA_SYSCIRQ_RST		38
+#define MT7629_INFRA_MIPI_CSI_RST		39
+#define MT7629_INFRA_GCE_FAXI_RST		40
+#define MT7629_INFRA_I2C_SRAM_RST		41
+#define MT7629_INFRA_IOMMU_RST			47
+
+/* PERICFG resets */
+#define MT7629_PERI_UART0_SW_RST		0
+#define MT7629_PERI_UART1_SW_RST		1
+#define MT7629_PERI_UART2_SW_RST		2
+#define MT7629_PERI_BTIF_SW_RST			6
+#define MT7629_PERI_PWN_SW_RST			8
+#define MT7629_PERI_DMA_SW_RST			11
+#define MT7629_PERI_NFI_SW_RST			14
+#define MT7629_PERI_I2C0_SW_RST			22
+#define MT7629_PERI_SPI0_SW_RST			33
+#define MT7629_PERI_SPI1_SW_RST			34
+#define MT7629_PERI_FLASHIF_SW_RST		36
+
+/* PCIe Subsystem resets */
+#define MT7629_PCIE1_CORE_RST			19
+#define MT7629_PCIE1_MMIO_RST			20
+#define MT7629_PCIE1_HRST			21
+#define MT7629_PCIE1_USER_RST			22
+#define MT7629_PCIE1_PIPE_RST			23
+#define MT7629_PCIE0_CORE_RST			27
+#define MT7629_PCIE0_MMIO_RST			28
+#define MT7629_PCIE0_HRST			29
+#define MT7629_PCIE0_USER_RST			30
+#define MT7629_PCIE0_PIPE_RST			31
+
+/* SSUSB Subsystem resets */
+#define MT7629_SSUSB_PHY_PWR_RST		3
+#define MT7629_SSUSB_MAC_PWR_RST		4
+
+/* ETH Subsystem resets */
+#define MT7629_ETHSYS_SYS_RST			0
+#define MT7629_ETHSYS_MCM_RST			2
+#define MT7629_ETHSYS_HSDMA_RST			5
+#define MT7629_ETHSYS_FE_RST			6
+#define MT7629_ETHSYS_ESW_RST			16
+#define MT7629_ETHSYS_GMAC_RST			23
+#define MT7629_ETHSYS_EPHY_RST			24
+#define MT7629_ETHSYS_CRYPTO_RST		29
+#define MT7629_ETHSYS_PPE_RST			31
+
+#endif  /* _DT_BINDINGS_RESET_CONTROLLER_MT7629 */
