From 925b969a16a2e3503803c47a87f093f88d1b2060 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Mon, 3 Dec 2018 13:15:20 +0000
Subject: [PATCH] staging: bcm2835-camera: Unify header inclusion
 defines

Most of the headers use ifndef FOO_H, whilst mmal-parameters.h
used ifndef __FOO_H.

Revise mmal-parameters.h to drop the underscores and make the
headers all consistent.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 .../staging/vc04_services/bcm2835-camera/mmal-parameters.h    | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/staging/vc04_services/bcm2835-camera/mmal-parameters.h
+++ b/drivers/staging/vc04_services/bcm2835-camera/mmal-parameters.h
@@ -19,8 +19,8 @@
  * @{
  */
 
-#ifndef __MMAL_PARAMETERS_H
-#define __MMAL_PARAMETERS_H
+#ifndef MMAL_PARAMETERS_H
+#define MMAL_PARAMETERS_H
 
 /** Common parameter ID group, used with many types of component. */
 #define MMAL_PARAMETER_GROUP_COMMON            (0 << 16)
