From 9f617ce19c5dab429a539d411204ae220b5b8cd6 Mon Sep 17 00:00:00 2001
From: Chunfeng Yun <chunfeng.yun@mediatek.com>
Date: Fri, 13 Oct 2017 16:26:33 +0800
Subject: [PATCH 126/224] usb: xhci-mtk: use dma_set_mask_and_coherent() in
 probe function

This patch uses the simpler dma_set_mask_and_coherent() instead of
doing these as separate steps

Signed-off-by: Chunfeng Yun <chunfeng.yun@mediatek.com>
Acked-by: Mathias Nyman <mathias.nyman@linux.intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/xhci-mtk.c | 7 +------
 1 file changed, 1 insertion(+), 6 deletions(-)

--- a/drivers/usb/host/xhci-mtk.c
+++ b/drivers/usb/host/xhci-mtk.c
@@ -606,15 +606,10 @@ static int xhci_mtk_probe(struct platfor
 	}
 
 	/* Initialize dma_mask and coherent_dma_mask to 32-bits */
-	ret = dma_set_coherent_mask(dev, DMA_BIT_MASK(32));
+	ret = dma_set_mask_and_coherent(dev, DMA_BIT_MASK(32));
 	if (ret)
 		goto disable_clk;
 
-	if (!dev->dma_mask)
-		dev->dma_mask = &dev->coherent_dma_mask;
-	else
-		dma_set_mask(dev, DMA_BIT_MASK(32));
-
 	hcd = usb_create_hcd(driver, dev, dev_name(dev));
 	if (!hcd) {
 		ret = -ENOMEM;
