// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "domywifi,dw33d", "qca,qca9558";
	model = "DomyWifi DW33D";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "blue:system";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		mmc {
			label = "blue:mmc";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port0>;
			linux,default-trigger = "usbport";
		};

		usb {
			label = "blue:usb";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port1>;
			linux,default-trigger = "usbport";
		};

		wlan2g {
			label = "blue:wlan2g";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		internet {
			label = "blue:internet";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0 0 0 0 0>;
	};
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	hub_port0: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&usb_phy1 {
	status = "okay";
};

&usb1 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	hub_port1: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
			};

			partition@50000 {
				label = "oem-firmware";
				reg = <0x50000 0xfa0000>;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "kernel";
			reg = <0x0 0x500000>;
		};

		partition@500000 {
			label = "ubi";
			reg = <0x500000 0x5b00000>;
		};

		partition@6000000 {
			label = "oem-backup";
			reg = <0x6000000 0x2000000>;
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;

		qca,ar8327-initvals = <
			0x04 0x87600000 /* PORT0 PAD MODE CTRL */
			0x0c 0x00080080 /* PORT6 PAD MODE CTRL */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x94 0x0000007e /* PORT6 STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
	pll-data = <0x56000000 0x00000101 0x00001616>;
	phy-handle = <&phy0>;
};

&eth1 {
	status = "okay";

	nvmem-cells = <&macaddr_art_6>;
	nvmem-cell-names = "mac-address";
	pll-data = <0x03000101 0x00000101 0x00001616>;
	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_art_c>;
	nvmem-cell-names = "mac-address";
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};

	macaddr_art_6: macaddr@6 {
		reg = <0x6 0x6>;
	};

	macaddr_art_c: macaddr@c {
		reg = <0xc 0x6>;
	};
};
