// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm63268.dtsi"

/ {
	model = "Comtrend VR-3032u";
	compatible = "comtrend,vr-3032u", "brcm,bcm63168", "brcm,bcm63268";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;

		led-dsl = &led_dsl_green;
		led-internet = &led_internet_green;
		led-usb = &led_usb_green;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio 32 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 33 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};
};

&ehci {
	status = "okay";
};

&ethernet {
	status = "okay";

	nvmem-cells = <&macaddr_cferom_6a0>;
	nvmem-cell-names = "mac-address";
};

&leds {
	status = "okay";

	brcm,serial-leds;
	brcm,serial-dat-low;
	brcm,serial-shift-inv;

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_serial_led>;

	led@0 {
		/* GPHY0 Spd 0 */
		reg = <0>;
		brcm,hardware-controlled;
		brcm,link-signal-sources = <0>;
	};

	led@1 {
		/* GPHY0 Spd 1 */
		reg = <1>;
		brcm,hardware-controlled;
		brcm,link-signal-sources = <1>;
	};

	led@2 {
		reg = <2>;
		active-low;
		label = "red:internet";
	};

	led_dsl_green: led@3 {
		reg = <3>;
		active-low;
		label = "green:dsl";
	};

	led_usb_green: led@4 {
		reg = <4>;
		active-low;
		label = "green:usb";
	};

	led@7 {
		reg = <7>;
		active-low;
		label = "green:wps";
	};

	led_internet_green: led@8 {
		reg = <8>;
		active-low;
		label = "green:internet";
	};

	led@9 {
		/* EPHY0 Act */
		reg = <9>;
		brcm,hardware-controlled;
	};

	led@10 {
		/* EPHY1 Act */
		reg = <10>;
		brcm,hardware-controlled;
	};

	led@11 {
		/* EPHY2 Act */
		reg = <11>;
		brcm,hardware-controlled;
	};

	led@12 {
		/* GPHY0 Act */
		reg = <12>;
		brcm,hardware-controlled;
	};

	led@13 {
		/* EPHY0 Spd */
		reg = <13>;
		brcm,hardware-controlled;
	};

	led@14 {
		/* EPHY1 Spd */
		reg = <14>;
		brcm,hardware-controlled;
	};

	led@15 {
		/* EPHY2 Spd */
		reg = <15>;
		brcm,hardware-controlled;
	};

	led_power_green: led@20 {
		reg = <20>;
		active-low;
		label = "green:power";
	};
};

&nflash {
	status = "okay";

	nandcs@0 {
		compatible = "brcm,nandcs";
		reg = <0>;
		nand-ecc-step-size = <512>;
		nand-ecc-strength = <15>;
		nand-on-flash-bbt;
		brcm,nand-oob-sector-size = <64>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			cferom: partition@0 {
				label = "cferom";
				reg = <0x0000000 0x0020000>;
				read-only;
			};

			partition@20000 {
				compatible = "brcm,wfi-split";
				label = "wfi";
				reg = <0x0020000 0x7ac0000>;
			};
		};
	};
};

&ohci {
	status = "okay";
};

&switch0 {
	ports {
		port@0 {
			reg = <0>;
			label = "lan2";

			phy-handle = <&phy1>;
		};

		port@1 {
			reg = <1>;
			label = "lan3";

			phy-handle = <&phy2>;
		};

		port@2 {
			reg = <2>;
			label = "lan4";

			phy-handle = <&phy3>;
		};

		port@3 {
			reg = <3>;
			label = "lan1";

			phy-handle = <&phy4>;
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};

&cferom {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_cferom_6a0: macaddr@6a0 {
		reg = <0x6a0 0x6>;
	};
};
