From 8c9eef96e24f34ff8b62b230700416b822691a37 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Thu, 1 Apr 2021 14:24:12 +0200
Subject: [PATCH] PCI: aardvark: Remove irq_mask_ack callback for INTx
 interrupts
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Callback for irq_mask_ack is the same as for irq_mask. As there is no
special handling for irq_ack, there is no need to define irq_mask_ack too.

Signed-off-by: Pali Rohár <pali@kernel.org>
Acked-by: Marc Zyngier <maz@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/pci/controller/pci-aardvark.c | 1 -
 1 file changed, 1 deletion(-)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -1422,7 +1422,6 @@ static int advk_pcie_init_irq_domain(str
 	}
 
 	irq_chip->irq_mask = advk_pcie_irq_mask;
-	irq_chip->irq_mask_ack = advk_pcie_irq_mask;
 	irq_chip->irq_unmask = advk_pcie_irq_unmask;
 
 	pcie->irq_domain =
