/* This file is released into the public domain */

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_g {
			label = "green:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		power_r {
			label = "red:power";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		client_g {
			label = "green:client";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};

		client_r {
			label = "red:client";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};

		router_g {
			label = "green:router";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		router_r {
			label = "red:router";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "green:wps";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
		};

		l_arrow {
			label = "blue:leftarrow";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};

		r_arrow {
			label = "blue:rightarrow";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x40000 0x7b0000>;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x10000>;
				read-only;
			};
		};
	};
};

&ethernet {
	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	ralink,mtd-eeprom = <&art 0x1000>;

	nvmem-cells = <&macaddr_art_6>;
	nvmem-cell-names = "mac-address";
};

&state_default {
	default {
		groups = "i2c", "uartf", "spi refclk";
		function = "gpio";
	};
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};

	macaddr_art_6: macaddr@6 {
		reg = <0x6 0x6>;
	};
};
