From adfa8e90db935da2b8bdfa9b8e8a3070f6c05818 Mon Sep 17 00:00:00 2001
From: Jonathan Bell <jonathan@raspberrypi.org>
Date: Wed, 12 Sep 2018 14:44:53 +0100
Subject: [PATCH] bcmgenet: constrain max DMA burst length

---
 drivers/net/ethernet/broadcom/genet/bcmgenet.h | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/broadcom/genet/bcmgenet.h
+++ b/drivers/net/ethernet/broadcom/genet/bcmgenet.h
@@ -29,7 +29,7 @@
 #define ENET_PAD		8
 #define ENET_MAX_MTU_SIZE	(ETH_DATA_LEN + ETH_HLEN + VLAN_HLEN + \
 				 ENET_BRCM_TAG_LEN + ETH_FCS_LEN + ENET_PAD)
-#define DMA_MAX_BURST_LENGTH    0x10
+#define DMA_MAX_BURST_LENGTH    0x08
 
 /* misc. configuration */
 #define MAX_NUM_OF_FS_RULES		16
