#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		label-mac-device = &gmac0;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_22>;
	nvmem-cell-names = "mac-address";
	label = "dsa";
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "eth0";
		};

		port@1 {
			status = "okay";
			label = "eth1";
			nvmem-cells = <&macaddr_factory_22>;
			nvmem-cell-names = "mac-address";
			mac-address-increment = <1>;
		};

		port@2 {
			status = "okay";
			label = "eth2";
			nvmem-cells = <&macaddr_factory_22>;
			nvmem-cell-names = "mac-address";
			mac-address-increment = <2>;
		};

		port@3 {
			status = "okay";
			label = "eth3";
			nvmem-cells = <&macaddr_factory_22>;
			nvmem-cell-names = "mac-address";
			mac-address-increment = <3>;
		};

		port@4 {
			status = "okay";
			label = "eth4";
			nvmem-cells = <&macaddr_factory_22>;
			nvmem-cell-names = "mac-address";
			mac-address-increment = <4>;
		};
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x80000>;
			read-only;
		};

		partition@80000 {
			label = "u-boot-env";
			reg = <0x80000 0x60000>;
			read-only;
		};

		factory: partition@e0000 {
			label = "factory";
			reg = <0xe0000 0x60000>;
		};

		partition@140000 {
			label = "kernel1";
			reg = <0x140000 0x300000>;
		};

		partition@440000 {
			label = "kernel2";
			reg = <0x440000 0x300000>;
		};

		partition@740000 {
			label = "ubi";
			reg = <0x740000 0xf7c0000>;
		};
	};
};

&state_default {
	gpio {
		groups = "uart2", "uart3", "pcie", "jtag";
		function = "gpio";
	};
};

&spi0 {
	/*
	 * This board has 2Mb spi flash soldered in and visible
	 * from manufacturer's firmware.
	 * But this SoC shares spi and nand pins,
	 * and current driver doesn't handle this sharing well
	 */
	status = "disabled";

	flash@1 {
		compatible = "jedec,spi-nor";
		reg = <1>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "spi";
				reg = <0x0 0x200000>;
				read-only;
			};
		};
	};
};

&xhci {
	status = "disabled";
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_22: macaddr@22 {
		reg = <0x22 0x6>;
	};
};
