From 216e8e80057a9f0b6366327881acf88eaf9f1fd4 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Tue, 23 Feb 2021 16:18:51 +0100
Subject: [PATCH 2/2] spi: bcm63xx-hsspi: fix pm_runtime
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The driver sets auto_runtime_pm to true, but it doesn't call
pm_runtime_enable(), which results in "Failed to power device" when PM support
is enabled.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Link: https://lore.kernel.org/r/20210223151851.4110-3-noltari@gmail.com
Signed-off-by: Mark Brown <broonie@kernel.org>
---
 drivers/spi/spi-bcm63xx-hsspi.c | 7 ++++++-
 1 file changed, 6 insertions(+), 1 deletion(-)

--- a/drivers/spi/spi-bcm63xx-hsspi.c
+++ b/drivers/spi/spi-bcm63xx-hsspi.c
@@ -21,6 +21,7 @@
 #include <linux/mutex.h>
 #include <linux/of.h>
 #include <linux/reset.h>
+#include <linux/pm_runtime.h>
 
 #define HSSPI_GLOBAL_CTRL_REG			0x0
 #define GLOBAL_CTRL_CS_POLARITY_SHIFT		0
@@ -439,13 +440,17 @@ static int bcm63xx_hsspi_probe(struct pl
 	if (ret)
 		goto out_put_master;
 
+	pm_runtime_enable(&pdev->dev);
+
 	/* register and we are done */
 	ret = devm_spi_register_master(dev, master);
 	if (ret)
-		goto out_put_master;
+		goto out_pm_disable;
 
 	return 0;
 
+out_pm_disable:
+	pm_runtime_disable(&pdev->dev);
 out_put_master:
 	spi_master_put(master);
 out_disable_pll_clk:
