From 5196c417854942e218a59ec87bf7d414b3bd581e Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@nbd.name>
Date: Thu, 22 Apr 2021 22:20:55 -0700
Subject: [PATCH] net: ethernet: mtk_eth_soc: unmap RX data before calling
 build_skb

Since build_skb accesses the data area (for initializing shinfo), dma unmap
needs to happen before that call

Signed-off-by: Felix Fietkau <nbd@nbd.name>
[Ilya: split build_skb cleanup fix into a separate commit]
Signed-off-by: Ilya Lipnitskiy <ilya.lipnitskiy@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 5 +++--
 1 file changed, 3 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -1334,6 +1334,9 @@ static int mtk_poll_rx(struct napi_struc
 			goto release_desc;
 		}
 
+		dma_unmap_single(eth->dev, trxd.rxd1,
+				 ring->buf_size, DMA_FROM_DEVICE);
+
 		/* receive data */
 		skb = build_skb(data, ring->frag_size);
 		if (unlikely(!skb)) {
@@ -1343,8 +1346,6 @@ static int mtk_poll_rx(struct napi_struc
 		}
 		skb_reserve(skb, NET_SKB_PAD + NET_IP_ALIGN);
 
-		dma_unmap_single(eth->dev, trxd.rxd1,
-				 ring->buf_size, DMA_FROM_DEVICE);
 		pktlen = RX_DMA_GET_PLEN0(trxd.rxd2);
 		skb->dev = netdev;
 		skb_put(skb, pktlen);
