From 2163477b39ed25362d5679d0cf9b843fe2c4bfbb Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Thu, 6 May 2021 17:01:46 +0200
Subject: [PATCH] drm/vc4: crtc: Pass the drm_atomic_state to config_pv

The vc4_crtc_config_pv will need to access the drm_atomic_state
structure and its only parent function, vc4_crtc_atomic_enable already
has access to it. Let's pass it as a parameter.

Fixes: 792c3132bc1b ("drm/vc4: encoder: Add finer-grained encoder callbacks")
Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/vc4_crtc.c | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_crtc.c
+++ b/drivers/gpu/drm/vc4/vc4_crtc.c
@@ -305,7 +305,7 @@ static void vc4_crtc_pixelvalve_reset(st
 	CRTC_WRITE(PV_CONTROL, CRTC_READ(PV_CONTROL) | PV_CONTROL_FIFO_CLR);
 }
 
-static void vc4_crtc_config_pv(struct drm_crtc *crtc)
+static void vc4_crtc_config_pv(struct drm_crtc *crtc, struct drm_atomic_state *state)
 {
 	struct drm_device *dev = crtc->dev;
 	struct vc4_dev *vc4 = to_vc4_dev(dev);
@@ -313,8 +313,8 @@ static void vc4_crtc_config_pv(struct dr
 	struct vc4_encoder *vc4_encoder = to_vc4_encoder(encoder);
 	struct vc4_crtc *vc4_crtc = to_vc4_crtc(crtc);
 	const struct vc4_pv_data *pv_data = vc4_crtc_to_vc4_pv_data(vc4_crtc);
-	struct drm_crtc_state *state = crtc->state;
-	struct drm_display_mode *mode = &state->adjusted_mode;
+	struct drm_crtc_state *crtc_state = crtc->state;
+	struct drm_display_mode *mode = &crtc_state->adjusted_mode;
 	bool interlace = mode->flags & DRM_MODE_FLAG_INTERLACE;
 	u32 pixel_rep = (mode->flags & DRM_MODE_FLAG_DBLCLK) ? 2 : 1;
 	bool is_dsi = (vc4_encoder->type == VC4_ENCODER_TYPE_DSI0 ||
@@ -541,7 +541,7 @@ static void vc4_crtc_atomic_enable(struc
 	if (vc4_encoder->pre_crtc_configure)
 		vc4_encoder->pre_crtc_configure(encoder, state);
 
-	vc4_crtc_config_pv(crtc);
+	vc4_crtc_config_pv(crtc, state);
 
 	CRTC_WRITE(PV_CONTROL, CRTC_READ(PV_CONTROL) | PV_CONTROL_EN);
 
