From 6131e50bfae6adb5ee52ad0d08cf12bfcbf8c606 Mon Sep 17 00:00:00 2001
From: David Plowman <david.plowman@raspberrypi.com>
Date: Tue, 11 May 2021 12:57:22 +0100
Subject: [PATCH] media: i2c: ov5647: Correct minimum VBLANK value

Trial and error reveals that the minimum vblank value appears to be 24
(the OV5647 data sheet does not give any clues). This fixes streaming
lock-ups in full resolution mode.

Fixes: 9b5a5ebedc303 ("media: i2c: ov5647: Add support for V4L2_CID_VBLANK")
Signed-off-by: David Plowman <david.plowman@raspberrypi.com>
---
 drivers/media/i2c/ov5647.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/media/i2c/ov5647.c
+++ b/drivers/media/i2c/ov5647.c
@@ -81,7 +81,7 @@
 #define OV5647_PIXEL_ARRAY_WIDTH	2592U
 #define OV5647_PIXEL_ARRAY_HEIGHT	1944U
 
-#define OV5647_VBLANK_MIN		4
+#define OV5647_VBLANK_MIN		24
 #define OV5647_VTS_MAX			32767
 
 #define OV5647_EXPOSURE_MIN		4
