// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9331_hak5_lan-turtle.dtsi"

/ {
	model = "Hak5 Packet Squirrel";
	compatible = "hak5,packet-squirrel", "qca,ar9331";

	aliases {
		led-boot = &led_system_green;
		led-failsafe = &led_system_green;
		led-running = &led_system_green;
		led-upgrade = &led_system_green;
	};

	leds {
		compatible = "gpio-leds";

		led_system_green: system-green {
			label = "green:system";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		system-blue {
			label = "blue:system";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		system-red {
			label = "red:system";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
	};
};

&keys {
	sw1 {
		label = "sw1";
		linux,code = <BTN_0>;
		gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
		debounce-interval = <60>;
	};

	sw2 {
		label = "sw2";
		linux,code = <BTN_1>;
		gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		debounce-interval = <60>;
	};

	sw3 {
		label = "sw3";
		linux,code = <BTN_2>;
		gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		debounce-interval = <60>;
	};

	sw4 {
		label = "sw4";
		linux,code = <BTN_3>;
		gpios = <&gpio 24 GPIO_ACTIVE_LOW>;
		debounce-interval = <60>;
	};
};
