// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Netgear EX7300 v2";
	compatible = "netgear,ex7300-v2", "qca,qcn5500", "qca,qca9560";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
		label-mac-device = &eth0;
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
		num-chipselects = <0>;

		led_gpio: led_gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <500000>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		led_power_amber: power_amber {
			label = "amber:power";
			gpios = <&led_gpio 7 GPIO_ACTIVE_LOW>;
		};

		wps_green {
			label = "green:wps";
			gpios = <&led_gpio 6 GPIO_ACTIVE_LOW>;
		};

		router_red {
			label = "red:router";
			gpios = <&led_gpio 5 GPIO_ACTIVE_LOW>;
		};

		router_green {
			label = "green:router";
			gpios = <&led_gpio 4 GPIO_ACTIVE_LOW>;
		};

		client_red {
			label = "red:client";
			gpios = <&led_gpio 3 GPIO_ACTIVE_LOW>;
		};

		client_green {
			label = "green:client";
			gpios = <&led_gpio 2 GPIO_ACTIVE_LOW>;
		};

		left_blue {
			label = "blue:left";
			gpios = <&led_gpio 1 GPIO_ACTIVE_LOW>;
		};

		right_blue {
			label = "blue:right";
			gpios = <&led_gpio 0 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		extender_apmode {
			label = "EXTENDER/APMODE switch";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
		};
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0 0 0 0 0>;

		nvmem-cells = <&macaddr_artmtd_c>, <&precal_art_5000>;
		nvmem-cell-names = "mac-address", "pre-calibration";
	};
};

&pll {
	clocks = <&extosc>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				label = "config";
				reg = <0x050000 0x010000>;
			};

			partition@60000 {
				label = "pot";
				reg = <0x060000 0x010000>;
				read-only;
			};

			partition@70000 {
				label = "firmware";
				reg = <0x70000 0xe30000>;
				compatible = "denx,uimage";
			};

			partition@ea0000 {
				label = "rae";
				reg = <0xea0000 0x100000>;
				read-only;
			};

			partition@fa0000 {
				label = "oopsdump";
				reg = <0xfa0000 0x40000>;
				read-only;
			};

			partition@fe0000 {
				label = "artmtd";
				reg = <0xfe0000 0x10000>;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_artmtd_0: macaddr@0 {
					reg = <0x0 0x6>;
				};

				macaddr_artmtd_6: macaddr@6 {
					reg = <0x6 0x6>;
				};

				macaddr_artmtd_c: macaddr@c {
					reg = <0xc 0x6>;
				};
			};

			partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x10000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				cal_art_1000: cal@1000 {
					reg = <0x1000 0x440>;
				};

				precal_art_5000: precal@5000 {
					reg = <0x5000 0x2f20>;
				};
			};
		};
	};
};


&wmac {
	/* Does not work due to lack of QCN5502 support in ath9k. */
	status = "disabled";

	nvmem-cells = <&macaddr_artmtd_6>, <&cal_art_1000>;
	nvmem-cell-names = "mac-address", "calibration";
};

&mdio0 {
	status = "okay";

	phy5: ethernet-phy@5 {
		reg = <5>;
		phy-mode = "sgmii";
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_artmtd_0>;
	nvmem-cell-names = "mac-address";

	phy-handle = <&phy5>;
	phy-mode = "sgmii";

	pll-data = <0x03000000 0x00000101 0x00001313>;
};
