From 23771cfafeedba325b6e9d7dedde11eb25381d67 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Mon, 14 Jun 2021 15:27:24 +0200
Subject: [PATCH] drm/vc4: crtc: Add encoder to vc4_crtc_config_pv
 prototype

vc4_crtc_config_pv() retrieves the encoder again, even though its only
caller, vc4_crtc_atomic_enable(), already did.

Pass the encoder pointer as an argument instead of going through all the
connectors to retrieve it again.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/vc4_crtc.c | 7 +++----
 1 file changed, 3 insertions(+), 4 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_crtc.c
+++ b/drivers/gpu/drm/vc4/vc4_crtc.c
@@ -313,12 +313,11 @@ static void vc4_crtc_pixelvalve_reset(st
 	CRTC_WRITE(PV_CONTROL, CRTC_READ(PV_CONTROL) | PV_CONTROL_FIFO_CLR);
 }
 
-static void vc4_crtc_config_pv(struct drm_crtc *crtc, struct drm_atomic_state *state)
+static void vc4_crtc_config_pv(struct drm_crtc *crtc, struct drm_encoder *encoder,
+			       struct drm_atomic_state *state)
 {
 	struct drm_device *dev = crtc->dev;
 	struct vc4_dev *vc4 = to_vc4_dev(dev);
-	struct drm_encoder *encoder = vc4_get_crtc_encoder(crtc, state,
-							   drm_atomic_get_new_connector_state);
 	struct vc4_encoder *vc4_encoder = to_vc4_encoder(encoder);
 	struct vc4_crtc *vc4_crtc = to_vc4_crtc(crtc);
 	const struct vc4_pv_data *pv_data = vc4_crtc_to_vc4_pv_data(vc4_crtc);
@@ -582,7 +581,7 @@ static void vc4_crtc_atomic_enable(struc
 	if (vc4_encoder->pre_crtc_configure)
 		vc4_encoder->pre_crtc_configure(encoder, state);
 
-	vc4_crtc_config_pv(crtc, state);
+	vc4_crtc_config_pv(crtc, encoder, state);
 
 	CRTC_WRITE(PV_CONTROL, CRTC_READ(PV_CONTROL) | PV_CONTROL_EN);
 
