#!/bin/sh /etc/rc.common
# NVRAM setup
#
# This file handles the NVRAM quirks of various hardware of the bcm47xx target.

START=02
alias debug=${DEBUG:-:}

nvram_default() {
	[ -z "$(nvram get $1)" ] && nvram set "$1=$2"
}

nvram_set() { # for the linksys fixup part
	[ "$(nvram get "$1")" = "$2" -a "$2" != "" ] || {
		COMMIT=1
		/usr/sbin/nvram set "$1=$2"
	}
}

fixup_linksys() {
	# work around braindead CFE defaults in linksys routers
	boardtype=$(nvram get boardtype)
	boardnum=$(nvram get boardnum)
	boardflags=$(($(nvram get boardflags)))
	adm_switch="$(( ($boardflags & 0x80) >> 7 ))"

	[ -n "$(nvram get vxkilled)" ] && boardtype=0 # don't mess with the ram settings on the hacked cfe
	case "$(( $boardtype ))" in
		"1800") #0x708
			if [ "$adm_switch" = 0 ]; then
				nvram_set sdram_init "$(printf 0x%04x $(( $(/usr/sbin/nvram get sdram_init) | 0x0100 )))"
				[ "$COMMIT" = 1 ] && {
					nvram_set clkfreq 216
					nvram_set sdram_ncdl 0x0
					nvram_set pa0itssit 62
					nvram_set pa0b0 0x15eb
					nvram_set pa0b1 0xfa82
					nvram_set pa0b2 0xfe66
					nvram_set pa0maxpwr 0x4e
				}
			fi
		;;
		"1127") #0x467
			nvram_set sdram_init "$(printf 0x%04x $(( $(/usr/sbin/nvram get sdram_init) | 0x0100 )))"
			[ "$COMMIT" = 1 ] && {
				nvram_set sdram_ncdl 0x0
				nvram_set pa0itssit 62
				nvram_set pa0b0 0x168b
				nvram_set pa0b1 0xfabf
				nvram_set pa0b2 0xfeaf
				nvram_set pa0maxpwr 0x4e
			}
		;;
		"1071") #0x042f
			# do sanity check first! max 0x0011 = 128mb
			SDRAM_INIT=$(printf %d $(/usr/sbin/nvram get sdram_init))
			[ "$SDRAM_INIT" -lt "9" -o "$SDRAM_INIT" -gt "17" ] && {
				# set this to default: 0x09 only if value is invaild like 16MB on Asus WL-500GP
				echo "sdram_init is invaild: $(printf 0x%04x $SDRAM_INIT), force to default!"
				nvram_set sdram_init 0x0009
			}
			# on WRT54G3GV2 set flag, so checksum errors of firmware image 2 don't stop the boot process
			noset_try_flag=$(nvram get noset_try_flag)
			[ "$noset_try_flag" = 0 ] && {
				echo "setting noset_try_flag to 1."
				nvram_set noset_try_flag 1
			}
			[ "$COMMIT" = 1 ] && {
				nvram_set sdram_ncdl 0x0
			}
	esac
}

boot() {
	# Don't do any fixups on the WGT634U
	[ "$(cat /proc/diag/model)" = "Netgear WGT634U" ] && return

	fixup_linksys

	# OFDM Power Offset is set incorrectly on many boards.
	# Setting it to 0 will increase the tx power to normal levels.
	nvram_set opo 0x0

	[ "$(nvram get il0macaddr)" = "00:90:4c:5f:00:2a" ] && {
		# if default wifi mac, set two higher than the lan mac
		nvram set il0macaddr=$(nvram get et0macaddr|
		awk '{OFS=FS=":";for(x=7,y=2;--x;){$x=sprintf("%02x",(y+="0x"$x)%256);y/=256}print}')
	}

	[ "$(nvram get et0macaddr)" = "00:90:4c:c0:00:08" ] && {
		# OvisLink WL-1600GL mac workaround
		nvram set et0macaddr=$(hexdump -n 6 -s 130976 -e '5/1 "%02x:" "%02x" ' /dev/mtd/0)
		nvram set il0macaddr=$(nvram get et0macaddr|
		awk '{OFS=FS=":";for(x=7,y=2;--x;){$x=sprintf("%02x",(y+="0x"$x)%256);y/=256}print}')
	}

	[ "$COMMIT" = "1" ] && nvram commit
}
