From ec5be4f79026282925ae383caa431a8d41e3456a Mon Sep 17 00:00:00 2001
From: Tobias Waldekranz <tobias@waldekranz.com>
Date: Sat, 16 Jan 2021 02:25:10 +0100
Subject: [PATCH] net: bridge: switchdev: Include local flag in FDB
 notifications

Some switchdev drivers, notably DSA, ignore all dynamically learned
address notifications (!added_by_user) as these are autonomously added
by the switch. Previously, such a notification was indistinguishable
from a local address notification. Include a local bit in the
notification so that the two classes can be discriminated.

This allows DSA-like devices to add local addresses to the hardware
FDB (with the CPU as the destination), thereby avoiding flows towards
the CPU being flooded by the switch as unknown unicast.

Signed-off-by: Tobias Waldekranz <tobias@waldekranz.com>
---
 include/net/switchdev.h   | 1 +
 net/bridge/br_switchdev.c | 1 +
 2 files changed, 2 insertions(+)

--- a/include/net/switchdev.h
+++ b/include/net/switchdev.h
@@ -226,6 +226,7 @@ struct switchdev_notifier_fdb_info {
 	const unsigned char *addr;
 	u16 vid;
 	u8 added_by_user:1,
+	   local:1,
 	   offloaded:1;
 };
 
--- a/net/bridge/br_switchdev.c
+++ b/net/bridge/br_switchdev.c
@@ -109,6 +109,7 @@ br_switchdev_fdb_notify(const struct net
 		.addr = fdb->key.addr.addr,
 		.vid = fdb->key.vlan_id,
 		.added_by_user = test_bit(BR_FDB_ADDED_BY_USER, &fdb->flags),
+		.local = test_bit(BR_FDB_LOCAL, &fdb->flags),
 		.offloaded = test_bit(BR_FDB_OFFLOADED, &fdb->flags),
 	};
 
