From bc75a1ca95c195508c7d9238a9dc31218ead3ad1 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Thu, 6 May 2021 17:07:07 +0200
Subject: [PATCH] drm/vc4: crtc: Fix vc4_get_crtc_encoder logic

The vc4_get_crtc_encoder function currently only works when the
connector->state->crtc pointer is set, which is only true when the
connector is currently enabled.

However, we use it as part of the disable path as well, and our lookup
will fail in that case, resulting in it returning a null pointer we
can't act on.

We can access the connector that used to be connected to that crtc
though using the old connector state in the disable path.

Since we want to support both the enable and disable path, we can
support it by passing the state accessor variant as a function pointer,
together with the atomic state.

Fixes: 792c3132bc1b ("drm/vc4: encoder: Add finer-grained encoder callbacks")
Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/vc4_crtc.c | 21 ++++++++++++++++-----
 1 file changed, 16 insertions(+), 5 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_crtc.c
+++ b/drivers/gpu/drm/vc4/vc4_crtc.c
@@ -279,14 +279,22 @@ static u32 vc4_crtc_get_fifo_full_level_
  * allows drivers to push pixels to more than one encoder from the
  * same CRTC.
  */
-static struct drm_encoder *vc4_get_crtc_encoder(struct drm_crtc *crtc)
+static struct drm_encoder *vc4_get_crtc_encoder(struct drm_crtc *crtc,
+						struct drm_atomic_state *state,
+						struct drm_connector_state *(*get_state)(struct drm_atomic_state *state,
+											 struct drm_connector *connector))
 {
 	struct drm_connector *connector;
 	struct drm_connector_list_iter conn_iter;
 
 	drm_connector_list_iter_begin(crtc->dev, &conn_iter);
 	drm_for_each_connector_iter(connector, &conn_iter) {
-		if (connector->state->crtc == crtc) {
+		struct drm_connector_state *conn_state = get_state(state, connector);
+
+		if (!conn_state)
+			continue;
+
+		if (conn_state->crtc == crtc) {
 			drm_connector_list_iter_end(&conn_iter);
 			return connector->encoder;
 		}
@@ -309,7 +317,8 @@ static void vc4_crtc_config_pv(struct dr
 {
 	struct drm_device *dev = crtc->dev;
 	struct vc4_dev *vc4 = to_vc4_dev(dev);
-	struct drm_encoder *encoder = vc4_get_crtc_encoder(crtc);
+	struct drm_encoder *encoder = vc4_get_crtc_encoder(crtc, state,
+							   drm_atomic_get_new_connector_state);
 	struct vc4_encoder *vc4_encoder = to_vc4_encoder(encoder);
 	struct vc4_crtc *vc4_crtc = to_vc4_crtc(crtc);
 	const struct vc4_pv_data *pv_data = vc4_crtc_to_vc4_pv_data(vc4_crtc);
@@ -426,7 +435,8 @@ static int vc4_crtc_disable(struct drm_c
 			    struct drm_atomic_state *state,
 			    unsigned int channel)
 {
-	struct drm_encoder *encoder = vc4_get_crtc_encoder(crtc);
+	struct drm_encoder *encoder = vc4_get_crtc_encoder(crtc, state,
+							   drm_atomic_get_old_connector_state);
 	struct vc4_encoder *vc4_encoder = to_vc4_encoder(encoder);
 	struct vc4_crtc *vc4_crtc = to_vc4_crtc(crtc);
 	struct drm_device *dev = crtc->dev;
@@ -526,7 +536,8 @@ static void vc4_crtc_atomic_enable(struc
 {
 	struct drm_device *dev = crtc->dev;
 	struct vc4_crtc *vc4_crtc = to_vc4_crtc(crtc);
-	struct drm_encoder *encoder = vc4_get_crtc_encoder(crtc);
+	struct drm_encoder *encoder = vc4_get_crtc_encoder(crtc, state,
+							   drm_atomic_get_new_connector_state);
 	struct vc4_encoder *vc4_encoder = to_vc4_encoder(encoder);
 
 	require_hvs_enabled(dev);
