From 5567ea58dd5814de7dd1c9756ab985fd0f753bce Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Thu, 13 Feb 2020 17:51:09 +0100
Subject: [PATCH] dt-bindings: clock: Add a binding for the RPi
 Firmware clocks

The firmare running on the RPi VideoCore can be used to discover and
change the various clocks running in the BCM2711. Since devices will
need to use them through the DT, let's add a pretty simple binding.

Cc: Michael Turquette <mturquette@baylibre.com>
Cc: Stephen Boyd <sboyd@kernel.org>
Cc: Rob Herring <robh+dt@kernel.org>
Cc: linux-clk@vger.kernel.org
Cc: devicetree@vger.kernel.org
Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 .../clock/raspberrypi,firmware-clocks.yaml    | 39 +++++++++++++++++++
 1 file changed, 39 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/clock/raspberrypi,firmware-clocks.yaml

--- /dev/null
+++ b/Documentation/devicetree/bindings/clock/raspberrypi,firmware-clocks.yaml
@@ -0,0 +1,39 @@
+# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/clock/raspberrypi,firmware-clocks.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: RaspberryPi Firmware Clocks Device Tree Bindings
+
+maintainers:
+  - Maxime Ripard <mripard@kernel.org>
+
+properties:
+  "#clock-cells":
+    const: 1
+
+  compatible:
+    const: raspberrypi,firmware-clocks
+
+  raspberrypi,firmware:
+    $ref: /schemas/types.yaml#/definitions/phandle
+    description: >
+      Phandle to the mailbox node to communicate with the firmware.
+
+required:
+  - "#clock-cells"
+  - compatible
+  - raspberrypi,firmware
+
+additionalProperties: false
+
+examples:
+  - |
+    firmware_clocks: firmware-clocks {
+        compatible = "raspberrypi,firmware-clocks";
+        raspberrypi,firmware = <&firmware>;
+        #clock-cells = <1>;
+    };
+
+...
